{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["1. 외벽 방수(코킹)공사 설계내역서","2. 내역서","3. 일위대가표(자재비-노임비 등 단가표)"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":35,"defined_names":311,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"1. 외벽 방수(코킹)공사 설계내역서","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[[27,0,27,2],[28,0,28,2],[23,0,23,2],[24,0,24,2],[25,0,25,2],[26,0,26,2],[0,0,0,5],[2,0,2,2],[21,0,21,2],[22,0,22,2]],"flags":["formulas_cached_only"]}
["1. 외벽 방수(코킹)공사 설계내역서"]
[" 공  사  명 [외벽 방수(코킹)공사 ] "]
["비                 목",null,null,"금 액","구    성    비","비         고"]
[null,"재","직  접  재  료  비",0]
["순","료","간  접  재  료  비",0]
[null,"비","작업설.부산물등(-)",0]
[null,null,"[소           계]",0]
["공","노","직  접  노  무  비",0]
[null,"무","간  접  노  무  비",0,"직접노무비의*7%"]
[null,"비","[소           계]",0]
["사",null,"운      반      비",0]
[null,"경","기   계    경   비",0]
[null,null,"산  재  보  험  료",0,"(직노+간노)*3.7%"]
["원",null,"안  전  관  리  비",0,"(재료비+직노)*1.24%"]
[null,null,"고  용  보  험  료",0,"노무비*0.69%"]
[null,null,"건  강  보  험  료"]
[null,null,"연  금  보  험  료"]
[null,null,"퇴 직 공 제 부금비"]
[null,null,"환  경  보  전  비"]
["가","비","기   타    경   비",0,"(재료비+노무비)*5.7%"]
[null,null,"[소           계]",0]
["계",null,null,0]
["일    반    관    리    비",null,null,0,0.055]
["이                      윤",null,null,0,"[노무비+경비+일반관리비]*12%이하"]
["공      급      가      액",null,null,0]
[]
["부    가    가    치    세",null,null,0,"공급가액*10%"]
["도          급          액",null,null,0]

{"sheet":"2. 내역서","index":1,"n_rows":8,"n_cols":13,"rows_kept":8,"cut":false,"hidden":false,"merged":[[1,12,2,12],[1,10,1,11],[1,6,1,7],[3,0,3,12],[0,0,0,12],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,1,5],[1,8,1,9]],"flags":["formulas_cached_only"]}
["2. 내 역 서(실란트)"]
["공         종","규       격","단 위","수 량","자       재       비",null,"노       무       비",null,"경            비",null,"합            계",null,"비고"]
[{"$nulls":4},"단    가","금      액","단    가","금      액","단   가","금     액","단   가","금     액"]
["외벽 방수(코킹)공사"]
["실란트","창호용","M",13433,0,0,0,0]
[null,"석재용","M",10384,0,0,0,0]
[]
["계",{"$nulls":4},0,null,0]

{"sheet":"3. 일위대가표(자재비-노임비 등 단가표)","index":2,"n_rows":12,"n_cols":13,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,10,1,11],[1,6,1,7],[3,0,3,12],[8,0,8,12],[0,0,0,12],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,1,5],[1,8,1,9],[1,12,2,12]],"flags":["formulas_cached_only"]}
["3. 일 위 대 가 표(자재비-노임비 등 단가표)"]
["공         종","규       격","단 위","수 량","자       재       비",null,"노       무       비",null,"경            비",null,"합            계",null,"비   고"]
[{"$nulls":4},"단    가","금      액","단    가","금      액","단   가","금     액","단   가","금     액"]
["1.수밀코킹(m당)-창호용"]
["일액형실리콘","창호용","L",0.12,{"$nulls":8},"물정442"]
[null,"방수공","인",0.018]
["소계"]
[]
["2.수밀코킹(m당)-석재용"]
["일액형실리콘","석재용","L",0.12,{"$nulls":8},"물정442"]
[null,"방수공","인",0.018]
["소계"]