{"text_format":"2","workbook":"xlsx","n_sheets":11,"sheets":["건축집계","건축내역","인테리어집계","인테리어내역","토목내역","조경내역","기계집계","기계내역","소방집계","소방내역","Sheet8"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":5,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"건축집계","index":0,"n_rows":52,"n_cols":20,"rows_kept":52,"cut":false,"hidden":false,"merged":[[2,18,3,18],[2,19,3,19],[2,12,3,12],[2,13,3,13],[2,14,3,14],[2,15,3,15],[2,16,3,16],[2,17,3,17],[0,0,0,12],[1,0,1,12],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,2,5],[2,6,2,7],[2,8,2,9],[2,10,2,11]]}
["공 종 별 집 계 표"]
["[ 국토연구원신청사건립공사 ]"]
["품      명","규      격","단위","수량","재  료  비",null,"노  무  비",null,"경      비",null,"합      계",null,"비  고","공종코드","변수","상위공종","공종구분","공종레벨","공종소계","원가계산서 연결금액"]
[{"$nulls":4},"단  가","금  액","단  가","금  액","단  가","금  액","단  가","금  액"]
["01  국토연구원신청사건립공사","","",1,{"$f":"F6","v":0},{"$f":"E5*D5","v":0},{"$f":"H6","v":0},{"$f":"G5*D5","v":0},{"$f":"J6","v":0},{"$f":"I5*D5","v":0},{"$f":"E5+G5+I5","v":0},0,"","01","","","",1,""]
["0101  ▶ 건축공사","","",1,{"$f":"F7+F8+F9+F10+F11+F12+F13+F14+F15+F16+F17+F18+F19+F20+F21+F22+F23+F24+F25+F26+F27+F28+F29+F30","v":0},0,{"$f":"H7+H8+H9+H10+H11+H12+H13+H14+H15+H16+H17+H18+H19+H20+H21+H22+H23+H24+H25+H26+H27+H28+H29+H30","v":0},0,{"$f":"J7+J8+J9+J10+J11+J12+J13+J14+J15+J16+J17+J18+J19+J20+J21+J22+J23+J24+J25+J26+J27+J28+J29+J30","v":0},0,0,0,"","0101","","01","",2,""]
["010101  공통가설공사","","",1,0,0,0,0,0,0,0,0,"","010101","","0101","",3,""]
["010102  가설공사","","",1,0,0,0,0,0,0,0,0,"","010102","","0101","",3,""]
["010103  철근콘크리트공사","","",1,0,0,0,0,0,0,0,0,"","010103","","0101","",3,""]
["010104  철골공사","","",1,0,0,0,0,0,0,0,0,"","010104","","0101","",3,""]
["010105  데크플레이트공사","","",1,0,0,0,0,0,0,0,0,"","010105","","0101","",3,""]
["010106  조적공사","","",1,0,0,0,0,0,0,0,0,"","010106","","0101","",3,""]
["010107  돌공사","","",1,0,0,0,0,0,0,0,0,"","010107","","0101","",3,""]
["010108  타일공사","","",1,0,0,0,0,0,0,0,0,"","010108","","0101","",3,""]
["010109  목공사","","",1,0,0,0,0,0,0,0,0,"","010109","","0101","",3,""]
["010110  방수공사","","",1,0,0,0,0,0,0,0,0,"","010110","","0101","",3,""]
["010111  지붕및홈통공사","","",1,0,0,0,0,0,0,0,0,"","010111","","0101","",3,""]
["010112  금속공사","","",1,0,0,0,0,0,0,0,0,"","010112","","0101","",3,""]
["010113  미장공사","","",1,0,0,0,0,0,0,0,0,"","010113","","0101","",3,""]
["010114  창호공사","","",1,0,0,0,0,0,0,0,0,"","010114","","0101","",3,""]
["010115  유리공사","","",1,0,0,0,0,0,0,0,0,"","010115","","0101","",3,""]
["010116  도장공사","","",1,0,0,0,0,0,0,0,0,"","010116","","0101","",3,""]
["010117  수장공사","","",1,0,0,0,0,0,0,0,0,"","010117","","0101","",3,""]
["010118  패널공사","","",1,0,0,0,0,0,0,0,0,"","010118","","0101","",3,""]
["010119  기타공사","","",1,0,0,0,0,0,0,0,0,"","010119","","0101","",3,""]
["010120  주요자재비","","",1,0,0,0,0,0,0,0,0,"","010120","","0101","",3,""]
["010121  운반비","","",1,0,0,0,0,0,0,0,0,"","010121","","0101","",3,""]
["010122  작업부산물","","",1,0,0,0,0,0,0,0,0,"","010122","","0101","",3,"<"]
["010123  관급자재비(도급자)","","",1,0,0,0,0,0,0,0,0,"","010123","","0101","",3,""]
["010124  관급자재비(관급자)","","",1,0,0,0,0,0,0,0,0,"","010124","","0101","",3,""]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"F5","v":0},null,{"$f":"H5","v":0},null,{"$f":"J5","v":0},null,{"$f":"L5","v":0}]

{"sheet":"건축내역","index":1,"n_rows":1095,"n_cols":48,"rows_kept":1095,"cut":false,"hidden":false,"merged":[[1,43,2,43],[1,44,2,44],[1,45,2,45],[1,46,2,46],[1,47,2,47],[1,42,2,42],[1,31,2,31],[1,32,2,32],[1,33,2,33],[1,34,2,34],[1,35,2,35],[1,36,2,36],[1,37,2,37],[1,38,2,38],[1,39,2,39],[1,40,2,40],[1,41,2,41],[1,30,2,30],[1,19,2,19],[1,20,2,20],[1,21,2,21],[1,22,2,22],[1,23,2,23],[1,24,2,24],[1,25,2,25],[1,26,2,26],[1,27,2,27],[1,28,2,28],[1,29,2,29],[1,18,2,18],[0,0,0,12],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,1,5],[1,6,1,7],[1,8,1,9],[1,10,1,11],[1,12,2,12],[1,13,2,13],[1,14,2,14],[1,15,2,15],[1,16,2,16],[1,17,2,17]]}
["[ 국토연구원신청사건립공사 ]"]
["품      명","규      격","단위","수량","재  료  비",null,"노  무  비",null,"경      비",null,"합      계",null,"비  고","품목코드","변수","설정","공종코드","일위","단산","자재","손료적용","손료저장","적용율","JUK1","JUK2","JUK3","JUK4","JUK5","JUK6","JUK7","JUK8","JUK9","JUK10","JUK11","JUK12","JUK13","JUK14","JUK15","JUK16","JUK17","JUK18","JUK19","JUK20","자재구분","공종구분","공종레벨","공종+자재","고유번호"]
[{"$nulls":4},"단  가","금  액","단  가","금  액","단  가","금  액","단  가","금  액"]
["010101  공통가설공사",{"$nulls":15},"010101"]
["조립식가설사무소","16개월","M2",180,null,{"$f":"TRUNC(E5*D5, 0)","v":0},null,{"$f":"TRUNC(G5*D5, 0)","v":0},null,{"$f":"TRUNC(I5*D5, 0)","v":0},{"$f":"TRUNC(E5+G5+I5, 0)","v":0},0,null,"502531702A3FE291486A801C23A425","","","010101","T","F","F",{"$nulls":23},"","",null,"010101502531702A3FE291486A801C23A425",838]
["조립식가설창고","16개월","M2",180,null,0,null,0,null,0,0,0,null,"502531702A3FD2F141FE8A638C9BCD","","","010101","T","F","F",{"$nulls":23},"","",null,"010101502531702A3FD2F141FE8A638C9BCD",839]
["조립식가설울타리/E.G.I철판","16개월,H=2.4m","M",350,null,0,null,0,null,0,0,0,null,"5025317019AC6261417AAEE27FEA5B","","","010101","T","F","F",{"$nulls":23},"","",null,"0101015025317019AC6261417AAEE27FEA5B",841]
["조립식가설시험실","16개월","M2",30,null,0,null,0,null,0,0,0,null,"502531702A3FD2F141FE88BA901F9E","","","010101","T","F","F",{"$nulls":23},"","",null,"010101502531702A3FD2F141FE88BA901F9E",840]
["조립식가설방음울타리/R.P.P","16개월,H=6.0m(방음판5m+분진망1m)","M",170,null,0,null,0,null,0,0,0,null,"5025317019AC62614177DB2B4D1F47","","","010101","T","F","F",{"$nulls":23},"","",null,"0101015025317019AC62614177DB2B4D1F47",842]
["조립식가설통용문설치","16개월,6000L*2400H+2400","EA",2,null,0,null,0,null,0,0,0,null,"5025317019AC62614786CED1294F68","","","010101","T","F","F",{"$nulls":23},"","",null,"0101015025317019AC62614786CED1294F68",843]
["타워크레인임대료","10ton","월",10,null,0,null,0,null,0,0,0,null,"502531703410D2C14FC5307CF0710B","","","010101","T","F","F",{"$nulls":23},"","",null,"010101502531703410D2C14FC5307CF0710B",83]
["타워크레인","수직이동","회",1,null,0,null,0,null,0,0,0,null,"502531703410D2C14D168FD7B56B6E","","","010101","T","F","F",{"$nulls":23},"","",null,"010101502531703410D2C14D168FD7B56B6E",84]
["타워크레인","가설 및 해체","대",1,null,0,null,0,null,0,0,0,null,"502531703410D2C14D168FD4E18C4E","","","010101","T","F","F",{"$nulls":23},"","",null,"010101502531703410D2C14D168FD4E18C4E",85]
["타워크레인기초","7*7*1.4m","개소",1,null,0,null,0,null,0,0,0,null,"502531703410D2C14FC5307D912A62","","","010101","T","F","F",{"$nulls":23},"","",null,"010101502531703410D2C14FC5307D912A62",86]
["타워크레인운반비(수송비)","10ton","대",1,null,0,null,0,null,0,0,0,null,"502531703410D2C14FC5307D9B5620","","","010101","T","F","F",{"$nulls":23},"","",null,"010101502531703410D2C14FC5307D9B5620",87]
["인화물용리프트","1톤*45m","개월",10,null,0,null,0,null,0,0,0,null,"5025317034B702E142467E56D19106","","","010101","T","F","F",{"$nulls":23},"","",null,"0101015025317034B702E142467E56D19106",89]
["인화물용리프트타워설치,해체","타워형","M",41,null,0,null,0,null,0,0,0,null,"5025317034D3E2714573F3BF70C4B1","","","010101","T","F","F",{"$nulls":23},"","",null,"0101015025317034D3E2714573F3BF70C4B1",90]
["인화물용리프트타워기초","2*2*0.6m","개소",1,null,0,null,0,null,0,0,0,null,"5025317034D3E2714573F3BF7193C7","","","010101","T","F","F",{"$nulls":23},"","",null,"0101015025317034D3E2714573F3BF7193C7",91]
["자재양중용장비","트럭크레인20톤,150HR/월","개월",1,null,0,null,0,null,0,0,0,null,"502531703410D2C14FC5307D904B78","","","010101","T","F","F",{"$nulls":23},"","",null,"010101502531703410D2C14FC5307D904B78",88]
["축중기설치,해체","3개월,이동식","회",1,null,0,null,0,null,0,0,0,null,"5025317046EBB23148A060B26622FA","","","010101","T","F","F",{"$nulls":23},"","",null,"0101015025317046EBB23148A060B26622FA",158]
["가설전력및용수비","인입및사용요금포함","식",1,null,0,null,0,null,0,0,0,null,"5198C172B06282714E04DB22BCC12F956BDDE5","","","010101","F","F","T",{"$nulls":23},"","",null,"0101015198C172B06282714E04DB22BCC12F956BDDE5",92]
["건설폐기물상차비","15톤덤프트럭기준","톤",620,null,0,null,0,null,0,0,0,null,"5025317046EBA21141996DB3248F31","","","010101","F","F","T",{"$nulls":23},"","",null,"0101015025317046EBA21141996DB3248F31",93]
["<품질시험비>","","",null,null,0,null,0,null,0,0,0,null,"5198C172B06282714E04DB22BCC12F956BDDE6","","","010101","F","F","T",{"$nulls":23},"","",null,"0101015198C172B06282714E04DB22BCC12F956BDDE6",94]
["레미콘","슬럼프","점",134,null,0,null,0,null,0,0,0,null,"5025317046D99291403BE0A7824433","","","010101","T","F","F",{"$nulls":23},"","",null,"0101015025317046D99291403BE0A7824433",919]
["레미콘","압축강도","점",134,null,0,null,0,null,0,0,0,null,"5025317046D99291403BE0A7836A36","","","010101","T","F","F",{"$nulls":23},"","",null,"0101015025317046D99291403BE0A7836A36",920]
["속빈콘크리트블록","치수","조",23,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAEA54F27","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAEA54F27",914]
["속빈콘크리트블록","압축강도","조",23,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAEA5494F","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAEA5494F",915]
["속빈콘크리트블록","흡수율","조",23,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAEA54B9C","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAEA54B9C",916]
["콘크리트벽돌","치수","조",17,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAEA77AFE","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAEA77AFE",886]
["콘크리트벽돌","압축강도","조",17,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAEA4A65F","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAEA4A65F",887]
["콘크리트벽돌","흡수율","조",17,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAEA54DEA","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAEA54DEA",888]
["타일","형상및치수","조",3,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAEAACFD3","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAEAACFD3",889]
["타일","뒤틀림","조",3,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAEABD58E","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAEABD58E",890]
["타일","꺽임강도","조",3,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAF4963DC","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAF4963DC",891]
["타일","흡수율","조",3,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAF485CCA","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAF485CCA",892]
["철근","인장강도","조",22,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAF4B1001","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAF4B1001",893]
["철근","항복강도","조",22,null,0,null,0,null,0,{"$f":"TRUNC(E37+G37+I37, 0)","v":0},0,null,"57A02175D3A7F251479584154783EEAF4B125E","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAF4B125E",917]
["철근","연신율","조",22,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAF4B14AC","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAF4B14AC",918]
["골재","밀도및흡수율","건",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAF4DDE34","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAF4DDE34",895]
["골재","단위중량","건",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAF4C377B","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAF4C377B",896]
["골재","점토덩어리","건",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAF4F8B79","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAF4F8B79",897]
["골재","0.08mm체 통과량","건",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAF4EE5C5","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAF4EE5C5",898]
["골재","마모율","건",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAF412D9C","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAF412D9C",899]
["골재","유기불순물","건",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEACF52425","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEACF52425",901]
["골재","염화물","건",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEACF41D13","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEACF41D13",902]
["시멘트방수재","응결시간","건",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEACF7D1A9","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEACF7D1A9",903]
["시멘트방수재","안정성","건",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEACF6CA87","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEACF6CA87",904]
["시멘트방수재","압축강도비","건",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEACF149F4","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEACF149F4",905]
["시멘트방수재","흡수비","건",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEACF0A27A","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEACF0A27A",906]
["시멘트방수재","투수비","건",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEACF37699","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEACF37699",907]
["발포폴리우레탄,폴리스틸렌","밀도","건",9,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEACF26FF7","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEACF26FF7",908]
["발포폴리우레탄,폴리스틸렌","흡수성","건",9,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEACFD7A4D","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEACFD7A4D",909]
["발포폴리우레탄,폴리스틸렌","연소성","건",9,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEACFC5353","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEACFC5353",910]
["발포폴리우레탄,폴리스틸렌","굽힘강도","건",9,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAD9AE089","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAD9AE089",912]
["발포폴리우레탄,폴리스틸렌","열전도율","건",9,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAD99DADE","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAD99DADE",913]
["지내력시험","평판재하(시외)","회",10,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154783EEAEA3805D","","","010101","F","F","T",{"$nulls":23},"","",null,"01010157A02175D3A7F251479584154783EEAEA3805D",882]
["MOCK-UP TEST","각종","SET",1,null,0,null,0,null,0,0,0,null,"5198C172B06282714E04DB22BCC12F956BDCD8","","","010101","F","F","T",{"$nulls":23},"","",null,"0101015198C172B06282714E04DB22BCC12F956BDCD8",733]
{"$rows_empty":23}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F5:F80)","v":0},null,{"$f":"SUM(H5:H80)","v":0},null,{"$f":"SUM(J5:J80)","v":0},null,{"$f":"SUM(L5:L80)","v":0},null,"TOTAL"]
["010102  가설공사",{"$nulls":15},"010102"]
["수평규준틀","평","개소",30,null,{"$f":"TRUNC(E83*D83, 0)","v":0},null,{"$f":"TRUNC(G83*D83, 0)","v":0},null,{"$f":"TRUNC(I83*D83, 0)","v":0},{"$f":"TRUNC(E83+G83+I83, 0)","v":0},0,null,"50253170198122A14102BF8EC738DF","","","010102","T","F","F",{"$nulls":23},"","",null,"01010250253170198122A14102BF8EC738DF",127]
["수평규준틀","귀","개소",9,null,0,null,0,null,0,0,0,null,"50253170198122A14102BF8D208F58","","","010102","T","F","F",{"$nulls":23},"","",null,"01010250253170198122A14102BF8D208F58",128]
["강관동바리/라멘구조","3개월, 4.2m이하","M2",6601.26,null,0,null,0,null,0,0,0,null,"50253170198112914B39BCC4F54A76","","","010102","T","F","F",{"$nulls":23},"","",null,"01010250253170198112914B39BCC4F54A76",129]
["강관동바리/라멘구조","3개월, 5.0m이하, 1단보강","M2",1134.6199999999999,null,0,null,0,null,0,0,0,null,"50253170198112914B39BCC2C97CF2","","","010102","T","F","F",{"$nulls":23},"","",null,"01010250253170198112914B39BCC2C97CF2",130]
["조립식강관동바리(시스템)","3개월, 10m이하","10공M3",919.2,null,0,null,0,null,0,0,0,null,"50253170198112914A1839FC567ADB","","","010102","T","F","F",{"$nulls":23},"","",null,"01010250253170198112914A1839FC567ADB",844]
["강관틀비계매기/내부공사용","3개월, 30m이하","M2",1807.38,null,0,null,0,null,0,0,0,null,"50253170198122A140793B1B0830F6","","","010102","T","F","F",{"$nulls":23},"","",null,"01010250253170198122A140793B1B0830F6",684]
["강관비계매기","6개월, 30m이하","M2",15080.29,null,0,null,0,null,0,0,0,null,"50253170198122A1407EA030CA68AD","","","010102","T","F","F",{"$nulls":23},"","",null,"01010250253170198122A1407EA030CA68AD",134]
["강관비계다리","6개월","M2",352.08,null,0,null,0,null,0,0,0,null,"50253170198122A1407F4C3CC839DF","","","010102","T","F","F",{"$nulls":23},"","",null,"01010250253170198122A1407F4C3CC839DF",135]
["강관비계안전발판","6개월","M2",360.36,null,0,null,0,null,0,0,0,null,"50253170198122A1407EA384C3D14A","","","010102","T","F","F",{"$nulls":23},"","",null,"01010250253170198122A1407EA384C3D14A",136]
["이동식강관말비계","3개월, 1단(2m)","대",176,null,0,null,0,null,0,0,0,null,"50253170198122A140781C46595633","","","010102","T","F","F",{"$nulls":23},"","",null,"01010250253170198122A140781C46595633",137]
["이동식강관말비계","3개월, 2단(4m)","대",13,null,0,null,0,null,0,0,0,null,"50253170198122A140781C45B2EC62","","","010102","T","F","F",{"$nulls":23},"","",null,"01010250253170198122A140781C45B2EC62",138]
["이동식강관말비계","3개월, 3단(6m)","대",11,null,0,null,0,null,0,0,0,null,"50253170198122A140781C44ABFA2A","","","010102","T","F","F",{"$nulls":23},"","",null,"01010250253170198122A140781C44ABFA2A",139]
["콘크리트보양","살수","M2",25795.87,null,0,null,0,null,0,0,0,null,"5025317046D982814BF746F0D4B362","","","010102","T","F","F",{"$nulls":23},"","",null,"0101025025317046D982814BF746F0D4B362",140]
["석재.타일보양","하드롱지","M2",970.93,null,0,null,0,null,0,0,0,null,"5025317046D982814BF48D413404A8","","","010102","T","F","F",{"$nulls":23},"","",null,"0101025025317046D982814BF48D413404A8",141]
["먹매김","일반(사무소등)","M2",19955.53,null,0,null,0,null,0,0,0,null,"5025317046D98281482325D3EBEF8F","","","010102","T","F","F",{"$nulls":23},"","",null,"0101025025317046D98281482325D3EBEF8F",142]
["건축물현장정리","철근콘크리트조","M2",19955.53,null,0,null,0,null,0,0,0,null,"5025317046EB92014AA33B11C70F3B","","","010102","T","F","F",{"$nulls":23},"","",null,"0101025025317046EB92014AA33B11C70F3B",143]
{"$rows_empty":8}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F83:F106)","v":0},null,{"$f":"SUM(H83:H106)","v":0},null,{"$f":"SUM(J83:J106)","v":0},null,{"$f":"SUM(L83:L106)","v":0},null,"TOTAL"]
["010103  철근콘크리트공사",{"$nulls":15},"010103"]
["레미콘[관급]/철근","25-27-15","M3",2496.13,null,{"$f":"TRUNC(E109*D109, 0)","v":0},null,{"$f":"TRUNC(G109*D109, 0)","v":0},null,{"$f":"TRUNC(I109*D109, 0)","v":0},{"$f":"TRUNC(E109+G109+I109, 0)","v":0},0,"관급별도","57008170BB4512214769AD0C84AD4E27B29487","","","010103","F","F","T",{"$nulls":23},"","",null,"01010357008170BB4512214769AD0C84AD4E27B29487",686]
["레미콘[관급]/철근","25-24-15","M3",8973.58,null,0,null,0,null,0,0,0,"관급별도","57008170BB4512214769AD0C84AD4E27B29486","","","010103","F","F","T",{"$nulls":23},"","",null,"01010357008170BB4512214769AD0C84AD4E27B29486",53]
["레미콘[관급]/철근","25-24-12","M3",5225.04,null,0,null,0,null,0,0,0,"관급별도","57008170BB4512214769AD0C84AD4E27B29485","","","010103","F","F","T",{"$nulls":23},"","",null,"01010357008170BB4512214769AD0C84AD4E27B29485",54]
["레미콘[관급]/무근","25-21-15","M3",2741.96,null,0,null,0,null,0,0,0,"관급별도","57008170BB4512214769AD0C84AD4E27B29483","","","010103","F","F","T",{"$nulls":23},"","",null,"01010357008170BB4512214769AD0C84AD4E27B29483",55]
["레미콘[관급]/버림","25-18-08","M3",367,null,0,null,0,null,0,0,0,"관급별도","57008170BB4512214769AD0C84AD4E27B29482","","","010103","F","F","T",{"$nulls":23},"","",null,"01010357008170BB4512214769AD0C84AD4E27B29482",56]
["철근콘크리트용봉강[관급]","HD-10, SD400","톤",239.541,null,0,null,0,null,0,0,0,"관급별도","57008170BB57621148C5B818B46297948AF465","","","010103","F","F","T",{"$nulls":23},"","",null,"01010357008170BB57621148C5B818B46297948AF465",57]
["철근콘크리트용봉강[관급]","HD-13, SD400","톤",427.32799999999997,null,0,null,0,null,0,0,0,"관급별도","57008170BB57621148C5B818B46297948AF466","","","010103","F","F","T",{"$nulls":23},"","",null,"01010357008170BB57621148C5B818B46297948AF466",58]
["철근콘크리트용봉강[관급]","HD-16, SD400","톤",113.881,null,0,null,0,null,0,0,0,"관급별도","57008170BB57621148C5B818B46297948AF467","","","010103","F","F","T",{"$nulls":23},"","",null,"01010357008170BB57621148C5B818B46297948AF467",59]
["철근콘크리트용봉강[관급]","HD-19, SD400","톤",155.256,null,0,null,0,null,0,0,0,"관급별도","57008170BB57621148C5B818B46297948AF460","","","010103","F","F","T",{"$nulls":23},"","",null,"01010357008170BB57621148C5B818B46297948AF460",60]
["철근콘크리트용봉강[관급]","HD-22, SD500","톤",1031.809,null,0,null,0,null,0,0,0,"관급별도","57008170BB57621148C5B818B46297948AF2B3","","","010103","F","F","T",{"$nulls":23},"","",null,"01010357008170BB57621148C5B818B46297948AF2B3",61]
["철근콘크리트타설/펌프카","슬럼프15cm, 300m3 이상/일, 붐타설","M3",11356.15,null,0,null,0,null,0,0,0,null,"5025617B3515E251405806AD4BCB07","","","010103","T","F","F",{"$nulls":23},"","",null,"0101035025617B3515E251405806AD4BCB07",65]
["철근콘크리트타설/펌프카","슬럼프8∼12cm, 300m3 이상/일, 붐타설","M3",5173.3,null,0,null,0,null,0,0,0,null,"5025617B3515E251405806AD4CD235","","","010103","T","F","F",{"$nulls":23},"","",null,"0101035025617B3515E251405806AD4CD235",66]
["무근콘크리트타설/펌프카","슬럼프15cm, 300m3 이상/일, 붐타설","M3",2688.2,null,0,null,0,null,0,0,0,null,"5025617B3526524141094E4115117D","","","010103","T","F","F",{"$nulls":23},"","",null,"0101035025617B3526524141094E4115117D",68]
["무근콘크리트타설/펌프카","슬럼프8∼12cm, 300m3 이상/일, 붐타설","M3",362.74,null,0,null,0,null,0,0,0,null,"5025617B3526524141094E411A9268","","","010103","T","F","F",{"$nulls":23},"","",null,"0101035025617B3526524141094E411A9268",67]
["철근현장가공조립","보통, 10톤이상","톤",1910.5,null,0,null,0,null,0,0,0,null,"5025617B7CE132E14211AE250BC3EA","","","010103","T","F","F",{"$nulls":23},"","",null,"0101035025617B7CE132E14211AE250BC3EA",69]
["합판거푸집","3회","M2",5030.25,null,0,null,0,null,0,0,0,null,"5025617B478682314AA3168C9707D4","","","010103","T","F","F",{"$nulls":23},"","",null,"0101035025617B478682314AA3168C9707D4",70]
["유로폼","벽","M2",46174.81,null,0,null,0,null,0,0,0,null,"5025617B47EF020141A65C2CA99CC4","","","010103","T","F","F",{"$nulls":23},"","",null,"0101035025617B47EF020141A65C2CA99CC4",71]
["노출콘크리트거푸집","벽,합판+코팅합판,면처리,메움","M2",737.68,null,0,null,0,null,0,0,0,null,"50255174F4A142D14C56C3013C21DC","","","010103","T","F","F",{"$nulls":23},"","",null,"01010350255174F4A142D14C56C3013C21DC",845]
["섬유보강재투입","친수성","M3",2407.85,null,0,null,0,null,0,0,0,null,"5025617A7A7E42714F8E59F624D0AC","","","010103","T","F","F",{"$nulls":23},"","",null,"0101035025617A7A7E42714F8E59F624D0AC",856]
["지수판설치","수팽창성지수재(시공조인트)","M",624.79,null,0,null,0,null,0,0,0,null,"5025617BD52DF2A14588F9DE0A0766","","","010103","T","F","F",{"$nulls":23},"","",null,"0101035025617BD52DF2A14588F9DE0A0766",73]
["방습필름설치(바닥)","0.1mm, 1겹","M2",14778.33,null,0,null,0,null,0,0,0,null,"5025D17006E9E2B1443BF853F6416B","","","010103","T","F","F",{"$nulls":23},"","",null,"0101035025D17006E9E2B1443BF853F6416B",75]
["콘크리트연석","300*150, 안전페인트","M",86.24,null,0,null,0,null,0,0,0,null,"5025617B352622814A86A69AED29AA","","","010103","T","F","F",{"$nulls":23},"","",null,"0101035025617B352622814A86A69AED29AA",76]
[]
[]
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F109:F132)","v":0},null,{"$f":"SUM(H109:H132)","v":0},null,{"$f":"SUM(J109:J132)","v":0},null,{"$f":"SUM(L109:L132)","v":0},null,"TOTAL"]
["010104  철골공사",{"$nulls":15},"010104"]
["H빔","SM400A, 200*200*8.0*12.0mm","톤",1.5860000000000001,null,{"$f":"TRUNC(E135*D135, 0)","v":0},null,{"$f":"TRUNC(G135*D135, 0)","v":0},null,{"$f":"TRUNC(I135*D135, 0)","v":0},{"$f":"TRUNC(E135+G135+I135, 0)","v":0},0,"","57008170BB57621149EBB0E6B4E5B7149F015C","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB57621149EBB0E6B4E5B7149F015C",794]
["H빔","SM400A, 250*125*6.0*9.0mm","톤",0.59499999999999997,null,0,null,0,null,0,0,0,"","57008170BB57621149EBB0E6B4E5B7149F0C6F","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB57621149EBB0E6B4E5B7149F0C6F",795]
["H빔","SM400A, 350*175*7.0*11.0mm","톤",0.83799999999999997,null,0,null,0,null,0,0,0,"","57008170BB57621149EBB0E6B4E5B7149F0309","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB57621149EBB0E6B4E5B7149F0309",796]
["H빔","SM400A, 600*200*11.0*17.0mm","톤",4.2569999999999997,null,0,null,0,null,0,0,0,"","57008170BB57621149EBB0E6B4E5B7149F0D05","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB57621149EBB0E6B4E5B7149F0D05",797]
["H빔","SM400A, 800*300*14.0*26.0mm","톤",8.4350000000000005,null,0,null,0,null,0,0,0,"","57008170BB57621149EBB0E6B4E5B714909F42","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB57621149EBB0E6B4E5B714909F42",798]
["H빔","SM490A, 350*175*7.0*11.0mm","톤",8.0239999999999991,null,0,null,0,null,0,0,0,"","57008170BB57621149EBB0E6B4E5B7149E7F0D","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB57621149EBB0E6B4E5B7149E7F0D",775]
["철강채널","150*75*6.5*10mm","톤",0.214,null,0,null,0,null,0,0,0,"","57008170BB5762114617127C2AB276DF29B4D3","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5762114617127C2AB276DF29B4D3",776]
["철강채널","250*90*9.0*13mm","톤",3.258,null,0,null,0,null,0,0,0,"","57008170BB5762114617127C2AB276DF29B4D6","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5762114617127C2AB276DF29B4D6",777]
["일반구조용탄소강관","STK400, Φ139.8*4.0mm","M",14.7,null,0,null,0,null,0,0,0,"","577B717798B7B24143C5BC74FC9AB3DFBF01D6","","","010104","F","F","T",{"$nulls":23},"","",null,"010104577B717798B7B24143C5BC74FC9AB3DFBF01D6",778]
["일반구조용탄소강관","STK400, Φ165.2*7.0mm","M",232.26,null,0,null,0,null,0,0,0,"","577B717798B7B24143C5BC74FC9AB3DFBF00C9","","","010104","F","F","T",{"$nulls":23},"","",null,"010104577B717798B7B24143C5BC74FC9AB3DFBF00C9",779]
["일반구조용탄소강관","STK400, Φ216.5*8.0mm","M",72.87,null,0,null,0,null,0,0,0,"","577B717798B7B24143C5BC74FC9AB3DFBF02FA","","","010104","F","F","T",{"$nulls":23},"","",null,"010104577B717798B7B24143C5BC74FC9AB3DFBF02FA",780]
["일반구조용각형강관","SPSR400,ㅁ-50*50*2.3mm","M",133.97999999999999,null,0,null,0,null,0,0,0,"","577B717798B7B24143C5BC74FC9AB3DFB24F68","","","010104","F","F","T",{"$nulls":23},"","",null,"010104577B717798B7B24143C5BC74FC9AB3DFB24F68",963]
["일반구조용각형강관","SPSR400,ㅁ-150*80*6.0mm","M",37.49,null,0,null,0,null,0,0,0,"","577B717798B7B24143C5BC74FC9AB3DFB24F69","","","010104","F","F","T",{"$nulls":23},"","",null,"010104577B717798B7B24143C5BC74FC9AB3DFB24F69",782]
["일반구조용각형강관","SPSR400,ㅁ-200*200*6.0mm","M",103.74,null,0,null,0,null,0,0,0,"","577B717798B7B24143C5BC74FC9AB3DFB35653","","","010104","F","F","T",{"$nulls":23},"","",null,"010104577B717798B7B24143C5BC74FC9AB3DFB35653",781]
["철근콘크리트용봉강[관급]","HD-22, SD500","톤",6.0999999999999999E-2,null,0,null,0,null,0,0,0,"관급별도","57008170BB57621148C5B818B46297948AF2B3","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB57621148C5B818B46297948AF2B3",783]
["용접구조용압연강판","SM400A, 4.5mm","톤",2.6179999999999999,null,0,null,0,null,0,0,0,"","57008170BB5752714AB7676DD6E6BDB0F49A92","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5752714AB7676DD6E6BDB0F49A92",964]
["용접구조용압연강판","SM400A, 6.0mm","톤",0.23799999999999999,null,0,null,0,null,0,0,0,"","57008170BB5752714AB7676DD6E6BDB0F49519","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5752714AB7676DD6E6BDB0F49519",799]
["용접구조용압연강판","SM400A, 7.0mm","톤",1.4999999999999999E-2,null,0,null,0,null,0,0,0,"","57008170BB5752714AB7676DD6E6BDB0F4951B","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5752714AB7676DD6E6BDB0F4951B",800]
["용접구조용압연강판","SM400A, 8.0mm","톤",0.29299999999999998,null,0,null,0,null,0,0,0,"","57008170BB5752714AB7676DD6E6BDB0F4951D","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5752714AB7676DD6E6BDB0F4951D",801]
["용접구조용압연강판","SM400A, 9.0mm","톤",0.13700000000000001,null,0,null,0,null,0,0,0,"","57008170BB5752714AB7676DD6E6BDB0F4951F","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5752714AB7676DD6E6BDB0F4951F",802]
["용접구조용압연강판","SM400A, 12.0mm","톤",0.90200000000000002,null,0,null,0,null,0,0,0,"","57008170BB5752714AB7676DD6E6BDB0F49511","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5752714AB7676DD6E6BDB0F49511",803]
["용접구조용압연강판","SM400A, 13.0mm","톤",0.16900000000000001,null,0,null,0,null,0,0,0,"","57008170BB5752714AB7676DD6E6BDB0F49472","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5752714AB7676DD6E6BDB0F49472",804]
["용접구조용압연강판","SM400A, 15.0mm","톤",0.498,null,0,null,0,null,0,0,0,"","57008170BB5752714AB7676DD6E6BDB0F49470","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5752714AB7676DD6E6BDB0F49470",805]
["용접구조용압연강판","SM400A, 20.0mm","톤",1.0820000000000001,null,0,null,0,null,0,0,0,"","57008170BB5752714AB7676DD6E6BDB0F49476","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5752714AB7676DD6E6BDB0F49476",806]
["용접구조용압연강판","SM400A, 22.0mm","톤",0.61299999999999999,null,0,null,0,null,0,0,0,"","57008170BB5752714AB7676DD6E6BDB0F49474","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5752714AB7676DD6E6BDB0F49474",807]
["용접구조용압연강판","SM400A, 25.0mm","톤",1.847,null,0,null,0,null,0,0,0,"","57008170BB5752714AB7676DD6E6BDB0F4947A","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5752714AB7676DD6E6BDB0F4947A",808]
["용접구조용압연강판","SM490A, 9.0mm","톤",1.2789999999999999,null,0,null,0,null,0,0,0,"","57008170BB5752714AB7676DD6E6BDB0F5A441","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5752714AB7676DD6E6BDB0F5A441",809]
["용접구조용압연강판","SM490A, 15.0mm","톤",0.34899999999999998,null,0,null,0,null,0,0,0,"","57008170BB5752714AB7676DD6E6BDB0F5A443","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5752714AB7676DD6E6BDB0F5A443",810]
["용접구조용압연강판","SM490A, 35.0mm","톤",7.24,null,0,null,0,null,0,0,0,"","57008170BB5752714AB7676DD6E6BDB0F5A445","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5752714AB7676DD6E6BDB0F5A445",811]
["용접구조용압연강판","SM490A, 40.0mm","톤",51.746000000000002,null,0,null,0,null,0,0,0,"","57008170BB5752714AB7676DD6E6BDB0F5A447","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB5752714AB7676DD6E6BDB0F5A447",812]
["철골가공조립(Rolled)","100톤~300톤미만","톤",103.181,null,0,null,0,null,0,0,0,null,"502571798FEEF2E1468800CA652CFA","","","010104","T","F","F",{"$nulls":23},"","",null,"010104502571798FEEF2E1468800CA652CFA",832]
["강판용접(Rolled)","100톤~200톤미만, 20m미만/톤","톤",103.181,null,0,null,0,null,0,0,0,null,"50257179E015220146C42540FBA9D4","","","010104","T","F","F",{"$nulls":23},"","",null,"01010450257179E015220146C42540FBA9D4",833]
["철골세우기(6층미만)","80톤~150톤미만","톤",103.181,null,0,null,0,null,0,{"$f":"TRUNC(E167+G167+I167, 0)","v":0},0,null,"50257179E0A4E241410FAF1B5D45B7","","","010104","T","F","F",{"$nulls":23},"","",null,"01010450257179E0A4E241410FAF1B5D45B7",834]
["고장력볼트 본조임","300톤미만, 20본/미만","톤",103.181,null,0,null,0,null,0,0,0,null,"50257179E0152201441799B9A6C26F","","","010104","T","F","F",{"$nulls":23},"","",null,"01010450257179E0152201441799B9A6C26F",928]
["고장력볼트","F10T, M20*55mm","조",399,null,0,null,0,null,0,0,0,null,"570091710FC262E1494749BB580E5C43951B3C","","","010104","F","F","T",{"$nulls":23},"","",null,"010104570091710FC262E1494749BB580E5C43951B3C",813]
["고장력볼트","F10T, M20*60mm","조",16,null,0,null,0,null,0,0,0,"","570091710FC262E1494749BB580E5C43951B3B","","","010104","F","F","T",{"$nulls":23},"","",null,"010104570091710FC262E1494749BB580E5C43951B3B",814]
["고장력볼트","F10T, M20*65mm","조",181,null,0,null,0,null,0,0,0,"","570091710FC262E1494749BB580E5C43951B3A","","","010104","F","F","T",{"$nulls":23},"","",null,"010104570091710FC262E1494749BB580E5C43951B3A",823]
["고장력볼트","F10T, M20*80mm","조",131,null,0,null,0,null,0,0,0,"","570091710FC262E1494749BB580E5C43951B37","","","010104","F","F","T",{"$nulls":23},"","",null,"010104570091710FC262E1494749BB580E5C43951B37",816]
["고장력볼트","F10T, M22*80mm","조",74,null,0,null,0,null,0,0,0,"","570091710FC262E1494749BB580E5C4395186D","","","010104","F","F","T",{"$nulls":23},"","",null,"010104570091710FC262E1494749BB580E5C4395186D",820]
["고장력볼트","F10T, M22*110mm","조",263,null,0,null,0,null,0,0,0,"","570091710FC262E1494749BB580E5C43951746","","","010104","F","F","T",{"$nulls":23},"","",null,"010104570091710FC262E1494749BB580E5C43951746",821]
["고장력볼트","F10T, M24*125mm","조",86,null,0,null,0,null,0,0,0,null,"570091710FC262E1494749BB580E5C43962791","","","010104","F","F","T",{"$nulls":23},"","",null,"010104570091710FC262E1494749BB580E5C43962791",822]
["스터드볼트설치/자동용접","M19*110","개소",352,null,0,null,0,null,0,0,0,null,"50257179986462614B0C85F3A73749","","","010104","T","F","F",{"$nulls":23},"","",null,"01010450257179986462614B0C85F3A73749",824]
["스터드볼트설치/자동용접","M19*150","개소",96,null,0,null,0,null,0,0,0,null,"50257179986462614B0C85F3A7357C","","","010104","T","F","F",{"$nulls":23},"","",null,"01010450257179986462614B0C85F3A7357C",825]
["스터드볼트설치/자동용접","M19*200","개소",156,null,0,null,0,null,0,0,0,null,"5025717998646261495E2928B732F5","","","010104","T","F","F",{"$nulls":23},"","",null,"0101045025717998646261495E2928B732F5",826]
["스터드볼트설치/자동용접","M22*200","개소",272,null,0,null,0,null,0,0,0,null,"5025717998646261495E2928B5048A","","","010104","T","F","F",{"$nulls":23},"","",null,"0101045025717998646261495E2928B5048A",827]
["앵커볼트","앵커볼트, M16*600mm","개",88,null,0,null,0,null,0,0,0,null,"570091710FC262E14946A2CD0C117B8A8117F4","","","010104","F","F","T",{"$nulls":23},"","",null,"010104570091710FC262E14946A2CD0C117B8A8117F4",828]
["앵커볼트","앵커볼트, M20*700mm","개",124,null,0,null,0,null,0,0,0,null,"570091710FC262E1494749BB580E5C439470D3","","","010104","F","F","T",{"$nulls":23},"","",null,"010104570091710FC262E1494749BB580E5C439470D3",829]
["앵커볼트설치","Ø16∼19mm, 주기둥","개",84,null,0,null,0,null,0,0,0,null,"5025717998647271427F83023333E7","","","010104","T","F","F",{"$nulls":23},"","",null,"0101045025717998647271427F83023333E7",989]
["앵커볼트설치","Ø22∼25mm, 주기둥","개",119,null,0,null,0,null,0,0,0,null,"5025717998647271427F82639E1312","","","010104","T","F","F",{"$nulls":23},"","",null,"0101045025717998647271427F82639E1312",149]
["방진고무패드깔기","25mm","M2",0.99,null,0,null,0,null,0,0,0,null,"5025D170799F12214F6508FDC0A20F","","","010104","T","F","F",{"$nulls":23},"","",null,"0101045025D170799F12214F6508FDC0A20F",955]
["기둥밑무수축고름모르타르","무수축그라우트","M3",0.21099999999999999,null,0,null,0,null,0,0,0,null,"50257179E01532214B217984BFFC43","","","010104","T","F","F",{"$nulls":23},"","",null,"01010450257179E01532214B217984BFFC43",153]
["녹막이페인트(뿜칠)","광명단프라이머, 30㎛","M2",861.53,null,0,null,0,null,0,0,0,null,"5025C171CE7312D14741F04789ADD0","","","010104","T","F","F",{"$nulls":23},"","",null,"0101045025C171CE7312D14741F04789ADD0",155]
["녹막이페인트(뿜칠)","무기질아연말프라이머,75㎛","M2",580.4,null,0,null,0,null,0,0,0,null,"5025C171CE7312D14741F04FDE7C5A","","","010104","T","F","F",{"$nulls":23},"","",null,"0101045025C171CE7312D14741F04FDE7C5A",156]
["내화피복재","2시간, 23mm","M2",822.02,null,0,null,0,null,0,0,0,null,"57008170BB19D2714DB7083DD960C6FEFCE233","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457008170BB19D2714DB7083DD960C6FEFCE233",154]
["유성페인트(뿜칠)","철재면, 2회. 1급","M2",39.51,null,0,null,0,null,0,0,0,null,"5025C171FBD5F2B1429816D21D9A02","","","010104","T","F","F",{"$nulls":23},"","",null,"0101045025C171FBD5F2B1429816D21D9A02",965]
["우레탄페인트(뿜칠)","철재면 3회","M2",580.4,null,0,null,0,null,0,0,0,null,"5025C171913952D14B049E081F6C21","","","010104","T","F","F",{"$nulls":23},"","",null,"0101045025C171913952D14B049E081F6C21",769]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F135:F210)","v":0},null,{"$f":"SUM(H135:H210)","v":0},null,{"$f":"SUM(J135:J210)","v":0},null,{"$f":"SUM(L135:L210)","v":0},null,"TOTAL"]
["010105  데크플레이트공사",{"$nulls":15},"010105"]
["덱플레이트[관급]","ED1A-5, 상부근1-D10/하부근2-D7/래티스Φ5","M2",1379.55,null,{"$f":"TRUNC(E213*D213, 0)","v":0},null,{"$f":"TRUNC(G213*D213, 0)","v":0},null,{"$f":"TRUNC(I213*D213, 0)","v":0},{"$f":"TRUNC(E213+G213+I213, 0)","v":0},0,"관급별도","57008170BBCAF2D1496E3A8A2716C069024E1E","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C069024E1E",176]
["덱플레이트[관급]","ED1A-6, 상부근1-D10/하부근2-D7/래티스Φ6","M2",43.89,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C0690080AA","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C0690080AA",177]
["덱플레이트[관급]","ED3-5, 상부근1-D13/하부근2-D8/래티스Φ5","M2",436.88,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C069073050","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C069073050",178]
["덱플레이트[관급]","ED3-6, 상부근1-D13/하부근2-D8/래티스Φ6","M2",102.41,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C06906294F","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C06906294F",179]
["덱플레이트[관급]","ED4-5, 상부근1-D13/하부근2-D10/래티스Φ5","M2",5549.66,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C069050255","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C069050255",180]
["덱플레이트[관급]","ED4-6, 상부근1-D13/하부근2-D10/래티스Φ6","M2",1005.31,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C069047B23","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C069047B23",181]
["덱플레이트[관급]","ED5-6, 상부근1-D13/하부근2-D13/래티스Φ6","M2",1254.6199999999999,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C0690A845E","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C0690A845E",183]
["덱플레이트[관급]","ND1A-5, 상부근1-D10/하부근2-D7/래티스Φ5","M2",591.53,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C1068BF6B3","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C1068BF6B3",508]
["덱플레이트[관급]","ND1A-6, 상부근1-D10/하부근2-D7/래티스Φ6","M2",479.45,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C1068822D5","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C1068822D5",509]
["덱플레이트[관급]","ND3-5, 상부근1-D13/하부근2-D8/래티스Φ5","M2",660.68,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C1022ED956","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C1022ED956",510]
["덱플레이트[관급]","ND3-6, 상부근1-D13/하부근2-D8/래티스Φ6","M2",759.07,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C1022D329D","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C1022D329D",511]
["덱플레이트[관급]","ND4-5, 상부근1-D13/하부근2-D10/래티스Φ5","M2",1122.31,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C10337F8A2","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C10337F8A2",512]
["덱플레이트[관급]","ND4-6, 상부근1-D13/하부근2-D10/래티스Φ6","M2",624.11,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C1033424C4","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C1033424C4",513]
["덱플레이트[관급]","ND5-5, 상부근1-D13/하부근2-D13/래티스Φ5","M2",1413.02,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C1006045E4","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C1006045E4",514]
["덱플레이트[관급]","ND5-6, 상부근1-D13/하부근2-D13/래티스Φ6","M2",1553.94,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C100631A79","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C100631A79",515]
["덱플레이트/압출법보온판[관급]","비중0.035,100mm","M2",1323.7,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C1006273EF","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C1006273EF",871]
["덱플레이트/압출법보온판[관급]","비중0.035,150mm","M2",1620.52,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C10065C7ED","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C10065C7ED",872]
["덱플레이트/압출법보온판[관급]","비중0.035,180mm","M2",4643.1499999999996,null,0,null,0,null,0,0,0,"관급별도","57008170BBCAF2D1496E3A8A2716C100642014","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BBCAF2D1496E3A8A2716C100642014",873]
["데크플레이트설치","자재별도","M2",16168.03,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCC555E0297A60D","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557A02175D3A7D2A149393C1BCC555E0297A60D",870]
["데크플레이트/CON'C STOPPER","PL-2.3t","KG",475,null,0,null,0,null,0,0,0,null,"50257179D623F2F143C92AAB2B452F","","","010105","T","F","F",{"$nulls":23},"","",null,"01010550257179D623F2F143C92AAB2B452F",161]
["데크플레이트/ANGLE","L-50*50*6","KG",34,null,0,null,0,null,0,0,0,null,"50257179D623F2F143C92AAB2C6B22","","","010105","T","F","F",{"$nulls":23},"","",null,"01010550257179D623F2F143C92AAB2C6B22",162]
["데크플레이트/FLAT BAR","FB-50*6","KG",150,null,0,null,0,null,0,0,0,null,"50257179D623F2F143C92AAB2D7233","","","010105","T","F","F",{"$nulls":23},"","",null,"01010550257179D623F2F143C92AAB2D7233",163]
["데크플레이트/STUD BOLT","M19×200","개소",2951,null,0,null,0,null,0,0,0,null,"50257179D623F2F143C92AAA039465","","","010105","T","F","F",{"$nulls":23},"","",null,"01010550257179D623F2F143C92AAA039465",165]
["철근콘크리트용봉강[관급]","HD-10, SD400","톤",62.771999999999998,null,0,null,0,null,0,0,0,null,"57008170BB57621148C5B818B46297948AF465","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BB57621148C5B818B46297948AF465",166]
["철근콘크리트용봉강[관급]","HD-13, SD400","톤",50.902999999999999,null,0,null,0,null,0,0,0,null,"57008170BB57621148C5B818B46297948AF466","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BB57621148C5B818B46297948AF466",167]
["철근콘크리트용봉강[관급]","HD-16, SD400","톤",6.64,null,0,null,0,null,0,0,0,null,"57008170BB57621148C5B818B46297948AF467","","","010105","F","F","T",{"$nulls":23},"","",null,"01010557008170BB57621148C5B818B46297948AF467",690]
["철근현장가공조립","보통, 10톤이상","톤",116.81100000000001,null,0,null,0,null,0,0,0,null,"5025617B7CE132E14211AE250BC3EA","","","010105","T","F","F",{"$nulls":23},"","",null,"0101055025617B7CE132E14211AE250BC3EA",159]
{"$rows_empty":23}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F213:F262)","v":0},null,{"$f":"SUM(H213:H262)","v":0},null,{"$f":"SUM(J213:J262)","v":0},null,{"$f":"SUM(L213:L262)","v":0},null,"TOTAL"]
["010106  조적공사",{"$nulls":15},"010106"]
["콘크리트벽돌[관급]","190*90*57mm","매",517187,null,{"$f":"TRUNC(E265*D265, 0)","v":0},null,{"$f":"TRUNC(G265*D265, 0)","v":0},null,{"$f":"TRUNC(I265*D265, 0)","v":0},{"$f":"TRUNC(E265+G265+I265, 0)","v":0},0,"관급별도","57008170BB61F2B140D00864F3530B747C739F","","","010106","F","F","T",{"$nulls":23},"","",null,"01010657008170BB61F2B140D00864F3530B747C739F",185]
["0.5B 시멘트벽돌 쌓기","3.6m 이하, 1층소운반","M2",60.33,null,0,null,0,null,0,0,0,null,"50254176646CA2B14F7B443FCEFBB6","","","010106","T","F","F",{"$nulls":23},"","",null,"01010650254176646CA2B14F7B443FCEFBB6",200]
["0.5B 시멘트벽돌 쌓기","3.6m 이하, 2층소운반","M2",60.49,null,0,null,0,null,0,0,0,null,"50254176646CA2B14F7B47F3B374AF","","","010106","T","F","F",{"$nulls":23},"","",null,"01010650254176646CA2B14F7B47F3B374AF",201]
["0.5B 시멘트벽돌 쌓기","3.6m 이하, 리프트소운반","M2",498.9,null,0,null,0,null,0,0,0,null,"50254176646CA2B14F7B46EC422476","","","010106","T","F","F",{"$nulls":23},"","",null,"01010650254176646CA2B14F7B46EC422476",202]
["1.0B 시멘트벽돌 쌓기","3.6m 이하, 1층소운반","M2",915.16,null,0,null,0,null,0,0,0,null,"50254176646CA2B14D49EE74BE0868","","","010106","T","F","F",{"$nulls":23},"","",null,"01010650254176646CA2B14D49EE74BE0868",197]
["1.0B 시멘트벽돌 쌓기","3.6m 이하, 2층소운반","M2",390.92,null,0,null,0,null,0,0,0,null,"50254176646CA2B14D49ED6D4D3893","","","010106","T","F","F",{"$nulls":23},"","",null,"01010650254176646CA2B14D49ED6D4D3893",198]
["1.0B 시멘트벽돌 쌓기","3.6m 이하, 리프트소운반","M2",1687.74,null,0,null,0,null,0,0,0,null,"50254176646CA2B14D49EC46A3D64D","","","010106","T","F","F",{"$nulls":23},"","",null,"01010650254176646CA2B14D49EC46A3D64D",199]
["속빈콘크리트블록[관급]","100×190×390mm","개",3335,null,0,null,0,null,0,0,0,"관급별도","57008170BB61F2B143A4E8E95BDD303A33749F","","","010106","F","F","T",{"$nulls":23},"","",null,"01010657008170BB61F2B143A4E8E95BDD303A33749F",186]
["속빈콘크리트블록[관급]","150×190×390mm","개",5763,null,0,null,0,null,0,0,0,"관급별도","57008170BB61F2B143A4E8E95BDD303A3377C4","","","010106","F","F","T",{"$nulls":23},"","",null,"01010657008170BB61F2B143A4E8E95BDD303A3377C4",187]
["속빈콘크리트블록[관급]","190×190×390mm","개",60197,null,0,null,0,null,0,0,0,"관급별도","57008170BB61F2B143A4E8E95BDD303A3376ED","","","010106","F","F","T",{"$nulls":23},"","",null,"01010657008170BB61F2B143A4E8E95BDD303A3376ED",188]
["4인치 블록보강쌓기(사춤1종)","100*190*390(철근,철망포함)","M2",256.51,null,0,null,0,null,0,0,0,null,"502541765A10C2514D647363CA637A","","","010106","T","F","F",{"$nulls":23},"","",null,"010106502541765A10C2514D647363CA637A",203]
["6인치 블록보강쌓기(사춤1종)","150*190*390(철근,철망포함)","M2",443.25,null,0,null,0,null,0,0,0,null,"502541765A10C2514E0DAB877D12F8","","","010106","T","F","F",{"$nulls":23},"","",null,"010106502541765A10C2514E0DAB877D12F8",204]
["8인치 블록보강쌓기(사춤1종)","190*190*390(철근,철망포함)","M2",4630.53,null,0,null,0,null,0,0,0,null,"502541765A10C2514E0EB2F84DAC63","","","010106","T","F","F",{"$nulls":23},"","",null,"010106502541765A10C2514E0EB2F84DAC63",205]
["철근콘크리트인방","200*200mm","M",143.9,null,0,null,0,null,0,0,0,null,"502541775CD3E2114F4B5E2E479E06","","","010106","T","F","F",{"$nulls":23},"","",null,"010106502541775CD3E2114F4B5E2E479E06",691]
["철근콘크리트인방","200*400mm","M",94.88,null,0,null,0,null,0,0,0,null,"502541775CD3E2114F4B5F338AD381","","","010106","T","F","F",{"$nulls":23},"","",null,"010106502541775CD3E2114F4B5F338AD381",208]
["콘크리트방수턱","100*100mm","M",245.71,null,0,null,0,null,0,0,0,null,"502541775C8BD2E14BF430F4AD49D2","","","010106","T","F","F",{"$nulls":23},"","",null,"010106502541775C8BD2E14BF430F4AD49D2",209]
["콘크리트방수턱","100*200mm","M",14.61,null,0,null,0,null,0,0,0,null,"502541775C8BD2E14BF430F4AE50C0","","","010106","T","F","F",{"$nulls":23},"","",null,"010106502541775C8BD2E14BF430F4AE50C0",210]
["콘크리트방수턱","150*200mm","M",66.06,null,0,null,0,null,0,0,0,null,"502541775C8BD2E14BF430F1DAF140","","","010106","T","F","F",{"$nulls":23},"","",null,"010106502541775C8BD2E14BF430F1DAF140",211]
["콘크리트방수턱","150*300mm","M",143.80000000000001,null,0,null,0,null,0,0,0,null,"502541775C8BD2E14BF430F1DB98F6","","","010106","T","F","F",{"$nulls":23},"","",null,"010106502541775C8BD2E14BF430F1DB98F6",212]
["콘크리트방수턱","200*100mm","M",521.04,null,0,null,0,null,0,0,0,null,"502541775C8BD2E14BF43348EAE377","","","010106","T","F","F",{"$nulls":23},"","",null,"010106502541775C8BD2E14BF43348EAE377",213]
["콘크리트방수턱","200*200mm","M",434.51,null,0,null,0,null,0,0,0,null,"502541775C8BD2E14BF43348E9DC59","","","010106","T","F","F",{"$nulls":23},"","",null,"010106502541775C8BD2E14BF43348E9DC59",214]
["콘크리트방수턱","200*300mm","M",237.9,null,0,null,0,null,0,0,0,null,"502541775C8BD2E14BF43348E83590","","","010106","T","F","F",{"$nulls":23},"","",null,"010106502541775C8BD2E14BF43348E83590",215]
["PVC통기구","Ø10,L:150","EA",144,null,0,null,0,null,0,0,0,null,"5025917EDC37C2714F8439A9F007EE","","","010106","T","F","F",{"$nulls":23},"","",null,"0101065025917EDC37C2714F8439A9F007EE",216]
["PVC통수관","Ø50,L:500","EA",72,null,0,null,0,null,0,0,0,null,"5025917EDC37C2714F8439A9F234F3","","","010106","T","F","F",{"$nulls":23},"","",null,"0101065025917EDC37C2714F8439A9F234F3",217]
["PVC통수관","Ø75,L:500","EA",10,null,0,null,0,null,0,0,0,null,"5025917EDC37C2714F8439A9F58E6A","","","010106","T","F","F",{"$nulls":23},"","",null,"0101065025917EDC37C2714F8439A9F58E6A",692]
["PVC슬리브","Ø100,L:1000","EA",44,null,0,null,0,null,0,0,0,null,"5025917EDC37C2714F8439A9F4E25E","","","010106","T","F","F",{"$nulls":23},"","",null,"0101065025917EDC37C2714F8439A9F4E25E",693]
["SST슬리브","Ø50,L:250","EA",3,null,0,null,0,null,0,0,0,null,"5025917EDC37C2714F8439A9F4E7D0","","","010106","T","F","F",{"$nulls":23},"","",null,"0101065025917EDC37C2714F8439A9F4E7D0",218]
["SST슬리브","Ø50,L:500","EA",9,null,0,null,0,null,0,0,0,null,"5025917EDC37C2714F8439A9F7B6FD","","","010106","T","F","F",{"$nulls":23},"","",null,"0101065025917EDC37C2714F8439A9F7B6FD",219]
{"$rows_empty":22}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F265:F314)","v":0},null,{"$f":"SUM(H265:H314)","v":0},null,{"$f":"SUM(J265:J314)","v":0},null,{"$f":"SUM(L265:L314)","v":0},null,"TOTAL"]
["010107  돌공사",{"$nulls":15},"010107"]
["자연석판석[관급]","수마, 30mm, 고흥석","M2",9.24,null,{"$f":"TRUNC(E317*D317, 0)","v":0},null,{"$f":"TRUNC(G317*D317, 0)","v":0},null,{"$f":"TRUNC(I317*D317, 0)","v":0},{"$f":"TRUNC(E317+G317+I317, 0)","v":0},0,"관급별도","57008170BB61F2B141F717B3F9CC1D14261BD1","","","010107","F","F","T",{"$nulls":23},"","",null,"01010757008170BB61F2B141F717B3F9CC1D14261BD1",861]
["자연석판석[관급]","버너, 30mm, 고흥석","M2",3087.34,null,0,null,0,null,0,0,0,"관급별도","57008170BB61F2B141F717B3F9CC1D14272095","","","010107","F","F","T",{"$nulls":23},"","",null,"01010757008170BB61F2B141F717B3F9CC1D14272095",221]
["자연석판석[관급]","잔다듬, 30mm, 고흥석","M2",4977.24,null,0,null,0,null,0,0,0,"관급별도","57008170BB61F2B141F717B3F9CC1D1428C677","","","010107","F","F","T",{"$nulls":23},"","",null,"01010757008170BB61F2B141F717B3F9CC1D1428C677",223]
["자연석판석[관급]","혼드, 30mm, 거창석","M2",914.5,null,0,null,0,null,0,0,0,"관급별도","57008170BB61F2B141F717B3F9CC1D15C193C3","","","010107","F","F","T",{"$nulls":23},"","",null,"01010757008170BB61F2B141F717B3F9CC1D15C193C3",222]
["자연석판석[관급]","잔다듬, 30mm, 거창석","M2",2091.94,null,0,null,0,null,0,0,0,"관급별도","57008170BB61F2B141F717B3F9CC1D15CF71C0","","","010107","F","F","T",{"$nulls":23},"","",null,"01010757008170BB61F2B141F717B3F9CC1D15CF71C0",224]
["화강석붙임(잔다듬,패턴시공)","바닥, 거창석 30mm, 모르타르 30mm","M2",35.82,null,0,null,0,null,0,0,0,null,"5025F175381DB2E14BDB95F4607023","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F175381DB2E14BDB95F4607023",959]
["화강석붙임(혼드,건식,패턴시공)","벽, 거창석 30mm","M2",831.36,null,0,null,0,null,0,0,0,null,"5025F1753838127140858EABE5192B","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F1753838127140858EABE5192B",847]
["화강석붙임(버너,건식,패턴시공)","벽, 고흥석 30mm","M2",2507.9299999999998,null,0,null,0,null,0,0,0,null,"5025F1753838127140858EA70A8E2B","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F1753838127140858EA70A8E2B",259]
["화강석붙임(잔다듬,건식,패턴시공)","벽, 거창석 30mm","M2",1749.69,null,0,null,0,null,0,0,0,null,"5025F175383832314E18BE89127B79","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F175383832314E18BE89127B79",261]
["화강석붙임(잔다듬,건식,패턴시공)","벽, 고흥석 30mm","M2",4418.63,null,0,null,0,null,0,0,0,null,"5025F175383832314E18B2DCE41C0A","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F175383832314E18B2DCE41C0A",262]
["화강석붙임(버너,TRUSS건식,패턴시공)","벽, 고흥석 30mm, 트러스포함","M2",22.91,null,0,null,0,null,0,0,0,null,"5025F175384AE2A142CA4496339580","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F175384AE2A142CA4496339580",235]
["화강석붙임(잔다듬,TRUSS건식,패턴시공)","벽, 고흥석 30mm, 트러스포함","M2",82.16,null,0,null,0,null,0,0,0,null,"5025F175384AF24149B436AE399C85","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F175384AF24149B436AE399C85",857]
["화강석걸레받이(잔다듬)","고흥석, 100*30mm, 건식","M",166.14,null,0,null,0,null,0,0,0,null,"5025F175385B724143048E14930F3D","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F175385B724143048E14930F3D",694]
["화강석두겁돌(버너)","고흥석, 400*30mm, 모르타르 30mm","M",490.67,null,0,null,0,null,0,0,0,null,"5025F175385B22C143F7DF3E186D13","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F175385B22C143F7DF3E186D13",246]
["화강석두겁돌(버너)","고흥석, 450*30mm, 모르타르 30mm","M",41.8,null,0,null,0,null,0,0,0,null,"5025F175385B22C143F7DF3D7390A7","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F175385B22C143F7DF3D7390A7",247]
["화강석두겁돌(버너)","고흥석, 500*30mm, 모르타르 30mm","M",9.6,null,0,null,0,null,0,0,0,null,"5025F175385B22C143F7DF3D70DC7E","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F175385B22C143F7DF3D70DC7E",859]
["화강석두겁돌(버너)","고흥석, 550*30mm, 모르타르 30mm","M",101.74,null,0,null,0,null,0,0,0,null,"5025F175385B22C143F7DF3D71E36C","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F175385B22C143F7DF3D71E36C",858]
["화강석두겁돌(잔다듬)","고흥석, 400*30mm, 모르타르 30mm","M",18.399999999999999,null,0,null,0,null,0,0,0,null,"5025F175385B22C143F7DF3C6B9859","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F175385B22C143F7DF3C6B9859",862]
["화강석두겁돌(잔다듬)","거창석, 400*30mm, 모르타르 30mm","M",290.63,null,0,null,0,null,0,0,0,null,"5025F175385B22C143F7DF3C6AF1D3","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F175385B22C143F7DF3C6AF1D3",248]
["화강석소변기턱(수마)","고흥석, 150*30mm, 모르타르 30mm","M",56,null,0,null,0,null,0,0,0,null,"5025F175385B22C145A765668E7876","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F175385B22C145A765668E7876",860]
["석재논슬립홈파기","5*5,계단3선","M",473.8,null,0,null,0,null,0,0,0,null,"5024217AFA7AB2914B03DB711BCD4D","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075024217AFA7AB2914B03DB711BCD4D",240]
["테라죠타일붙임","바닥, 400*400*25mm, 모르타르 35mm","M2",499.78,null,0,null,0,null,0,0,0,null,"5025F175381DA2C14785FBCF4A39F1","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075025F175381DA2C14785FBCF4A39F1",924]
["인조대리석세면대","W:600*12t,틀포함","M",37.549999999999997,null,0,null,0,null,0,0,0,null,"5024217AFA7AB2914B03DB711FD094","","","010107","T","F","F",{"$nulls":23},"","",null,"0101075024217AFA7AB2914B03DB711FD094",239]
[]
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F317:F340)","v":0},null,{"$f":"SUM(H317:H340)","v":0},null,{"$f":"SUM(J317:J340)","v":0},null,{"$f":"SUM(L317:L340)","v":0},null,"TOTAL"]
["010108  타일공사",{"$nulls":15},"010108"]
["도기질타일[관급]","300*600*7mm","M2",1410.89,null,{"$f":"TRUNC(E343*D343, 0)","v":0},null,{"$f":"TRUNC(G343*D343, 0)","v":0},null,{"$f":"TRUNC(I343*D343, 0)","v":0},{"$f":"TRUNC(E343+G343+I343, 0)","v":0},0,"관급별도","57008170BB61F2B141F7112A8F09CA4050FAB2","","","010108","F","F","T",{"$nulls":23},"","",null,"01010857008170BB61F2B141F7112A8F09CA4050FAB2",848]
["자기질타일(논슬립)[관급]","300*300*7mm","M2",435.61,null,0,null,0,null,0,0,0,"관급별도","57008170BB61F2B141F7112A8CBC3A908C6EED","","","010108","F","F","T",{"$nulls":23},"","",null,"01010857008170BB61F2B141F7112A8CBC3A908C6EED",850]
["자기질타일(석재타일)[관급]","200*200*15mm","M2",12.78,null,0,null,0,null,0,0,0,"관급별도","57008170BB61F2B141F7112A8CBC3A934015F3","","","010108","F","F","T",{"$nulls":23},"","",null,"01010857008170BB61F2B141F7112A8CBC3A934015F3",852]
["타일압착붙임(바탕 85mm+압착 5mm)","바닥, 200*200(타일C, 백색줄눈)","M2",12.41,null,0,null,0,null,0,0,0,null,"5025F1750CD102A141DA35CA76F686","","","010108","T","F","F",{"$nulls":23},"","",null,"0101085025F1750CD102A141DA35CA76F686",256]
["타일압착붙임(바탕 93mm+압착 5mm)","바닥, 300*300(타일C, 백색줄눈)","M2",422.92,null,0,null,0,null,0,0,0,null,"5025F1750CD102A141DA343F7A8FA6","","","010108","T","F","F",{"$nulls":23},"","",null,"0101085025F1750CD102A141DA343F7A8FA6",257]
["타일압착붙임(바탕 23mm+압착 6mm)","벽, 300*600(타일C, 백색줄눈)","M2",1369.8,null,0,null,0,null,0,0,0,null,"5025F1750CFDF2914EB82230FA9435","","","010108","T","F","F",{"$nulls":23},"","",null,"0101085025F1750CFDF2914EB82230FA9435",258]
{"$rows_empty":18}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F343:F366)","v":0},null,{"$f":"SUM(H343:H366)","v":0},null,{"$f":"SUM(J343:J366)","v":0},null,{"$f":"SUM(L343:L366)","v":0},null,"TOTAL"]
["010109  목공사",{"$nulls":15},"010109"]
["합성목재데크[관급]","20mm","M2",213.71,null,{"$f":"TRUNC(E369*D369, 0)","v":0},null,{"$f":"TRUNC(G369*D369, 0)","v":0},null,{"$f":"TRUNC(I369*D369, 0)","v":0},{"$f":"TRUNC(E369+G369+I369, 0)","v":0},0,"관급별도","57008170BB34B2D1402942481922B29B338409","","","010109","F","F","T",{"$nulls":23},"","",null,"01010957008170BB34B2D1402942481922B29B338409",699]
["합성목재데크설치","20mm(자재별도/관급), 하부틀포함","M2",194.28,null,0,null,0,null,0,0,0,null,"57A02175D3A7F251479584154204AD45A655FC","","","010109","F","F","T",{"$nulls":23},"","",null,"01010957A02175D3A7F251479584154204AD45A655FC",846]
["목재계단판설치/휴게실계단","40mm,10mm접착매트고정","M2",29.04,null,0,null,0,null,0,0,0,null,"5025B17375FD82F146DB318418F5B2","","","010109","T","F","F",{"$nulls":23},"","",null,"0101095025B17375FD82F146DB318418F5B2",930]
["원목마루","9.2mm*75*900","M2",365.43,null,0,null,0,null,0,0,0,null,"57008170BB34B2D1402942481922B29B32FF15","","","010109","F","F","T",{"$nulls":23},"","",null,"01010957008170BB34B2D1402942481922B29B32FF15",695]
["마루귀틀설치","라왕, 60*150, 바니시","M",16.38,null,0,null,0,null,0,0,0,null,"5025D170FD32E2B14E1CBB61D32BE4","","","010109","T","F","F",{"$nulls":23},"","",null,"0101095025D170FD32E2B14E1CBB61D32BE4",663]
["목재걸레받이설치","MDF, H:100*9mm, 무늬목시트","M",66.45,null,0,null,0,null,0,0,0,null,"5025D17079D6F2C14FE6CE54FB1CA8","","","010109","T","F","F",{"$nulls":23},"","",null,"0101095025D17079D6F2C14FE6CE54FB1CA8",696]
{"$rows_empty":18}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F369:F392)","v":0},null,{"$f":"SUM(H369:H392)","v":0},null,{"$f":"SUM(J369:J392)","v":0},null,{"$f":"SUM(L369:L392)","v":0},null,"TOTAL"]
["010110  방수공사",{"$nulls":15},"010110"]
["침투성방수","2회","M2",4145.28,null,{"$f":"TRUNC(E395*D395, 0)","v":0},null,{"$f":"TRUNC(G395*D395, 0)","v":0},null,{"$f":"TRUNC(I395*D395, 0)","v":0},{"$f":"TRUNC(E395+G395+I395, 0)","v":0},0,null,"5025A17D41CFC211472425D125E868","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17D41CFC211472425D125E868",263]
["에폭시코팅방수","3회","M2",726.25,null,0,null,0,null,0,0,0,null,"5025A17D41FB22814AA335578559E1","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17D41FB22814AA335578559E1",270]
["우레탄도막방수","바닥, 비노출","M2",891.57,null,0,null,0,null,0,0,0,null,"5025A17D37CA12314D3699639C63F7","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17D37CA12314D3699639C63F7",265]
["우레탄도막방수","벽체, 비노출","M2",1487.16,null,0,null,0,null,0,0,0,null,"5025A17D37CA12314D3699639F3716","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17D37CA12314D3699639F3716",266]
["우레탄복합방수","바닥, 비노출","M2",7369.38,null,0,null,0,null,0,0,0,null,"5025A17D37CA12314D37A787F4CF7D","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17D37CA12314D37A787F4CF7D",267]
["우레탄복합방수","벽체, 비노출","M2",822.26,null,0,null,0,null,0,0,0,null,"5025A17D37CA12314D37A787F328A4","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17D37CA12314D37A787F328A4",268]
["우레탄도막방수","접합부위, 비노출","M",1181.77,null,0,null,0,null,0,0,0,null,"5025A17D37CA12314D37A0570279F2","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17D37CA12314D37A0570279F2",264]
["방수보호재설치","벽체 30mm","M2",212.23,null,0,null,0,null,0,0,0,null,"5025A17DAA4C125147E1386D858283","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17DAA4C125147E1386D858283",863]
["실리콘발수제바름","2회, 뿜칠, 노츨콘크리트면","M2",737.68,null,0,null,0,null,0,0,0,null,"5025A17D41FB22814AA333AA30E22F","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17D41FB22814AA333AA30E22F",929]
["방수모르타르바름","바닥, 21mm","M2",265.72000000000003,null,0,null,0,null,0,0,0,null,"5025A17D7D0632314A9F1A22F9D82F","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17D7D0632314A9F1A22F9D82F",271]
["방수모르타르바름","벽, 21mm","M2",458.32,null,0,null,0,null,0,0,0,null,"5025A17D7D1082F14F1006B3621445","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17D7D1082F14F1006B3621445",272]
["보호모르타르바름","벽, 18mm","M2",663.45,null,0,null,0,null,0,0,0,null,"5025A17DAA5E62B142CB8A5C31626D","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17DAA5E62B142CB8A5C31626D",274]
["배수판설치","500*500*45mm","M2",4888.82,null,0,null,0,null,0,0,0,null,"5025A17DD79462D14A3ABEC2C06216","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17DD79462D14A3ABEC2C06216",276]
["신축줄눈설치(주차장)","SAW CUT+코킹","M",1064.3,null,0,null,0,null,0,0,0,null,"5025617BD57412C1487D9FEA0A4ED2","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025617BD57412C1487D9FEA0A4ED2",700]
["신축줄눈설치(옥상)","SAW CUT+코킹","M",3182.02,null,0,null,0,null,0,0,0,null,"5025617BD57412C1487D9FEA0BA92B","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025617BD57412C1487D9FEA0BA92B",282]
["신축줄눈설치(옥상)","W:170*20t+코킹","M",1087.04,null,0,null,0,null,0,0,0,null,"5025617BD57412C1487CF90A81B5CD","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025617BD57412C1487CF90A81B5CD",281]
["신축조인트재설치(램프)","W:300*20t+코킹","M",86.24,null,0,null,0,null,0,0,0,null,"5025617BD57412C1487CF90BA89A9C","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025617BD57412C1487CF90BA89A9C",864]
["수밀코킹(실리콘)","삼각, 5mm, 방균용","M",202.05,null,0,null,0,null,0,0,0,null,"5025A17D6CB3F2F14ABA3E23EF72F2","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17D6CB3F2F14ABA3E23EF72F2",280]
["수밀코킹(실리콘)","삼각, 10mm, 창호주위","M",16912.009999999998,null,0,null,0,null,0,0,0,null,"5025A17D6CB3F2F14AB91673A32AFC","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17D6CB3F2F14AB91673A32AFC",279]
["수밀코킹(실리콘)","사각, 20mm, 장비패드주위","M",146.1,null,0,null,0,null,0,0,0,null,"5025A17D6CB3F2F14993177FF262D0","","","010110","T","F","F",{"$nulls":23},"","",null,"0101105025A17D6CB3F2F14993177FF262D0",278]
[]
[]
[]
[]
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F395:F418)","v":0},null,{"$f":"SUM(H395:H418)","v":0},null,{"$f":"SUM(J395:J418)","v":0},null,{"$f":"SUM(L395:L418)","v":0},null,"TOTAL"]
["010111  지붕및홈통공사",{"$nulls":15},"010111"]
["루프드레인설치","수직형, 100mm","개소",53,null,{"$f":"TRUNC(E421*D421, 0)","v":0},null,{"$f":"TRUNC(G421*D421, 0)","v":0},null,{"$f":"TRUNC(I421*D421, 0)","v":0},{"$f":"TRUNC(E421+G421+I421, 0)","v":0},0,null,"5025917EA0FF52A1402713B0CA9576","","","010111","T","F","F",{"$nulls":23},"","",null,"0101115025917EA0FF52A1402713B0CA9576",284]
["루프드레인설치","L형, 100mm","개소",20,null,{"$f":"TRUNC(E422*D422, 0)","v":0},null,{"$f":"TRUNC(G422*D422, 0)","v":0},null,{"$f":"TRUNC(I422*D422, 0)","v":0},0,0,null,"5025917EA0C2120142BD4637B7E49F","","","010111","T","F","F",{"$nulls":23},"","",null,"0101115025917EA0C2120142BD4637B7E49F",676]
["스테레스선홈통","Ø100*1.5t","M",115.1,null,{"$f":"TRUNC(E423*D423, 0)","v":0},null,{"$f":"TRUNC(G423*D423, 0)","v":0},null,{"$f":"TRUNC(I423*D423, 0)","v":0},0,0,null,"5025917EB15C62F146F6F7EC109369","","","010111","T","F","F",{"$nulls":23},"","",null,"0101115025917EB15C62F146F6F7EC109369",285]
["스텐레스상자홈통설치","250*250*250*1.5t","EA",20,null,{"$f":"TRUNC(E424*D424, 0)","v":0},null,{"$f":"TRUNC(G424*D424, 0)","v":0},null,{"$f":"TRUNC(I424*D424, 0)","v":0},0,0,null,"5025917EB10432D14705C7F08F0B3C","","","010111","T","F","F",{"$nulls":23},"","",null,"0101115025917EB10432D14705C7F08F0B3C",617]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F421:F444)","v":0},null,{"$f":"SUM(H421:H444)","v":0},null,{"$f":"SUM(J421:J444)","v":0},null,{"$f":"SUM(L421:L444)","v":0},null,"TOTAL"]
["010112  금속공사",{"$nulls":15},"010112"]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",4463.51,null,{"$f":"TRUNC(E447*D447, 0)","v":0},null,{"$f":"TRUNC(G447*D447, 0)","v":0},null,{"$f":"TRUNC(I447*D447, 0)","v":0},{"$f":"TRUNC(E447+G447+I447, 0)","v":0},0,null,"50258178BEBD12D14BA0DB838A43FD","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178BEBD12D14BA0DB838A43FD",596]
["경량철골천정틀","TH-BAR, H:1m이상, 인서트 유","M2",6562.31,null,0,null,0,null,0,0,0,null,"50258178BEEA429143BA06797F28A1","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178BEEA429143BA06797F28A1",598]
["AL몰딩설치(ㄷ형)","15*30*15*1.0mm","M",1140.1400000000001,null,0,null,0,null,0,0,0,null,"5025D170D27A12414F2BB08D52DC6F","","","010112","T","F","F",{"$nulls":23},"","",null,"0101125025D170D27A12414F2BB08D52DC6F",600]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",6875.92,null,0,null,0,null,0,0,0,null,"5025D170D27A12414F2BB08D53E371","","","010112","T","F","F",{"$nulls":23},"","",null,"0101125025D170D27A12414F2BB08D53E371",599]
["알루미늄천장재/내풍압용","600*600*0.7mm, 무공","M2",1881.29,null,0,null,0,null,0,0,0,null,"57008170BB34B2D14130B0C72AC83A6CBA4FDA","","","010112","F","F","T",{"$nulls":23},"","",null,"01011257008170BB34B2D14130B0C72AC83A6CBA4FDA",736]
["알루미늄컨벡터커버","W:300, 바닥그릴형","M",34.6,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD7D0BF99693A1","","","010112","F","F","T",{"$nulls":23},"","",null,"01011257A02175D3A7D2A149393C1BCD7D0BF99693A1",869]
["팬코일유니트커버","W:350*H:450*1.2t","M",304,null,0,null,0,null,0,0,0,null,"57008170BB0F7291403C4F7B9871EF55387E93","","","010112","F","F","T",{"$nulls":23},"","",null,"01011257008170BB0F7291403C4F7B9871EF55387E93",931]
["조명박스","460*250*1.2t,STL, 도장","M",37.549999999999997,null,0,null,0,null,0,0,0,null,"57008170BB34B2D14139A79DBC42B796866C75","","","010112","F","F","T",{"$nulls":23},"","",null,"01011257008170BB34B2D14139A79DBC42B796866C75",601]
["철재커텐박스설치(ㄱ자)","200*200*1.2t, STL. 도장","M",43.38,null,0,null,0,null,0,0,0,null,"5025D170C1FA92A14C2EC03F1C1C0A","","","010112","T","F","F",{"$nulls":23},"","",null,"0101125025D170C1FA92A14C2EC03F1C1C0A",761]
["철재커텐박스설치(ㄱ자)","200*250*1.2t, STL. 도장","M",1322.6,null,0,null,0,null,0,0,0,null,"5025D170C1FA92A14C2EC03F1D67D6","","","010112","T","F","F",{"$nulls":23},"","",null,"0101125025D170C1FA92A14C2EC03F1D67D6",762]
["철재커텐박스설치(ㄱ자)","200*300*1.2t, STL. 도장","M",92.8,null,0,null,0,null,0,0,0,null,"5025D170C1FA92A14C2EC03F1A2B0A","","","010112","T","F","F",{"$nulls":23},"","",null,"0101125025D170C1FA92A14C2EC03F1A2B0A",763]
["철재커텐박스설치(ㄱ자)","200*500*1.2t, STL. 도장","M",23.83,null,0,null,0,null,0,0,0,null,"5025D170C1FA92A14C2EC03F18F923","","","010112","T","F","F",{"$nulls":23},"","",null,"0101125025D170C1FA92A14C2EC03F18F923",765]
["철재커텐박스설치(ㄱ자)","200*550*1.2t, STL. 도장","M",86.26,null,0,null,0,null,0,0,0,null,"5025D170C1FA92A14C2EC03F19C085","","","010112","T","F","F",{"$nulls":23},"","",null,"0101125025D170C1FA92A14C2EC03F19C085",766]
["철재커텐박스설치(ㄱ자)","200*600*1.2t, STL. 도장","M",17,null,0,null,0,null,0,0,0,null,"5025D170C1FA92A14C2EC03F16B4FC","","","010112","T","F","F",{"$nulls":23},"","",null,"0101125025D170C1FA92A14C2EC03F16B4FC",767]
["철재커텐박스설치(ㄱ자)","200*900*1.2t, STL. 도장","M",19.18,null,0,null,0,null,0,0,0,null,"5025D170C1FA92A14C2EC03F179EEA","","","010112","T","F","F",{"$nulls":23},"","",null,"0101125025D170C1FA92A14C2EC03F179EEA",768]
["계단논슬립설치","스테인리스 ,50mm(박킹 1줄)","M",18,null,0,null,0,null,0,0,0,null,"5025D1705EDC72314DD6D7109C0DF2","","","010112","T","F","F",{"$nulls":23},"","",null,"0101125025D1705EDC72314DD6D7109C0DF2",602]
["메탈라스설치/모르타르탈락방지","W:300","M",283.95,null,0,null,0,null,0,0,0,null,"502581786683122145C1B2318DAA66","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502581786683122145C1B2318DAA66",634]
["미장용코너비드","AL, H=13mm","M",1528.1,null,0,null,0,null,0,0,0,null,"502551744A4D42014032276E660A96","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502551744A4D42014032276E660A96",607]
["미장용인코너비드","AL, H=13mm","M",423.1,null,0,null,0,null,0,0,0,null,"502551744A4D42014032276E660F14","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502551744A4D42014032276E660F14",608]
["걸레받이비드","AL, H=10mm","M",2667.56,null,0,null,0,null,0,0,0,null,"502551744A4D4201403105C9B34035","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502551744A4D4201403105C9B34035",609]
["창호주위비드","AL, H=10mm","M",6317.51,null,0,null,0,null,0,0,0,null,"502551744A4D420145B5C82A540F4C","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502551744A4D420145B5C82A540F4C",674]
["죠인트비드","AL, H=12mm(크랙방지)","M",159.5,null,0,null,0,null,0,0,0,null,"502551744A4D42014033CFBE2B5206","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502551744A4D42014033CFBE2B5206",610]
["벽코너보강","W:300,메탈라스(조적+콘크리트)","M",261.8,null,0,null,0,null,0,0,0,null,"502551744A4D4201477ED99558E9BF","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502551744A4D4201477ED99558E9BF",611]
["타일벽코너비드","SST,W:15*15*1.2t","M",161.4,null,0,null,0,null,0,0,0,null,"502551744A4D420145B16D3BB21EE6","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502551744A4D420145B16D3BB21EE6",675]
["스텐레스공후레임/화장실","1100*2100.W250*1.2t코킹","개소",6,null,0,null,0,null,0,0,0,null,"50258178939DB29149039E3349F9B0","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178939DB29149039E3349F9B0",932]
["스텐레스공후레임/화장실","1200*2100.W250*1.2t코킹","개소",10,null,0,null,0,null,0,0,0,null,"50258178939DB29149039E334A80E2","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178939DB29149039E334A80E2",933]
["오픈트렌치","한면,L-25*25*3T,아연도금","M",670.2,null,0,null,0,null,0,0,0,null,"50258178546A82B14061B48D305DD9","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178546A82B14061B48D305DD9",615]
["오픈트렌치","양면,L-25*25*3T,아연도금","M",403.49,null,0,null,0,null,0,0,0,null,"50258178546A82B14061B48D305858","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178546A82B14061B48D305858",616]
["트렌치","아연도그레이팅, W200. I-25*5*3t","M",94.95,null,0,null,0,null,0,0,0,null,"50258178546A82B143340C1C211EE8","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178546A82B143340C1C211EE8",635]
["트렌치","주철제그레이팅,W300,무소음","M",13,null,0,null,0,null,0,0,0,null,"50258178546A82B143363A17BE1A2B","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178546A82B143363A17BE1A2B",620]
["트렌치","스테인리스, W100*3t","M",25.3,null,0,null,0,null,0,0,0,null,"50258178546AA2714EF5C735EC02DB","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178546AA2714EF5C735EC02DB",739]
["트렌치","스테인리스, W200*3t","M",32.01,null,0,null,0,null,0,0,0,null,"50258178546AA2714EF5C735EC02A3","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178546AA2714EF5C735EC02A3",738]
["스틸핸드레일/TYPE-A(3F옥상정원)","Ø60+FB60*3*2단,H:1000","M",146.05000000000001,null,0,null,0,null,0,{"$f":"TRUNC(E479+G479+I479, 0)","v":0},0,null,"502581781E5D1201432656C4EE38F8","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502581781E5D1201432656C4EE38F8",934]
["스틸핸드레일/TYPE-B(2F테라스)","FB50*3*3단,H:750","M",40.9,null,0,null,0,null,0,0,0,null,"502581781E5D1201432656C4ED118F","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502581781E5D1201432656C4ED118F",935]
["스틸핸드레일/TYPE-C(5F,7F테라스)","Ø60+FB60*3*2단,H:950","M",31.3,null,0,null,0,null,0,0,0,null,"502581781E5D1201432656C4EC0BD4","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502581781E5D1201432656C4EC0BD4",936]
["스틸핸드레일/TYPE-D(4F옥상정원,RF지붕)","Ø60+FB60*3*2단,H:950","M",451.54,null,0,null,0,null,0,0,0,null,"502581781E5D1201432656C4EB6459","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502581781E5D1201432656C4EB6459",937]
["스틸핸드레일/TYPE-E(RF/옥상전망데크)","FB50*3*3단,H:900","M",15.2,null,0,null,0,null,0,0,0,null,"502581781E5D1201432656C4EA5D48","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502581781E5D1201432656C4EA5D48",938]
["스틸핸드레일/내부계단","FB65*12+RB9*4단,H:1200","M",110.48,null,0,null,0,null,0,0,0,null,"502581781E5D1201432656C4E9B63E","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502581781E5D1201432656C4E9B63E",939]
["스틸핸드레일/계단#1,2","FB50*9+50*3*3단,H:900","M",174.74,null,0,null,0,null,0,0,0,null,"502581781E5D1201432656C4E8903B","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502581781E5D1201432656C4E8903B",940]
["스틸핸드레일/1F하역공간","FB50*3*5단,H:1200","M",15.5,null,0,null,0,null,0,0,0,null,"502581781E5D1201432656C4E78929","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502581781E5D1201432656C4E78929",941]
["스틸핸드레일/3F옥상정원","FB50*3*2단,H:600","M",55.5,null,0,null,0,null,0,0,0,null,"502581781E5D1201432656C4E6E29F","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502581781E5D1201432656C4E6E29F",942]
["강화유리핸드레일/2F,3F로비","구로철판1.6t+강화유리12mm,H:1200","M",82.4,null,0,null,0,null,0,0,0,null,"502581781E5D1201432656C7A2FF15","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502581781E5D1201432656C7A2FF15",944]
["스텐레스사다리/PIT,우수조","W:400,Ø38.1+22.3*2t","M",12.4,null,0,null,0,null,0,0,0,null,"502581780C3482E14DA44332830372","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502581780C3482E14DA44332830372",741]
["스텐레스사다리/옥탑점검","W:600*4400,Ø38.1*2t+25.4*1.5t","개",2,null,0,null,0,null,0,0,0,null,"502581780C3482E14DA44332830AD9","","","010112","T","F","F",{"$nulls":23},"","",null,"010112502581780C3482E14DA44332830AD9",945]
["스틸점검구뚜껑/점검구","1000*1000*3.2t 무늬강판","개",3,null,0,null,0,null,0,0,0,null,"50258178541262B145C669B7ADAA99","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178541262B145C669B7ADAA99",946]
["스틸점검구뚜껑/집수정","1000*1000.I-50*6*3 아연GT","개",4,null,0,null,0,null,0,0,0,null,"50258178541262B14420C6072CB5BD","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178541262B14420C6072CB5BD",947]
["스틸점검구뚜껑/집수정","1500*1500.I-50*6*3 아연GT","개",4,null,0,null,0,null,0,0,0,null,"50258178541262B14420C6072F0A52","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178541262B14420C6072F0A52",948]
["스틸점검구뚜껑/집수정","2000*2000.I-50*6*3 아연GT","개",1,null,0,null,0,null,0,0,0,null,"50258178541262B14420C6072E63D8","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178541262B14420C6072E63D8",949]
["스틸점검구뚜껑/집수정","1200*1800.I-50*6*3 아연GT","개",1,null,0,null,0,null,0,0,0,null,"50258178541262B14420C60729E11E","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178541262B14420C60729E11E",950]
["AL환기용그릴/방습벽","400*200*2.0t","개",144,null,0,null,0,null,0,0,0,null,"50258178541242814A826B54DE1199","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178541242814A826B54DE1199",623]
["천장점검구설치","450*450mm","EA",86,null,0,null,0,null,0,0,0,null,"50258178BECF82E1450CB8F38F3940","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178BECF82E1450CB8F38F3940",880]
["주방배식대","스테인리스, W600*1.2t","M",3,null,0,null,0,null,0,0,0,null,"50258178F41822A14E70EB6117C258","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178F41822A14E70EB6117C258",624]
["파라펫링","스테인리스, D100*19t","개",216,null,0,null,0,null,0,0,0,null,"50258178F41822A14E7299DD97867B","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178F41822A14E7299DD97867B",625]
["엘리베이터후크","Ø100*22t STL","개",6,null,0,null,0,null,0,0,0,null,"50258178F41832B1445D7EB08AB4B2","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178F41832B1445D7EB08AB4B2",626]
["스틸후레임설치/계단형(옥상정원3층)","ㅁ-50*50*2.3t,@600*600,H:1050","M2",57.24,null,0,null,0,null,0,0,0,null,"50258178F41832B1445D79C8A42A25","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178F41832B1445D79C8A42A25",754]
["창호상부보강/커튼월상부","ㅁ-150*100*3.2t,@900","M2",277.20999999999998,null,0,null,0,null,0,0,0,null,"50258178F41832B1445D79C8A53137","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178F41832B1445D79C8A53137",951]
["창호상부보강/스텐도어상부","ㅁ-100*50*2.3t,@900","M2",365.16,null,0,null,0,null,0,0,0,null,"50258178F41832B1445D79C8A6D880","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178F41832B1445D79C8A6D880",952]
["스틸판접기/커튼월+기둥및벽","1.2t,조합","M2",88.52,null,0,null,0,null,0,0,0,null,"50258178F41832B1445D782A568C53","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178F41832B1445D782A568C53",881]
["스틸판접기/단차천정,누드ELEV벽등","1.2t,갈바","M2",426.06,null,0,null,0,null,0,0,0,null,"50258178F41832B1445D782A56892F","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178F41832B1445D782A56892F",756]
["스틸판접기/방화셔터상부","1.6t+L-50*50*6,방청","M2",155.08000000000001,null,0,null,0,null,0,0,0,null,"50258178F41832B1445D782A55E295","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178F41832B1445D782A55E295",758]
["스텐레스재료분리대","바닥, W15*H20*1.5t","M",248.14,null,0,null,0,null,0,0,0,null,"5025D1703209A28143EAE8685CB471","","","010112","T","F","F",{"$nulls":23},"","",null,"0101125025D1703209A28143EAE8685CB471",759]
["스텐레스재료분리대","바닥, W50*H20*2.0t","M",99.74,null,0,null,0,null,0,0,0,null,"5025D1703209A28143E83BD47F8600","","","010112","T","F","F",{"$nulls":23},"","",null,"0101125025D1703209A28143E83BD47F8600",760]
["카스톱퍼","네오프렌계, 150*120*750mm","개소",110,null,0,null,0,null,0,0,0,null,"5025D170A51142714592BCD116AB9C","","","010112","T","F","F",{"$nulls":23},"","",null,"0101125025D170A51142714592BCD116AB9C",629]
["주차장코너가드","네오프렌계, 90*90*15*1000mm","M",64,null,0,null,0,null,0,0,0,null,"5025D170A51172C149AFBDB4BAD315","","","010112","T","F","F",{"$nulls":23},"","",null,"0101125025D170A51172C149AFBDB4BAD315",630]
["주차반사경설치","Ø1000, 스텐레스","개소",6,null,{"$f":"TRUNC(E511*D511, 0)","v":0},null,{"$f":"TRUNC(G511*D511, 0)","v":0},null,{"$f":"TRUNC(I511*D511, 0)","v":0},{"$f":"TRUNC(E511+G511+I511, 0)","v":0},0,null,"5025D170A51172C149ABC4FAD28E7D","","","010112","T","F","F",{"$nulls":23},"","",null,"0101125025D170A51172C149ABC4FAD28E7D",631]
["그리스트랩설치","900*600*600,SST","개소",2,null,0,null,0,null,0,0,0,null,"50258178F41832B1445D7709D36149","","","010112","T","F","F",{"$nulls":23},"","",null,"01011250258178F41832B1445D7709D36149",633]
["EXPANSION JOINT","바닥,W:50mm","M",4.8,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD7D0BF8F1D625","","","010112","F","F","T",{"$nulls":23},"","",null,"01011257A02175D3A7D2A149393C1BCD7D0BF8F1D625",679]
["EXPANSION JOINT","천정,W:50mm","M",4.8,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD7D0BF8F2FD1E","","","010112","F","F","T",{"$nulls":23},"","",null,"01011257A02175D3A7D2A149393C1BCD7D0BF8F2FD1E",680]
["EXPANSION JOINT","내벽,W:50mm","M",12,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD7D0BF8F38441","","","010112","F","F","T",{"$nulls":23},"","",null,"01011257A02175D3A7D2A149393C1BCD7D0BF8F38441",681]
["EXPANSION JOINT","외벽,W:50mm","M",21.6,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD7D0BF8F4AA43","","","010112","F","F","T",{"$nulls":23},"","",null,"01011257A02175D3A7D2A149393C1BCD7D0BF8F4AA43",682]
["EXPANSION JOINT","지붕,W:50mm","M",4.8,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD7D0BF8F5B155","","","010112","F","F","T",{"$nulls":23},"","",null,"01011257A02175D3A7D2A149393C1BCD7D0BF8F5B155",683]
[]
[]
[]
[]
[]
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F447:F522)","v":0},null,{"$f":"SUM(H447:H522)","v":0},null,{"$f":"SUM(J447:J522)","v":0},null,{"$f":"SUM(L447:L522)","v":0},null,"TOTAL"]
["010113  미장공사",{"$nulls":15},"010113"]
["폴리머수지모르타르","3mm","M2",1945.19,null,{"$f":"TRUNC(E525*D525, 0)","v":0},null,{"$f":"TRUNC(G525*D525, 0)","v":0},null,{"$f":"TRUNC(I525*D525, 0)","v":0},{"$f":"TRUNC(E525+G525+I525, 0)","v":0},0,null,"57008170BB0F7291403514FB26538811DF4FF0","","","010113","F","F","T",{"$nulls":23},"","",null,"01011357008170BB0F7291403514FB26538811DF4FF0",702]
["시멘트모르타르바름","바닥, 23mm","M2",710.78,null,0,null,0,null,0,0,0,null,"50255174F4F9125144E93A8D78DC5D","","","010113","T","F","F",{"$nulls":23},"","",null,"01011350255174F4F9125144E93A8D78DC5D",530]
["시멘트모르타르바름","바닥, 27mm","M2",1118.83,null,0,null,0,null,0,0,0,null,"50255174F4F9125144E93A8D78D826","","","010113","T","F","F",{"$nulls":23},"","",null,"01011350255174F4F9125144E93A8D78D826",529]
["시멘트모르타르바름","바닥, 77mm","M2",59.87,null,0,null,0,null,0,0,0,null,"50255174F4F9125144E93A8D7D46F5","","","010113","T","F","F",{"$nulls":23},"","",null,"01011350255174F4F9125144E93A8D7D46F5",532]
["시멘트모르타르바름","내벽, 18mm","M2",8212.67,null,0,null,0,null,0,0,0,null,"50255174F4F9320147CA90C63879E3","","","010113","T","F","F",{"$nulls":23},"","",null,"01011350255174F4F9320147CA90C63879E3",533]
["시멘트모르타르바름","외벽, 24mm","M2",810.19,null,0,null,0,null,0,0,0,null,"50255174F4F9320147CE0B10CA4D75","","","010113","T","F","F",{"$nulls":23},"","",null,"01011350255174F4F9320147CE0B10CA4D75",534]
["쇠흙손마감","콘크리트면","M2",645.89,null,0,null,0,null,0,0,0,null,"5025617A7A30B2914CC3BA47FD1052","","","010113","T","F","F",{"$nulls":23},"","",null,"0101135025617A7A30B2914CC3BA47FD1052",535]
["조면처리","콘크리트면","M2",210.99,null,0,null,0,null,0,0,0,null,"5025617A7A30B2914CC3BA47FD15D0","","","010113","T","F","F",{"$nulls":23},"","",null,"0101135025617A7A30B2914CC3BA47FD15D0",536]
["기계휘니셔마감","콘크리트면","M2",25447.89,null,0,null,0,null,0,0,0,null,"50255174F4A1221142FFF4EF51E9C0","","","010113","T","F","F",{"$nulls":23},"","",null,"01011350255174F4A1221142FFF4EF51E9C0",537]
["콘크리트면마무리","내벽","M2",1455.99,null,0,null,0,null,0,0,0,null,"50255174F4CDF2514FCE3B803AD8DB","","","010113","T","F","F",{"$nulls":23},"","",null,"01011350255174F4CDF2514FCE3B803AD8DB",538]
["콘크리트면마무리","외벽","M2",1430.73,null,0,null,0,null,0,0,0,null,"50255174F4CDC2814B6FFCD4388C2E","","","010113","T","F","F",{"$nulls":23},"","",null,"01011350255174F4CDC2814B6FFCD4388C2E",835]
["콘크리트면마무리","내부천정","M2",417.59,null,0,null,0,null,0,0,0,null,"50255174F4CDF2514C7916858867D1","","","010113","T","F","F",{"$nulls":23},"","",null,"01011350255174F4CDF2514C7916858867D1",539]
["창틀주위모르타르충진/습식벽체","창호주위","M",7201.61,null,0,null,0,null,0,0,0,null,"5025E176D6BE02714F124EC7B895CB","","","010113","T","F","F",{"$nulls":23},"","",null,"0101135025E176D6BE02714F124EC7B895CB",525]
["창틀주위암면충진/건식벽체","창호주위","M",627.20000000000005,null,0,null,0,null,0,0,0,null,"5025E176D6BE02714E0B5D16B39657","","","010113","T","F","F",{"$nulls":23},"","",null,"0101135025E176D6BE02714E0B5D16B39657",703]
["판넬히팅","단열30mm+은박단열매트3mm+몰탈57mm","M2",21.14,null,0,null,0,null,0,0,0,null,"5025517481D0E20149B71ABE13B443","","","010113","T","F","F",{"$nulls":23},"","",null,"0101135025517481D0E20149B71ABE13B443",704]
["판넬히팅","단열75mm+은박단열매트3mm+몰탈57mm","M2",238.59,null,0,null,0,null,0,0,0,null,"5025517481D0E20149B71ABE10E024","","","010113","T","F","F",{"$nulls":23},"","",null,"0101135025517481D0E20149B71ABE10E024",705]
{"$rows_empty":8}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F525:F548)","v":0},null,{"$f":"SUM(H525:H548)","v":0},null,{"$f":"SUM(J525:J548)","v":0},null,{"$f":"SUM(L525:L548)","v":0},null,"TOTAL"]
["010114  창호공사",{"$nulls":15},"010114"]
["CW17(180*60mm*1.5t,MPG SYSTEM)","4.800 x 33.100 = 158.880, 접합유리, H/W포함","EA",1,null,{"$f":"TRUNC(E551*D551, 0)","v":0},null,{"$f":"TRUNC(G551*D551, 0)","v":0},null,{"$f":"TRUNC(I551*D551, 0)","v":0},{"$f":"TRUNC(E551+G551+I551, 0)","v":0},0,null,"5769617FEB94D2E14997F1C830C3","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C830C3",342]
["CW18(180*60mm*1.5t,MPG SYSTEM)","4.800 x 33.100 = 158.880, 접합유리, H/W포함","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C830C5","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C830C5",343]
["DFSD01(240*45*1.6t,갑종방화문,이중문)","2.000 x 2.400 = 4.800","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C830C7","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C830C7",344]
["DFSD02(240*45*1.6t,갑종방화문,이중문)","2.000 x 2.100 = 4.200","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C830C9","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C830C9",345]
["DSD01(240*45*1.6t,일반철재문,이중문)","2.000 x 2.400 = 4.800","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83395","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83395",346]
["FSD01(240*45*1.6t,갑종방화문)","0.800 x 2.100 = 1.680","EA",23,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83397","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83397",347]
["FSD02(240*45*1.6t,갑종방화문)","0.900 x 2.100 = 1.890","EA",51,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83391","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83391",348]
["FSD03(240*45*1.6t,갑종방화문)","1.000 x 1.600 = 1.600","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83393","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83393",349]
["FSD03A(240*45*1.6t,갑종방화문)","1.000 x 2.100 = 2.100","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8339C","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8339C",953]
["FSD04(240*45*1.6t,갑종방화문)","1.000 x 2.400 = 2.400","EA",41,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8339D","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8339D",350]
["FSD05(240*45*1.6t,갑종방화문)","2.000 x 2.400 = 4.800","EA",7,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8328C","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8328C",351]
["FSD06(240*45*1.6t,갑종방화문)","2.500 x 3.000 = 7.500","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8328E","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8328E",352]
["FSD07(240*45*1.6t,갑종방화문)","3.000 x 3.000 = 9.000","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83288","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83288",353]
["FSS101(방화셔터,개폐기포함)","11.150 x 3.000 = 33.450","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8328A","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8328A",354]
["FSS102(방화셔터,개폐기포함)","2.500 x 3.000 = 7.500","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83284","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83284",355]
["FSS201(방화셔터,개폐기포함)","9.750 x 2.700 = 26.325","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83540","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83540",356]
["FSS301(방화셔터,개폐기포함)","6.200 x 2.700 = 16.740","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83542","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83542",357]
["FSS302(방화셔터,개폐기포함)","3.500 x 2.700 = 9.450","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83544","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83544",358]
["FSS303(방화셔터,개폐기포함)","9.000 x 2.700 = 24.300","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83546","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83546",359]
["FSS304(방화셔터,개폐기포함)","6.950 x 2.700 = 18.765","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83548","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83548",360]
["FSS305(방화셔터,개폐기포함)","6.950 x 2.700 = 18.765","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C834BA","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C834BA",361]
["FSS306(방화셔터,개폐기포함)","5.800 x 2.700 = 15.660","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C834B8","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C834B8",362]
["FSS307(방화셔터,개폐기포함)","1.350 x 2.700 = 3.645","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C834BE","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C834BE",363]
["FSS501(방화셔터,개폐기포함)","9.500 x 2.700 = 25.650","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C834BC","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C834BC",364]
["FSS502(방화셔터,개폐기포함)","1.550 x 2.700 = 4.185","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C834B2","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C834B2",365]
["FSS503(방화셔터,개폐기포함)","9.500 x 2.700 = 25.650","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8370E","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8370E",366]
["FSS504(방화셔터,개폐기포함)","1.550 x 2.700 = 4.185","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8370C","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8370C",367]
["FSS701(방화셔터,개폐기포함)","9.500 x 2.700 = 25.650","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8370A","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8370A",368]
["FSS702(방화셔터,개폐기포함)","2.700 x 2.700 = 7.290","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83708","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83708",369]
["FSS703(방화셔터,개폐기포함)","9.500 x 2.700 = 25.650","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83706","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83706",370]
["FSS704(방화셔터,개폐기포함)","2.700 x 2.700 = 7.290","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83669","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83669",371]
["PFSD01(방화방음문)","1.200 x 2.400 = 2.880","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8366B","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8366B",372]
["PFSD02(방화방음문)","2.000 x 2.400 = 4.800","EA",3,null,0,null,0,null,0,{"$f":"TRUNC(E583+G583+I583, 0)","v":0},0,null,"5769617FEB94D2E14997F1C8366D","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8366D",373]
["PSD01(철재방음문)","1.000 x 2.400 = 2.400","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8366F","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8366F",374]
["PSD02(철재방음문)","2.000 x 2.400 = 4.800","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83661","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83661",375]
["SD01(240*45*1.6t,일반철재문)","0.800 x 2.100 = 1.680","EA",18,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8393D","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8393D",376]
["SD01A(240*45*1.6t,일반철재문)","1.000 x 1.500 = 1.500","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8393E","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8393E",954]
["SD02(240*45*1.6t,일반철재문)","1.000 x 2.100 = 2.100","EA",6,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8393F","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8393F",377]
["SD03(240*45*1.6t,일반철재문)","1.000 x 2.400 = 2.400","EA",16,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83939","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83939",378]
["SD04(240*45*1.6t,일반철재문)","1.200 x 2.400 = 2.880","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8393B","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8393B",379]
["SD05(240*45*1.6t,일반철재문)","2.000 x 2.100 = 4.200","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83935","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83935",380]
["SD06(240*45*1.6t,일반철재문)","2.000 x 2.400 = 4.800","EA",15,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83814","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83814",381]
["SD07(240*45*1.6t,일반철재문)","2.000 x 3.000 = 6.000","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83816","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83816",382]
["SLD01(장애인용자동문)","1.000 x 2.100 = 2.100","EA",14,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83810","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83810",383]
["SS101(스텐레스웨이브셔터,개폐기포함)","7.140 x 4.550 = 32.487","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C83812","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C83812",384]
["SSB01(단열셔터,개폐기포함)/장비반입구","3.550 x 4.700 = 16.685","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8381D","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8381D",966]
["SSD01(100*50*1.5t,H/L)","2.000 x 3.000 = 6.000","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C8381C","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1C8381C",385]
["SSD02(100*50*1.5t,H/L)","3.000 x 3.000 = 9.000","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB85E5","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB85E5",386]
["SSD03(100*50*1.5t,H/L)","2.000 x 3.000 = 6.000","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB85E7","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB85E7",387]
["SSD04(100*50*1.5t,H/L)","3.800 x 2.700 = 10.260","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB85E1","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB85E1",388]
["SSD05(100*50*1.5t,H/L)","11.300 x 3.000 = 33.900","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB85E3","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB85E3",389]
["SSD06(100*50*1.5t,H/L)","2.000 x 3.000 = 6.000","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB85ED","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB85ED",390]
["SSD07(100*50*1.5t,H/L)","6.000 x 3.300 = 19.800","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB84DF","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB84DF",391]
["SSD08(100*50*1.5t,H/L)","4.280 x 3.000 = 12.840","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB84DD","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB84DD",392]
["SSD09(100*50*1.5t,H/L)","5.080 x 3.000 = 15.240","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB84DB","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB84DB",393]
["SSD10(100*50*1.5t,H/L)","2.615 x 2.700 = 7.060","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB84D9","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB84D9",394]
["SSD11(100*50*1.5t,H/L)","0.800 x 2.700 = 2.160","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB84D7","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB84D7",395]
["SSD12(100*50*1.5t,H/L)","0.800 x 2.700 = 2.160","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8793","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8793",396]
["SSD13(100*50*1.5t,H/L)","7.700 x 3.300 = 25.410","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8791","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8791",397]
["SSD14(100*50*1.5t,H/L)","4.030 x 2.700 = 10.881","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8797","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8797",398]
["SSD15(100*50*1.5t,H/L)","6.030 x 2.700 = 16.281","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8795","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8795",399]
["SSD16(100*50*1.5t,H/L)","8.980 x 2.700 = 24.246","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB879B","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB879B",400]
["SSD17(100*50*1.5t,H/L)","5.540 x 2.700 = 14.958","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB868A","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB868A",401]
["SSD18(100*50*1.5t,H/L)","3.200 x 2.700 = 8.640","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8688","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8688",402]
["SSD19(100*50*1.5t,H/L)","3.000 x 2.700 = 8.100","EA",1,null,{"$f":"TRUNC(E615*D615, 0)","v":0},null,{"$f":"TRUNC(G615*D615, 0)","v":0},null,{"$f":"TRUNC(I615*D615, 0)","v":0},{"$f":"TRUNC(E615+G615+I615, 0)","v":0},0,null,"5769617FEB94D2E14997F1CB868E","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB868E",403]
["SSD20(100*50*1.5t,H/L)","2.860 x 2.700 = 7.722","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB868C","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB868C",404]
["SSD21(100*50*1.5t,H/L)","12.730 x 2.700 = 34.371","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8682","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8682",405]
["SSD22(100*50*1.5t,H/L)","3.405 x 2.700 = 9.193","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8108","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8108",406]
["SSD22A(100*50*1.5t,H/L)","6.165 x 2.700 = 16.645","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB810B","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB810B",990]
["SSD23(100*50*1.5t,H/L)","3.405 x 2.700 = 9.193","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB810A","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB810A",407]
["SSD25(100*50*1.5t,H/L)","2.650 x 2.700 = 7.155","EA",3,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB810E","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB810E",409]
["SSD26(100*50*1.5t,H/L)","2.714 x 2.700 = 7.327","EA",3,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8100","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8100",410]
["SSD27(100*50*1.5t,H/L)","3.015 x 2.700 = 8.140","EA",3,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8062","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8062",411]
["SSD28(100*50*1.5t,H/L)","2.965 x 2.700 = 8.005","EA",3,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8060","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8060",412]
["SSD29(100*50*1.5t,H/L)","3.405 x 2.700 = 9.193","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8066","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8066",413]
["SSD30(100*50*1.5t,H/L)","6.430 x 2.700 = 17.361","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8064","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8064",414]
["SSD31(100*50*1.5t,H/L)","6.405 x 2.700 = 17.293","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB806A","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB806A",415]
["SSD32(100*50*1.5t,H/L)","6.510 x 2.700 = 17.577","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8336","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8336",416]
["SSD33(100*50*1.5t,H/L)","6.240 x 2.700 = 16.848","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8334","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8334",417]
["SSD34(100*50*1.5t,H/L)","3.490 x 2.700 = 9.423","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8332","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8332",418]
["SSD35(100*50*1.5t,H/L)","3.680 x 2.700 = 9.936","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8330","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8330",419]
["SSD36(100*50*1.5t,H/L)","6.430 x 2.700 = 17.361","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB833E","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB833E",420]
["SSD37(100*50*1.5t,H/L)","6.405 x 2.700 = 17.293","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8211","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8211",421]
["SSD38(100*50*1.5t,H/L)","6.510 x 2.700 = 17.577","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8213","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8213",422]
["SSD39(100*50*1.5t,H/L)","6.240 x 2.700 = 16.848","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8215","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8215",423]
["SSD40(100*50*1.5t,H/L)","3.490 x 2.700 = 9.423","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8217","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8217",424]
["SSD41(100*50*1.5t,H/L)","3.130 x 2.700 = 8.451","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8219","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8219",425]
["SSD42(100*50*1.5t,H/L)","3.679 x 2.700 = 9.933","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8D3B","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8D3B",426]
["SSD43(100*50*1.5t,H/L)","6.240 x 2.700 = 16.848","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8D39","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8D39",427]
["SSD44(100*50*1.5t,H/L)","6.490 x 2.700 = 17.523","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8D3F","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8D3F",428]
["SSD45(100*50*1.5t,H/L)","6.155 x 2.700 = 16.618","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8D3D","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8D3D",429]
["SSD46(100*50*1.5t,H/L)","6.240 x 2.700 = 16.848","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8D33","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8D33",430]
["SSD47(100*50*1.5t,H/L)","6.790 x 2.700 = 18.333","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CB8C15","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CB8C15",431]
["SSD48(100*50*1.5t,H/L)","1.300 x 2.700 = 3.510","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CAFE11","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CAFE11",437]
["SSD49(100*50*1.5t,H/L)","3.130 x 2.700 = 8.451","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CAFE17","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CAFE17",438]
["SSW01(100*50*1.5t,H/L)","1.200 x 1.500 = 1.800","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CAFF39","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CAFF39",967]
["SSW02(100*50*1.5t,H/L)","4.600 x 2.100 = 9.660","EA",1,null,0,null,0,null,0,{"$f":"TRUNC(E647+G647+I647, 0)","v":0},0,null,"5769617FEB94D2E14997F1CAFF3B","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CAFF3B",968]
["SSW03(100*50*1.5t,H/L)","3.180 x 1.800 = 5.724","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CAFF3D","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CAFF3D",969]
["SSW04(100*50*1.5t,H/L)","4.000 x 1.600 = 6.400","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CAFF3F","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CAFF3F",970]
["SSW05(100*50*1.5t,H/L)","1.450 x 3.000 = 4.350","EA",4,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CAFF31","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CAFF31",971]
["T11(100*50*1.5t,H/L)","1.000 x 2.700 = 2.700","EA",98,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1CAFB5E","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145769617FEB94D2E14997F1CAFB5E",439]
["강화유리자동문","2.000 x 3.000, 양개형, 하드웨어포함","SET",2,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD7F39F539232D","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD7F39F539232D",505]
["강화유리폴딩도어","8.800 x 3.000, 8mm강화유리, 하드웨어포함","SET",2,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD78843D3CE6A6","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD78843D3CE6A6",507]
["복층유리폴딩도어","7.950 x 3.000, 16mm복층유리, 하드웨어포함","SET",4,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD78843D3FBAC5","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD78843D3FBAC5",991]
["배연창개폐기/개폐기","2CHAIN TYPE","SET",119,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD799365B57F55","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD799365B57F55",502]
["배연창개폐기/연동제어기","2CHAIN TYPE","EA",10,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD799365B60687","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD799365B60687",503]
["배연창개폐기/DC전원반","2CHAIN TYPE","EA",2,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD799365B72C9A","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD799365B72C9A",504]
["BUTT HINGE 4.5\"*4.0\"","BB1279 NRP","EA",162,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925C9485C0","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925C9485C0",460]
["BUTT HINGE 5.0\"*4.0\"","BB1279 NRP","EA",733,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925C94804E","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925C94804E",461]
["BUTT HINGE 4.5\"*4.0\"","BB1191 NRP","EA",24,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925C948DF6","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925C948DF6",462]
["BUTT HINGE 5.0\"*4.0\"","BB1191 NRP","EA",3,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925C975A45","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925C975A45",463]
["SPRING HINGE 4.5\"*4.0\"","1250","EA",126,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925C96B3CB","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925C96B3CB",464]
["PIVOT HINGE","H195","EA",6,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925C902A30","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925C902A30",465]
["INTERMEDIATE PIVOT","H19","EA",18,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925C93FFF4","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925C93FFF4",466]
["CONTINUOUS HINGE","780-112HD 95\"","EA",14,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925C93FA72","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925C93FA72",467]
["FLOOR HINGE","TSF-300A","EA",20,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925C92D89B","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925C92D89B",468]
["FLOOR HINGE","K-8300WP","EA",2,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925C9DE27A","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925C9DE27A",469]
["FLOOR HINGE","K-8500","EA",98,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925C9CDB68","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925C9CDB68",470]
["MORTISE LOCKSET/ENT","MCS-13-GALA","EA",22,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925F6B384E","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925F6B384E",471]
["MORTISE LOCKSET/CLA","MCS-05-GALA","EA",17,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925F6DE629","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925F6DE629",472]
["DUMMY TRIM","MCS-42-GALA","EA",17,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925F6F935E","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925F6F935E",473]
["LOCKSET/ENT","HC5081L","EA",141,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925F6E8DA3","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925F6E8DA3",474]
["LOCKSET/PRI","HC5076L","EA",8,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925F6135F1","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925F6135F1",475]
["LATCHSET/PASS","HC5075L","EA",7,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925F602EEF","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925F602EEF",476]
["DUMMY TRIM","HC50DT","EA",18,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925E430812","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925E430812",477]
["MORTISE DEAD LOCK","HI-DB300","EA",72,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925E415AF6","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925E415AF6",478]
["BOTTOM RAIL DEAD LOCK","HI-BL300","EA",108,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925E40B453","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925E40B453",479]
["MORTISE CYLINDER","TS-MC","EA",236,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925E46DCF0","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925E46DCF0",480]
["MORTISE THUMBTURN","HI-TT300","EA",180,null,{"$f":"TRUNC(E679*D679, 0)","v":0},null,{"$f":"TRUNC(G679*D679, 0)","v":0},null,{"$f":"TRUNC(I679*D679, 0)","v":0},{"$f":"TRUNC(E679+G679+I679, 0)","v":0},0,null,"57A02175D3A7D2A149393C1BCD79925E442F0C","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925E442F0C",481]
["DOOR CLOSER 일반형","TDC-40","EA",77,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925E4B5EBA","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925E4B5EBA",482]
["EXIT DEVICE","ED5500-08","EA",17,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD799259C1C858","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD799259C1C858",483]
["HANDLE","HI-S2690","EA",14,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD799259C02767","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD799259C02767",484]
["HANDLE","HI-F52","EA",100,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD799259C3FBC5","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD799259C3FBC5",485]
["HANDLE","HI-S51","EA",20,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD799259C2D4EB","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD799259C2D4EB",486]
["DOOR COORDINATOR","COR60FL20","EA",5,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD799259C48277","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD799259C48277",487]
["AUTO DOOR BOTTOM","420APKL 40\"","EA",10,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD799259C75696","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD799259C75696",488]
["AUTO DOOR BOTTOM","420APKL 50\"","EA",4,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD799259C903DB","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD799259C903DB",489]
["PUSH PULL PLATE","PP304-5","EA",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD799259C87D8F","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD799259C87D8F",490]
["FLUSH RING","HI-551","EA",136,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD7992583B4313","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD7992583B4313",491]
["INTEGRAL LATCH","HI-552","EA",5,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD799258388FDC","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD799258388FDC",492]
["FLUSH BOLT/UL","HI-282","EA",56,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD7992583D7027","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD7992583D7027",493]
["FLUSH BOLT/UL/L","HI-282L","EA",34,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD799258326658","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD799258326658",494]
["DUST PROOF STRIKE","HI-489","EA",153,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD799258330DD2","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD799258330DD2",495]
["FLOOR STOP","HI-410","EA",381,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925B8F4124","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925B8F4124",496]
["WALL BUMPER","HI-411","EA",8,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925B8C8DED","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925B8C8DED",497]
["KEY CABINET","HI-KCB300","EA",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCD79925B8D94FF","","","010114","F","F","T",{"$nulls":23},"","",null,"01011457A02175D3A7D2A149393C1BCD79925B8D94FF",498]
["도아록설치","강재문, 재료비 별도","개소",646,null,0,null,0,null,0,0,0,null,"5025E176D6EB7291406A69BAFF086E","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145025E176D6EB7291406A69BAFF086E",499]
["도아체크달기","재료비 별도","개소",77,null,0,null,0,null,0,0,0,null,"5025E176D6EB2211401C87684C375F","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145025E176D6EB2211401C87684C375F",500]
["플로어힌지설치","재료비 별도","개소",120,null,0,null,0,null,0,0,0,null,"5025E176D6DAF291496FFDE9BB150F","","","010114","T","F","F",{"$nulls":23},"","",null,"0101145025E176D6DAF291496FFDE9BB150F",501]
[]
[]
[]
[]
[]
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F551:F704)","v":0},null,{"$f":"SUM(H551:H704)","v":0},null,{"$f":"SUM(J551:J704)","v":0},null,{"$f":"SUM(L551:L704)","v":0},null,"TOTAL"]
["010115  유리공사",{"$nulls":15},"010115"]
["강화유리","투명, 10mm","M2",630.98,null,{"$f":"TRUNC(E707*D707, 0)","v":0},null,{"$f":"TRUNC(G707*D707, 0)","v":0},null,{"$f":"TRUNC(I707*D707, 0)","v":0},{"$f":"TRUNC(E707+G707+I707, 0)","v":0},0,null,"57008170BB2A22A1470A33F8368DA4F87F0EF6","","","010115","F","F","T",{"$nulls":23},"","",null,"01011557008170BB2A22A1470A33F8368DA4F87F0EF6",444]
["투명싱글로이복층유리(일면반강화)","24mm(6LOW-E+12Ar+6CL H/S)","M2",1137.51,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCE05E7DC422363","","","010115","F","F","T",{"$nulls":23},"","",null,"01011557A02175D3A7D2A149393C1BCE05E7DC422363",440]
["투명싱글로이복층유리(양면반강화)","24mm(6LOW-E H/S+12Ar+6CL H/S)","M2",85.9,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCE05E7DF168222","","","010115","F","F","T",{"$nulls":23},"","",null,"01011557A02175D3A7D2A149393C1BCE05E7DF168222",441]
["칼라싱글로이복층유리(일면반강화)","24mm(6LOW-E,Silver H/S+12Ar+6CL)","M2",2281.29,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCE05E7D8E7F244","","","010115","F","F","T",{"$nulls":23},"","",null,"01011557A02175D3A7D2A149393C1BCE05E7D8E7F244",442]
["칼라싱글로이복층유리(양면반강화)","24mm(6LOW-E,Silver H/S+12Ar+6CL H/S)","M2",2035.58,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCE05E7D8E2705A","","","010115","F","F","T",{"$nulls":23},"","",null,"01011557A02175D3A7D2A149393C1BCE05E7D8E2705A",443]
["칼라더블로이복층유리(일면반강화)","24mm(6LOW-E,Silver H/S+12Ar+6CL)","M2",173.31,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCE05E7D8E043B6","","","010115","F","F","T",{"$nulls":23},"","",null,"01011557A02175D3A7D2A149393C1BCE05E7D8E043B6",992]
["칼라더블로이복층유리(양면반강화)","24mm(6LOW-E,Silver H/S+12Ar+6CL H/S)","M2",91.92,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCE05E7D8EFC80C","","","010115","F","F","T",{"$nulls":23},"","",null,"01011557A02175D3A7D2A149393C1BCE05E7D8EFC80C",993]
["유리끼우고닦기-판유리","10mm 이상","M2",573.61,null,0,null,0,null,0,0,0,null,"5025E176C49582D1404A05536B34BB","","","010115","T","F","F",{"$nulls":23},"","",null,"0101155025E176C49582D1404A05536B34BB",445]
["유리끼우고닦기-복층유리, 커튼월","24mm(6+12A+6)","M2",5805.51,null,0,null,0,null,0,0,0,null,"5025E17636B072B14CBC9796752E42","","","010115","T","F","F",{"$nulls":23},"","",null,"0101155025E17636B072B14CBC9796752E42",447]
["유리주위코킹","5*5, 실리콘","M",2420.2800000000002,null,0,null,0,null,0,0,0,null,"5025A17D6CB3F2F14AB9171CDAA86A","","","010115","T","F","F",{"$nulls":23},"","",null,"0101155025A17D6CB3F2F14AB9171CDAA86A",448]
["유리접합코킹","10*10, 실리콘","M",245.4,null,0,null,0,null,0,0,0,null,"5025A17D6CB3A2714B7452C3CAF499","","","010115","T","F","F",{"$nulls":23},"","",null,"0101155025A17D6CB3A2714B7452C3CAF499",449]
["웨더코킹","10*16, 실리콘","M",18711.86,null,0,null,0,null,0,0,0,null,"5025A17D6CB3A2714B7452C3CAFE9C","","","010115","T","F","F",{"$nulls":23},"","",null,"0101155025A17D6CB3A2714B7452C3CAFE9C",451]
["구조용코킹","18*8, 실리콘","M",18711.86,null,0,null,0,null,0,0,0,null,"5025A17D6CB3A2714B7452C3CB829A","","","010115","T","F","F",{"$nulls":23},"","",null,"0101155025A17D6CB3A2714B7452C3CB829A",452]
["노턴테이프","10mm","M",18711.86,null,0,null,0,null,0,0,0,null,"5025A17D6CB3A2714B7452C3C9D0D3","","","010115","T","F","F",{"$nulls":23},"","",null,"0101155025A17D6CB3A2714B7452C3C9D0D3",450]
["샤워부스설치","2000*2100*10t,강화유리","EA",2,null,0,null,0,null,0,0,0,null,"5025E176241A82814C140814C48A61","","","010115","T","F","F",{"$nulls":23},"","",null,"0101155025E176241A82814C140814C48A61",706]
["샤워칸막이설치","450*1550*12t,강화유리,불투명","EA",16,null,0,null,0,null,0,0,0,null,"5025E176241A82814C140813259F0D","","","010115","T","F","F",{"$nulls":23},"","",null,"0101155025E176241A82814C140813259F0D",707]
["유리캐노피설치","2300*900*12.3mm,접합유리,틀포함","EA",3,null,0,null,0,null,0,0,0,null,"5025E176241A82814C14081ECBF55F","","","010115","T","F","F",{"$nulls":23},"","",null,"0101155025E176241A82814C14081ECBF55F",958]
["방습거울설치","5mm, 틀 포함","M2",49.07,null,0,null,0,null,0,0,0,null,"5025E176241A82814C14093F4B4CE4","","","010115","T","F","F",{"$nulls":23},"","",null,"0101155025E176241A82814C14093F4B4CE4",453]
["강화거울설치","5mm, 틀 포함","M2",56.7,null,0,null,0,null,0,0,0,null,"5025E176241A82814C14093F4AA502","","","010115","T","F","F",{"$nulls":23},"","",null,"0101155025E176241A82814C14093F4AA502",457]
["장애인경사거울설치","600*900mm","EA",8,null,0,null,0,null,0,0,0,null,"5025E176241A82814C14093F4D7A87","","","010115","T","F","F",{"$nulls":23},"","",null,"0101155025E176241A82814C14093F4D7A87",454]
["강화유리문(후레임포함)","12*800*2700mm, 투명, 세이프강화도어(고급형)","개",2,null,0,null,0,null,0,0,0,null,"57008170BB2A22A1455D617A0C37A2C81C426E","","","010115","F","F","T",{"$nulls":23},"","",null,"01011557008170BB2A22A1455D617A0C37A2C81C426E",708]
["강화유리문(후레임포함)","12*900*2700mm, 투명, 세이프강화도어(고급형)","개",79,null,0,null,0,null,0,0,0,null,"57008170BB2A22A1455D617A0C37A2C81F17E4","","","010115","F","F","T",{"$nulls":23},"","",null,"01011557008170BB2A22A1455D617A0C37A2C81F17E4",709]
["강화유리문(후레임포함)","12*900*3000mm, 투명, 세이프강화도어(고급형)","개",4,null,0,null,0,null,0,0,0,null,"57008170BB2A22A1455D617A0C37A2C81F1597","","","010115","F","F","T",{"$nulls":23},"","",null,"01011557008170BB2A22A1455D617A0C37A2C81F1597",710]
["강화유리문(후레임포함)","12*1000*2400mm, 투명, 세이프강화도어(고급형)","개",1,null,0,null,0,null,0,0,0,null,"57008170BB2A22A1455D617A0C37A2C8109176","","","010115","F","F","T",{"$nulls":23},"","",null,"01011557008170BB2A22A1455D617A0C37A2C8109176",458]
["강화유리문(후레임포함)","12*1000*2600mm, 투명, 세이프강화도어(고급형)","개",8,null,0,null,0,null,0,0,0,null,"57008170BB2A22A1455D617A0C37A2C81094BA","","","010115","F","F","T",{"$nulls":23},"","",null,"01011557008170BB2A22A1455D617A0C37A2C81094BA",960]
["강화유리문(후레임포함)","12*1000*2700mm, 투명, 세이프강화도어(고급형)","개",2,null,0,null,0,null,0,0,0,null,"57008170BB2A22A1455D617A0C37A2C77204D0","","","010115","F","F","T",{"$nulls":23},"","",null,"01011557008170BB2A22A1455D617A0C37A2C77204D0",459]
["강화유리문(후레임포함)","12*1000*3000mm, 투명, 세이프강화도어(고급형)","개",22,null,0,null,0,null,0,0,0,null,"57008170BB2A22A1455D617A0C37A2C77201AB","","","010115","F","F","T",{"$nulls":23},"","",null,"01011557008170BB2A22A1455D617A0C37A2C77201AB",711]
["강화유리문(후레임포함)","12*1000*3300mm, 투명, 세이프강화도어(고급형)","개",4,null,0,null,0,null,0,0,0,null,"57008170BB2A22A1455D617A0C37A2C77203F9","","","010115","F","F","T",{"$nulls":23},"","",null,"01011557008170BB2A22A1455D617A0C37A2C77203F9",712]
{"$rows_empty":22}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F707:F756)","v":0},null,{"$f":"SUM(H707:H756)","v":0},null,{"$f":"SUM(J707:J756)","v":0},null,{"$f":"SUM(L707:L756)","v":0},null,"TOTAL"]
["010116  도장공사",{"$nulls":15},"010116"]
["에폭시코팅","0.3mm","M2",1912.6,null,{"$f":"TRUNC(E759*D759, 0)","v":0},null,{"$f":"TRUNC(G759*D759, 0)","v":0},null,{"$f":"TRUNC(I759*D759, 0)","v":0},{"$f":"TRUNC(E759+G759+I759, 0)","v":0},0,null,"5025C171766DF291451C425206AD0F","","","010116","T","F","F",{"$nulls":23},"","",null,"0101165025C171766DF291451C425206AD0F",541]
["분진방지코팅","0.3mm","M2",7666.5,null,0,null,0,null,0,0,0,null,"5025A17D37CA12314D323F1D121E95","","","010116","T","F","F",{"$nulls":23},"","",null,"0101165025A17D37CA12314D323F1D121E95",542]
["안전페인트칠(붓칠)","2회. 2급","M2",43.2,null,0,null,0,null,0,0,0,null,"5025C1712E48427144B9C247868FF4","","","010116","T","F","F",{"$nulls":23},"","",null,"0101165025C1712E48427144B9C247868FF4",544]
["친환경수성페인트(로울러칠)","내벽 3회. 친환경","M2",11030.93,null,0,null,0,null,0,0,0,null,"5025C171E94852A145654C9D53445E","","","010116","T","F","F",{"$nulls":23},"","",null,"0101165025C171E94852A145654C9D53445E",545]
["친환경수성페인트(로울러칠)","내벽 3회. 친환경(GB면)","M2",5224.5,null,0,null,0,null,0,0,0,null,"5025C171E94852A145654C9A9FE5B1","","","010116","T","F","F",{"$nulls":23},"","",null,"0101165025C171E94852A145654C9A9FE5B1",546]
["친환경수성페인트(로울러칠)","내천장 3회. 친환경","M2",361.08,null,0,null,0,null,0,0,0,null,"5025C171E94852A14565467222B432","","","010116","T","F","F",{"$nulls":23},"","",null,"0101165025C171E94852A14565467222B432",547]
["친환경수성페인트(로울러칠)","내천장 3회. 친환경(GB면)","M2",3110.42,null,0,null,0,null,0,0,0,null,"5025C171E94852A1456546769D2463","","","010116","T","F","F",{"$nulls":23},"","",null,"0101165025C171E94852A1456546769D2463",548]
["친환경수성페인트(로울러칠)","외벽 3회. 친환경","M2",810.19,null,0,null,0,null,0,0,0,null,"5025C171E94852A1456549C620A643","","","010116","T","F","F",{"$nulls":23},"","",null,"0101165025C171E94852A1456549C620A643",549]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",422.54,null,0,null,0,null,0,0,0,null,"5025C171E94852A14F52C92BC8D977","","","010116","T","F","F",{"$nulls":23},"","",null,"0101165025C171E94852A14F52C92BC8D977",550]
["걸레받이용페인트칠","2회","M2",369.91,null,0,null,0,null,0,0,0,null,"5025C171FBF0A2514E57EE19DB6AF6","","","010116","T","F","F",{"$nulls":23},"","",null,"0101165025C171FBF0A2514E57EE19DB6AF6",551]
["걸레받이용페인트칠","2회(GB면)","M2",196.11,null,0,null,0,null,0,0,0,null,"5025C171FBF0A2514E57EE19DB6884","","","010116","T","F","F",{"$nulls":23},"","",null,"0101165025C171FBF0A2514E57EE19DB6884",555]
["주차표시페인트(융착식)","W:150(실선)","M",741.3,null,0,null,0,null,0,0,0,null,"5025C170D62892D14A73CB1FC47ADE","","","010116","T","F","F",{"$nulls":23},"","",null,"0101165025C170D62892D14A73CB1FC47ADE",552]
["주차표시페인트(융착식)","기호(방향표시)","개소",6,null,0,null,0,null,0,0,0,null,"5025C170D62892D14A73CB1FC7CED0","","","010116","T","F","F",{"$nulls":23},"","",null,"0101165025C170D62892D14A73CB1FC7CED0",553]
["주차표시페인트(융착식)","기호(장애인주차표시)","개소",4,null,0,null,0,null,0,0,0,null,"5025C170D62892D14A73CB1FC9FCD4","","","010116","T","F","F",{"$nulls":23},"","",null,"0101165025C170D62892D14A73CB1FC9FCD4",554]
{"$rows_empty":10}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F759:F782)","v":0},null,{"$f":"SUM(H759:H782)","v":0},null,{"$f":"SUM(J759:J782)","v":0},null,{"$f":"SUM(L759:L782)","v":0},null,"TOTAL"]
["010117  수장공사",{"$nulls":15},"010117"]
["석고보드","석고보드, 평보드, 9.5*900*2400mm(㎡)","M2",3385.96,null,{"$f":"TRUNC(E785*D785, 0)","v":0},null,{"$f":"TRUNC(G785*D785, 0)","v":0},null,{"$f":"TRUNC(I785*D785, 0)","v":0},{"$f":"TRUNC(E785+G785+I785, 0)","v":0},0,null,"57008170BB34B2D142D7F2681676436532D5A9","","","010117","F","F","T",{"$nulls":23},"","",null,"01011757008170BB34B2D142D7F2681676436532D5A9",639]
["석고보드","석고보드, 평보드, 방수, 9.5*900*2400mm(㎡)","M2",323.64999999999998,null,0,null,0,null,0,0,0,null,"57008170BB34B2D142D7F26BEA95BBEA54473F","","","010117","F","F","T",{"$nulls":23},"","",null,"01011757008170BB34B2D142D7F26BEA95BBEA54473F",640]
["불연천장재","6*300*600mm","M2",417.31,null,0,null,0,null,0,0,0,null,"57008170BB34B2D14130B0C7281E7E412B45BF","","","010117","F","F","T",{"$nulls":23},"","",null,"01011757008170BB34B2D14130B0C7281E7E412B45BF",713]
["불연천장재","12*300*600mm","M2",559.76,null,0,null,0,null,0,0,0,null,"57008170BB34B2D14130B0C7281E7E412B476A","","","010117","F","F","T",{"$nulls":23},"","",null,"01011757008170BB34B2D14130B0C7281E7E412B476A",714]
["불연천장재","15*600*600mm","M2",6890.43,null,0,null,0,null,0,0,0,null,"57008170BB34B2D14130B0C7281BA459BBF904","","","010117","F","F","T",{"$nulls":23},"","",null,"01011757008170BB34B2D14130B0C7281BA459BBF904",923]
["열경화성수지천장재","1.2*300*300mm, 틀포함","M2",149.87,null,0,null,0,null,0,0,0,null,"57008170BB34B2D14130B0C7281BA459BAD278","","","010117","F","F","T",{"$nulls":23},"","",null,"01011757008170BB34B2D14130B0C7281BA459BAD278",641]
["화장실칸막이","20mm, HPM","M2",215.06,null,0,null,0,null,0,0,0,null,"57008170BBD4C2514244F95DF995A43B6E7C0B","","","010117","F","F","T",{"$nulls":23},"","",null,"01011757008170BBD4C2514244F95DF995A43B6E7C0B",642]
["소변기칸막이","750*1100*12t","EA",8,null,0,null,0,null,0,0,0,null,"57008170BBD4C2514244F95DF995A43B6D5608","","","010117","F","F","T",{"$nulls":23},"","",null,"01011757008170BBD4C2514244F95DF995A43B6D5608",643]
["악세스후로아(STEEL PANEL/마감재별도)","600*600","M2",332.03,null,0,null,0,null,0,0,0,null,"5025D1705EEEA2614870CC0A0AE8B5","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D1705EEEA2614870CC0A0AE8B5",637]
["O.A후로아(무기질/마감재별도)","500*500mm","M2",7334.47,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCF2CF1A781979C","","","010117","F","F","T",{"$nulls":23},"","",null,"01011757A02175D3A7D2A149393C1BCF2CF1A781979C",854]
["악세스후로아(출입전실용계단)","W:1200*H:300*2단","개소",1,null,0,null,0,null,0,0,0,null,"57008170BB34B2D14028BDA7092D90980A9632","","","010117","F","F","T",{"$nulls":23},"","",null,"01011757008170BB34B2D14028BDA7092D90980A9632",720]
["악세스후로아(출입전실용경사로)","W:1200*L:1200기준","개소",1,null,0,null,0,null,0,0,0,null,"57008170BB34B2D14028BDA7092D90980A97D8","","","010117","F","F","T",{"$nulls":23},"","",null,"01011757008170BB34B2D14028BDA7092D90980A97D8",866]
["비닐무석면타일깔기","450*450*3.0mm","M2",1405.43,null,0,null,0,null,0,0,0,null,"5025D1705EEEA261491A0A3E3B31BA","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D1705EEEA261491A0A3E3B31BA",647]
["전도성타일깔기","600*600*3.0mm","M2",332.03,null,0,null,0,null,0,0,0,null,"5025D1705EEEA261491DDE5C1E4BD5","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D1705EEEA261491DDE5C1E4BD5",645]
["O.A전용타일깔기","500*500*5.0mm","M2",7334.47,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1BCF2CF1A782BD9F","","","010117","F","F","T",{"$nulls":23},"","",null,"01011757A02175D3A7D2A149393C1BCF2CF1A782BD9F",855]
["비닐시트깔기","2.0mm, 전면접합","M2",259.73,null,0,null,0,null,0,0,0,null,"5025D1705EEEA2614870CC0EFEE5E9","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D1705EEEA2614870CC0EFEE5E9",649]
["PVC탄성바닥재깔기","4.5mm, 전면접합","M2",247.05,null,0,null,0,null,0,0,0,null,"5025D1705EEEA2614870CC0EF97A2B","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D1705EEEA2614870CC0EF97A2B",722]
["타일카펫 깔기","500*500*7.0mm","M2",710.78,null,0,null,0,null,0,0,0,null,"5025D1705EEEA261491F8C3844BF53","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D1705EEEA261491F8C3844BF53",650]
["PVC걸레받이","H:100mm","M",159.07,null,0,null,0,null,0,0,0,null,"5025D1705EA722114D587CF8D3584D","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D1705EA722114D587CF8D3584D",721]
["벽지바름","지정실크벽지","M2",330.58,null,0,null,0,null,0,0,0,null,"5025D1706F4372A1437EC635EC008E","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D1706F4372A1437EC635EC008E",723]
["석고판본드붙임","천장, 일반 9.5mm","M2",3224.73,null,0,null,0,null,0,0,0,null,"5025D17079F192C14D8A986D440C3D","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D17079F192C14D8A986D440C3D",669]
["석고판본드붙임","천장, 방수 9.5mm","M2",308.24,null,0,null,0,null,0,0,0,null,"5025D17079F192C14E918BCB0161B4","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D17079F192C14E918BCB0161B4",671]
["DRY WALL(단열120t)/D1","일반12.5t*2겹,한면","M2",289.11,null,0,null,0,null,0,0,0,null,"5025D17079BA02914117A1441F4249","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D17079BA02914117A1441F4249",724]
["DRY WALL(C-100,단열50t)/D2","일반12.5t*2겹(양면)","M2",2671.18,null,0,null,0,null,0,0,0,null,"5025D17079BA02914117A1441EBB06","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D17079BA02914117A1441EBB06",725]
["DRY WALL(C-100)/D3","일반12.5t*2겹(양면)","M2",98.55,null,0,null,0,null,0,0,0,null,"5025D17079BA02914117A1441D942D","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D17079BA02914117A1441D942D",726]
["흡음뿜칠","퍼라이트, 뿜칠, 10mm","M2",4361.67,null,0,null,0,null,0,0,0,null,"57008170BB19D2714DB709C1971A9B0246D6D3","","","010117","F","F","T",{"$nulls":23},"","",null,"01011757008170BB19D2714DB709C1971A9B0246D6D3",718]
["석재뿜칠","램프벽체","M2",148.02000000000001,null,0,null,0,null,0,0,0,null,"57008170BB19D2714DB709C1971A9B0246D5FB","","","010117","F","F","T",{"$nulls":23},"","",null,"01011757008170BB19D2714DB709C1971A9B0246D5FB",956]
["경질우레탄폼단열재","50mm","M2",831.36,null,0,null,0,null,0,0,0,null,"57008170BB19D2714E4501166090F87F777F67","","","010117","F","F","T",{"$nulls":23},"","",null,"01011757008170BB19D2714E4501166090F87F777F67",961]
["압출스치로폼본드붙임/공조실패드주위","벽, 비중 0.035, 25mm","M2",26.24,null,0,null,0,null,0,0,0,null,"5025D17006CD32F144C4080DB8E36E","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D17006CD32F144C4080DB8E36E",962]
["압출스치로폼본드붙임/외벽","벽, 비중 0.035, 120mm","M2",6844.84,null,0,null,0,null,0,0,0,null,"5025D17006CD32F144C4080DB8E445","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D17006CD32F144C4080DB8E445",727]
["압출발포폴리스티렌깔기/최하층바닥","바닥, 비중 0.035, 100mm","M2",1561.19,null,0,null,0,null,0,0,0,null,"5025D17006CD12C14AA714F9FFD926","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D17006CD12C14AA714F9FFD926",728]
["유리면벽격자넣기","100mm, #48","M2",126.72,null,0,null,0,null,0,0,0,null,"5025D17006FA72514577ABFE73190D","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D17006FA72514577ABFE73190D",652]
["유리면천장틀사이넣기","100mm, #48","M2",71.52,null,0,null,0,null,0,0,0,null,"5025D170EC9692214F1C793722265C","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D170EC9692214F1C793722265C",651]
["방진고무패드깔기","25mm","M2",101.02,null,0,null,0,null,0,0,0,null,"5025D170799F12214F6508FDC0A20F","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D170799F12214F6508FDC0A20F",867]
["방진고무패드깔기","50mm","M2",15.84,null,0,null,0,null,0,0,0,null,"5025D170799F12214F6508FDC14999","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D170799F12214F6508FDC14999",657]
["유리면흡음판설치(벽)","100T+G/C","M2",784.52,null,0,null,0,null,0,0,0,null,"5025D170948742C14113AFE91FE61B","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D170948742C14113AFE91FE61B",661]
["유리면흡음판설치(천정)","100T+G/C","M2",410.82,null,0,null,0,null,0,0,0,null,"5025D170948742C14113AFE91D308A","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D170948742C14113AFE91D308A",660]
["착탈식흡음보드설치(벽)","25mm,패브릭","M2",83.4,null,0,null,0,null,0,0,0,null,"5025D170948742C14113AA667DC031","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D170948742C14113AA667DC031",729]
["패브릭흡음판설치(벽)","벽틀+합판9mm+MDF9mm,방염패브릭","M2",85.15,null,0,null,0,null,0,0,0,null,"5025D170948742C14113AA667F8D4E","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D170948742C14113AA667F8D4E",730]
["층간방화구획설치","1.2mm갈바+단열100mm+코킹","M",659.49,null,0,null,0,null,0,0,0,null,"5025D17006FA428142B591DA20D292","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D17006FA428142B591DA20D292",658]
["커텐월백패널설치","1.2mm갈바+단열100mm+0.8mm","M2",1477.43,null,0,null,0,null,0,0,0,null,"5025D17006FA428142B591D03E6326","","","010117","T","F","F",{"$nulls":23},"","",null,"0101175025D17006FA428142B591D03E6326",659]
{"$rows_empty":9}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F785:F834)","v":0},null,{"$f":"SUM(H785:H834)","v":0},null,{"$f":"SUM(J785:J834)","v":0},null,{"$f":"SUM(L785:L834)","v":0},null,"TOTAL"]
["010118  패널공사",{"$nulls":15},"010118"]
["접합스텐레스패널(돌출이음)","0.6t강판@530+2.0t방수시트+12t내수,틀포함","M2",43.79,null,{"$f":"TRUNC(E837*D837, 0)","v":0},null,{"$f":"TRUNC(G837*D837, 0)","v":0},null,{"$f":"TRUNC(I837*D837, 0)","v":0},{"$f":"TRUNC(E837+G837+I837, 0)","v":0},0,null,"57A02175D3A7D2A149393C191FC17DF7DF949F","","","010118","F","F","T",{"$nulls":23},"","",null,"01011857A02175D3A7D2A149393C191FC17DF7DF949F",677]
["접합스텐레스패널","1.5t,틀포함","M2",354.15,null,{"$f":"TRUNC(E838*D838, 0)","v":0},null,{"$f":"TRUNC(G838*D838, 0)","v":0},null,{"$f":"TRUNC(I838*D838, 0)","v":0},0,0,null,"57A02175D3A7D2A149393C191FC17DF7DCC071","","","010118","F","F","T",{"$nulls":23},"","",null,"01011857A02175D3A7D2A149393C191FC17DF7DCC071",678]
["알루미늄시트패널","평판,T=3.0,불소수지,틀포함","M2",195.06,null,{"$f":"TRUNC(E839*D839, 0)","v":0},null,{"$f":"TRUNC(G839*D839, 0)","v":0},null,{"$f":"TRUNC(I839*D839, 0)","v":0},0,0,null,"57008170BB0F7291403C4E5012F0315963F5A3","","","010118","F","F","T",{"$nulls":23},"","",null,"01011857008170BB0F7291403C4E5012F0315963F5A3",868]
["AL.수직루버","ㅁ-500*50,H=3800","EA",139,null,{"$f":"TRUNC(E840*D840, 0)","v":0},null,{"$f":"TRUNC(G840*D840, 0)","v":0},null,{"$f":"TRUNC(I840*D840, 0)","v":0},0,0,null,"57A02175D3A7D2A149393C191FC17DF7DDE673","","","010118","F","F","T",{"$nulls":23},"","",null,"01011857A02175D3A7D2A149393C191FC17DF7DDE673",716]
["AL.수직루버","ㅁ-500*50,H=4000","EA",51,null,{"$f":"TRUNC(E841*D841, 0)","v":0},null,{"$f":"TRUNC(G841*D841, 0)","v":0},null,{"$f":"TRUNC(I841*D841, 0)","v":0},0,0,null,"57A02175D3A7D2A149393C191FC17DF7DA1296","","","010118","F","F","T",{"$nulls":23},"","",null,"01011857A02175D3A7D2A149393C191FC17DF7DA1296",717]
{"$rows_empty":19}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F837:F860)","v":0},null,{"$f":"SUM(H837:H860)","v":0},null,{"$f":"SUM(J837:J860)","v":0},null,{"$f":"SUM(L837:L860)","v":0},null,"TOTAL"]
["010119  기타공사",{"$nulls":15},"010119"]
["승객용엘리베이터(MRL,장애인겸용,전망용)","17인승, 120m/min, 7/7Stop, 방화도어","대",4,null,{"$f":"TRUNC(E863*D863, 0)","v":0},null,{"$f":"TRUNC(G863*D863, 0)","v":0},null,{"$f":"TRUNC(I863*D863, 0)","v":0},{"$f":"TRUNC(E863+G863+I863, 0)","v":0},0,null,"57A02175D3A7D2A149393C13FF70534AE6E474","","","010119","F","F","T",{"$nulls":23},"","",null,"01011957A02175D3A7D2A149393C13FF70534AE6E474",341]
["승객용엘리베이터(MRL)","17인승, 105m/min, 7/7Stop, 방화도어","대",2,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C13FF70534AE78B8E","","","010119","F","F","T",{"$nulls":23},"","",null,"01011957A02175D3A7D2A149393C13FF70534AE78B8E",566]
["전동롤스크린","Fabric(방염),Motor,하드웨어포함","M2",632.79999999999995,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1DF8A302FC303CAA","","","010119","F","F","T",{"$nulls":23},"","",null,"01011957A02175D3A7D2A149393C1DF8A302FC303CAA",878]
["장애인대변기용손잡이","STS304 Ø38,1.5t(L형)","EA",14,null,0,null,0,null,0,0,0,null,"5024217AFA4EE2F14D5BB1FF10D13E","","","010119","T","F","F",{"$nulls":23},"","",null,"0101195024217AFA4EE2F14D5BB1FF10D13E",561]
["장애인대변기용손잡이","STS304 Ø38,1.5t(T형)","EA",14,null,0,null,0,null,0,0,0,null,"5024217AFA4EE2F14D5BB1FF10D559","","","010119","T","F","F",{"$nulls":23},"","",null,"0101195024217AFA4EE2F14D5BB1FF10D559",564]
["장애인소변기용손잡이","STS304 Ø38,1.5t","EA",12,null,0,null,0,null,0,0,0,null,"5024217AFA4EE2F14D5BB1FF10D6B0","","","010119","T","F","F",{"$nulls":23},"","",null,"0101195024217AFA4EE2F14D5BB1FF10D6B0",563]
["장애인세면대용손잡이","STS304 Ø38,1.5t","EA",16,null,0,null,0,null,0,0,0,null,"5024217AFA4EE2F14D5BB1FF10D9E4","","","010119","T","F","F",{"$nulls":23},"","",null,"0101195024217AFA4EE2F14D5BB1FF10D9E4",562]
["장애인핸드레일촉지판","AL120*Ø38,인쇄+점자타공","EA",66,null,0,null,0,null,0,0,0,null,"5024217AFA4EE2F14D5BB1FF13A55D","","","010119","T","F","F",{"$nulls":23},"","",null,"0101195024217AFA4EE2F14D5BB1FF13A55D",578]
["장애인용안내촉지판","배면인쇄+아크릴+점자렉산","EA",42,null,0,null,0,null,0,0,0,null,"5024217AFA4EE2F14D5BB1FF129B07","","","010119","T","F","F",{"$nulls":23},"","",null,"0101195024217AFA4EE2F14D5BB1FF129B07",579]
["장애인종합안내촉지도","스탠드형,음성유도기내장","EA",1,null,0,null,0,null,0,0,0,null,"5024217AFA4EE2F14D5BB1FF144CD7","","","010119","T","F","F",{"$nulls":23},"","",null,"0101195024217AFA4EE2F14D5BB1FF144CD7",582]
["장애인용주차안내표지판","700*600*1500mm,지주형","EA",7,null,0,null,0,null,0,0,0,null,"5024217AFA4EE2F14D5BB1FF17002E","","","010119","T","F","F",{"$nulls":23},"","",null,"0101195024217AFA4EE2F14D5BB1FF17002E",583]
["장애인용점자블럭/내부","300*300*18t,점형","EA",171,null,0,null,0,null,0,0,0,null,"5024217AFA4EE2F14D5BB1FF182285","","","010119","T","F","F",{"$nulls":23},"","",null,"0101195024217AFA4EE2F14D5BB1FF182285",587]
["실내용분리수거용기함","300*300*670(80L)","EA",42,null,0,null,0,null,0,0,0,null,"577B017C893562214CD548D07815CA9F6D6D38","","","010119","F","F","T",{"$nulls":23},"","",null,"010119577B017C893562214CD548D07815CA9F6D6D38",592]
["국기게양대설치(구체및화강석)","Ø100+80,H:10m3봉,4.2*1.2","개소",1,null,0,null,0,null,0,0,0,null,"50258178EBCFC2314474A03C81FEF3","","","010119","T","F","F",{"$nulls":23},"","",null,"01011950258178EBCFC2314474A03C81FEF3",957]
["차수판설치","W:8290*H:500","SET",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C1DF8A302FC33F020","","","010119","F","F","T",{"$nulls":23},"","",null,"01011957A02175D3A7D2A149393C1DF8A302FC33F020",877]
{"$rows_empty":9}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F863:F886)","v":0},null,{"$f":"SUM(H863:H886)","v":0},null,{"$f":"SUM(J863:J886)","v":0},null,{"$f":"SUM(L863:L886)","v":0},null,"TOTAL"]
["010120  주요자재비",{"$nulls":15},"010120"]
["시멘트[관급]","40kg/포","포",9717,null,{"$f":"TRUNC(E889*D889, 0)","v":0},null,{"$f":"TRUNC(G889*D889, 0)","v":0},null,{"$f":"TRUNC(I889*D889, 0)","v":0},{"$f":"TRUNC(E889+G889+I889, 0)","v":0},0,"관급별도","57008170BB45122144942348667942BB489565","","","010120","F","F","T",{"$nulls":23},"","",null,"01012057008170BB45122144942348667942BB489565",43]
["모래","도착도","M3",833.99,null,{"$f":"TRUNC(E890*D890, 0)","v":0},null,{"$f":"TRUNC(G890*D890, 0)","v":0},null,{"$f":"TRUNC(I890*D890, 0)","v":0},0,0,"","5723417597BB92514B1C916CC2E6C0FB9160D0","","","010120","F","F","T",{"$nulls":23},"","",null,"0101205723417597BB92514B1C916CC2E6C0FB9160D0",46]
["자갈","도착도, #57(25mm)","M3",12.52,null,{"$f":"TRUNC(E891*D891, 0)","v":0},null,{"$f":"TRUNC(G891*D891, 0)","v":0},null,{"$f":"TRUNC(I891*D891, 0)","v":0},0,0,"","5723417597BB92514A741EBC50E5EC39EFECB2","","","010120","F","F","T",{"$nulls":23},"","",null,"0101205723417597BB92514A741EBC50E5EC39EFECB2",47]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F889:F912)","v":0},null,{"$f":"SUM(H889:H912)","v":0},null,{"$f":"SUM(J889:J912)","v":0},null,{"$f":"SUM(L889:L912)","v":0},null,"TOTAL"]
["010121  운반비",{"$nulls":15},"010121"]
["시멘트운반","L:10km, 덤프8톤","포",9717,null,{"$f":"TRUNC(E915*D915, 0)","v":0},null,{"$f":"TRUNC(G915*D915, 0)","v":0},null,{"$f":"TRUNC(I915*D915, 0)","v":0},{"$f":"TRUNC(E915+G915+I915, 0)","v":0},0,null,"5024617C81ABC2614B77C2BFDFF89C","","","010121","F","T","F",{"$nulls":23},"","",null,"0101215024617C81ABC2614B77C2BFDFF89C",49]
["철근운반비","L:15km, 트레일러20톤","톤",2104,null,{"$f":"TRUNC(E916*D916, 0)","v":0},null,{"$f":"TRUNC(G916*D916, 0)","v":0},null,{"$f":"TRUNC(I916*D916, 0)","v":0},0,0,null,"5024617C81D70211426D6C29F837D3","","","010121","F","T","F",{"$nulls":23},"","",null,"0101215024617C81D70211426D6C29F837D3",52]
["철골운반비","L:30km, 트레일러20톤+크레인10톤","톤",103,null,{"$f":"TRUNC(E917*D917, 0)","v":0},null,{"$f":"TRUNC(G917*D917, 0)","v":0},null,{"$f":"TRUNC(I917*D917, 0)","v":0},0,0,null,"5024617C81D70211426D6C2BA3DAB2","","","010121","F","T","F",{"$nulls":23},"","",null,"0101215024617C81D70211426D6C2BA3DAB2",50]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F915:F938)","v":0},null,{"$f":"SUM(H915:H938)","v":0},null,{"$f":"SUM(J915:J938)","v":0},null,{"$f":"SUM(L915:L938)","v":0},null,"TOTAL"]
["010122  작업부산물",{"$nulls":15},"010122"]
["철강설(철근)","철강설, 고철, 작업설부산물","톤",-42.893999999999998,null,{"$f":"TRUNC(E941*D941, 0)","v":0},null,{"$f":"TRUNC(G941*D941, 0)","v":0},null,{"$f":"TRUNC(I941*D941, 0)","v":0},{"$f":"TRUNC(E941+G941+I941, 0)","v":0},{"$f":"TRUNC(F941+H941+J941, 0)","v":0},null,"57234175973632E14251503F831494CFA793F2","","","010122","F","F","T",{"$nulls":23},"","",null,"01012257234175973632E14251503F831494CFA793F2",44]
["철강설(철골)","철강설, 고철, 작업설부산물","톤",-5.0549999999999997,null,{"$f":"TRUNC(E942*D942, 0)","v":0},null,{"$f":"TRUNC(G942*D942, 0)","v":0},null,{"$f":"TRUNC(I942*D942, 0)","v":0},{"$f":"TRUNC(E942+G942+I942, 0)","v":0},{"$f":"TRUNC(F942+H942+J942, 0)","v":0},null,"57234175973632E14251503F831494CFA7938B","","","010122","F","F","T",{"$nulls":23},"","",null,"01012257234175973632E14251503F831494CFA7938B",45]
{"$rows_empty":22}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F941:F964)","v":0},null,{"$f":"SUM(H941:H964)","v":0},null,{"$f":"SUM(J941:J964)","v":0},null,{"$f":"SUM(L941:L964)","v":0},null,"TOTAL"]
["010123  관급자재비(도급자)"]
["레미콘","대전,세종,충남, 25-18-08","M3",387.57,null,{"$f":"TRUNC(E967*D967, 0)","v":0},null,{"$f":"TRUNC(G967*D967, 0)","v":0},null,{"$f":"TRUNC(I967*D967, 0)","v":0},{"$f":"TRUNC(E967+G967+I967, 0)","v":0},0]
["레미콘","대전,세종,충남, 25-21-15","M3",2746.18,null,0,null,0,null,0,0,0]
["레미콘","대전,세종,충남, 25-24-12","M3",5225.04,null,0,null,0,null,0,0,0]
["레미콘","대전,세종,충남, 25-24-15","M3",9103.6299999999992,null,0,null,0,null,0,0,0]
["레미콘","대전,세종,충남, 25-27-15","M3",2496.13,null,0,null,0,null,0,0,0]
["철근콘크리트용봉강","이형봉강(SD400), HD-10, 하치장상차도","톤",310.09300000000002,null,0,null,0,null,0,0,0]
["철근콘크리트용봉강","이형봉강(SD400), HD-13, 하치장상차도","톤",479.18299999999999,null,0,null,0,null,0,0,0]
["철근콘크리트용봉강","이형봉강(SD400), HD-16, 하치장상차도","톤",121.895,null,0,null,0,null,0,0,0]
["철근콘크리트용봉강","이형봉강(SD400), HD-19, 하치장상차도","톤",155.256,null,0,null,0,null,0,0,0]
["철근콘크리트용봉강","이형봉강(SD500), SH-22, 하치장상차도","톤",1037.425,null,0,null,0,null,0,0,0]
["시멘트","40kg/포, 하치장도","포",9717,null,0,null,0,null,0,0,0]
["덱플레이트","ED1A-5, 0.5mm, 상부근1-D10/하부근2-D7/래티스Φ5","M2",1379.55,null,0,null,0,null,0,0,0]
["덱플레이트","ED1A-6, 0.5mm, 상부근1-D10/하부근2-D7/래티스Φ6","M2",43.89,null,0,null,0,null,0,0,0]
["덱플레이트","ED3-5, 0.5mm, 상부근1-D13/하부근2-D8/래티스Φ5","M2",436.88,null,0,null,0,null,0,0,0]
["덱플레이트","ED3-6, 0.5mm, 상부근1-D13/하부근2-D8/래티스Φ6","M2",102.41,null,0,null,0,null,0,0,0]
["덱플레이트","ED4-5, 0.5mm, 상부근1-D13/하부근2-D10/래티스Φ5","M2",5549.66,null,0,null,0,null,0,0,0]
["덱플레이트","ED4-6, 0.5mm,상부근1-D13/하부근2-D10/래티스Φ6","M2",1005.31,null,0,null,0,null,0,0,0]
["덱플레이트","ED5-6, 0.5mm,상부근1-D13/하부근2-D13/래티스Φ6","M2",1254.6199999999999,null,0,null,0,null,0,0,0]
["덱플레이트","ND1A-5, 상부근1-D10/하부근2-D7/래티스Φ5","M2",591.53,null,0,null,0,null,0,0,0]
["덱플레이트","ND1A-6, 상부근1-D10/하부근2-D7/래티스Φ6","M2",479.45,null,0,null,0,null,0,0,0]
["덱플레이트","ND3-5, 상부근1-D13/하부근2-D8/래티스Φ5","M2",660.68,null,0,null,0,null,0,0,0]
["덱플레이트","ND3-6, 상부근1-D13/하부근2-D8/래티스Φ6","M2",759.07,null,0,null,0,null,0,0,0]
["덱플레이트","ND4-5, 상부근1-D13/하부근2-D10/래티스Φ5","M2",1122.31,null,0,null,0,null,0,0,0]
["덱플레이트","ND4-6, 상부근1-D13/하부근2-D10/래티스Φ6","M2",624.11,null,0,null,0,null,0,0,0]
["덱플레이트","ND5-5, 상부근1-D13/하부근2-D13/래티스Φ5","M2",1413.02,null,0,null,0,null,0,0,0]
["덱플레이트","ND5-6, 상부근1-D13/하부근2-D13/래티스Φ6","M2",1553.94,null,0,null,0,null,0,0,0]
["덱플레이트/압출법보온판","비중0.035,100mm","M2",1323.7,null,0,null,0,null,0,0,0]
["덱플레이트/압출법보온판","비중0.035,150mm","M2",1620.52,null,0,null,0,null,0,0,0]
["덱플레이트/압출법보온판","비중0.035,180mm","M2",4643.1499999999996,null,0,null,0,null,0,0,0]
["콘크리트벽돌","190*57*90mm, C종2급","매",517187,null,0,null,0,null,0,0,0]
["속빈콘크리트블록","100*190*390mm","매",3335,null,0,null,0,null,0,0,0]
["속빈콘크리트블록","150*190*390mm","매",5763,null,0,null,0,null,0,0,0]
["속빈콘크리트블록","190*190*390mm","매",60197,null,0,null,0,null,0,0,0]
["자연석판석","수마, 30mm, 고흥석","M2",9.24,null,0,null,0,null,0,0,0]
["자연석판석","버너, 30mm, 고흥석","M2",3087.34,null,0,null,0,null,0,0,0]
["자연석판석","잔다듬, 30mm, 고흥석","M2",4994.66,null,0,null,0,null,0,0,0]
["자연석판석","혼드, 30mm, 거창석","M2",914.5,null,0,null,0,null,0,0,0]
["자연석판석","잔다듬, 30mm, 거창석","M2",2091.94,null,0,null,0,null,0,0,0]
["도기질타일","300*600*7mm","M2",1410.89,null,0,null,0,null,0,0,0]
["자기질타일(논슬립)","300*300*7mm","M2",435.61,null,0,null,0,null,0,0,0]
["자기질타일(석재타일)","200*200*15mm","M2",12.78,null,0,null,0,null,0,0,0]
["합성목재데크","20mm*140mm","M2",213.71,null,0,null,0,null,0,0,0]
{"$rows_empty":8}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F967:F1016)","v":0},null,{"$f":"SUM(H967:H1016)","v":0},null,{"$f":"SUM(J967:J1016)","v":0},null,{"$f":"SUM(L967:L1016)","v":0},null,"TOTAL"]
["010124  관급자재비(관급자)",{"$nulls":15},"010124"]
["1. 알루미늄커튼월","","",null,null,{"$f":"TRUNC(E1019*D1019, 0)","v":0},null,{"$f":"TRUNC(G1019*D1019, 0)","v":0},null,{"$f":"TRUNC(I1019*D1019, 0)","v":0},{"$f":"TRUNC(E1019+G1019+I1019, 0)","v":0},0,"","5198C172B06282714E04DB22BCC12F956BDCDB","","","010124","F","F","T",{"$nulls":23},"","",null,"0101245198C172B06282714E04DB22BCC12F956BDCDB",978]
["AG01(AL.갤러리,PVDF2)","2.450 x 2.200 = 5.390(76.1kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D82E","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D82E",286]
["AG02(AL.갤러리,PVDF2)","2.250 x 2.200 = 4.950(65.9kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D82D","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D82D",287]
["AG03(AL.갤러리,PVDF2)","1.100 x 3.000 = 3.300(44.9kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D82C","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D82C",288]
["AG04(AL.갤러리,PVDF2)","2.000 x 3.040 = 6.080(80.0kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D82B","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D82B",289]
["AG05(AL.갤러리,PVDF2)","2.700 x 3.040 = 8.208(108.7kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D82A","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D82A",290]
["AG06(AL.갤러리,PVDF2)","1.450 x 2.345 = 3.400(50.5kg)","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D829","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D829",291]
["AG07(AL.갤러리,PVDF2)","1.650 x 2.345 = 3.869(55.3kg)","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D828","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D828",292]
["AG08(AL.갤러리,PVDF2)","2.400 x 2.000 = 4.800(63.9kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D827","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D827",293]
["AG09(AL.갤러리,PVDF2)","2.700 x 3.000 = 8.100(71.5kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D826","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D826",294]
["AD01(AL,단열창,PVDF2,시스템도어)","1.000 x 2.300 = 2.300(132.1kg)","EA",3,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D937","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D937",972]
["AD02(AL,단열창,PVDF2,시스템도어)","2.150 x 3.000 = 6.450(179.7kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D934","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D934",973]
["AD03(AL,단열창,PVDF2,시스템도어)","2.350 x 3.000 = 7.050(183.2kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D935","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D935",974]
["AD04(AL,단열창,PVDF2,시스템도어)","2.150 x 3.000 = 6.450(179.7kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D932","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D932",975]
["AD05(AL,단열창,PVDF2,시스템도어)","2.150 x 3.000 = 6.450(179.7kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D930","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D930",976]
["AD06(AL,단열창,PVDF2,시스템도어)","1.650 x 3.000 = 4.950(156.07kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D931","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D931",988]
["AW01(AL,단열창,PVDF2,롤방충망)","2.400 x 3.800 = 9.120(145.8kg)","EA",66,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D93F","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D93F",295]
["AW02(AL,단열창,PVDF2,롤방충망)","2.400 x 4.000 = 9.600(149.7kg)","EA",24,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DADC","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DADC",296]
["AW03(AL,단열창,PVDF2,롤방충망)","2.400 x 3.800 = 9.120(145.8kg)","EA",73,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DADE","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DADE",297]
["AW04(AL,단열창,PVDF2,롤방충망)","2.400 x 4.000 = 9.600(149.7kg)","EA",27,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DAD8","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DAD8",298]
["AW05(AL,단열창,PVDF2,롤방충망)","1.500 x 2.400 = 3.600(69.5kg)","EA",4,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DADA","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DADA",299]
["AW06A(AL,단열창,PVDF2,롤방충망)","1.100 x 2.400 = 2.640(51.0kg)","EA",19,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DAD4","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DAD4",300]
["AW06B(AL,단열창,PVDF2,롤방충망)","1.100 x 2.400 = 2.640(51.0kg)","EA",8,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DBE4","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DBE4",879]
["AW07(AL,단열창,PVDF2,롤방충망)","1.100 x 3.000 = 3.300(55.6kg)","EA",5,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DBE5","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DBE5",301]
["AW08(AL,단열창,PVDF2,롤방충망)","1.100 x 3.000 = 3.300(55.6kg)","EA",8,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DBE7","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DBE7",302]
["AW09(AL,단열창,PVDF2,롤방충망)","1.450 x 1.520 = 2.204(65.5kg)","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DBE1","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DBE1",303]
["AW10(AL,단열창,PVDF2)","0.725 x 1.140 = 0.826(14.3kg)","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DBE3","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DBE3",304]
["AW11(AL,단열창,PVDF2)","1.100 x 1.140 = 1.254(17.1kg)","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DBED","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DBED",305]
["AW12(AL,단열창,PVDF2,롤방충망)","9.900 x 1.200 = 11.880(422.6kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DC8B","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DC8B",306]
["AW13(AL,단열창,PVDF2,롤방충망)","9.900 x 1.200 = 11.880(422.6kg)","EA",2,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DC89","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DC89",307]
["AW14(AL,단열창,PVDF2,롤방충망)","5.550 x 1.800 = 9.990(375.8kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DC8F","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DC8F",308]
["AW15(AL,단열창,PVDF2,롤방충망)","2.550 x 1.800 = 4.590(140.0kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DC8D","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DC8D",309]
["AW16(AL,단열창,PVDF2,롤방충망)","1.650 x 1.520 = 2.508(114.5kg)","EA",14,null,0,null,0,null,0,{"$f":"TRUNC(E1051+G1051+I1051, 0)","v":0},0,null,"5769617FEB94D2E14997F1C9DC83","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DC83",310]
["AW17(AL,단열창,PVDF2,롤방충망)","1.650 x 1.520 = 2.508(114.5kg)","EA",5,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DD90","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DD90",311]
["AW18(AL,단열창,PVDF2,롤방충망)","4.950 x 1.520 = 7.524(321.3kg)","EA",3,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DD92","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DD92",312]
["AW19(AL,단열창,PVDF2,롤방충망)","4.950 x 1.520 = 7.524(321.3kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DD94","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DD94",313]
["AW20(AL,단열창,PVDF2,롤방충망)","7.890 x 1.520 = 11.992(495.2kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DD96","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DD96",314]
["AW21(AL,단열창,PVDF2,롤방충망)","7.890 x 1.520 = 11.992(495.2kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DD98","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DD98",315]
["AW22(AL,단열창,PVDF2,롤방충망)","7.890 x 1.520 = 11.992(495.2kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DEB9","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DEB9",316]
["AW23(AL,단열창,PVDF2,시스템도어,롤방충망)","8.330 x 3.000 = 24.990(456.7kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DEBD","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DEBD",318]
["AW25(AL,단열창,PVDF2)","8.980 x 5.700 = 51.186(402.3kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DF5A","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DF5A",323]
["AW26(AL,단열창,PVDF2,롤방충망)","1.450 x 5.900 = 8.555(345.4kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DF58","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DF58",324]
["AW27(AL,단열창,PVDF2,롤방충망)","1.450 x 5.900 = 8.555(345.4kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9DF56","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9DF56",325]
["CW01(AL,단열창,PVDF2,롤방충망)","A=387.441(4442.1kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D0D8","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D0D8",326]
["CW02(AL,단열창,PVDF2,시스템도어,롤방충망)","24.680 x 7.800 = 192.504(4500.6kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D0DA","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D0DA",327]
["CW03(AL,단열창,PVDF2,시스템도어,롤방충망)","45.430 x 3.600 = 163.548(2999.1kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D0DC","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D0DC",328]
["CW04(AL,단열창,PVDF2,시스템도어,롤방충망)","A=399.764(3566.0kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D0DE","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D0DE",329]
["CW05(AL,단열창,PVDF2,시스템도어,롤방충망)","9.180 x 3.200 = 29.376(642.5kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D0D0","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D0D0",330]
["CW06(AL,단열창,PVDF2,시스템도어,롤방충망)","A=68.646(1291.0kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D1E1","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D1E1",331]
["CW07(AL,단열창,PVDF2,롤방충망)","14.455 x 13.600 = 196.588(2279.6kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D1E3","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D1E3",332]
["CW08(AL,단열창,PVDF2,시스템도어,롤방충망)","A=746.765(10453.0kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D1E5","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D1E5",333]
["CW09(AL,단열창,PVDF2,시스템도어,롤방충망)","A=746.765(10005.7kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D1E7","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D1E7",334]
["CW10(AL,단열창,PVDF2,롤방충망)","17.514 x 5.300 = 92.824(1211.2kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C9D1E9","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C9D1E9",335]
["CW11(AL,단열창,PVDF2,롤방충망)","17.514 x 5.300 = 92.824(1211.2kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C831E7","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C831E7",336]
["CW12(AL,단열창,PVDF2)","4.680 x 9.600 = 44.928(492.8kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C831E5","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C831E5",337]
["CW13(AL,단열창,PVDF2,롤방충망)","9.820 x 14.800 = 145.336(2135.4kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C831E3","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C831E3",338]
["CW14(AL,단열창,PVDF2,롤방충망)","7.900 x 14.800 = 116.920(1767.8kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C831E1","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C831E1",339]
["CW15(AL,단열창,PVDF2,롤방충망)","10.100 x 14.800 = 149.480(2160.7kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C831EF","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C831EF",340]
["CW16(AL,단열창,PVDF2,롤방충망)","7.900 x 14.800 = 116.920(1767.8kg)","EA",1,null,0,null,0,null,0,0,0,null,"5769617FEB94D2E14997F1C830C1","","","010124","T","F","F",{"$nulls":23},"","",null,"0101245769617FEB94D2E14997F1C830C1",565]
["소    계","","",null,null,{"$f":"SUM(F1019:F1077)","v":0},null,{"$f":"SUM(H1019:H1077)","v":0},null,{"$f":"SUM(J1019:J1077)","v":0},null,{"$f":"SUM(L1019:L1077)","v":0},null,"5199717519F3E2414AB780AE71F3","","","","F","F","F",{"$nulls":23},"","",null,"0101245199717519F3E2414AB780AE71F3",979]
["2. 스틸커튼월","","",null,null,{"$f":"TRUNC(E1079*D1079, 0)","v":0},null,{"$f":"TRUNC(G1079*D1079, 0)","v":0},null,{"$f":"TRUNC(I1079*D1079, 0)","v":0},{"$f":"TRUNC(E1079+G1079+I1079, 0)","v":0},0,null,"5198C172B06282714E04DB22BCC12F956BDCDA","","","010124","F","F","T",{"$nulls":23},"","",null,"0101245198C172B06282714E04DB22BCC12F956BDCDA",980]
["SCW01(STEEL.단열창)","19.860 x 8.100 = 160.866(4928.0kg)","EA",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C13FF7050F6A4C904","","","010124","F","F","T",null,null,null,1,{"$nulls":19},"","",null,"01012457A02175D3A7D2A149393C13FF7050F6A4C904",981]
["SCW02(STEEL.단열창)","38.730 x 8.400 = 325.332(8292.0kg)","EA",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C13FF7050F6A79DA2","","","010124","F","F","T",null,null,null,1,{"$nulls":19},"","",null,"01012457A02175D3A7D2A149393C13FF7050F6A79DA2",982]
["SCW03(STEEL.단열창)","9.930 x 17.800 = 176.754(5431.0kg)","EA",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C13FF7050F6A6F628","","","010124","F","F","T",null,null,null,1,{"$nulls":19},"","",null,"01012457A02175D3A7D2A149393C13FF7050F6A6F628",983]
["SCW04(STEEL.단열창)","9.930 x 17.800 = 176.754(5401.0kg)","EA",1,null,0,null,0,null,0,0,0,null,"57A02175D3A7D2A149393C13FF7050F6A17505","","","010124","F","F","T",null,null,null,1,{"$nulls":19},"","",null,"01012457A02175D3A7D2A149393C13FF7050F6A17505",984]
["부가가치세","합계의 10%","식",1,null,0,null,0,null,0,0,0,null,"51335177232932214EEDED8E8C731","","","010124","F","F","F",3,0,0.1,{"$nulls":20},"","",null,"01012451335177232932214EEDED8E8C731",987]
["소    계","","",null,null,{"$f":"SUM(F1079:F1084)","v":0},null,{"$f":"SUM(H1079:H1084)","v":0},null,{"$f":"SUM(J1079:J1084)","v":0},null,{"$f":"SUM(L1079:L1084)","v":0},"","5199717519F3E2414AB780AE71F3","","","","F","F","F",{"$nulls":23},"","",null,"0101245199717519F3E2414AB780AE71F3",985]
{"$rows_empty":9}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1019:F1094) -F1078-F1085","v":0},null,{"$f":"SUM(H1019:H1094) -H1078-H1085","v":0},null,{"$f":"SUM(J1019:J1094) -J1078-J1085","v":0},null,{"$f":"SUM(L1019:L1094) -L1078-L1085","v":0},null,"TOTAL"]

{"sheet":"인테리어집계","index":2,"n_rows":165,"n_cols":20,"rows_kept":165,"cut":false,"hidden":false,"merged":[[2,18,3,18],[2,19,3,19],[2,12,3,12],[2,13,3,13],[2,14,3,14],[2,15,3,15],[2,16,3,16],[2,17,3,17],[0,0,0,12],[1,0,1,12],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,2,5],[2,6,2,7],[2,8,2,9],[2,10,2,11]]}
["공 종 별 집 계 표"]
["[ 국토연구원 인테리어공사 ]"]
["품      명","규      격","단위","수량","재  료  비",null,"노  무  비",null,"경      비",null,"합      계",null,"비  고","공종코드","변수","상위공종","공종구분","공종레벨","공종소계","원가계산서 연결금액"]
[{"$nulls":4},"단  가","금  액","단  가","금  액","단  가","금  액","단  가","금  액"]
["01  국토연구원 인테리어공사","","",1,{"$f":"F6+F146","v":0},{"$f":"E5*D5","v":0},{"$f":"H6+H146","v":0},{"$f":"G5*D5","v":0},{"$f":"J6+J146","v":0},{"$f":"I5*D5","v":0},{"$f":"E5+G5+I5","v":0},0,"","01","","","",1,""]
["0101  ■ 인테리어공사","","",1,{"$f":"F7+F40+F88+F145","v":0},0,{"$f":"H7+H40+H88+H145","v":0},0,{"$f":"J7+J40+J88+J145","v":0},0,0,0,"","0101","","01","",2,""]
["010101  ▶ 지상1층","","",1,{"$f":"F8+F13+F18+F22+F26+F31+F36","v":0},0,{"$f":"H8+H13+H18+H22+H26+H31+H36","v":0},0,{"$f":"J8+J13+J18+J22+J26+J31+J36","v":0},0,0,0,"","010101","","0101","",3,""]
["01010101  실명 : 101.로비     개소 :1","","",1,{"$f":"F9+F10+F11+F12","v":0},0,{"$f":"H9+H10+H11+H12","v":0},0,{"$f":"J9+J10+J11+J12","v":0},0,0,0,"","01010101","","010101","",4,""]
["0101010101  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010101","","01010101","",5,""]
["0101010102  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101010102","","01010101","",5,""]
["0101010103  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010103","","01010101","",5,""]
["0101010104  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010104","","01010101","",5,""]
["01010102  실명 : 102a.직원식당     개소 :1","","",1,{"$f":"F14+F15+F16+F17","v":0},0,{"$f":"H14+H15+H16+H17","v":0},0,{"$f":"J14+J15+J16+J17","v":0},0,0,0,"","01010102","","010101","",4,""]
["0101010201  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010201","","01010102","",5,""]
["0101010202  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101010202","","01010102","",5,""]
["0101010203  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010203","","01010102","",5,""]
["0101010204  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010204","","01010102","",5,""]
["01010103  실명 : 102b.직원식당방풍실     개소 :1","","",1,{"$f":"F19+F20+F21","v":0},0,{"$f":"H19+H20+H21","v":0},0,{"$f":"J19+J20+J21","v":0},0,0,0,"","01010103","","010101","",4,""]
["0101010301  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010301","","01010103","",5,""]
["0101010302  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101010302","","01010103","",5,""]
["0101010303  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010303","","01010103","",5,""]
["01010104  실명 : 103.PDR ROOM     개소 :1","","",1,{"$f":"F23+F24+F25","v":0},0,{"$f":"H23+H24+H25","v":0},0,{"$f":"J23+J24+J25","v":0},0,0,0,"","01010104","","010101","",4,""]
["0101010401  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010401","","01010104","",5,""]
["0101010402  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101010402","","01010104","",5,""]
["0101010403  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010403","","01010104","",5,""]
["01010105  실명 : 104.공용화장실(남)     개소 :1","","",1,{"$f":"F27+F28+F29+F30","v":0},0,{"$f":"H27+H28+H29+H30","v":0},0,{"$f":"J27+J28+J29+J30","v":0},0,0,0,"","01010105","","010101","",4,""]
["0101010501  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010501","","01010105","",5,""]
["0101010502  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101010502","","01010105","",5,""]
["0101010503  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010503","","01010105","",5,""]
["0101010504  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010504","","01010105","",5,""]
["01010106  실명 : 105.공용화장실(여)     개소 :1","","",1,{"$f":"F32+F33+F34+F35","v":0},0,{"$f":"H32+H33+H34+H35","v":0},0,{"$f":"J32+J33+J34+J35","v":0},0,0,0,"","01010106","","010101","",4,""]
["0101010601  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010601","","01010106","",5,""]
["0101010602  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101010602","","01010106","",5,""]
["0101010603  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010603","","01010106","",5,""]
["0101010604  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010604","","01010106","",5,""]
["01010107  실명 : 106.청소도구함     개소 :1","","",1,{"$f":"F37+F38+F39","v":0},0,{"$f":"H37+H38+H39","v":0},0,{"$f":"J37+J38+J39","v":0},0,0,0,"","01010107","","010101","",4,""]
["0101010701  바  닥  공  사","","",1,0,0,0,0,0,0,{"$f":"E37+G37+I37","v":0},0,"","0101010701","","01010107","",5,""]
["0101010702  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101010702","","01010107","",5,""]
["0101010703  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101010703","","01010107","",5,""]
["010102  ▶ 지상2층","","",1,{"$f":"F41+F47+F52+F54+F56+F61+F66+F70+F74+F79+F84","v":0},0,{"$f":"H41+H47+H52+H54+H56+H61+H66+H70+H74+H79+H84","v":0},0,{"$f":"J41+J47+J52+J54+J56+J61+J66+J70+J74+J79+J84","v":0},0,0,0,"","010102","","0101","",3,""]
["01010201  실명 : 201.로비     개소 :1","","",1,{"$f":"F42+F43+F44+F45+F46","v":0},0,{"$f":"H42+H43+H44+H45+H46","v":0},0,{"$f":"J42+J43+J44+J45+J46","v":0},0,0,0,"","01010201","","010102","",4,""]
["0101020101  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020101","","01010201","",5,""]
["0101020102  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101020102","","01010201","",5,""]
["0101020103  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020103","","01010201","",5,""]
["0101020104  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020104","","01010201","",5,""]
["0101020105  미 팅 박 스 공 사","","",1,0,0,0,0,0,0,0,0,"","0101020105","","01010201","",5,""]
["01010202  실명 : 202.대강당     개소 :1","","",1,{"$f":"F48+F49+F50+F51","v":0},0,{"$f":"H48+H49+H50+H51","v":0},0,{"$f":"J48+J49+J50+J51","v":0},0,0,0,"","01010202","","010102","",4,""]
["0101020201  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020201","","01010202","",5,""]
["0101020202  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101020202","","01010202","",5,""]
["0101020203  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020203","","01010202","",5,""]
["0101020204  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020204","","01010202","",5,""]
["01010203  실명 : 202d.준비실-1    개소:1","","",1,{"$f":"F53","v":0},0,{"$f":"H53","v":0},0,{"$f":"J53","v":0},0,0,0,"","01010203","","010102","",4,""]
["0101020301  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020301","","01010203","",5,""]
["01010204  실명 : 202e.준비실-2    개소:1","","",1,{"$f":"F55","v":0},0,{"$f":"H55","v":0},0,{"$f":"J55","v":0},0,0,0,"","01010204","","010102","",4,""]
["0101020401  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020401","","01010204","",5,""]
["01010205  실명 : 202f.대강당화장실(남)     개소 :1","","",1,{"$f":"F57+F58+F59+F60","v":0},0,{"$f":"H57+H58+H59+H60","v":0},0,{"$f":"J57+J58+J59+J60","v":0},0,0,0,"","01010205","","010102","",4,""]
["0101020501  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020501","","01010205","",5,""]
["0101020502  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101020502","","01010205","",5,""]
["0101020503  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020503","","01010205","",5,""]
["0101020504  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020504","","01010205","",5,""]
["01010206  실명 : 202f.대강당화장실(여)     개소 :1","","",1,{"$f":"F62+F63+F64+F65","v":0},0,{"$f":"H62+H63+H64+H65","v":0},0,{"$f":"J62+J63+J64+J65","v":0},0,0,0,"","01010206","","010102","",4,""]
["0101020601  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020601","","01010206","",5,""]
["0101020602  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101020602","","01010206","",5,""]
["0101020603  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020603","","01010206","",5,""]
["0101020604  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020604","","01010206","",5,""]
["01010207  실명 : 203.전실-1(대강당)     개소 :1","","",1,{"$f":"F67+F68+F69","v":0},0,{"$f":"H67+H68+H69","v":0},0,{"$f":"J67+J68+J69","v":0},0,0,0,"","01010207","","010102","",4,""]
["0101020701  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020701","","01010207","",5,""]
["0101020702  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101020702","","01010207","",5,""]
["0101020703  천  장  공  사","","",1,0,{"$f":"E69*D69","v":0},0,{"$f":"G69*D69","v":0},0,{"$f":"I69*D69","v":0},{"$f":"E69+G69+I69","v":0},0,"","0101020703","","01010207","",5,""]
["01010208  실명 : 204.전실-2(대강당)     개소 :1","","",1,{"$f":"F71+F72+F73","v":0},0,{"$f":"H71+H72+H73","v":0},0,{"$f":"J71+J72+J73","v":0},0,0,0,"","01010208","","010102","",4,""]
["0101020801  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020801","","01010208","",5,""]
["0101020802  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101020802","","01010208","",5,""]
["0101020803  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020803","","01010208","",5,""]
["01010209  실명 : 205.공용화장실(남)     개소 :1","","",1,{"$f":"F75+F76+F77+F78","v":0},0,{"$f":"H75+H76+H77+H78","v":0},0,{"$f":"J75+J76+J77+J78","v":0},0,0,0,"","01010209","","010102","",4,""]
["0101020901  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020901","","01010209","",5,""]
["0101020902  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101020902","","01010209","",5,""]
["0101020903  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020903","","01010209","",5,""]
["0101020904  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101020904","","01010209","",5,""]
["01010210  실명 : 206.공용화장실(여)     개소 :1","","",1,{"$f":"F80+F81+F82+F83","v":0},0,{"$f":"H80+H81+H82+H83","v":0},0,{"$f":"J80+J81+J82+J83","v":0},0,0,0,"","01010210","","010102","",4,""]
["0101021001  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101021001","","01010210","",5,""]
["0101021002  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101021002","","01010210","",5,""]
["0101021003  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101021003","","01010210","",5,""]
["0101021004  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101021004","","01010210","",5,""]
["01010211  실명 : 207.청소도구함     개소 :1","","",1,{"$f":"F85+F86+F87","v":0},0,{"$f":"H85+H86+H87","v":0},0,{"$f":"J85+J86+J87","v":0},0,0,0,"","01010211","","010102","",4,""]
["0101021101  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101021101","","01010211","",5,""]
["0101021102  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101021102","","01010211","",5,""]
["0101021103  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101021103","","01010211","",5,""]
["010103  ▶ 지상3층","","",1,{"$f":"F89+F93+F98+F103+F108+F112+F117+F122+F127+F131+F136+F141","v":0},0,{"$f":"H89+H93+H98+H103+H108+H112+H117+H122+H127+H131+H136+H141","v":0},0,{"$f":"J89+J93+J98+J103+J108+J112+J117+J122+J127+J131+J136+J141","v":0},0,0,0,"","010103","","0101","",3,""]
["01010301  실명 : 301.로비     개소 :1","","",1,{"$f":"F90+F91+F92","v":0},0,{"$f":"H90+H91+H92","v":0},0,{"$f":"J90+J91+J92","v":0},0,0,0,"","01010301","","010103","",4,""]
["0101030101  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030101","","01010301","",5,""]
["0101030102  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101030102","","01010301","",5,""]
["0101030103  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030103","","01010301","",5,""]
["01010302  실명 : 302.원장실     개소 :1","","",1,{"$f":"F94+F95+F96+F97","v":0},0,{"$f":"H94+H95+H96+H97","v":0},0,{"$f":"J94+J95+J96+J97","v":0},0,0,0,"","01010302","","010103","",4,""]
["0101030201  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030201","","01010302","",5,""]
["0101030202  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101030202","","01010302","",5,""]
["0101030203  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030203","","01010302","",5,""]
["0101030204  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030204","","01010302","",5,""]
["01010303  실명 : 303.접견실     개소 :1","","",1,{"$f":"F99+F100+F101+F102","v":0},0,{"$f":"H99+H100+H101+H102","v":0},0,{"$f":"J99+J100+J101+J102","v":0},0,0,0,"","01010303","","010103","",4,""]
["0101030301  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030301","","01010303","",5,""]
["0101030302  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101030302","","01010303","",5,""]
["0101030303  천  장  공  사","","",1,0,0,0,0,0,0,{"$f":"E101+G101+I101","v":0},0,"","0101030303","","01010303","",5,""]
["0101030304  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030304","","01010303","",5,""]
["01010304  실명 : 304.원장 행정실     개소 :1","","",1,{"$f":"F104+F105+F106+F107","v":0},0,{"$f":"H104+H105+H106+H107","v":0},0,{"$f":"J104+J105+J106+J107","v":0},0,0,0,"","01010304","","010103","",4,""]
["0101030401  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030401","","01010304","",5,""]
["0101030402  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101030402","","01010304","",5,""]
["0101030403  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030403","","01010304","",5,""]
["0101030404  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030404","","01010304","",5,""]
["01010305  실명 : 305.원장 창고     개소 :1","","",1,{"$f":"F109+F110+F111","v":0},0,{"$f":"H109+H110+H111","v":0},0,{"$f":"J109+J110+J111","v":0},0,0,0,"","01010305","","010103","",4,""]
["0101030501  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030501","","01010305","",5,""]
["0101030502  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101030502","","01010305","",5,""]
["0101030503  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030503","","01010305","",5,""]
["01010306  실명 : 306.원장 화장실     개소 :1","","",1,{"$f":"F113+F114+F115+F116","v":0},0,{"$f":"H113+H114+H115+H116","v":0},0,{"$f":"J113+J114+J115+J116","v":0},0,0,0,"","01010306","","010103","",4,""]
["0101030601  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030601","","01010306","",5,""]
["0101030602  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101030602","","01010306","",5,""]
["0101030603  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030603","","01010306","",5,""]
["0101030604  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030604","","01010306","",5,""]
["01010307  실명 : 307.부원장실     개소 :1","","",1,{"$f":"F118+F119+F120+F121","v":0},0,{"$f":"H118+H119+H120+H121","v":0},0,{"$f":"J118+J119+J120+J121","v":0},0,0,0,"","01010307","","010103","",4,""]
["0101030701  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030701","","01010307","",5,""]
["0101030702  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101030702","","01010307","",5,""]
["0101030703  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030703","","01010307","",5,""]
["0101030704  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030704","","01010307","",5,""]
["01010308  실명 : 308.부원장 행정실     개소 :1","","",1,{"$f":"F123+F124+F125+F126","v":0},0,{"$f":"H123+H124+H125+H126","v":0},0,{"$f":"J123+J124+J125+J126","v":0},0,0,0,"","01010308","","010103","",4,""]
["0101030801  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030801","","01010308","",5,""]
["0101030802  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101030802","","01010308","",5,""]
["0101030803  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030803","","01010308","",5,""]
["0101030804  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030804","","01010308","",5,""]
["01010309  실명 : 309.대회의실     개소 :1","","",1,{"$f":"F128+F129+F130","v":0},0,{"$f":"H128+H129+H130","v":0},0,{"$f":"J128+J129+J130","v":0},0,0,0,"","01010309","","010103","",4,""]
["0101030901  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030901","","01010309","",5,""]
["0101030902  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101030902","","01010309","",5,""]
["0101030903  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101030903","","01010309","",5,""]
["01010310  실명 : 310.공용화장실(남)     개소 :1","","",1,{"$f":"F132+F133+F134+F135","v":0},0,{"$f":"H132+H133+H134+H135","v":0},0,{"$f":"J132+J133+J134+J135","v":0},0,0,0,"","01010310","","010103","",4,""]
["0101031001  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101031001","","01010310","",5,""]
["0101031002  벽    공    사","","",1,0,{"$f":"E133*D133","v":0},0,{"$f":"G133*D133","v":0},0,{"$f":"I133*D133","v":0},{"$f":"E133+G133+I133","v":0},0,"","0101031002","","01010310","",5,""]
["0101031003  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101031003","","01010310","",5,""]
["0101031004  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101031004","","01010310","",5,""]
["01010311  실명 : 311.공용화장실(여)     개소 :1","","",1,{"$f":"F137+F138+F139+F140","v":0},0,{"$f":"H137+H138+H139+H140","v":0},0,{"$f":"J137+J138+J139+J140","v":0},0,0,0,"","01010311","","010103","",4,""]
["0101031101  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101031101","","01010311","",5,""]
["0101031102  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101031102","","01010311","",5,""]
["0101031103  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101031103","","01010311","",5,""]
["0101031104  기  타  공  사","","",1,0,0,0,0,0,0,0,0,"","0101031104","","01010311","",5,""]
["01010312  실명 : 312.청소도구함     개소 :1","","",1,{"$f":"F142+F143+F144","v":0},0,{"$f":"H142+H143+H144","v":0},0,{"$f":"J142+J143+J144","v":0},0,0,0,"","01010312","","010103","",4,""]
["0101031201  바  닥  공  사","","",1,0,0,0,0,0,0,0,0,"","0101031201","","01010312","",5,""]
["0101031202  벽    공    사","","",1,0,0,0,0,0,0,0,0,"","0101031202","","01010312","",5,""]
["0101031203  천  장  공  사","","",1,0,0,0,0,0,0,0,0,"","0101031203","","01010312","",5,""]
["010104  ▶ 골재비및운반비","","",1,0,0,0,0,0,0,0,0,"","010104","","0101","",3,""]
["0102  ■ 관급공사","","",1,{"$f":"F147","v":0},0,{"$f":"H147","v":0},0,{"$f":"J147","v":0},0,0,0,"","0102","","01","",2,""]
["010201  ▶ 도급자설치관급자재비","","",1,0,0,0,0,0,0,0,0,"","010201","","0102","",3,""]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"F5","v":0},null,{"$f":"H5","v":0},null,{"$f":"J5","v":0},null,{"$f":"L5","v":0}]

{"sheet":"인테리어내역","index":3,"n_rows":2678,"n_cols":48,"rows_kept":2678,"cut":false,"hidden":false,"merged":[[1,43,2,43],[1,44,2,44],[1,45,2,45],[1,46,2,46],[1,47,2,47],[1,42,2,42],[1,31,2,31],[1,32,2,32],[1,33,2,33],[1,34,2,34],[1,35,2,35],[1,36,2,36],[1,37,2,37],[1,38,2,38],[1,39,2,39],[1,40,2,40],[1,41,2,41],[1,30,2,30],[1,19,2,19],[1,20,2,20],[1,21,2,21],[1,22,2,22],[1,23,2,23],[1,24,2,24],[1,25,2,25],[1,26,2,26],[1,27,2,27],[1,28,2,28],[1,29,2,29],[1,18,2,18],[0,0,0,12],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,1,5],[1,6,1,7],[1,8,1,9],[1,10,1,11],[1,12,2,12],[1,13,2,13],[1,14,2,14],[1,15,2,15],[1,16,2,16],[1,17,2,17]]}
["[ 국토연구원 인테리어공사 ]"]
["품      명","규      격","단위","수량","재  료  비",null,"노  무  비",null,"경      비",null,"합      계",null,"비  고","품목코드","변수","설정","공종코드","일위","단산","자재","손료적용","손료저장","적용율","JUK1","JUK2","JUK3","JUK4","JUK5","JUK6","JUK7","JUK8","JUK9","JUK10","JUK11","JUK12","JUK13","JUK14","JUK15","JUK16","JUK17","JUK18","JUK19","JUK20","자재구분","공종구분","공종레벨","공종+자재","고유번호"]
[{"$nulls":4},"단  가","금  액","단  가","금  액","단  가","금  액","단  가","금  액"]
["0101010101  바  닥  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 101.로비     개소 :1",{"$nulls":14},"0101010101"]
["석재.타일보양","하드롱지","M2",793.93,null,{"$f":"TRUNC(E5*D5, 0)","v":0},null,{"$f":"TRUNC(G5*D5, 0)","v":0},null,{"$f":"TRUNC(I5*D5, 0)","v":0},{"$f":"TRUNC(E5+G5+I5, 0)","v":0},{"$f":"TRUNC(F5+H5+J5, 0)","v":0},null,"50FA026009B9885A1F2BAC10AA64C9","","","0101010101","T","F","F",{"$nulls":23},"","",null,"010101010150FA026009B9885A1F2BAC10AA64C9",5]
["지정타일압착붙임 /홀 (타일관급)","바닥, 바탕 65mm+압 5mm","M2",793.93,null,{"$f":"TRUNC(E6*D6, 0)","v":0},null,{"$f":"TRUNC(G6*D6, 0)","v":0},null,{"$f":"TRUNC(I6*D6, 0)","v":0},{"$f":"TRUNC(E6+G6+I6, 0)","v":0},{"$f":"TRUNC(F6+H6+J6, 0)","v":0},null,"50FAC240091DE2698B2F0344CE27B2","","","0101010101","T","F","F",{"$nulls":23},"","",null,"010101010150FAC240091DE2698B2F0344CE27B2",6]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F5:F27)","v":0},null,{"$f":"SUM(H5:H27)","v":0},null,{"$f":"SUM(J5:J27)","v":0},null,{"$f":"SUM(L5:L27)","v":0},null,"TOTAL"]
["0101010102  벽    공    사","■ 인테리어공사 ▶ 지상1층 실명 : 101.로비     개소 :1",{"$nulls":14},"0101010102"]
["벽마감용 각파이프틀설치","ㅁ-30*30","M2",54.18,null,{"$f":"TRUNC(E30*D30, 0)","v":0},null,{"$f":"TRUNC(G30*D30, 0)","v":0},null,{"$f":"TRUNC(I30*D30, 0)","v":0},{"$f":"TRUNC(E30+G30+I30, 0)","v":0},0,null,"50FAB25009099778C12BFF07E62024","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAB25009099778C12BFF07E62024",9]
["벤치설치용 각파이프틀설치","W:400*H:600, ㅁ-30*30","M",21.1,null,0,null,0,null,0,0,0,null,"50FAB25009099778C12BFF07E62027","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAB25009099778C12BFF07E62027",682]
["수벽몰딩","STL 10*80*1.6mm, 지정도장","M",5.25,null,0,null,0,null,0,0,0,null,"50FAB25009099778C12BFF07E62022","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAB25009099778C12BFF07E62022",10]
["엘리베이터출입구 마구리","구로철판1.6t, W:400","M",12.4,null,0,null,0,null,0,0,0,null,"50FAB25009099778C12BFF07E62023","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAB25009099778C12BFF07E62023",795]
["걸레받이","구로철판1.6t, W:100","M",3,null,0,null,0,null,0,0,0,null,"50FAB25009099778C12BFF07E6202C","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAB25009099778C12BFF07E6202C",796]
["지정청고벽돌타일붙임","벽, 본드붙임","M2",48.87,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CC79D3","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAC240091DE2698B2F0344CC79D3",11]
["화강석붙임(버너,건식,패턴시공)","벽, 고흥석 30mm","M2",328.93,null,0,null,0,null,0,0,0,null,"50FAC240092E2412022A0C87E3B371","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAC240092E2412022A0C87E3B371",12]
["화강석붙임(혼드,건식,패턴시공)","벽, 고흥석 30mm","M2",29.34,null,0,null,0,null,0,0,0,null,"50FAC240092E243ED527AEED2DD81F","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAC240092E243ED527AEED2DD81F",13]
["화강석붙임(버너,본드붙임,패턴시공)","벽, 고흥석 30mm","M2",29.74,null,0,null,0,null,0,0,0,null,"50FAC240092E2412022A0C87E3B370","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAC240092E2412022A0C87E3B370",898]
["화강석붙임(버너,TRUSS건식,패턴시공)","벽, 고흥석 30mm, 트러스포함","M2",56.37,null,0,null,0,null,0,0,0,null,"50FAC240092E51B27A27DE4C0D5B4E","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAC240092E51B27A27DE4C0D5B4E",793]
["친환경수성페인트(로울러칠)","내벽 3회. 친환경","M2",222.66,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FEC02D76A50311ED","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAF2F0097711FEC02D76A50311ED",14]
["친환경수성페인트(로울러칠)","내벽 3회. 친환경(GB면)","M2",9.4499999999999993,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FEC02D76A24F126A","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAF2F0097711FEC02D76A24F126A",15]
["걸레받이용페인트칠","2회","M2",6.91,null,0,null,0,null,0,0,0,null,"50FAF2F00966A2A451265A9E70BECD","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAF2F00966A2A451265A9E70BECD",16]
["MDF붙임(벽)","9mm","M2",160.57,null,0,null,0,null,0,0,0,null,"50FAE28009EE89516723B7798FD4FC","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAE28009EE89516723B7798FD4FC",17]
["석고판 붙임","벽, 일반 9.5mm 2겹","M2",9.4499999999999993,null,0,null,0,null,0,0,0,null,"50FAE28009EEB69F052002C24F1E0B","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAE28009EEB69F052002C24F1E0B",794]
["합판붙임(벽)","9mm","M2",74.47,null,0,null,0,null,0,0,0,null,"50FAE28009EED176C1217BAD90B52A","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FAE28009EED176C1217BAD90B52A",19]
["지정무늬목마감","티크","M2",108.63,null,0,null,0,null,0,0,0,null,"50FB62500938F8AF6C2BA268B4F296","","","0101010102","T","F","F",{"$nulls":23},"","",null,"010101010250FB62500938F8AF6C2BA268B4F296",20]
["지정개비온월판넬","THK150mm, H:3000, STS304 6mm, 일반석채움","M2",27.59,null,0,null,0,null,0,0,0,null,"51422250099FA2F9AC22E5D3FAE6313ABA6085","","","0101010102","F","F","T",{"$nulls":23},"","",null,"010101010251422250099FA2F9AC22E5D3FAE6313ABA6085",636]
[]
[]
[]
[]
[]
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F30:F52)","v":0},null,{"$f":"SUM(H30:H52)","v":0},null,{"$f":"SUM(J30:J52)","v":0},null,{"$f":"SUM(L30:L52)","v":0},null,"TOTAL"]
["0101010103  천  장  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 101.로비     개소 :1",{"$nulls":14},"0101010103"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",393.52,null,{"$f":"TRUNC(E55*D55, 0)","v":0},null,{"$f":"TRUNC(G55*D55, 0)","v":0},null,{"$f":"TRUNC(I55*D55, 0)","v":0},{"$f":"TRUNC(E55+G55+I55, 0)","v":0},0,null,"57D3722009F9710BAE2ED981ED5CFCF4080C3E","","","0101010103","F","F","T",{"$nulls":23},"","",null,"010101010357D3722009F9710BAE2ED981ED5CFCF4080C3E",23]
["등기구타공","다운라이트","EA",106,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101010103","F","F","T",{"$nulls":23},"","",null,"010101010357D3722009F9710B9C21B6DD9D2E4747ACE111",24]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",374.79,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101010103","T","F","F",{"$nulls":23},"","",null,"010101010350FAB2500909EF985820B87BB6AB0D",25]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",374.79,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101010103","T","F","F",{"$nulls":23},"","",null,"010101010350FAF2F0097711FE6F2FE675585AF3",26]
["석고판본드붙임","천장, 일반 9.5mm","M2",374.79,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403B220C4D6970C9E","","","0101010103","T","F","F",{"$nulls":23},"","",null,"010101010350FAE28009EEA403B220C4D6970C9E",798]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",184.7,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101010103","T","F","F",{"$nulls":23},"","",null,"010101010350FAE280094E44060A2808FF6AAFE4",28]
["픽쳐레일","","M",18.100000000000001,null,0,null,0,null,0,0,0,null,"51422250099FA2F9AC22E5D3FAE6313ABA61AD","","","0101010103","F","F","T",{"$nulls":23},"","",null,"010101010351422250099FA2F9AC22E5D3FAE6313ABA61AD",690]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F55:F77)","v":0},null,{"$f":"SUM(H55:H77)","v":0},null,{"$f":"SUM(J55:J77)","v":0},null,{"$f":"SUM(L55:L77)","v":0},null,"TOTAL"]
["0101010104  기  타  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 101.로비     개소 :1",{"$nulls":14},"0101010104"]
["벤치설치","L:1200","개소",9,null,{"$f":"TRUNC(E80*D80, 0)","v":0},null,{"$f":"TRUNC(G80*D80, 0)","v":0},null,{"$f":"TRUNC(I80*D80, 0)","v":0},{"$f":"TRUNC(E80+G80+I80, 0)","v":0},{"$f":"TRUNC(F80+H80+J80, 0)","v":0},null,"50FB6250091C3241552590DC69BEE0","","","0101010104","T","F","F",{"$nulls":23},"","",null,"010101010450FB6250091C3241552590DC69BEE0",637]
["카페테리아 가구","","개",1,null,{"$f":"TRUNC(E81*D81, 0)","v":0},null,{"$f":"TRUNC(G81*D81, 0)","v":0},null,{"$f":"TRUNC(I81*D81, 0)","v":0},{"$f":"TRUNC(E81+G81+I81, 0)","v":0},{"$f":"TRUNC(F81+H81+J81, 0)","v":0},null,"57D3722009F9710B9C28E90B723AB022DF8680","","","0101010104","F","F","T",{"$nulls":23},"","",null,"010101010457D3722009F9710B9C28E90B723AB022DF8680",31]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F80:F102)","v":0},null,{"$f":"SUM(H80:H102)","v":0},null,{"$f":"SUM(J80:J102)","v":0},null,{"$f":"SUM(L80:L102)","v":0},null,"TOTAL"]
["0101010201  바  닥  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 102a.직원식당     개소 :1",{"$nulls":14},"0101010201"]
["시멘트모르타르바름","바닥, 80mm","M2",338.71,null,{"$f":"TRUNC(E105*D105, 0)","v":0},null,{"$f":"TRUNC(G105*D105, 0)","v":0},null,{"$f":"TRUNC(I105*D105, 0)","v":0},{"$f":"TRUNC(E105+G105+I105, 0)","v":0},0,null,"50FA62D00969ADB3282ADD819B33AE","","","0101010201","T","F","F",{"$nulls":23},"","",null,"010101020150FA62D00969ADB3282ADD819B33AE",685]
["콘플로어마감","바닥","M2",338.71,null,{"$f":"TRUNC(E106*D106, 0)","v":0},null,{"$f":"TRUNC(G106*D106, 0)","v":0},null,{"$f":"TRUNC(I106*D106, 0)","v":0},0,0,null,"50FAF2F009EBFFC42A231C985BAF9A","","","0101010201","T","F","F",{"$nulls":23},"","",null,"010101020150FAF2F009EBFFC42A231C985BAF9A",35]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",2.8,null,{"$f":"TRUNC(E107*D107, 0)","v":0},null,{"$f":"TRUNC(G107*D107, 0)","v":0},null,{"$f":"TRUNC(I107*D107, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101010201","T","F","F",{"$nulls":23},"","",null,"010101020150FAE28009A0F313FA23F4CCF30D36",799]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F105:F127)","v":0},null,{"$f":"SUM(H105:H127)","v":0},null,{"$f":"SUM(J105:J127)","v":0},null,{"$f":"SUM(L105:L127)","v":0},null,"TOTAL"]
["0101010202  벽    공    사","■ 인테리어공사 ▶ 지상1층 실명 : 102a.직원식당     개소 :1",{"$nulls":14},"0101010202"]
["지정흑철판마감","바탕틀, 도장포함","M2",63.32,null,{"$f":"TRUNC(E130*D130, 0)","v":0},null,{"$f":"TRUNC(G130*D130, 0)","v":0},null,{"$f":"TRUNC(I130*D130, 0)","v":0},{"$f":"TRUNC(E130+G130+I130, 0)","v":0},0,null,"50FAB2500947EC87B42F88E3127BAE","","","0101010202","T","F","F",{"$nulls":23},"","",null,"010101020250FAB2500947EC87B42F88E3127BAE",38]
["지정청고벽돌타일붙임","벽, 본드붙임","M2",87.06,null,{"$f":"TRUNC(E131*D131, 0)","v":0},null,{"$f":"TRUNC(G131*D131, 0)","v":0},null,{"$f":"TRUNC(I131*D131, 0)","v":0},0,0,null,"50FAC240091DE2698B2F0344CC79D3","","","0101010202","T","F","F",{"$nulls":23},"","",null,"010101020250FAC240091DE2698B2F0344CC79D3",39]
["지정도장마감","건축도어면","M2",6.6,null,{"$f":"TRUNC(E132*D132, 0)","v":0},null,{"$f":"TRUNC(G132*D132, 0)","v":0},null,{"$f":"TRUNC(I132*D132, 0)","v":0},0,0,null,"50FAF2F0097711FE6F2FE675585AFC","","","0101010202","T","F","F",{"$nulls":23},"","",null,"010101020250FAF2F0097711FE6F2FE675585AFC",974]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F130:F152)","v":0},null,{"$f":"SUM(H130:H152)","v":0},null,{"$f":"SUM(J130:J152)","v":0},null,{"$f":"SUM(L130:L152)","v":0},null,"TOTAL"]
["0101010203  천  장  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 102a.직원식당     개소 :1",{"$nulls":14},"0101010203"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",180.81,null,{"$f":"TRUNC(E155*D155, 0)","v":0},null,{"$f":"TRUNC(G155*D155, 0)","v":0},null,{"$f":"TRUNC(I155*D155, 0)","v":0},{"$f":"TRUNC(E155+G155+I155, 0)","v":0},0,null,"57D3722009F9710BAE2ED981ED5CFCF4080C3E","","","0101010203","F","F","T",{"$nulls":23},"","",null,"010101020357D3722009F9710BAE2ED981ED5CFCF4080C3E",43]
["보통합판","보통합판, 1급, 9.0*1220*2440mm","M2",171.5,null,0,null,0,null,0,0,0,null,"57FE5240098541A8F625467ED95EBC89C0B2EB","","","0101010203","F","F","T",{"$nulls":23},"","",null,"010101020357FE5240098541A8F625467ED95EBC89C0B2EB",860]
["등기구타공","다운라이트","EA",100,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101010203","F","F","T",{"$nulls":23},"","",null,"010101020357D3722009F9710B9C21B6DD9D2E4747ACE111",44]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",338.71,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101010203","T","F","F",{"$nulls":23},"","",null,"010101020350FAB2500909EF985820B87BB6AB0D",45]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",338.71,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101010203","T","F","F",{"$nulls":23},"","",null,"010101020350FAF2F0097711FE6F2FE675585AF3",48]
["석고판본드붙임","천장, 일반 9.5mm","M2",338.71,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403B220C4D6970C9E","","","0101010203","T","F","F",{"$nulls":23},"","",null,"010101020350FAE28009EEA403B220C4D6970C9E",49]
["철재커텐박스설치(ㄱ자)","200*200*1.2t, STL. 도장","M",20.07,null,0,null,0,null,0,0,0,null,"50FAE2800958DF9CBC23EFCCF16A9D","","","0101010203","T","F","F",{"$nulls":23},"","",null,"010101020350FAE2800958DF9CBC23EFCCF16A9D",50]
["천장단차보강 /직원식당","H:300*1.6t갈바/도장, 각파이프틀및달대포함","M",54.14,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D2822A1B8D","","","0101010203","T","F","F",{"$nulls":23},"","",null,"010101020350FAE2800958DFBF8327D2822A1B8D",861]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",79.02,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101010203","T","F","F",{"$nulls":23},"","",null,"010101020350FAE280094E44060A2808FF6AAFE4",51]
["지정스크린루버천정재","AL 50*150@180/인테리어필름마감, 경량철골천정틀별도","M2",166.51,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A265A034A13DA","","","0101010203","T","F","F",{"$nulls":23},"","",null,"010101020350FAE280094E44060A265A034A13DA",52]
{"$rows_empty":13}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F155:F177)","v":0},null,{"$f":"SUM(H155:H177)","v":0},null,{"$f":"SUM(J155:J177)","v":0},null,{"$f":"SUM(L155:L177)","v":0},null,"TOTAL"]
["0101010204  기  타  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 102a.직원식당     개소 :1",{"$nulls":14},"0101010204"]
["식당 빠 테이블","","개",1,null,{"$f":"TRUNC(E180*D180, 0)","v":0},null,{"$f":"TRUNC(G180*D180, 0)","v":0},null,{"$f":"TRUNC(I180*D180, 0)","v":0},{"$f":"TRUNC(E180+G180+I180, 0)","v":0},{"$f":"TRUNC(F180+H180+J180, 0)","v":0},null,"57D3722009F9710B9C28E90B723AB022DF8687","","","0101010204","F","F","T",{"$nulls":23},"","",null,"010101020457D3722009F9710B9C28E90B723AB022DF8687",54]
{"$rows_empty":22}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F180:F202)","v":0},null,{"$f":"SUM(H180:H202)","v":0},null,{"$f":"SUM(J180:J202)","v":0},null,{"$f":"SUM(L180:L202)","v":0},null,"TOTAL"]
["0101010301  바  닥  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 102b.직원식당방풍실     개소 :1",{"$nulls":14},"0101010301"]
["시멘트모르타르바름","바닥, 80mm","M2",4.78,null,{"$f":"TRUNC(E205*D205, 0)","v":0},null,{"$f":"TRUNC(G205*D205, 0)","v":0},null,{"$f":"TRUNC(I205*D205, 0)","v":0},{"$f":"TRUNC(E205+G205+I205, 0)","v":0},{"$f":"TRUNC(F205+H205+J205, 0)","v":0},null,"50FA62D00969ADB3282ADD819B33AE","","","0101010301","T","F","F",{"$nulls":23},"","",null,"010101030150FA62D00969ADB3282ADD819B33AE",977]
["콘플로어마감","바닥","M2",4.78,null,{"$f":"TRUNC(E206*D206, 0)","v":0},null,{"$f":"TRUNC(G206*D206, 0)","v":0},null,{"$f":"TRUNC(I206*D206, 0)","v":0},{"$f":"TRUNC(E206+G206+I206, 0)","v":0},{"$f":"TRUNC(F206+H206+J206, 0)","v":0},null,"50FAF2F009EBFFC42A231C985BAF9A","","","0101010301","T","F","F",{"$nulls":23},"","",null,"010101030150FAF2F009EBFFC42A231C985BAF9A",978]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F205:F227)","v":0},null,{"$f":"SUM(H205:H227)","v":0},null,{"$f":"SUM(J205:J227)","v":0},null,{"$f":"SUM(L205:L227)","v":0},null,"TOTAL"]
["0101010302  벽    공    사","■ 인테리어공사 ▶ 지상1층 실명 : 102b.직원식당방풍실     개소 :1",{"$nulls":14},"0101010302"]
["지정청고벽돌타일붙임","벽, 본드붙임","M2",16.649999999999999,null,{"$f":"TRUNC(E230*D230, 0)","v":0},null,{"$f":"TRUNC(G230*D230, 0)","v":0},null,{"$f":"TRUNC(I230*D230, 0)","v":0},{"$f":"TRUNC(E230+G230+I230, 0)","v":0},{"$f":"TRUNC(F230+H230+J230, 0)","v":0},null,"50FAC240091DE2698B2F0344CC79D3","","","0101010302","T","F","F",{"$nulls":23},"","",null,"010101030250FAC240091DE2698B2F0344CC79D3",980]
{"$rows_empty":22}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F230:F252)","v":0},null,{"$f":"SUM(H230:H252)","v":0},null,{"$f":"SUM(J230:J252)","v":0},null,{"$f":"SUM(L230:L252)","v":0},null,"TOTAL"]
["0101010303  천  장  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 102b.직원식당방풍실     개소 :1",{"$nulls":14},"0101010303"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",5.0199999999999996,null,{"$f":"TRUNC(E255*D255, 0)","v":0},null,{"$f":"TRUNC(G255*D255, 0)","v":0},null,{"$f":"TRUNC(I255*D255, 0)","v":0},{"$f":"TRUNC(E255+G255+I255, 0)","v":0},0,null,"57D3722009F9710BAE2ED981ED5CFCF4080C3E","","","0101010303","F","F","T",{"$nulls":23},"","",null,"010101030357D3722009F9710BAE2ED981ED5CFCF4080C3E",982]
["등기구타공","다운라이트","EA",1,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101010303","F","F","T",{"$nulls":23},"","",null,"010101030357D3722009F9710B9C21B6DD9D2E4747ACE111",983]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",4.78,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101010303","T","F","F",{"$nulls":23},"","",null,"010101030350FAB2500909EF985820B87BB6AB0D",984]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",4.78,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101010303","T","F","F",{"$nulls":23},"","",null,"010101030350FAF2F0097711FE6F2FE675585AF3",985]
["석고판본드붙임","천장, 일반 9.5mm","M2",4.78,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403B220C4D6970C9E","","","0101010303","T","F","F",{"$nulls":23},"","",null,"010101030350FAE28009EEA403B220C4D6970C9E",986]
["철재커텐박스설치(ㄱ자)","200*200*1.2t, STL. 도장","M",2.74,null,0,null,0,null,0,0,0,null,"50FAE2800958DF9CBC23EFCCF16A9D","","","0101010303","T","F","F",{"$nulls":23},"","",null,"010101030350FAE2800958DF9CBC23EFCCF16A9D",987]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",6.23,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101010303","T","F","F",{"$nulls":23},"","",null,"010101030350FAE280094E44060A2808FF6AAFE4",988]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F255:F277)","v":0},null,{"$f":"SUM(H255:H277)","v":0},null,{"$f":"SUM(J255:J277)","v":0},null,{"$f":"SUM(L255:L277)","v":0},null,"TOTAL"]
["0101010401  바  닥  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 103.PDR ROOM     개소 :1",{"$nulls":14},"0101010401"]
["시멘트모르타르바름","바닥, 77mm","M2",12.89,null,{"$f":"TRUNC(E280*D280, 0)","v":0},null,{"$f":"TRUNC(G280*D280, 0)","v":0},null,{"$f":"TRUNC(I280*D280, 0)","v":0},{"$f":"TRUNC(E280+G280+I280, 0)","v":0},0,null,"50FA62D00969ADB3282ADD819A2D22","","","0101010401","T","F","F",{"$nulls":23},"","",null,"010101040150FA62D00969ADB3282ADD819A2D22",686]
["지정카펫타일 깔기","7.0mm","M2",12.89,null,{"$f":"TRUNC(E281*D281, 0)","v":0},null,{"$f":"TRUNC(G281*D281, 0)","v":0},null,{"$f":"TRUNC(I281*D281, 0)","v":0},0,0,null,"50FAE28009C3DCCF2C2E7219497839","","","0101010401","T","F","F",{"$nulls":23},"","",null,"010101040150FAE28009C3DCCF2C2E7219497839",58]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",1.8,null,{"$f":"TRUNC(E282*D282, 0)","v":0},null,{"$f":"TRUNC(G282*D282, 0)","v":0},null,{"$f":"TRUNC(I282*D282, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101010401","T","F","F",{"$nulls":23},"","",null,"010101040150FAE28009A0F313FA23F4CCF30D36",802]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F280:F302)","v":0},null,{"$f":"SUM(H280:H302)","v":0},null,{"$f":"SUM(J280:J302)","v":0},null,{"$f":"SUM(L280:L302)","v":0},null,"TOTAL"]
["0101010402  벽    공    사","■ 인테리어공사 ▶ 지상1층 실명 : 103.PDR ROOM     개소 :1",{"$nulls":14},"0101010402"]
["스텐걸레받이","SUS H/L 1.6t, H:100","M",5.5,null,{"$f":"TRUNC(E305*D305, 0)","v":0},null,{"$f":"TRUNC(G305*D305, 0)","v":0},null,{"$f":"TRUNC(I305*D305, 0)","v":0},{"$f":"TRUNC(E305+G305+I305, 0)","v":0},0,null,"50FAB2500947ECFABD256D4BC0E986","","","0101010402","T","F","F",{"$nulls":23},"","",null,"010101040250FAB2500947ECFABD256D4BC0E986",914]
["합판붙임(벽)","9mm","M2",17.04,null,{"$f":"TRUNC(E306*D306, 0)","v":0},null,{"$f":"TRUNC(G306*D306, 0)","v":0},null,{"$f":"TRUNC(I306*D306, 0)","v":0},0,0,null,"50FAE28009EED176C1217BAD90B52A","","","0101010402","T","F","F",{"$nulls":23},"","",null,"010101040250FAE28009EED176C1217BAD90B52A",62]
["지정패브릭마감","흡음보드+패브릭마감","M2",16.489999999999998,null,{"$f":"TRUNC(E307*D307, 0)","v":0},null,{"$f":"TRUNC(G307*D307, 0)","v":0},null,{"$f":"TRUNC(I307*D307, 0)","v":0},0,0,null,"50FB62500938F8AF6C2BA268B4F294","","","0101010402","T","F","F",{"$nulls":23},"","",null,"010101040250FB62500938F8AF6C2BA268B4F294",64]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F305:F327)","v":0},null,{"$f":"SUM(H305:H327)","v":0},null,{"$f":"SUM(J305:J327)","v":0},null,{"$f":"SUM(L305:L327)","v":0},null,"TOTAL"]
["0101010403  천  장  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 103.PDR ROOM     개소 :1",{"$nulls":14},"0101010403"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",13.53,null,{"$f":"TRUNC(E330*D330, 0)","v":0},null,{"$f":"TRUNC(G330*D330, 0)","v":0},null,{"$f":"TRUNC(I330*D330, 0)","v":0},{"$f":"TRUNC(E330+G330+I330, 0)","v":0},0,null,"57D3722009F9710BAE2ED981ED5CFCF4080C3E","","","0101010403","F","F","T",{"$nulls":23},"","",null,"010101040357D3722009F9710BAE2ED981ED5CFCF4080C3E",66]
["등기구타공","다운라이트","EA",7,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101010403","F","F","T",{"$nulls":23},"","",null,"010101040357D3722009F9710B9C21B6DD9D2E4747ACE111",67]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",12.89,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101010403","T","F","F",{"$nulls":23},"","",null,"010101040350FAB2500909EF985820B87BB6AB0D",68]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",12.89,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101010403","T","F","F",{"$nulls":23},"","",null,"010101040350FAF2F0097711FE6F2FE675585AF3",69]
["석고판본드붙임","천장, 일반 9.5mm","M2",12.89,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403B220C4D6970C9E","","","0101010403","T","F","F",{"$nulls":23},"","",null,"010101040350FAE28009EEA403B220C4D6970C9E",70]
["철재커텐박스설치(ㄱ자)","200*200*1.2t, STL. 도장","M",6.08,null,0,null,0,null,0,0,0,null,"50FAE2800958DF9CBC23EFCCF16A9D","","","0101010403","T","F","F",{"$nulls":23},"","",null,"010101040350FAE2800958DF9CBC23EFCCF16A9D",71]
["천장단차보강 /PDR ROOM","H:250*1.6t갈바/도장, 각파이프틀및달대포함","M",7,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D2822A1B8B","","","0101010403","T","F","F",{"$nulls":23},"","",null,"010101040350FAE2800958DFBF8327D2822A1B8B",863]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",8.26,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101010403","T","F","F",{"$nulls":23},"","",null,"010101040350FAE280094E44060A2808FF6AAFE4",73]
{"$rows_empty":15}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F330:F352)","v":0},null,{"$f":"SUM(H330:H352)","v":0},null,{"$f":"SUM(J330:J352)","v":0},null,{"$f":"SUM(L330:L352)","v":0},null,"TOTAL"]
["0101010501  바  닥  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 104.공용화장실(남)     개소 :1",{"$nulls":14},"0101010501"]
["석재.타일보양","하드롱지","M2",13.02,null,{"$f":"TRUNC(E355*D355, 0)","v":0},null,{"$f":"TRUNC(G355*D355, 0)","v":0},null,{"$f":"TRUNC(I355*D355, 0)","v":0},{"$f":"TRUNC(E355+G355+I355, 0)","v":0},0,null,"50FA026009B9885A1F2BAC10AA64C9","","","0101010501","T","F","F",{"$nulls":23},"","",null,"010101050150FA026009B9885A1F2BAC10AA64C9",76]
["지정타일압착붙임 /화장실 (타일 관급)","바닥, 바탕 65mm+압 5mm","M2",13.02,null,{"$f":"TRUNC(E356*D356, 0)","v":0},null,{"$f":"TRUNC(G356*D356, 0)","v":0},null,{"$f":"TRUNC(I356*D356, 0)","v":0},0,0,null,"50FAC240091DE2698B2F0344CE27B1","","","0101010501","T","F","F",{"$nulls":23},"","",null,"010101050150FAC240091DE2698B2F0344CE27B1",77]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",1.1000000000000001,null,{"$f":"TRUNC(E357*D357, 0)","v":0},null,{"$f":"TRUNC(G357*D357, 0)","v":0},null,{"$f":"TRUNC(I357*D357, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101010501","T","F","F",{"$nulls":23},"","",null,"010101050150FAE28009A0F313FA23F4CCF30D36",78]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F355:F377)","v":0},null,{"$f":"SUM(H355:H377)","v":0},null,{"$f":"SUM(J355:J377)","v":0},null,{"$f":"SUM(L355:L377)","v":0},null,"TOTAL"]
["0101010502  벽    공    사","■ 인테리어공사 ▶ 지상1층 실명 : 104.공용화장실(남)     개소 :1",{"$nulls":14},"0101010502"]
["소변기턱설치용 각파이프틀설치","W:200*H:1250, ㅁ-30*30","M",2,null,{"$f":"TRUNC(E380*D380, 0)","v":0},null,{"$f":"TRUNC(G380*D380, 0)","v":0},null,{"$f":"TRUNC(I380*D380, 0)","v":0},{"$f":"TRUNC(E380+G380+I380, 0)","v":0},0,null,"50FAB25009099778C12BFF07E62020","","","0101010502","T","F","F",{"$nulls":23},"","",null,"010101050250FAB25009099778C12BFF07E62020",864]
["대변기턱설치용 각파이프틀설치","W:200*H:1000, ㅁ-30*30","M",2,null,0,null,0,null,0,0,0,null,"50FAB25009099778C12BFF07E62021","","","0101010502","T","F","F",{"$nulls":23},"","",null,"010101050250FAB25009099778C12BFF07E62021",865]
["지정타일떠붙임 /화장실 (타일 관급)","벽, 몰탈18mm","M2",40.799999999999997,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD6","","","0101010502","T","F","F",{"$nulls":23},"","",null,"010101050250FAC240091DE2698B2F0344CFCDD6",80]
["지정타일본드붙임 /화장실 (타일관급)","벽","M2",4.5,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD1","","","0101010502","T","F","F",{"$nulls":23},"","",null,"010101050250FAC240091DE2698B2F0344CFCDD1",866]
["우레탄도막방수","벽체, 비노출","M2",5.3,null,0,null,0,null,0,0,0,null,"50FA92000987C572F62EA1806E70A5","","","0101010502","T","F","F",{"$nulls":23},"","",null,"010101050250FA92000987C572F62EA1806E70A5",867]
["인조대리석 변기턱","180*30mm, 몰탈30mm","M",4,null,0,null,0,null,0,0,0,null,"50FAC240092E47393F289B71873F55","","","0101010502","T","F","F",{"$nulls":23},"","",null,"010101050250FAC240092E47393F289B71873F55",81]
["벽, 합판붙임","방수 12mm 1겹","M2",5.3,null,0,null,0,null,0,0,0,null,"50FAE28009EED176C1217BDCCD06F7","","","0101010502","T","F","F",{"$nulls":23},"","",null,"010101050250FAE28009EED176C1217BDCCD06F7",868]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F380:F402)","v":0},null,{"$f":"SUM(H380:H402)","v":0},null,{"$f":"SUM(J380:J402)","v":0},null,{"$f":"SUM(L380:L402)","v":0},null,"TOTAL"]
["0101010503  천  장  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 104.공용화장실(남)     개소 :1",{"$nulls":14},"0101010503"]
["석고보드","석고보드, 평보드, 방수, 9.5*900*1800mm(㎡)","M2",13.67,null,{"$f":"TRUNC(E405*D405, 0)","v":0},null,{"$f":"TRUNC(G405*D405, 0)","v":0},null,{"$f":"TRUNC(I405*D405, 0)","v":0},{"$f":"TRUNC(E405+G405+I405, 0)","v":0},0,null,"57D3722009F9710BAE2ED982F3A1AA138880B3","","","0101010503","F","F","T",{"$nulls":23},"","",null,"010101050357D3722009F9710BAE2ED982F3A1AA138880B3",83]
["등기구타공","다운라이트","EA",6,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101010503","F","F","T",{"$nulls":23},"","",null,"010101050357D3722009F9710B9C21B6DD9D2E4747ACE111",84]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",13.02,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101010503","T","F","F",{"$nulls":23},"","",null,"010101050350FAB2500909EF985820B87BB6AB0D",85]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",13.02,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101010503","T","F","F",{"$nulls":23},"","",null,"010101050350FAF2F0097711FE6F2FE675585AF3",86]
["석고판본드붙임","천장, 방수 9.5mm","M2",13.02,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403862C1FD18B8962","","","0101010503","T","F","F",{"$nulls":23},"","",null,"010101050350FAE28009EEA403862C1FD18B8962",87]
["조명박스(J형) /화장실","(160+160+400+400)*1.6t갈바/도장, 각파이프틀및달대포함","M",6.3,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D286850A91","","","0101010503","T","F","F",{"$nulls":23},"","",null,"010101050350FAE2800958DFBF8327D286850A91",88]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",18.010000000000002,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101010503","T","F","F",{"$nulls":23},"","",null,"010101050350FAE280094E44060A2808FF6AAFE4",89]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F405:F427)","v":0},null,{"$f":"SUM(H405:H427)","v":0},null,{"$f":"SUM(J405:J427)","v":0},null,{"$f":"SUM(L405:L427)","v":0},null,"TOTAL"]
["0101010504  기  타  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 104.공용화장실(남)     개소 :1",{"$nulls":14},"0101010504"]
["지정화장실칸막이","자작나무합판마감","M2",8.73,null,{"$f":"TRUNC(E430*D430, 0)","v":0},null,{"$f":"TRUNC(G430*D430, 0)","v":0},null,{"$f":"TRUNC(I430*D430, 0)","v":0},{"$f":"TRUNC(E430+G430+I430, 0)","v":0},0,null,"57D3722009F99DF9C123903DCBC8B9718F30A1","","","0101010504","F","F","T",{"$nulls":23},"","",null,"010101050457D3722009F99DF9C123903DCBC8B9718F30A1",91]
["장애인소변기용손잡이","STS304 Ø38,1.5t","EA",1,null,0,null,0,null,0,0,0,null,"50FB12C009000A0DE123F9CD7ADDE2","","","0101010504","T","F","F",{"$nulls":23},"","",null,"010101050450FB12C009000A0DE123F9CD7ADDE2",92]
["수밀코킹(실리콘)","삼각, 5mm이하, 방균용","M",10.7,null,0,null,0,null,0,0,0,null,"50FA920009DF72024B2E486FEF08DE","","","0101010504","T","F","F",{"$nulls":23},"","",null,"010101050450FA920009DF72024B2E486FEF08DE",93]
["방습거울후레임","스테인리스, W50*1.5t","M",6.7,null,0,null,0,null,0,0,0,null,"50FAB2500924C55AE02DCC1BFE2175","","","0101010504","T","F","F",{"$nulls":23},"","",null,"010101050450FAB2500924C55AE02DCC1BFE2175",94]
["출입구 공프레임","구로철판1.6t, 1220*2150","개소",1,null,0,null,0,null,0,0,0,null,"50FAB2500924980282224F9EC8AE99","","","0101010504","T","F","F",{"$nulls":23},"","",null,"010101050450FAB2500924980282224F9EC8AE99",95]
["방습거울설치","5mm, 틀 포함","M2",2.42,null,0,null,0,null,0,0,0,null,"50FAD2A009FE1520552E7181DB95CE","","","0101010504","T","F","F",{"$nulls":23},"","",null,"010101050450FAD2A009FE1520552E7181DB95CE",96]
["인조대리석세면대","W:600*12t,틀포함","M",2.2999999999999998,null,0,null,0,null,0,0,0,null,"50FB12C0090037D9682873AC4EB01D","","","0101010504","T","F","F",{"$nulls":23},"","",null,"010101050450FB12C0090037D9682873AC4EB01D",97]
["소변기칸막이","400*900, 인조대리석13mm","개소",1,null,0,null,0,null,0,0,0,null,"50FB6250091C32460A2B63C3F2AE4D","","","0101010504","T","F","F",{"$nulls":23},"","",null,"010101050450FB6250091C32460A2B63C3F2AE4D",687]
{"$rows_empty":15}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F430:F452)","v":0},null,{"$f":"SUM(H430:H452)","v":0},null,{"$f":"SUM(J430:J452)","v":0},null,{"$f":"SUM(L430:L452)","v":0},null,"TOTAL"]
["0101010601  바  닥  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 105.공용화장실(여)     개소 :1",{"$nulls":14},"0101010601"]
["석재.타일보양","하드롱지","M2",14.53,null,{"$f":"TRUNC(E455*D455, 0)","v":0},null,{"$f":"TRUNC(G455*D455, 0)","v":0},null,{"$f":"TRUNC(I455*D455, 0)","v":0},{"$f":"TRUNC(E455+G455+I455, 0)","v":0},0,null,"50FA026009B9885A1F2BAC10AA64C9","","","0101010601","T","F","F",{"$nulls":23},"","",null,"010101060150FA026009B9885A1F2BAC10AA64C9",717]
["지정타일압착붙임 /화장실 (타일 관급)","바닥, 바탕 65mm+압 5mm","M2",14.53,null,{"$f":"TRUNC(E456*D456, 0)","v":0},null,{"$f":"TRUNC(G456*D456, 0)","v":0},null,{"$f":"TRUNC(I456*D456, 0)","v":0},0,0,null,"50FAC240091DE2698B2F0344CE27B1","","","0101010601","T","F","F",{"$nulls":23},"","",null,"010101060150FAC240091DE2698B2F0344CE27B1",718]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",1.1000000000000001,null,{"$f":"TRUNC(E457*D457, 0)","v":0},null,{"$f":"TRUNC(G457*D457, 0)","v":0},null,{"$f":"TRUNC(I457*D457, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101010601","T","F","F",{"$nulls":23},"","",null,"010101060150FAE28009A0F313FA23F4CCF30D36",719]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F455:F477)","v":0},null,{"$f":"SUM(H455:H477)","v":0},null,{"$f":"SUM(J455:J477)","v":0},null,{"$f":"SUM(L455:L477)","v":0},null,"TOTAL"]
["0101010602  벽    공    사","■ 인테리어공사 ▶ 지상1층 실명 : 105.공용화장실(여)     개소 :1",{"$nulls":14},"0101010602"]
["대변기턱설치용 각파이프틀설치","W:200*H:1000, ㅁ-30*30","M",4,null,{"$f":"TRUNC(E480*D480, 0)","v":0},null,{"$f":"TRUNC(G480*D480, 0)","v":0},null,{"$f":"TRUNC(I480*D480, 0)","v":0},{"$f":"TRUNC(E480+G480+I480, 0)","v":0},0,null,"50FAB25009099778C12BFF07E62021","","","0101010602","T","F","F",{"$nulls":23},"","",null,"010101060250FAB25009099778C12BFF07E62021",869]
["지정타일떠붙임 /화장실 (타일 관급)","벽, 몰탈18mm","M2",46.61,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD6","","","0101010602","T","F","F",{"$nulls":23},"","",null,"010101060250FAC240091DE2698B2F0344CFCDD6",111]
["지정타일본드붙임 /화장실 (타일관급)","벽","M2",4,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD1","","","0101010602","T","F","F",{"$nulls":23},"","",null,"010101060250FAC240091DE2698B2F0344CFCDD1",870]
["우레탄도막방수","벽체, 비노출","M2",4.8,null,0,null,0,null,0,0,0,null,"50FA92000987C572F62EA1806E70A5","","","0101010602","T","F","F",{"$nulls":23},"","",null,"010101060250FA92000987C572F62EA1806E70A5",871]
["인조대리석 변기턱","180*30mm, 몰탈30mm","M",4,null,0,null,0,null,0,0,0,null,"50FAC240092E47393F289B71873F55","","","0101010602","T","F","F",{"$nulls":23},"","",null,"010101060250FAC240092E47393F289B71873F55",112]
["벽, 합판붙임","방수 12mm 1겹","M2",4.8,null,0,null,0,null,0,0,0,null,"50FAE28009EED176C1217BDCCD06F7","","","0101010602","T","F","F",{"$nulls":23},"","",null,"010101060250FAE28009EED176C1217BDCCD06F7",872]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F480:F502)","v":0},null,{"$f":"SUM(H480:H502)","v":0},null,{"$f":"SUM(J480:J502)","v":0},null,{"$f":"SUM(L480:L502)","v":0},null,"TOTAL"]
["0101010603  천  장  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 105.공용화장실(여)     개소 :1",{"$nulls":14},"0101010603"]
["석고보드","석고보드, 평보드, 방수, 9.5*900*1800mm(㎡)","M2",15.25,null,{"$f":"TRUNC(E505*D505, 0)","v":0},null,{"$f":"TRUNC(G505*D505, 0)","v":0},null,{"$f":"TRUNC(I505*D505, 0)","v":0},{"$f":"TRUNC(E505+G505+I505, 0)","v":0},0,null,"57D3722009F9710BAE2ED982F3A1AA138880B3","","","0101010603","F","F","T",{"$nulls":23},"","",null,"010101060357D3722009F9710BAE2ED982F3A1AA138880B3",114]
["등기구타공","다운라이트","EA",6,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101010603","F","F","T",{"$nulls":23},"","",null,"010101060357D3722009F9710B9C21B6DD9D2E4747ACE111",115]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",14.53,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101010603","T","F","F",{"$nulls":23},"","",null,"010101060350FAB2500909EF985820B87BB6AB0D",116]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",14.53,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101010603","T","F","F",{"$nulls":23},"","",null,"010101060350FAF2F0097711FE6F2FE675585AF3",117]
["석고판본드붙임","천장, 방수 9.5mm","M2",14.53,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403862C1FD18B8962","","","0101010603","T","F","F",{"$nulls":23},"","",null,"010101060350FAE28009EEA403862C1FD18B8962",118]
["조명박스(J형) /화장실","(160+160+400+400)*1.6t갈바/도장, 각파이프틀및달대포함","M",6.12,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D286850A91","","","0101010603","T","F","F",{"$nulls":23},"","",null,"010101060350FAE2800958DFBF8327D286850A91",119]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",19.149999999999999,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101010603","T","F","F",{"$nulls":23},"","",null,"010101060350FAE280094E44060A2808FF6AAFE4",120]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F505:F527)","v":0},null,{"$f":"SUM(H505:H527)","v":0},null,{"$f":"SUM(J505:J527)","v":0},null,{"$f":"SUM(L505:L527)","v":0},null,"TOTAL"]
["0101010604  기  타  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 105.공용화장실(여)     개소 :1",{"$nulls":14},"0101010604"]
["지정화장실칸막이","자작나무합판마감","M2",17.45,null,{"$f":"TRUNC(E530*D530, 0)","v":0},null,{"$f":"TRUNC(G530*D530, 0)","v":0},null,{"$f":"TRUNC(I530*D530, 0)","v":0},{"$f":"TRUNC(E530+G530+I530, 0)","v":0},0,null,"57D3722009F99DF9C123903DCBC8B9718F30A1","","","0101010604","F","F","T",{"$nulls":23},"","",null,"010101060457D3722009F99DF9C123903DCBC8B9718F30A1",122]
["수밀코킹(실리콘)","삼각, 5mm이하, 방균용","M",10.16,null,0,null,0,null,0,0,0,null,"50FA920009DF72024B2E486FEF08DE","","","0101010604","T","F","F",{"$nulls":23},"","",null,"010101060450FA920009DF72024B2E486FEF08DE",123]
["방습거울후레임","스테인리스, W50*1.5t","M",6.34,null,0,null,0,null,0,0,0,null,"50FAB2500924C55AE02DCC1BFE2175","","","0101010604","T","F","F",{"$nulls":23},"","",null,"010101060450FAB2500924C55AE02DCC1BFE2175",124]
["출입구 공프레임","구로철판1.6t, 1220*2150","개소",1,null,0,null,0,null,0,0,0,null,"50FAB2500924980282224F9EC8AE99","","","0101010604","T","F","F",{"$nulls":23},"","",null,"010101060450FAB2500924980282224F9EC8AE99",125]
["방습거울설치","5mm, 틀 포함","M2",2.23,null,0,null,0,null,0,0,0,null,"50FAD2A009FE1520552E7181DB95CE","","","0101010604","T","F","F",{"$nulls":23},"","",null,"010101060450FAD2A009FE1520552E7181DB95CE",126]
["인조대리석세면대","W:600*12t,틀포함","M",2.12,null,0,null,0,null,0,0,0,null,"50FB12C0090037D9682873AC4EB01D","","","0101010604","T","F","F",{"$nulls":23},"","",null,"010101060450FB12C0090037D9682873AC4EB01D",127]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F530:F552)","v":0},null,{"$f":"SUM(H530:H552)","v":0},null,{"$f":"SUM(J530:J552)","v":0},null,{"$f":"SUM(L530:L552)","v":0},null,"TOTAL"]
["0101010701  바  닥  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 106.청소도구함     개소 :1",{"$nulls":14},"0101010701"]
["석재.타일보양","하드롱지","M2",1.3,null,{"$f":"TRUNC(E555*D555, 0)","v":0},null,{"$f":"TRUNC(G555*D555, 0)","v":0},null,{"$f":"TRUNC(I555*D555, 0)","v":0},{"$f":"TRUNC(E555+G555+I555, 0)","v":0},0,null,"50FA026009B9885A1F2BAC10AA64C9","","","0101010701","T","F","F",{"$nulls":23},"","",null,"010101070150FA026009B9885A1F2BAC10AA64C9",134]
["지정타일압착붙임 /화장실 (타일 관급)","바닥, 바탕 65mm+압 5mm","M2",1.3,null,{"$f":"TRUNC(E556*D556, 0)","v":0},null,{"$f":"TRUNC(G556*D556, 0)","v":0},null,{"$f":"TRUNC(I556*D556, 0)","v":0},0,0,null,"50FAC240091DE2698B2F0344CE27B1","","","0101010701","T","F","F",{"$nulls":23},"","",null,"010101070150FAC240091DE2698B2F0344CE27B1",135]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",0.82,null,{"$f":"TRUNC(E557*D557, 0)","v":0},null,{"$f":"TRUNC(G557*D557, 0)","v":0},null,{"$f":"TRUNC(I557*D557, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101010701","T","F","F",{"$nulls":23},"","",null,"010101070150FAE28009A0F313FA23F4CCF30D36",136]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F555:F577)","v":0},null,{"$f":"SUM(H555:H577)","v":0},null,{"$f":"SUM(J555:J577)","v":0},null,{"$f":"SUM(L555:L577)","v":0},null,"TOTAL"]
["0101010702  벽    공    사","■ 인테리어공사 ▶ 지상1층 실명 : 106.청소도구함     개소 :1",{"$nulls":14},"0101010702"]
["지정타일떠붙임 /화장실 (타일 관급)","벽, 몰탈18mm","M2",11.09,null,{"$f":"TRUNC(E580*D580, 0)","v":0},null,{"$f":"TRUNC(G580*D580, 0)","v":0},null,{"$f":"TRUNC(I580*D580, 0)","v":0},{"$f":"TRUNC(E580+G580+I580, 0)","v":0},{"$f":"TRUNC(F580+H580+J580, 0)","v":0},null,"50FAC240091DE2698B2F0344CFCDD6","","","0101010702","T","F","F",{"$nulls":23},"","",null,"010101070250FAC240091DE2698B2F0344CFCDD6",138]
{"$rows_empty":22}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F580:F602)","v":0},null,{"$f":"SUM(H580:H602)","v":0},null,{"$f":"SUM(J580:J602)","v":0},null,{"$f":"SUM(L580:L602)","v":0},null,"TOTAL"]
["0101010703  천  장  공  사","■ 인테리어공사 ▶ 지상1층 실명 : 106.청소도구함     개소 :1",{"$nulls":14},"0101010703"]
["석고보드","석고보드, 평보드, 방수, 9.5*900*1800mm(㎡)","M2",1.19,null,{"$f":"TRUNC(E605*D605, 0)","v":0},null,{"$f":"TRUNC(G605*D605, 0)","v":0},null,{"$f":"TRUNC(I605*D605, 0)","v":0},{"$f":"TRUNC(E605+G605+I605, 0)","v":0},0,null,"57D3722009F9710BAE2ED982F3A1AA138880B3","","","0101010703","F","F","T",{"$nulls":23},"","",null,"010101070357D3722009F9710BAE2ED982F3A1AA138880B3",140]
["등기구타공","다운라이트","EA",1,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101010703","F","F","T",{"$nulls":23},"","",null,"010101070357D3722009F9710B9C21B6DD9D2E4747ACE111",141]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",1.1299999999999999,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101010703","T","F","F",{"$nulls":23},"","",null,"010101070350FAB2500909EF985820B87BB6AB0D",142]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",1.1299999999999999,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101010703","T","F","F",{"$nulls":23},"","",null,"010101070350FAF2F0097711FE6F2FE675585AF3",143]
["석고판본드붙임","천장, 방수 9.5mm","M2",1.1299999999999999,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403862C1FD18B8962","","","0101010703","T","F","F",{"$nulls":23},"","",null,"010101070350FAE28009EEA403862C1FD18B8962",144]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",4.5599999999999996,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101010703","T","F","F",{"$nulls":23},"","",null,"010101070350FAE280094E44060A2808FF6AAFE4",145]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F605:F627)","v":0},null,{"$f":"SUM(H605:H627)","v":0},null,{"$f":"SUM(J605:J627)","v":0},null,{"$f":"SUM(L605:L627)","v":0},null,"TOTAL"]
["0101020101  바  닥  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 201.로비     개소 :1",{"$nulls":14},"0101020101"]
["석재.타일보양","하드롱지","M2",794.8,null,{"$f":"TRUNC(E630*D630, 0)","v":0},null,{"$f":"TRUNC(G630*D630, 0)","v":0},null,{"$f":"TRUNC(I630*D630, 0)","v":0},{"$f":"TRUNC(E630+G630+I630, 0)","v":0},0,null,"50FA026009B9885A1F2BAC10AA64C9","","","0101020101","T","F","F",{"$nulls":23},"","",null,"010102010150FA026009B9885A1F2BAC10AA64C9",151]
["시멘트모르타르바름","바닥, 77mm","M2",121.97,null,{"$f":"TRUNC(E631*D631, 0)","v":0},null,{"$f":"TRUNC(G631*D631, 0)","v":0},null,{"$f":"TRUNC(I631*D631, 0)","v":0},0,0,null,"50FA62D00969ADB3282ADD819A2D22","","","0101020101","T","F","F",{"$nulls":23},"","",null,"010102010150FA62D00969ADB3282ADD819A2D22",812]
["지정타일압착붙임 /홀 (타일관급)","바닥, 바탕 65mm+압 5mm","M2",794.8,null,{"$f":"TRUNC(E632*D632, 0)","v":0},null,{"$f":"TRUNC(G632*D632, 0)","v":0},null,{"$f":"TRUNC(I632*D632, 0)","v":0},0,0,null,"50FAC240091DE2698B2F0344CE27B2","","","0101020101","T","F","F",{"$nulls":23},"","",null,"010102010150FAC240091DE2698B2F0344CE27B2",152]
["지정카펫타일 깔기 /포인트","7.0mm","M2",121.97,null,{"$f":"TRUNC(E633*D633, 0)","v":0},null,{"$f":"TRUNC(G633*D633, 0)","v":0},null,{"$f":"TRUNC(I633*D633, 0)","v":0},0,0,null,"50FAE28009C3DCCF2C2E721949783A","","","0101020101","T","F","F",{"$nulls":23},"","",null,"010102010150FAE28009C3DCCF2C2E721949783A",620]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",34.54,null,{"$f":"TRUNC(E634*D634, 0)","v":0},null,{"$f":"TRUNC(G634*D634, 0)","v":0},null,{"$f":"TRUNC(I634*D634, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101020101","T","F","F",{"$nulls":23},"","",null,"010102010150FAE28009A0F313FA23F4CCF30D36",803]
{"$rows_empty":18}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F630:F652)","v":0},null,{"$f":"SUM(H630:H652)","v":0},null,{"$f":"SUM(J630:J652)","v":0},null,{"$f":"SUM(L630:L652)","v":0},null,"TOTAL"]
["0101020102  벽    공    사","■ 인테리어공사 ▶ 지상2층 실명 : 201.로비     개소 :1",{"$nulls":14},"0101020102"]
["벽마감용 각파이프틀설치","ㅁ-30*30","M2",59,null,{"$f":"TRUNC(E655*D655, 0)","v":0},null,{"$f":"TRUNC(G655*D655, 0)","v":0},null,{"$f":"TRUNC(I655*D655, 0)","v":0},{"$f":"TRUNC(E655+G655+I655, 0)","v":0},0,null,"50FAB25009099778C12BFF07E62024","","","0101020102","T","F","F",{"$nulls":23},"","",null,"010102010250FAB25009099778C12BFF07E62024",156]
["수벽몰딩","STL 10*80*1.6mm, 지정도장","M",32.78,null,0,null,0,null,0,0,0,null,"50FAB25009099778C12BFF07E62022","","","0101020102","T","F","F",{"$nulls":23},"","",null,"010102010250FAB25009099778C12BFF07E62022",157]
["엘리베이터출입구 마구리","구로철판1.6t, W:400","M",12.4,null,0,null,0,null,0,0,0,null,"50FAB25009099778C12BFF07E62023","","","0101020102","T","F","F",{"$nulls":23},"","",null,"010102010250FAB25009099778C12BFF07E62023",804]
["걸레받이","구로철판1.6t, W:100","M",3,null,0,null,0,null,0,0,0,null,"50FAB25009099778C12BFF07E6202C","","","0101020102","T","F","F",{"$nulls":23},"","",null,"010102010250FAB25009099778C12BFF07E6202C",805]
["화강석붙임(버너,건식,패턴시공)","벽, 고흥석 30mm","M2",236.1,null,0,null,0,null,0,0,0,null,"50FAC240092E2412022A0C87E3B371","","","0101020102","T","F","F",{"$nulls":23},"","",null,"010102010250FAC240092E2412022A0C87E3B371",158]
["화강석붙임(버너,TRUSS건식,패턴시공)","벽, 고흥석 30mm, 트러스포함","M2",170.49,null,0,null,0,null,0,0,0,null,"50FAC240092E51B27A27DE4C0D5B4E","","","0101020102","T","F","F",{"$nulls":23},"","",null,"010102010250FAC240092E51B27A27DE4C0D5B4E",806]
["친환경수성페인트(로울러칠)","내벽 3회. 친환경","M2",62.64,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FEC02D76A50311ED","","","0101020102","T","F","F",{"$nulls":23},"","",null,"010102010250FAF2F0097711FEC02D76A50311ED",159]
["친환경수성페인트(로울러칠)","내벽 3회. 친환경(GB면)","M2",59,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FEC02D76A24F126A","","","0101020102","T","F","F",{"$nulls":23},"","",null,"010102010250FAF2F0097711FEC02D76A24F126A",160]
["걸레받이용페인트칠","2회","M2",2.0299999999999998,null,0,null,0,null,0,0,0,null,"50FAF2F00966A2A451265A9E70BECD","","","0101020102","T","F","F",{"$nulls":23},"","",null,"010102010250FAF2F00966A2A451265A9E70BECD",161]
["MDF붙임(벽)","9mm","M2",67.73,null,0,null,0,null,0,0,0,null,"50FAE28009EE89516723B7798FD4FC","","","0101020102","T","F","F",{"$nulls":23},"","",null,"010102010250FAE28009EE89516723B7798FD4FC",162]
["석고판 붙임","벽, 일반 9.5mm 2겹","M2",59,null,0,null,0,null,0,0,0,null,"50FAE28009EEB69F052002C24F1E0B","","","0101020102","T","F","F",{"$nulls":23},"","",null,"010102010250FAE28009EEB69F052002C24F1E0B",807]
["지정무늬목마감","티크","M2",66.64,null,0,null,0,null,0,0,0,null,"50FB62500938F8AF6C2BA268B4F296","","","0101020102","T","F","F",{"$nulls":23},"","",null,"010102010250FB62500938F8AF6C2BA268B4F296",165]
["벽면조각파사드","","식",1,null,0,null,0,null,0,0,0,null,"51422250099FA2F9AC22E5D3FAE6313ABA60F5","","","0101020102","F","F","T",{"$nulls":23},"","",null,"010102010251422250099FA2F9AC22E5D3FAE6313ABA60F5",647]
{"$rows_empty":10}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F655:F677)","v":0},null,{"$f":"SUM(H655:H677)","v":0},null,{"$f":"SUM(J655:J677)","v":0},null,{"$f":"SUM(L655:L677)","v":0},null,"TOTAL"]
["0101020103  천  장  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 201.로비     개소 :1",{"$nulls":14},"0101020103"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",89.16,null,{"$f":"TRUNC(E680*D680, 0)","v":0},null,{"$f":"TRUNC(G680*D680, 0)","v":0},null,{"$f":"TRUNC(I680*D680, 0)","v":0},{"$f":"TRUNC(E680+G680+I680, 0)","v":0},0,null,"57D3722009F9710BAE2ED981ED5CFCF4080C3E","","","0101020103","F","F","T",{"$nulls":23},"","",null,"010102010357D3722009F9710BAE2ED981ED5CFCF4080C3E",808]
["지정타공패널","600*1200","M2",901.54,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C28EF935560ACE7D5C386","","","0101020103","F","F","T",{"$nulls":23},"","",null,"010102010357D3722009F9710B9C28EF935560ACE7D5C386",168]
["등기구타공","다운라이트","EA",152,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101020103","F","F","T",{"$nulls":23},"","",null,"010102010357D3722009F9710B9C21B6DD9D2E4747ACE111",809]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",943.52,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101020103","T","F","F",{"$nulls":23},"","",null,"010102010350FAB2500909EF985820B87BB6AB0D",171]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",84.91,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101020103","T","F","F",{"$nulls":23},"","",null,"010102010350FAF2F0097711FE6F2FE675585AF3",810]
["석고판본드붙임","천장, 일반 9.5mm","M2",84.91,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403B220C4D6970C9E","","","0101020103","T","F","F",{"$nulls":23},"","",null,"010102010350FAE28009EEA403B220C4D6970C9E",811]
["철재커텐박스설치(ㄱ자)","200*200*1.2t, STL. 도장","M",31.87,null,0,null,0,null,0,0,0,null,"50FAE2800958DF9CBC23EFCCF16A9D","","","0101020103","T","F","F",{"$nulls":23},"","",null,"010102010350FAE2800958DF9CBC23EFCCF16A9D",174]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",250.45,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101020103","T","F","F",{"$nulls":23},"","",null,"010102010350FAE280094E44060A2808FF6AAFE4",175]
["픽쳐레일","","M",29.96,null,0,null,0,null,0,0,0,null,"51422250099FA2F9AC22E5D3FAE6313ABA61AD","","","0101020103","F","F","T",{"$nulls":23},"","",null,"010102010351422250099FA2F9AC22E5D3FAE6313ABA61AD",695]
{"$rows_empty":14}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F680:F702)","v":0},null,{"$f":"SUM(H680:H702)","v":0},null,{"$f":"SUM(J680:J702)","v":0},null,{"$f":"SUM(L680:L702)","v":0},null,"TOTAL"]
["0101020104  기  타  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 201.로비     개소 :1",{"$nulls":14},"0101020104"]
["인포데스크","전면화강석포함","개",1,null,{"$f":"TRUNC(E705*D705, 0)","v":0},null,{"$f":"TRUNC(G705*D705, 0)","v":0},null,{"$f":"TRUNC(I705*D705, 0)","v":0},{"$f":"TRUNC(E705+G705+I705, 0)","v":0},{"$f":"TRUNC(F705+H705+J705, 0)","v":0},null,"57D3722009F9710B9C28E90B723AB022DF8682","","","0101020104","F","F","T",{"$nulls":23},"","",null,"010102010457D3722009F9710B9C28E90B723AB022DF8682",177]
{"$rows_empty":22}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F705:F727)","v":0},null,{"$f":"SUM(H705:H727)","v":0},null,{"$f":"SUM(J705:J727)","v":0},null,{"$f":"SUM(L705:L727)","v":0},null,"TOTAL"]
["0101020105  미 팅 박 스 공 사","■ 인테리어공사 ▶ 지상2층 실명 : 201.로비     개소 :1",{"$nulls":14},"0101020105"]
["지정카펫타일 깔기 /포인트","7.0mm","M2",19.899999999999999,null,{"$f":"TRUNC(E730*D730, 0)","v":0},null,{"$f":"TRUNC(G730*D730, 0)","v":0},null,{"$f":"TRUNC(I730*D730, 0)","v":0},{"$f":"TRUNC(E730+G730+I730, 0)","v":0},0,null,"50FAE28009C3DCCF2C2E721949783A","","","0101020105","T","F","F",{"$nulls":23},"","",null,"010102010550FAE28009C3DCCF2C2E721949783A",661]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",1.8,null,0,null,0,null,0,0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101020105","T","F","F",{"$nulls":23},"","",null,"010102010550FAE28009A0F313FA23F4CCF30D36",660]
["강화유리","투명, 12mm","M2",23.34,null,0,null,0,null,0,0,0,null,"57D3722009F960B7C12B8D2FBF841CFA000E37","","","0101020105","F","F","T",{"$nulls":23},"","",null,"010102010557D3722009F960B7C12B8D2FBF841CFA000E37",662]
["유리끼우고닦기-판유리","10mm 이상","M2",23.34,null,0,null,0,null,0,0,0,null,"50FAD2A0091066B2C12CC02B332AB3","","","0101020105","T","F","F",{"$nulls":23},"","",null,"010102010550FAD2A0091066B2C12CC02B332AB3",663]
["유리주위코킹","5*5, 실리콘","M",69.94,null,0,null,0,null,0,0,0,null,"50FA920009DF46C7E62DFAAF94BA94","","","0101020105","T","F","F",{"$nulls":23},"","",null,"010102010550FA920009DF46C7E62DFAAF94BA94",664]
["유리문/일반형(손잡이별도)","유리문, 12*900*2400mm, 손보호, 투명, 강화유리문","개",2,null,0,null,0,null,0,0,0,null,"57D3722009F960B7EC29579D2341316C335C59","","","0101020105","F","F","T",{"$nulls":23},"","",null,"010102010557D3722009F960B7EC29579D2341316C335C59",665]
["강화유리문손잡이","","조",2,null,0,null,0,null,0,0,0,null,"577D425009F25E57222FF358D48C8ABA906323","","","0101020105","F","F","T",{"$nulls":23},"","",null,"0101020105577D425009F25E57222FF358D48C8ABA906323",666]
["플로어힌지","플로어힌지, KS3호, 105kg, 강화유리문(K-8300)","조",2,null,0,null,0,null,0,0,0,null,"57D36200096DC153FB230EE5945C304AA724F2","","","0101020105","F","F","T",{"$nulls":23},"","",null,"010102010557D36200096DC153FB230EE5945C304AA724F2",667]
["플로어힌지설치","재료비 별도","개소",2,null,0,null,0,null,0,0,0,null,"50FAD2A009062B4FBC2976BE36780A","","","0101020105","T","F","F",{"$nulls":23},"","",null,"010102010550FAD2A009062B4FBC2976BE36780A",668]
["스텐후레임","W:85*1.6t","M",16.059999999999999,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D286850BB5","","","0101020105","T","F","F",{"$nulls":23},"","",null,"010102010550FAE2800958DFBF8327D286850BB5",669]
["미팅박스벽설치","9tMDF/유색분체도장+9t합판+9t석고판 양면, ㅁ-30*30각파이프틀","M2",51.1,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D286850BB4","","","0101020105","T","F","F",{"$nulls":23},"","",null,"010102010550FAE2800958DFBF8327D286850BB4",670]
{"$rows_empty":12}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F730:F752)","v":0},null,{"$f":"SUM(H730:H752)","v":0},null,{"$f":"SUM(J730:J752)","v":0},null,{"$f":"SUM(L730:L752)","v":0},null,"TOTAL"]
["0101020201  바  닥  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 202.대강당     개소 :1",{"$nulls":14},"0101020201"]
["레미콘[관급]/무근","25-21-15","M3",57.96,null,{"$f":"TRUNC(E755*D755, 0)","v":0},null,{"$f":"TRUNC(G755*D755, 0)","v":0},null,{"$f":"TRUNC(I755*D755, 0)","v":0},{"$f":"TRUNC(E755+G755+I755, 0)","v":0},0,"관급별도","57D3722009F90E35882C07B7FC6D95A56A0FC9","","","0101020201","F","F","T",{"$nulls":23},"","",null,"010102020157D3722009F90E35882C07B7FC6D95A56A0FC9",897]
["무근콘크리트타설/펌프카","슬럼프15cm, 300m3 이상/일, 붐타설","M3",56.82,null,0,null,0,null,0,0,0,null,"50FA52F0096F1AF06E2FC29253E8FC","","","0101020201","T","F","F",{"$nulls":23},"","",null,"010102020150FA52F0096F1AF06E2FC29253E8FC",896]
["섬유보강재투입","친수성","M3",56.82,null,0,null,0,null,0,0,0,null,"50FA52E00928C5307F27373ECEC016","","","0101020201","T","F","F",{"$nulls":23},"","",null,"010102020150FA52E00928C5307F27373ECEC016",895]
["시멘트모르타르바름","바닥, 47mm","M2",378.83,null,0,null,0,null,0,0,0,null,"50FA62D00969ADB3282ADD819B33AC","","","0101020201","T","F","F",{"$nulls":23},"","",null,"010102020150FA62D00969ADB3282ADD819B33AC",815]
["무대마루틀 설치(H:600)","동바리+장선목+내수합판12t","M2",63.67,null,0,null,0,null,0,0,0,null,"50FA82200948B1DDFE2B035B16A511","","","0101020201","T","F","F",{"$nulls":23},"","",null,"010102020150FA82200948B1DDFE2B035B16A511",182]
["무대계단 설치","W:1000*L:840*H:900, 라왕30t디딤판, 45*90미송각재틀포함","개소",2,null,0,null,0,null,0,0,0,null,"50FA82200948B1DDFE2B035B16A512","","","0101020201","T","F","F",{"$nulls":23},"","",null,"010102020150FA82200948B1DDFE2B035B16A512",183]
["무대전면 설치","H:900, 합판5t+MDF10t/무늬목시트, 45*45미송각재틀포함","M",13.89,null,0,null,0,null,0,0,0,null,"50FA82200948B1DDFE2B035B16A513","","","0101020201","T","F","F",{"$nulls":23},"","",null,"010102020150FA82200948B1DDFE2B035B16A513",184]
["무대전면몰딩 설치","라왕90*65/우레탄락카","M",13.89,null,0,null,0,null,0,0,0,null,"50FA82200948B1DDFE2B035B16A514","","","0101020201","T","F","F",{"$nulls":23},"","",null,"010102020150FA82200948B1DDFE2B035B16A514",185]
["무대전면걸레받이 설치","라왕24*90/우레탄락카","M",13.89,null,0,null,0,null,0,0,0,null,"50FA82200948B1DDFE2B035B16A515","","","0101020201","T","F","F",{"$nulls":23},"","",null,"010102020150FA82200948B1DDFE2B035B16A515",186]
["지정우드후로링 깔기","14mm","M2",63.67,null,0,null,0,null,0,0,0,null,"50FA82200948B1DDF82D3FF31EC069","","","0101020201","T","F","F",{"$nulls":23},"","",null,"010102020150FA82200948B1DDF82D3FF31EC069",187]
["지정카펫타일 깔기","7.0mm","M2",315.16000000000003,null,0,null,0,null,0,0,0,null,"50FAE28009C3DCCF2C2E7219497839","","","0101020201","T","F","F",{"$nulls":23},"","",null,"010102020150FAE28009C3DCCF2C2E7219497839",188]
{"$rows_empty":12}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F755:F777)","v":0},null,{"$f":"SUM(H755:H777)","v":0},null,{"$f":"SUM(J755:J777)","v":0},null,{"$f":"SUM(L755:L777)","v":0},null,"TOTAL"]
["0101020202  벽    공    사","■ 인테리어공사 ▶ 지상2층 실명 : 202.대강당     개소 :1",{"$nulls":14},"0101020202"]
["친환경수성페인트(로울러칠)","내벽 3회. 친환경(GB면)","M2",47.75,null,{"$f":"TRUNC(E780*D780, 0)","v":0},null,{"$f":"TRUNC(G780*D780, 0)","v":0},null,{"$f":"TRUNC(I780*D780, 0)","v":0},{"$f":"TRUNC(E780+G780+I780, 0)","v":0},0,null,"50FAF2F0097711FEC02D76A24F126A","","","0101020202","T","F","F",{"$nulls":23},"","",null,"010102020250FAF2F0097711FEC02D76A24F126A",191]
["걸레받이용페인트칠","2회","M2",1.9,null,0,null,0,null,0,0,0,null,"50FAF2F00966A2A451265A9E70BECD","","","0101020202","T","F","F",{"$nulls":23},"","",null,"010102020250FAF2F00966A2A451265A9E70BECD",192]
["석고판 붙임","벽, 일반 12.5mm 1겹","M2",49.64,null,0,null,0,null,0,0,0,null,"50FAE28009EEB69F052005962D179A","","","0101020202","T","F","F",{"$nulls":23},"","",null,"010102020250FAE28009EEB69F052005962D179A",816]
["MDF붙임(벽)","9mm","M2",7.81,null,0,null,0,null,0,0,0,null,"50FAE28009EE89516723B7798FD4FC","","","0101020202","T","F","F",{"$nulls":23},"","",null,"010102020250FAE28009EE89516723B7798FD4FC",195]
["지정흡음보드붙임","벽, 라인흡음보드","M2",186.49,null,0,null,0,null,0,0,0,null,"50FB62500938F8AF6C2BA31164A680","","","0101020202","T","F","F",{"$nulls":23},"","",null,"010102020250FB62500938F8AF6C2BA31164A680",197]
["지정무늬목마감","티크","M2",12.74,null,0,null,0,null,0,0,0,null,"50FB62500938F8AF6C2BA268B4F296","","","0101020202","T","F","F",{"$nulls":23},"","",null,"010102020250FB62500938F8AF6C2BA268B4F296",198]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F780:F802)","v":0},null,{"$f":"SUM(H780:H802)","v":0},null,{"$f":"SUM(J780:J802)","v":0},null,{"$f":"SUM(L780:L802)","v":0},null,"TOTAL"]
["0101020203  천  장  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 202.대강당     개소 :1",{"$nulls":14},"0101020203"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",371.15,null,{"$f":"TRUNC(E805*D805, 0)","v":0},null,{"$f":"TRUNC(G805*D805, 0)","v":0},null,{"$f":"TRUNC(I805*D805, 0)","v":0},{"$f":"TRUNC(E805+G805+I805, 0)","v":0},0,"","57D3722009F9710BAE2ED981ED5CFCF4080C3E","","","0101020203","F","F","T",{"$nulls":23},"","",null,"010102020357D3722009F9710BAE2ED981ED5CFCF4080C3E",200]
["등기구타공","다운라이트","EA",43,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101020203","F","F","T",{"$nulls":23},"","",null,"010102020357D3722009F9710B9C21B6DD9D2E4747ACE111",201]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",353.47,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101020203","T","F","F",{"$nulls":23},"","",null,"010102020350FAB2500909EF985820B87BB6AB0D",202]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",197.77,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101020203","T","F","F",{"$nulls":23},"","",null,"010102020350FAF2F0097711FE6F2FE675585AF3",203]
["석고판본드붙임","천장, 일반 9.5mm","M2",197.77,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403B220C4D6970C9E","","","0101020203","T","F","F",{"$nulls":23},"","",null,"010102020350FAE28009EEA403B220C4D6970C9E",204]
["조명박스(ㄷ형) /대강당","(150+300+150)*1.6t갈바/도장, 각파이프틀및달대포함","M",79.849999999999994,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D2822A1B8C","","","0101020203","T","F","F",{"$nulls":23},"","",null,"010102020350FAE2800958DFBF8327D2822A1B8C",205]
["천장단차보강 /대강당","H:700*1.6t갈바/도장, 각파이프틀및달대포함","M",54.44,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D287AC1478","","","0101020203","T","F","F",{"$nulls":23},"","",null,"010102020350FAE2800958DFBF8327D287AC1478",206]
["지정흡음보드붙임","천장, 라인흡음보드","M2",155.71,null,0,null,0,null,0,0,0,null,"50FB62500938F8AF6C2BA31164A683","","","0101020203","T","F","F",{"$nulls":23},"","",null,"010102020350FB62500938F8AF6C2BA31164A683",207]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",95.65,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101020203","T","F","F",{"$nulls":23},"","",null,"010102020350FAE280094E44060A2808FF6AAFE4",208]
{"$rows_empty":14}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F805:F827)","v":0},null,{"$f":"SUM(H805:H827)","v":0},null,{"$f":"SUM(J805:J827)","v":0},null,{"$f":"SUM(L805:L827)","v":0},null,"TOTAL"]
["0101020204  기  타  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 202.대강당     개소 :1",{"$nulls":14},"0101020204"]
["※ 차음형무빙월공사","100t, 방음성적 STC-48, 최종마감 PB, 세미오토(원터치)고정","",null,null,{"$f":"TRUNC(E830*D830, 0)","v":0},null,{"$f":"TRUNC(G830*D830, 0)","v":0},null,{"$f":"TRUNC(I830*D830, 0)","v":0},{"$f":"TRUNC(E830+G830+I830, 0)","v":0},0,"","","","","0101020204","F","F","F",{"$nulls":23},"","",null,"0101020204",691]
["레일","KMW-A14","M",30,null,0,null,0,null,0,0,0,"","51422250099FA2F9AC22E5D3FAE6313ABA6087","","","0101020204","F","F","T",{"$nulls":23},"","",null,"010102020451422250099FA2F9AC22E5D3FAE6313ABA6087",649]
["격납레일","더블격납기준","조",12,null,0,null,0,null,0,0,0,"","51422250099FA2F9AC22E5D3FAE6313ABA6080","","","0101020204","F","F","T",{"$nulls":23},"","",null,"010102020451422250099FA2F9AC22E5D3FAE6313ABA6080",651]
["레일보강철물","","M",42,null,0,null,0,null,0,0,0,"","51422250099FA2F9AC22E5D3FAE6313ABA60F6","","","0101020204","F","F","T",{"$nulls":23},"","",null,"010102020451422250099FA2F9AC22E5D3FAE6313ABA60F6",652]
["트롤리","KMW-AT14","EA",53,null,0,null,0,null,0,0,0,"","51422250099FA2F9AC22E5D3FAE6313ABA6082","","","0101020204","F","F","T",{"$nulls":23},"","",null,"010102020451422250099FA2F9AC22E5D3FAE6313ABA6082",653]
["판넬","2450*3000(3장)","SET",1,null,0,null,0,null,0,0,0,"","51422250099FA2F9AC22E5D3FAE6313ABA61AC","","","0101020204","F","F","T",{"$nulls":23},"","",null,"010102020451422250099FA2F9AC22E5D3FAE6313ABA61AC",692]
["판넬","11000*3000(10장)","SET",1,null,0,null,0,null,0,0,0,"","51422250099FA2F9AC22E5D3FAE6313ABA61A3","","","0101020204","F","F","T",{"$nulls":23},"","",null,"010102020451422250099FA2F9AC22E5D3FAE6313ABA61A3",693]
["판넬","16235*3000(15장)","SET",1,null,0,null,0,null,0,0,0,"","51422250099FA2F9AC22E5D3FAE6313ABA61A2","","","0101020204","F","F","T",{"$nulls":23},"","",null,"010102020451422250099FA2F9AC22E5D3FAE6313ABA61A2",694]
["레버클로져","","EA",3,null,0,null,0,null,0,0,0,"","51422250099FA2F9AC22E5D3FAE6313ABA608C","","","0101020204","F","F","T",{"$nulls":23},"","",null,"010102020451422250099FA2F9AC22E5D3FAE6313ABA608C",655]
["레일설치","","M",42,null,0,null,0,null,0,0,0,"","51422250099FA2F9AC22E5D3FAE6313ABA61AB","","","0101020204","F","F","T",{"$nulls":23},"","",null,"010102020451422250099FA2F9AC22E5D3FAE6313ABA61AB",657]
["판넬설치","","SET",1,null,0,null,0,null,0,0,0,"","51422250099FA2F9AC22E5D3FAE6313ABA61AA","","","0101020204","F","F","T",{"$nulls":23},"","",null,"010102020451422250099FA2F9AC22E5D3FAE6313ABA61AA",658]
{"$rows_empty":12}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F830:F852)","v":0},null,{"$f":"SUM(H830:H852)","v":0},null,{"$f":"SUM(J830:J852)","v":0},null,{"$f":"SUM(L830:L852)","v":0},null,"TOTAL"]
["0101020301  바  닥  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 202d.준비실-1    개소:1",{"$nulls":14},"0101020301"]
["레미콘[관급]/무근","25-21-15","M3",3.29,null,{"$f":"TRUNC(E855*D855, 0)","v":0},null,{"$f":"TRUNC(G855*D855, 0)","v":0},null,{"$f":"TRUNC(I855*D855, 0)","v":0},{"$f":"TRUNC(E855+G855+I855, 0)","v":0},0,"관급별도","57D3722009F90E35882C07B7FC6D95A56A0FC9","","","0101020301","F","F","T",{"$nulls":23},"","",null,"010102030157D3722009F90E35882C07B7FC6D95A56A0FC9",905]
["무근콘크리트타설/펌프카","슬럼프15cm, 300m3 이상/일, 붐타설","M3",3.23,null,0,null,0,null,0,0,0,null,"50FA52F0096F1AF06E2FC29253E8FC","","","0101020301","T","F","F",{"$nulls":23},"","",null,"010102030150FA52F0096F1AF06E2FC29253E8FC",819]
["섬유보강재투입","친수성","M3",3.23,null,0,null,0,null,0,0,0,null,"50FA52E00928C5307F27373ECEC016","","","0101020301","T","F","F",{"$nulls":23},"","",null,"010102030150FA52E00928C5307F27373ECEC016",906]
["시멘트모르타르바름","바닥, 47mm","M2",21.56,null,0,null,0,null,0,0,0,null,"50FA62D00969ADB3282ADD819B33AC","","","0101020301","T","F","F",{"$nulls":23},"","",null,"010102030150FA62D00969ADB3282ADD819B33AC",821]
["무대마루틀 설치(H:600)","동바리+장선목+내수합판12t","M2",21.56,null,0,null,0,null,0,0,0,null,"50FA82200948B1DDFE2B035B16A511","","","0101020301","T","F","F",{"$nulls":23},"","",null,"010102030150FA82200948B1DDFE2B035B16A511",822]
["지정우드후로링 깔기","14mm","M2",21.56,null,0,null,0,null,0,0,0,null,"50FA82200948B1DDF82D3FF31EC069","","","0101020301","T","F","F",{"$nulls":23},"","",null,"010102030150FA82200948B1DDF82D3FF31EC069",823]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F855:F877)","v":0},null,{"$f":"SUM(H855:H877)","v":0},null,{"$f":"SUM(J855:J877)","v":0},null,{"$f":"SUM(L855:L877)","v":0},null,"TOTAL"]
["0101020401  바  닥  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 202e.준비실-2    개소:1",{"$nulls":14},"0101020401"]
["레미콘[관급]/무근","25-21-15","M3",4.72,null,{"$f":"TRUNC(E880*D880, 0)","v":0},null,{"$f":"TRUNC(G880*D880, 0)","v":0},null,{"$f":"TRUNC(I880*D880, 0)","v":0},{"$f":"TRUNC(E880+G880+I880, 0)","v":0},0,"관급별도","57D3722009F90E35882C07B7FC6D95A56A0FC9","","","0101020401","F","F","T",{"$nulls":23},"","",null,"010102040157D3722009F90E35882C07B7FC6D95A56A0FC9",907]
["무근콘크리트타설/펌프카","슬럼프15cm, 300m3 이상/일, 붐타설","M3",4.63,null,0,null,0,null,0,0,0,null,"50FA52F0096F1AF06E2FC29253E8FC","","","0101020401","T","F","F",{"$nulls":23},"","",null,"010102040150FA52F0096F1AF06E2FC29253E8FC",826]
["섬유보강재투입","친수성","M3",4.63,null,0,null,0,null,0,0,0,null,"50FA52E00928C5307F27373ECEC016","","","0101020401","T","F","F",{"$nulls":23},"","",null,"010102040150FA52E00928C5307F27373ECEC016",908]
["시멘트모르타르바름","바닥, 47mm","M2",30.86,null,0,null,0,null,0,0,0,null,"50FA62D00969ADB3282ADD819B33AC","","","0101020401","T","F","F",{"$nulls":23},"","",null,"010102040150FA62D00969ADB3282ADD819B33AC",828]
["무대마루틀 설치(H:600)","동바리+장선목+내수합판12t","M2",30.86,null,0,null,0,null,0,0,0,null,"50FA82200948B1DDFE2B035B16A511","","","0101020401","T","F","F",{"$nulls":23},"","",null,"010102040150FA82200948B1DDFE2B035B16A511",829]
["지정우드후로링 깔기","14mm","M2",30.86,null,0,null,0,null,0,0,0,null,"50FA82200948B1DDF82D3FF31EC069","","","0101020401","T","F","F",{"$nulls":23},"","",null,"010102040150FA82200948B1DDF82D3FF31EC069",830]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F880:F902)","v":0},null,{"$f":"SUM(H880:H902)","v":0},null,{"$f":"SUM(J880:J902)","v":0},null,{"$f":"SUM(L880:L902)","v":0},null,"TOTAL"]
["0101020501  바  닥  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 202f.대강당화장실(남)     개소 :1",{"$nulls":14},"0101020501"]
["석재.타일보양","하드롱지","M2",21.31,null,{"$f":"TRUNC(E905*D905, 0)","v":0},null,{"$f":"TRUNC(G905*D905, 0)","v":0},null,{"$f":"TRUNC(I905*D905, 0)","v":0},{"$f":"TRUNC(E905+G905+I905, 0)","v":0},0,null,"50FA026009B9885A1F2BAC10AA64C9","","","0101020501","T","F","F",{"$nulls":23},"","",null,"010102050150FA026009B9885A1F2BAC10AA64C9",917]
["지정타일압착붙임 /화장실 (타일 관급)","바닥, 바탕 65mm+압 5mm","M2",21.31,null,{"$f":"TRUNC(E906*D906, 0)","v":0},null,{"$f":"TRUNC(G906*D906, 0)","v":0},null,{"$f":"TRUNC(I906*D906, 0)","v":0},0,0,null,"50FAC240091DE2698B2F0344CE27B1","","","0101020501","T","F","F",{"$nulls":23},"","",null,"010102050150FAC240091DE2698B2F0344CE27B1",918]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",1,null,{"$f":"TRUNC(E907*D907, 0)","v":0},null,{"$f":"TRUNC(G907*D907, 0)","v":0},null,{"$f":"TRUNC(I907*D907, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101020501","T","F","F",{"$nulls":23},"","",null,"010102050150FAE28009A0F313FA23F4CCF30D36",919]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F905:F927)","v":0},null,{"$f":"SUM(H905:H927)","v":0},null,{"$f":"SUM(J905:J927)","v":0},null,{"$f":"SUM(L905:L927)","v":0},null,"TOTAL"]
["0101020502  벽    공    사","■ 인테리어공사 ▶ 지상2층 실명 : 202f.대강당화장실(남)     개소 :1",{"$nulls":14},"0101020502"]
["소변기턱설치용 각파이프틀설치","W:200*H:1250, ㅁ-30*30","M",4.4000000000000004,null,{"$f":"TRUNC(E930*D930, 0)","v":0},null,{"$f":"TRUNC(G930*D930, 0)","v":0},null,{"$f":"TRUNC(I930*D930, 0)","v":0},{"$f":"TRUNC(E930+G930+I930, 0)","v":0},0,null,"50FAB25009099778C12BFF07E62020","","","0101020502","T","F","F",{"$nulls":23},"","",null,"010102050250FAB25009099778C12BFF07E62020",921]
["대변기턱설치용 각파이프틀설치","W:200*H:1000, ㅁ-30*30","M",4.55,null,0,null,0,null,0,0,0,null,"50FAB25009099778C12BFF07E62021","","","0101020502","T","F","F",{"$nulls":23},"","",null,"010102050250FAB25009099778C12BFF07E62021",922]
["지정타일떠붙임 /화장실 (타일 관급)","벽, 몰탈18mm","M2",63.87,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD6","","","0101020502","T","F","F",{"$nulls":23},"","",null,"010102050250FAC240091DE2698B2F0344CFCDD6",923]
["지정타일본드붙임 /화장실 (타일관급)","벽","M2",7.5,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD1","","","0101020502","T","F","F",{"$nulls":23},"","",null,"010102050250FAC240091DE2698B2F0344CFCDD1",924]
["우레탄도막방수","벽체, 비노출","M2",11.84,null,0,null,0,null,0,0,0,null,"50FA92000987C572F62EA1806E70A5","","","0101020502","T","F","F",{"$nulls":23},"","",null,"010102050250FA92000987C572F62EA1806E70A5",925]
["인조대리석 변기턱","180*30mm, 몰탈30mm","M",8.9499999999999993,null,0,null,0,null,0,0,0,null,"50FAC240092E47393F289B71873F55","","","0101020502","T","F","F",{"$nulls":23},"","",null,"010102050250FAC240092E47393F289B71873F55",926]
["벽, 합판붙임","방수 12mm 1겹","M2",11.84,null,0,null,0,null,0,0,0,null,"50FAE28009EED176C1217BDCCD06F7","","","0101020502","T","F","F",{"$nulls":23},"","",null,"010102050250FAE28009EED176C1217BDCCD06F7",927]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F930:F952)","v":0},null,{"$f":"SUM(H930:H952)","v":0},null,{"$f":"SUM(J930:J952)","v":0},null,{"$f":"SUM(L930:L952)","v":0},null,"TOTAL"]
["0101020503  천  장  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 202f.대강당화장실(남)     개소 :1",{"$nulls":14},"0101020503"]
["석고보드","석고보드, 평보드, 방수, 9.5*900*1800mm(㎡)","M2",22.376000000000001,null,{"$f":"TRUNC(E955*D955, 0)","v":0},null,{"$f":"TRUNC(G955*D955, 0)","v":0},null,{"$f":"TRUNC(I955*D955, 0)","v":0},{"$f":"TRUNC(E955+G955+I955, 0)","v":0},0,"","57D3722009F9710BAE2ED982F3A1AA138880B3","","","0101020503","F","F","T",{"$nulls":23},"","",null,"010102050357D3722009F9710BAE2ED982F3A1AA138880B3",929]
["등기구타공","다운라이트","EA",10,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101020503","F","F","T",{"$nulls":23},"","",null,"010102050357D3722009F9710B9C21B6DD9D2E4747ACE111",930]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",21.31,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101020503","T","F","F",{"$nulls":23},"","",null,"010102050350FAB2500909EF985820B87BB6AB0D",931]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",21.31,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101020503","T","F","F",{"$nulls":23},"","",null,"010102050350FAF2F0097711FE6F2FE675585AF3",932]
["석고판본드붙임","천장, 방수 9.5mm","M2",21.31,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403862C1FD18B8962","","","0101020503","T","F","F",{"$nulls":23},"","",null,"010102050350FAE28009EEA403862C1FD18B8962",933]
["조명박스(J형) /화장실","(160+160+400+400)*1.6t갈바/도장, 각파이프틀및달대포함","M",8.9499999999999993,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D286850A91","","","0101020503","T","F","F",{"$nulls":23},"","",null,"010102050350FAE2800958DFBF8327D286850A91",934]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",26.24,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101020503","T","F","F",{"$nulls":23},"","",null,"010102050350FAE280094E44060A2808FF6AAFE4",935]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F955:F977)","v":0},null,{"$f":"SUM(H955:H977)","v":0},null,{"$f":"SUM(J955:J977)","v":0},null,{"$f":"SUM(L955:L977)","v":0},null,"TOTAL"]
["0101020504  기  타  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 202f.대강당화장실(남)     개소 :1",{"$nulls":14},"0101020504"]
["지정화장실칸막이","자작나무합판마감","M2",8.89,null,{"$f":"TRUNC(E980*D980, 0)","v":0},null,{"$f":"TRUNC(G980*D980, 0)","v":0},null,{"$f":"TRUNC(I980*D980, 0)","v":0},{"$f":"TRUNC(E980+G980+I980, 0)","v":0},0]
["장애인소변기용손잡이","STS304 Ø38,1.5t","EA",1,null,0,null,0,null,0,0,0]
["수밀코킹(실리콘)","삼각, 5mm이하, 방균용","M",11.45,null,0,null,0,null,0,0,0]
["방습거울후레임","스테인리스, W50*1.5t","M",7.2,null,0,null,0,null,0,0,0]
["방습거울설치","5mm, 틀 포함","M2",2.68,null,0,null,0,null,0,0,0]
["인조대리석세면대","W:600*12t,틀포함","M",2.5499999999999998,null,0,null,0,null,0,0,0]
["소변기칸막이","400*900, 인조대리석13mm","개소",3,null,0,null,0,null,0,0,0]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F980:F1002)","v":0},null,{"$f":"SUM(H980:H1002)","v":0},null,{"$f":"SUM(J980:J1002)","v":0},null,{"$f":"SUM(L980:L1002)","v":0},null,"TOTAL"]
["0101020601  바  닥  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 202f.대강당화장실(여)     개소 :1",{"$nulls":14},"0101020601"]
["석재.타일보양","하드롱지","M2",24.98,null,{"$f":"TRUNC(E1005*D1005, 0)","v":0},null,{"$f":"TRUNC(G1005*D1005, 0)","v":0},null,{"$f":"TRUNC(I1005*D1005, 0)","v":0},{"$f":"TRUNC(E1005+G1005+I1005, 0)","v":0},0,null,"50FA026009B9885A1F2BAC10AA64C9","","","0101020601","T","F","F",{"$nulls":23},"","",null,"010102060150FA026009B9885A1F2BAC10AA64C9",947]
["지정타일압착붙임 /화장실 (타일 관급)","바닥, 바탕 65mm+압 5mm","M2",24.98,null,{"$f":"TRUNC(E1006*D1006, 0)","v":0},null,{"$f":"TRUNC(G1006*D1006, 0)","v":0},null,{"$f":"TRUNC(I1006*D1006, 0)","v":0},0,0,null,"50FAC240091DE2698B2F0344CE27B1","","","0101020601","T","F","F",{"$nulls":23},"","",null,"010102060150FAC240091DE2698B2F0344CE27B1",948]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",1,null,{"$f":"TRUNC(E1007*D1007, 0)","v":0},null,{"$f":"TRUNC(G1007*D1007, 0)","v":0},null,{"$f":"TRUNC(I1007*D1007, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101020601","T","F","F",{"$nulls":23},"","",null,"010102060150FAE28009A0F313FA23F4CCF30D36",949]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1005:F1027)","v":0},null,{"$f":"SUM(H1005:H1027)","v":0},null,{"$f":"SUM(J1005:J1027)","v":0},null,{"$f":"SUM(L1005:L1027)","v":0},null,"TOTAL"]
["0101020602  벽    공    사","■ 인테리어공사 ▶ 지상2층 실명 : 202f.대강당화장실(여)     개소 :1",{"$nulls":14},"0101020602"]
["대변기턱설치용 각파이프틀설치","W:200*H:1000, ㅁ-30*30","M",8.85,null,{"$f":"TRUNC(E1030*D1030, 0)","v":0},null,{"$f":"TRUNC(G1030*D1030, 0)","v":0},null,{"$f":"TRUNC(I1030*D1030, 0)","v":0},{"$f":"TRUNC(E1030+G1030+I1030, 0)","v":0},0,null,"50FAB25009099778C12BFF07E62021","","","0101020602","T","F","F",{"$nulls":23},"","",null,"010102060250FAB25009099778C12BFF07E62021",952]
["지정타일떠붙임 /화장실 (타일 관급)","벽, 몰탈18mm","M2",66.89,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD6","","","0101020602","T","F","F",{"$nulls":23},"","",null,"010102060250FAC240091DE2698B2F0344CFCDD6",953]
["지정타일본드붙임 /화장실 (타일관급)","벽","M2",8.85,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD1","","","0101020602","T","F","F",{"$nulls":23},"","",null,"010102060250FAC240091DE2698B2F0344CFCDD1",954]
["우레탄도막방수","벽체, 비노출","M2",10.62,null,0,null,0,null,0,0,0,null,"50FA92000987C572F62EA1806E70A5","","","0101020602","T","F","F",{"$nulls":23},"","",null,"010102060250FA92000987C572F62EA1806E70A5",955]
["인조대리석 변기턱","180*30mm, 몰탈30mm","M",8.85,null,0,null,0,null,0,0,0,null,"50FAC240092E47393F289B71873F55","","","0101020602","T","F","F",{"$nulls":23},"","",null,"010102060250FAC240092E47393F289B71873F55",956]
["벽, 합판붙임","방수 12mm 1겹","M2",10.62,null,0,null,0,null,0,0,0,null,"50FAE28009EED176C1217BDCCD06F7","","","0101020602","T","F","F",{"$nulls":23},"","",null,"010102060250FAE28009EED176C1217BDCCD06F7",957]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1030:F1052)","v":0},null,{"$f":"SUM(H1030:H1052)","v":0},null,{"$f":"SUM(J1030:J1052)","v":0},null,{"$f":"SUM(L1030:L1052)","v":0},null,"TOTAL"]
["0101020603  천  장  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 202f.대강당화장실(여)     개소 :1",{"$nulls":14},"0101020603"]
["석고보드","석고보드, 평보드, 방수, 9.5*900*1800mm(㎡)","M2",24.98,null,{"$f":"TRUNC(E1055*D1055, 0)","v":0},null,{"$f":"TRUNC(G1055*D1055, 0)","v":0},null,{"$f":"TRUNC(I1055*D1055, 0)","v":0},{"$f":"TRUNC(E1055+G1055+I1055, 0)","v":0},0,"","57D3722009F9710BAE2ED982F3A1AA138880B3","","","0101020603","F","F","T",{"$nulls":23},"","",null,"010102060357D3722009F9710BAE2ED982F3A1AA138880B3",959]
["등기구타공","다운라이트","EA",10,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101020603","F","F","T",{"$nulls":23},"","",null,"010102060357D3722009F9710B9C21B6DD9D2E4747ACE111",960]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",24.98,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101020603","T","F","F",{"$nulls":23},"","",null,"010102060350FAB2500909EF985820B87BB6AB0D",961]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",24.98,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101020603","T","F","F",{"$nulls":23},"","",null,"010102060350FAF2F0097711FE6F2FE675585AF3",962]
["석고판본드붙임","천장, 방수 9.5mm","M2",24.98,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403862C1FD18B8962","","","0101020603","T","F","F",{"$nulls":23},"","",null,"010102060350FAE28009EEA403862C1FD18B8962",963]
["조명박스(J형) /화장실","(160+160+400+400)*1.6t갈바/도장, 각파이프틀및달대포함","M",8.85,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D286850A91","","","0101020603","T","F","F",{"$nulls":23},"","",null,"010102060350FAE2800958DFBF8327D286850A91",964]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",27.94,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101020603","T","F","F",{"$nulls":23},"","",null,"010102060350FAE280094E44060A2808FF6AAFE4",965]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1055:F1077)","v":0},null,{"$f":"SUM(H1055:H1077)","v":0},null,{"$f":"SUM(J1055:J1077)","v":0},null,{"$f":"SUM(L1055:L1077)","v":0},null,"TOTAL"]
["0101020604  기  타  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 202f.대강당화장실(여)     개소 :1",{"$nulls":14},"0101020604"]
["지정화장실칸막이","자작나무합판마감","M2",31.72,null,{"$f":"TRUNC(E1080*D1080, 0)","v":0},null,{"$f":"TRUNC(G1080*D1080, 0)","v":0},null,{"$f":"TRUNC(I1080*D1080, 0)","v":0},{"$f":"TRUNC(E1080+G1080+I1080, 0)","v":0},0,null,"57D3722009F99DF9C123903DCBC8B9718F30A1","","","0101020604","F","F","T",{"$nulls":23},"","",null,"010102060457D3722009F99DF9C123903DCBC8B9718F30A1",967]
["수밀코킹(실리콘)","삼각, 5mm이하, 방균용","M",11.15,null,{"$f":"TRUNC(E1081*D1081, 0)","v":0},null,{"$f":"TRUNC(G1081*D1081, 0)","v":0},null,{"$f":"TRUNC(I1081*D1081, 0)","v":0},0,0,null,"50FA920009DF72024B2E486FEF08DE","","","0101020604","T","F","F",{"$nulls":23},"","",null,"010102060450FA920009DF72024B2E486FEF08DE",969]
["방습거울후레임","스테인리스, W50*1.5t","M",7,null,{"$f":"TRUNC(E1082*D1082, 0)","v":0},null,{"$f":"TRUNC(G1082*D1082, 0)","v":0},null,{"$f":"TRUNC(I1082*D1082, 0)","v":0},0,0,null,"50FAB2500924C55AE02DCC1BFE2175","","","0101020604","T","F","F",{"$nulls":23},"","",null,"010102060450FAB2500924C55AE02DCC1BFE2175",970]
["방습거울설치","5mm, 틀 포함","M2",2.57,null,{"$f":"TRUNC(E1083*D1083, 0)","v":0},null,{"$f":"TRUNC(G1083*D1083, 0)","v":0},null,{"$f":"TRUNC(I1083*D1083, 0)","v":0},0,0,null,"50FAD2A009FE1520552E7181DB95CE","","","0101020604","T","F","F",{"$nulls":23},"","",null,"010102060450FAD2A009FE1520552E7181DB95CE",972]
["인조대리석세면대","W:600*12t,틀포함","M",2.4500000000000002,null,{"$f":"TRUNC(E1084*D1084, 0)","v":0},null,{"$f":"TRUNC(G1084*D1084, 0)","v":0},null,{"$f":"TRUNC(I1084*D1084, 0)","v":0},0,0,null,"50FB12C0090037D9682873AC4EB01D","","","0101020604","T","F","F",{"$nulls":23},"","",null,"010102060450FB12C0090037D9682873AC4EB01D",973]
{"$rows_empty":18}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1080:F1102)","v":0},null,{"$f":"SUM(H1080:H1102)","v":0},null,{"$f":"SUM(J1080:J1102)","v":0},null,{"$f":"SUM(L1080:L1102)","v":0},null,"TOTAL"]
["0101020701  바  닥  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 203.전실-1(대강당)     개소 :1",{"$nulls":14},"0101020701"]
["레미콘[관급]/무근","25-21-15","M3",0.86,null,{"$f":"TRUNC(E1105*D1105, 0)","v":0},null,{"$f":"TRUNC(G1105*D1105, 0)","v":0},null,{"$f":"TRUNC(I1105*D1105, 0)","v":0},{"$f":"TRUNC(E1105+G1105+I1105, 0)","v":0},0,"관급별도","57D3722009F90E35882C07B7FC6D95A56A0FC9","","","0101020701","F","F","T",{"$nulls":23},"","",null,"010102070157D3722009F90E35882C07B7FC6D95A56A0FC9",909]
["무근콘크리트타설/펌프카","슬럼프15cm, 300m3 이상/일, 붐타설","M3",0.84,null,0,null,0,null,0,0,0,null,"50FA52F0096F1AF06E2FC29253E8FC","","","0101020701","T","F","F",{"$nulls":23},"","",null,"010102070150FA52F0096F1AF06E2FC29253E8FC",831]
["섬유보강재투입","친수성","M3",0.84,null,0,null,0,null,0,0,0,null,"50FA52E00928C5307F27373ECEC016","","","0101020701","T","F","F",{"$nulls":23},"","",null,"010102070150FA52E00928C5307F27373ECEC016",910]
["시멘트모르타르바름","바닥, 47mm","M2",5.62,null,0,null,0,null,0,0,0,null,"50FA62D00969ADB3282ADD819B33AC","","","0101020701","T","F","F",{"$nulls":23},"","",null,"010102070150FA62D00969ADB3282ADD819B33AC",833]
["지정카펫타일 깔기","7.0mm","M2",5.62,null,0,null,0,null,0,0,0,null,"50FAE28009C3DCCF2C2E7219497839","","","0101020701","T","F","F",{"$nulls":23},"","",null,"010102070150FAE28009C3DCCF2C2E7219497839",212]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",2,null,0,null,0,null,0,0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101020701","T","F","F",{"$nulls":23},"","",null,"010102070150FAE28009A0F313FA23F4CCF30D36",834]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1105:F1127)","v":0},null,{"$f":"SUM(H1105:H1127)","v":0},null,{"$f":"SUM(J1105:J1127)","v":0},null,{"$f":"SUM(L1105:L1127)","v":0},null,"TOTAL"]
["0101020702  벽    공    사","■ 인테리어공사 ▶ 지상2층 실명 : 203.전실-1(대강당)     개소 :1",{"$nulls":14},"0101020702"]
["친환경수성페인트(로울러칠)","내벽 3회. 친환경","M2",22.14,null,{"$f":"TRUNC(E1130*D1130, 0)","v":0},null,{"$f":"TRUNC(G1130*D1130, 0)","v":0},null,{"$f":"TRUNC(I1130*D1130, 0)","v":0},{"$f":"TRUNC(E1130+G1130+I1130, 0)","v":0},{"$f":"TRUNC(F1130+H1130+J1130, 0)","v":0},null,"50FAF2F0097711FEC02D76A50311ED","","","0101020702","T","F","F",{"$nulls":23},"","",null,"010102070250FAF2F0097711FEC02D76A50311ED",835]
["걸레받이용페인트칠","2회","M2",0.52,null,{"$f":"TRUNC(E1131*D1131, 0)","v":0},null,{"$f":"TRUNC(G1131*D1131, 0)","v":0},null,{"$f":"TRUNC(I1131*D1131, 0)","v":0},{"$f":"TRUNC(E1131+G1131+I1131, 0)","v":0},{"$f":"TRUNC(F1131+H1131+J1131, 0)","v":0},null,"50FAF2F00966A2A451265A9E70BECD","","","0101020702","T","F","F",{"$nulls":23},"","",null,"010102070250FAF2F00966A2A451265A9E70BECD",836]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1130:F1152)","v":0},null,{"$f":"SUM(H1130:H1152)","v":0},null,{"$f":"SUM(J1130:J1152)","v":0},null,{"$f":"SUM(L1130:L1152)","v":0},null,"TOTAL"]
["0101020703  천  장  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 203.전실-1(대강당)     개소 :1",{"$nulls":14},"0101020703"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",5.9,null,{"$f":"TRUNC(E1155*D1155, 0)","v":0},null,{"$f":"TRUNC(G1155*D1155, 0)","v":0},null,{"$f":"TRUNC(I1155*D1155, 0)","v":0},{"$f":"TRUNC(E1155+G1155+I1155, 0)","v":0},0,null,"57D3722009F9710BAE2ED981ED5CFCF4080C3E","","","0101020703","F","F","T",{"$nulls":23},"","",null,"010102070357D3722009F9710BAE2ED981ED5CFCF4080C3E",219]
["등기구타공","다운라이트","EA",1,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101020703","F","F","T",{"$nulls":23},"","",null,"010102070357D3722009F9710B9C21B6DD9D2E4747ACE111",220]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",5.62,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101020703","T","F","F",{"$nulls":23},"","",null,"010102070350FAB2500909EF985820B87BB6AB0D",221]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",5.62,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101020703","T","F","F",{"$nulls":23},"","",null,"010102070350FAF2F0097711FE6F2FE675585AF3",222]
["석고판본드붙임","천장, 일반 9.5mm","M2",5.62,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403B220C4D6970C9E","","","0101020703","T","F","F",{"$nulls":23},"","",null,"010102070350FAE28009EEA403B220C4D6970C9E",223]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",9.48,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101020703","T","F","F",{"$nulls":23},"","",null,"010102070350FAE280094E44060A2808FF6AAFE4",224]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1155:F1177)","v":0},null,{"$f":"SUM(H1155:H1177)","v":0},null,{"$f":"SUM(J1155:J1177)","v":0},null,{"$f":"SUM(L1155:L1177)","v":0},null,"TOTAL"]
["0101020801  바  닥  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 204.전실-2(대강당)     개소 :1",{"$nulls":14},"0101020801"]
["레미콘[관급]/무근","25-21-15","M3",0.86,null,{"$f":"TRUNC(E1180*D1180, 0)","v":0},null,{"$f":"TRUNC(G1180*D1180, 0)","v":0},null,{"$f":"TRUNC(I1180*D1180, 0)","v":0},{"$f":"TRUNC(E1180+G1180+I1180, 0)","v":0},0,"관급별도","57D3722009F90E35882C07B7FC6D95A56A0FC9","","","0101020801","F","F","T",{"$nulls":23},"","",null,"010102080157D3722009F90E35882C07B7FC6D95A56A0FC9",911]
["무근콘크리트타설/펌프카","슬럼프15cm, 300m3 이상/일, 붐타설","M3",0.84,null,0,null,0,null,0,0,0,null,"50FA52F0096F1AF06E2FC29253E8FC","","","0101020801","T","F","F",{"$nulls":23},"","",null,"010102080150FA52F0096F1AF06E2FC29253E8FC",837]
["섬유보강재투입","친수성","M3",0.84,null,0,null,0,null,0,0,0,null,"50FA52E00928C5307F27373ECEC016","","","0101020801","T","F","F",{"$nulls":23},"","",null,"010102080150FA52E00928C5307F27373ECEC016",912]
["시멘트모르타르바름","바닥, 47mm","M2",5.62,null,0,null,0,null,0,0,0,null,"50FA62D00969ADB3282ADD819B33AC","","","0101020801","T","F","F",{"$nulls":23},"","",null,"010102080150FA62D00969ADB3282ADD819B33AC",839]
["지정카펫타일 깔기","7.0mm","M2",5.62,null,0,null,0,null,0,0,0,null,"50FAE28009C3DCCF2C2E7219497839","","","0101020801","T","F","F",{"$nulls":23},"","",null,"010102080150FAE28009C3DCCF2C2E7219497839",228]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",2,null,0,null,0,null,0,0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101020801","T","F","F",{"$nulls":23},"","",null,"010102080150FAE28009A0F313FA23F4CCF30D36",840]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1180:F1202)","v":0},null,{"$f":"SUM(H1180:H1202)","v":0},null,{"$f":"SUM(J1180:J1202)","v":0},null,{"$f":"SUM(L1180:L1202)","v":0},null,"TOTAL"]
["0101020802  벽    공    사","■ 인테리어공사 ▶ 지상2층 실명 : 204.전실-2(대강당)     개소 :1",{"$nulls":14},"0101020802"]
["친환경수성페인트(로울러칠)","내벽 3회. 친환경","M2",21,null,{"$f":"TRUNC(E1205*D1205, 0)","v":0},null,{"$f":"TRUNC(G1205*D1205, 0)","v":0},null,{"$f":"TRUNC(I1205*D1205, 0)","v":0},{"$f":"TRUNC(E1205+G1205+I1205, 0)","v":0},{"$f":"TRUNC(F1205+H1205+J1205, 0)","v":0},null,"50FAF2F0097711FEC02D76A50311ED","","","0101020802","T","F","F",{"$nulls":23},"","",null,"010102080250FAF2F0097711FEC02D76A50311ED",841]
["걸레받이용페인트칠","2회","M2",0.44,null,{"$f":"TRUNC(E1206*D1206, 0)","v":0},null,{"$f":"TRUNC(G1206*D1206, 0)","v":0},null,{"$f":"TRUNC(I1206*D1206, 0)","v":0},{"$f":"TRUNC(E1206+G1206+I1206, 0)","v":0},{"$f":"TRUNC(F1206+H1206+J1206, 0)","v":0},null,"50FAF2F00966A2A451265A9E70BECD","","","0101020802","T","F","F",{"$nulls":23},"","",null,"010102080250FAF2F00966A2A451265A9E70BECD",842]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1205:F1227)","v":0},null,{"$f":"SUM(H1205:H1227)","v":0},null,{"$f":"SUM(J1205:J1227)","v":0},null,{"$f":"SUM(L1205:L1227)","v":0},null,"TOTAL"]
["0101020803  천  장  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 204.전실-2(대강당)     개소 :1"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",5.9,null,{"$f":"TRUNC(E1230*D1230, 0)","v":0},null,{"$f":"TRUNC(G1230*D1230, 0)","v":0},null,{"$f":"TRUNC(I1230*D1230, 0)","v":0},{"$f":"TRUNC(E1230+G1230+I1230, 0)","v":0},0]
["등기구타공","다운라이트","EA",1,null,0,null,0,null,0,0,0]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",5.62,null,0,null,0,null,0,0,0]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",5.62,null,0,null,0,null,0,0,0]
["석고판본드붙임","천장, 일반 9.5mm","M2",5.62,null,0,null,0,null,0,0,0]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",9.48,null,0,null,0,null,0,0,0]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1230:F1252)","v":0},null,{"$f":"SUM(H1230:H1252)","v":0},null,{"$f":"SUM(J1230:J1252)","v":0},null,{"$f":"SUM(L1230:L1252)","v":0},null,"TOTAL"]
["0101020901  바  닥  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 205.공용화장실(남)     개소 :1",{"$nulls":14},"0101020901"]
["석재.타일보양","하드롱지","M2",21.38,null,{"$f":"TRUNC(E1255*D1255, 0)","v":0},null,{"$f":"TRUNC(G1255*D1255, 0)","v":0},null,{"$f":"TRUNC(I1255*D1255, 0)","v":0},{"$f":"TRUNC(E1255+G1255+I1255, 0)","v":0},0,null,"50FA026009B9885A1F2BAC10AA64C9","","","0101020901","T","F","F",{"$nulls":23},"","",null,"010102090150FA026009B9885A1F2BAC10AA64C9",243]
["지정타일압착붙임 /화장실 (타일 관급)","바닥, 바탕 65mm+압 5mm","M2",21.38,null,{"$f":"TRUNC(E1256*D1256, 0)","v":0},null,{"$f":"TRUNC(G1256*D1256, 0)","v":0},null,{"$f":"TRUNC(I1256*D1256, 0)","v":0},0,0,null,"50FAC240091DE2698B2F0344CE27B1","","","0101020901","T","F","F",{"$nulls":23},"","",null,"010102090150FAC240091DE2698B2F0344CE27B1",244]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",1.1000000000000001,null,{"$f":"TRUNC(E1257*D1257, 0)","v":0},null,{"$f":"TRUNC(G1257*D1257, 0)","v":0},null,{"$f":"TRUNC(I1257*D1257, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101020901","T","F","F",{"$nulls":23},"","",null,"010102090150FAE28009A0F313FA23F4CCF30D36",245]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1255:F1277)","v":0},null,{"$f":"SUM(H1255:H1277)","v":0},null,{"$f":"SUM(J1255:J1277)","v":0},null,{"$f":"SUM(L1255:L1277)","v":0},null,"TOTAL"]
["0101020902  벽    공    사","■ 인테리어공사 ▶ 지상2층 실명 : 205.공용화장실(남)     개소 :1",{"$nulls":14},"0101020902"]
["소변기턱설치용 각파이프틀설치","W:200*H:1250, ㅁ-30*30","M",3.25,null,{"$f":"TRUNC(E1280*D1280, 0)","v":0},null,{"$f":"TRUNC(G1280*D1280, 0)","v":0},null,{"$f":"TRUNC(I1280*D1280, 0)","v":0},{"$f":"TRUNC(E1280+G1280+I1280, 0)","v":0},0,null,"50FAB25009099778C12BFF07E62020","","","0101020902","T","F","F",{"$nulls":23},"","",null,"010102090250FAB25009099778C12BFF07E62020",873]
["대변기턱설치용 각파이프틀설치","W:200*H:1000, ㅁ-30*30","M",4,null,0,null,0,null,0,0,0,null,"50FAB25009099778C12BFF07E62021","","","0101020902","T","F","F",{"$nulls":23},"","",null,"010102090250FAB25009099778C12BFF07E62021",874]
["지정타일떠붙임 /화장실 (타일 관급)","벽, 몰탈18mm","M2",50.89,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD6","","","0101020902","T","F","F",{"$nulls":23},"","",null,"010102090250FAC240091DE2698B2F0344CFCDD6",247]
["지정타일본드붙임 /화장실 (타일관급)","벽","M2",8.06,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD1","","","0101020902","T","F","F",{"$nulls":23},"","",null,"010102090250FAC240091DE2698B2F0344CFCDD1",875]
["우레탄도막방수","벽체, 비노출","M2",9.51,null,0,null,0,null,0,0,0,null,"50FA92000987C572F62EA1806E70A5","","","0101020902","T","F","F",{"$nulls":23},"","",null,"010102090250FA92000987C572F62EA1806E70A5",876]
["인조대리석 변기턱","180*30mm, 몰탈30mm","M",7.25,null,0,null,0,null,0,0,0,null,"50FAC240092E47393F289B71873F55","","","0101020902","T","F","F",{"$nulls":23},"","",null,"010102090250FAC240092E47393F289B71873F55",248]
["벽, 합판붙임","방수 12mm 1겹","M2",9.51,null,0,null,0,null,0,0,0,null,"50FAE28009EED176C1217BDCCD06F7","","","0101020902","T","F","F",{"$nulls":23},"","",null,"010102090250FAE28009EED176C1217BDCCD06F7",877]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1280:F1302)","v":0},null,{"$f":"SUM(H1280:H1302)","v":0},null,{"$f":"SUM(J1280:J1302)","v":0},null,{"$f":"SUM(L1280:L1302)","v":0},null,"TOTAL"]
["0101020903  천  장  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 205.공용화장실(남)     개소 :1",{"$nulls":14},"0101020903"]
["석고보드","석고보드, 평보드, 방수, 9.5*900*1800mm(㎡)","M2",22.45,null,{"$f":"TRUNC(E1305*D1305, 0)","v":0},null,{"$f":"TRUNC(G1305*D1305, 0)","v":0},null,{"$f":"TRUNC(I1305*D1305, 0)","v":0},{"$f":"TRUNC(E1305+G1305+I1305, 0)","v":0},0,"","57D3722009F9710BAE2ED982F3A1AA138880B3","","","0101020903","F","F","T",{"$nulls":23},"","",null,"010102090357D3722009F9710BAE2ED982F3A1AA138880B3",250]
["등기구타공","다운라이트","EA",7,null,0,null,0,null,0,0,0,"","57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101020903","F","F","T",{"$nulls":23},"","",null,"010102090357D3722009F9710B9C21B6DD9D2E4747ACE111",251]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",21.38,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101020903","T","F","F",{"$nulls":23},"","",null,"010102090350FAB2500909EF985820B87BB6AB0D",252]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",21.38,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101020903","T","F","F",{"$nulls":23},"","",null,"010102090350FAF2F0097711FE6F2FE675585AF3",253]
["석고판본드붙임","천장, 방수 9.5mm","M2",21.38,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403862C1FD18B8962","","","0101020903","T","F","F",{"$nulls":23},"","",null,"010102090350FAE28009EEA403862C1FD18B8962",254]
["조명박스(J형) /화장실","(160+160+400+400)*1.6t갈바/도장, 각파이프틀및달대포함","M",9.5500000000000007,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D286850A91","","","0101020903","T","F","F",{"$nulls":23},"","",null,"010102090350FAE2800958DFBF8327D286850A91",255]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",22.88,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101020903","T","F","F",{"$nulls":23},"","",null,"010102090350FAE280094E44060A2808FF6AAFE4",256]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1305:F1327)","v":0},null,{"$f":"SUM(H1305:H1327)","v":0},null,{"$f":"SUM(J1305:J1327)","v":0},null,{"$f":"SUM(L1305:L1327)","v":0},null,"TOTAL"]
["0101020904  기  타  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 205.공용화장실(남)     개소 :1",{"$nulls":14},"0101020904"]
["지정화장실칸막이","자작나무합판마감","M2",21.59,null,{"$f":"TRUNC(E1330*D1330, 0)","v":0},null,{"$f":"TRUNC(G1330*D1330, 0)","v":0},null,{"$f":"TRUNC(I1330*D1330, 0)","v":0},{"$f":"TRUNC(E1330+G1330+I1330, 0)","v":0},0,"","57D3722009F99DF9C123903DCBC8B9718F30A1","","","0101020904","F","F","T",{"$nulls":23},"","",null,"010102090457D3722009F99DF9C123903DCBC8B9718F30A1",258]
["장애인소변기용손잡이","STS304 Ø38,1.5t","EA",1,null,0,null,0,null,0,0,0,null,"50FB12C009000A0DE123F9CD7ADDE2","","","0101020904","T","F","F",{"$nulls":23},"","",null,"010102090450FB12C009000A0DE123F9CD7ADDE2",259]
["수밀코킹(실리콘)","삼각, 5mm이하, 방균용","M",10.7,null,0,null,0,null,0,0,0,null,"50FA920009DF72024B2E486FEF08DE","","","0101020904","T","F","F",{"$nulls":23},"","",null,"010102090450FA920009DF72024B2E486FEF08DE",260]
["방습거울후레임","스테인리스, W50*1.5t","M",6.7,null,0,null,0,null,0,0,0,null,"50FAB2500924C55AE02DCC1BFE2175","","","0101020904","T","F","F",{"$nulls":23},"","",null,"010102090450FAB2500924C55AE02DCC1BFE2175",261]
["출입구 공프레임","구로철판1.6t, 1220*2150","개소",1,null,0,null,0,null,0,0,0,null,"50FAB2500924980282224F9EC8AE99","","","0101020904","T","F","F",{"$nulls":23},"","",null,"010102090450FAB2500924980282224F9EC8AE99",262]
["방습거울설치","5mm, 틀 포함","M2",2.42,null,0,null,0,null,0,0,0,null,"50FAD2A009FE1520552E7181DB95CE","","","0101020904","T","F","F",{"$nulls":23},"","",null,"010102090450FAD2A009FE1520552E7181DB95CE",263]
["인조대리석세면대","W:600*12t,틀포함","M",2.2999999999999998,null,0,null,0,null,0,0,0,null,"50FB12C0090037D9682873AC4EB01D","","","0101020904","T","F","F",{"$nulls":23},"","",null,"010102090450FB12C0090037D9682873AC4EB01D",264]
["소변기칸막이","400*900, 인조대리석13mm","개소",2,null,0,null,0,null,0,0,0,null,"50FB6250091C32460A2B63C3F2AE4D","","","0101020904","T","F","F",{"$nulls":23},"","",null,"010102090450FB6250091C32460A2B63C3F2AE4D",271]
{"$rows_empty":15}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1330:F1352)","v":0},null,{"$f":"SUM(H1330:H1352)","v":0},null,{"$f":"SUM(J1330:J1352)","v":0},null,{"$f":"SUM(L1330:L1352)","v":0},null,"TOTAL"]
["0101021001  바  닥  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 206.공용화장실(여)     개소 :1",{"$nulls":14},"0101021001"]
["석재.타일보양","하드롱지","M2",24.4,null,{"$f":"TRUNC(E1355*D1355, 0)","v":0},null,{"$f":"TRUNC(G1355*D1355, 0)","v":0},null,{"$f":"TRUNC(I1355*D1355, 0)","v":0},{"$f":"TRUNC(E1355+G1355+I1355, 0)","v":0},0,null,"50FA026009B9885A1F2BAC10AA64C9","","","0101021001","T","F","F",{"$nulls":23},"","",null,"010102100150FA026009B9885A1F2BAC10AA64C9",274]
["지정타일압착붙임 /화장실 (타일 관급)","바닥, 바탕 65mm+압 5mm","M2",24.4,null,{"$f":"TRUNC(E1356*D1356, 0)","v":0},null,{"$f":"TRUNC(G1356*D1356, 0)","v":0},null,{"$f":"TRUNC(I1356*D1356, 0)","v":0},0,0,null,"50FAC240091DE2698B2F0344CE27B1","","","0101021001","T","F","F",{"$nulls":23},"","",null,"010102100150FAC240091DE2698B2F0344CE27B1",275]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",1.1000000000000001,null,{"$f":"TRUNC(E1357*D1357, 0)","v":0},null,{"$f":"TRUNC(G1357*D1357, 0)","v":0},null,{"$f":"TRUNC(I1357*D1357, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101021001","T","F","F",{"$nulls":23},"","",null,"010102100150FAE28009A0F313FA23F4CCF30D36",276]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1355:F1377)","v":0},null,{"$f":"SUM(H1355:H1377)","v":0},null,{"$f":"SUM(J1355:J1377)","v":0},null,{"$f":"SUM(L1355:L1377)","v":0},null,"TOTAL"]
["0101021002  벽    공    사","■ 인테리어공사 ▶ 지상2층 실명 : 206.공용화장실(여)     개소 :1",{"$nulls":14},"0101021002"]
["대변기턱설치용 각파이프틀설치","W:200*H:1000, ㅁ-30*30","M",8,null,{"$f":"TRUNC(E1380*D1380, 0)","v":0},null,{"$f":"TRUNC(G1380*D1380, 0)","v":0},null,{"$f":"TRUNC(I1380*D1380, 0)","v":0},{"$f":"TRUNC(E1380+G1380+I1380, 0)","v":0},0,null,"50FAB25009099778C12BFF07E62021","","","0101021002","T","F","F",{"$nulls":23},"","",null,"010102100250FAB25009099778C12BFF07E62021",878]
["지정타일떠붙임 /화장실 (타일 관급)","벽, 몰탈18mm","M2",53.3,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD6","","","0101021002","T","F","F",{"$nulls":23},"","",null,"010102100250FAC240091DE2698B2F0344CFCDD6",278]
["지정타일본드붙임 /화장실 (타일관급)","벽","M2",8,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD1","","","0101021002","T","F","F",{"$nulls":23},"","",null,"010102100250FAC240091DE2698B2F0344CFCDD1",879]
["우레탄도막방수","벽체, 비노출","M2",9.6,null,0,null,0,null,0,0,0,null,"50FA92000987C572F62EA1806E70A5","","","0101021002","T","F","F",{"$nulls":23},"","",null,"010102100250FA92000987C572F62EA1806E70A5",880]
["인조대리석 변기턱","180*30mm, 몰탈30mm","M",8,null,0,null,0,null,0,0,0,null,"50FAC240092E47393F289B71873F55","","","0101021002","T","F","F",{"$nulls":23},"","",null,"010102100250FAC240092E47393F289B71873F55",279]
["벽, 합판붙임","방수 12mm 1겹","M2",9.6,null,0,null,0,null,0,0,0,null,"50FAE28009EED176C1217BDCCD06F7","","","0101021002","T","F","F",{"$nulls":23},"","",null,"010102100250FAE28009EED176C1217BDCCD06F7",881]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1380:F1402)","v":0},null,{"$f":"SUM(H1380:H1402)","v":0},null,{"$f":"SUM(J1380:J1402)","v":0},null,{"$f":"SUM(L1380:L1402)","v":0},null,"TOTAL"]
["0101021003  천  장  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 206.공용화장실(여)     개소 :1",{"$nulls":14},"0101021003"]
["석고보드","석고보드, 평보드, 방수, 9.5*900*1800mm(㎡)","M2",25.62,null,{"$f":"TRUNC(E1405*D1405, 0)","v":0},null,{"$f":"TRUNC(G1405*D1405, 0)","v":0},null,{"$f":"TRUNC(I1405*D1405, 0)","v":0},{"$f":"TRUNC(E1405+G1405+I1405, 0)","v":0},0,"","57D3722009F9710BAE2ED982F3A1AA138880B3","","","0101021003","F","F","T",{"$nulls":23},"","",null,"010102100357D3722009F9710BAE2ED982F3A1AA138880B3",281]
["등기구타공","다운라이트","EA",7,null,0,null,0,null,0,0,0,"","57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101021003","F","F","T",{"$nulls":23},"","",null,"010102100357D3722009F9710B9C21B6DD9D2E4747ACE111",282]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",24.4,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101021003","T","F","F",{"$nulls":23},"","",null,"010102100350FAB2500909EF985820B87BB6AB0D",283]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",24.4,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101021003","T","F","F",{"$nulls":23},"","",null,"010102100350FAF2F0097711FE6F2FE675585AF3",284]
["석고판본드붙임","천장, 방수 9.5mm","M2",24.4,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403862C1FD18B8962","","","0101021003","T","F","F",{"$nulls":23},"","",null,"010102100350FAE28009EEA403862C1FD18B8962",285]
["조명박스(J형) /화장실","(160+160+400+400)*1.6t갈바/도장, 각파이프틀및달대포함","M",10.1,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D286850A91","","","0101021003","T","F","F",{"$nulls":23},"","",null,"010102100350FAE2800958DFBF8327D286850A91",286]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",23.72,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101021003","T","F","F",{"$nulls":23},"","",null,"010102100350FAE280094E44060A2808FF6AAFE4",287]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1405:F1427)","v":0},null,{"$f":"SUM(H1405:H1427)","v":0},null,{"$f":"SUM(J1405:J1427)","v":0},null,{"$f":"SUM(L1405:L1427)","v":0},null,"TOTAL"]
["0101021004  기  타  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 206.공용화장실(여)     개소 :1",{"$nulls":14},"0101021004"]
["지정화장실칸막이","자작나무합판마감","M2",43.17,null,{"$f":"TRUNC(E1430*D1430, 0)","v":0},null,{"$f":"TRUNC(G1430*D1430, 0)","v":0},null,{"$f":"TRUNC(I1430*D1430, 0)","v":0},{"$f":"TRUNC(E1430+G1430+I1430, 0)","v":0},0,null,"57D3722009F99DF9C123903DCBC8B9718F30A1","","","0101021004","F","F","T",{"$nulls":23},"","",null,"010102100457D3722009F99DF9C123903DCBC8B9718F30A1",289]
["수밀코킹(실리콘)","삼각, 5mm이하, 방균용","M",10.1,null,0,null,0,null,0,0,0,null,"50FA920009DF72024B2E486FEF08DE","","","0101021004","T","F","F",{"$nulls":23},"","",null,"010102100450FA920009DF72024B2E486FEF08DE",290]
["방습거울후레임","스테인리스, W50*1.5t","M",6.3,null,0,null,0,null,0,0,0,null,"50FAB2500924C55AE02DCC1BFE2175","","","0101021004","T","F","F",{"$nulls":23},"","",null,"010102100450FAB2500924C55AE02DCC1BFE2175",291]
["출입구 공프레임","구로철판1.6t, 1220*2150","개소",1,null,0,null,0,null,0,0,0,null,"50FAB2500924980282224F9EC8AE99","","","0101021004","T","F","F",{"$nulls":23},"","",null,"010102100450FAB2500924980282224F9EC8AE99",292]
["방습거울설치","5mm, 틀 포함","M2",2.21,null,0,null,0,null,0,0,0,null,"50FAD2A009FE1520552E7181DB95CE","","","0101021004","T","F","F",{"$nulls":23},"","",null,"010102100450FAD2A009FE1520552E7181DB95CE",293]
["인조대리석세면대","W:600*12t,틀포함","M",2.1,null,0,null,0,null,0,0,0,null,"50FB12C0090037D9682873AC4EB01D","","","0101021004","T","F","F",{"$nulls":23},"","",null,"010102100450FB12C0090037D9682873AC4EB01D",294]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1430:F1452)","v":0},null,{"$f":"SUM(H1430:H1452)","v":0},null,{"$f":"SUM(J1430:J1452)","v":0},null,{"$f":"SUM(L1430:L1452)","v":0},null,"TOTAL"]
["0101021101  바  닥  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 207.청소도구함     개소 :1",{"$nulls":14},"0101021101"]
["석재.타일보양","하드롱지","M2",1.52,null,{"$f":"TRUNC(E1455*D1455, 0)","v":0},null,{"$f":"TRUNC(G1455*D1455, 0)","v":0},null,{"$f":"TRUNC(I1455*D1455, 0)","v":0},{"$f":"TRUNC(E1455+G1455+I1455, 0)","v":0},0,null,"50FA026009B9885A1F2BAC10AA64C9","","","0101021101","T","F","F",{"$nulls":23},"","",null,"010102110150FA026009B9885A1F2BAC10AA64C9",301]
["지정타일압착붙임 /화장실 (타일 관급)","바닥, 바탕 65mm+압 5mm","M2",1.52,null,{"$f":"TRUNC(E1456*D1456, 0)","v":0},null,{"$f":"TRUNC(G1456*D1456, 0)","v":0},null,{"$f":"TRUNC(I1456*D1456, 0)","v":0},0,0,null,"50FAC240091DE2698B2F0344CE27B1","","","0101021101","T","F","F",{"$nulls":23},"","",null,"010102110150FAC240091DE2698B2F0344CE27B1",302]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",0.82,null,{"$f":"TRUNC(E1457*D1457, 0)","v":0},null,{"$f":"TRUNC(G1457*D1457, 0)","v":0},null,{"$f":"TRUNC(I1457*D1457, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101021101","T","F","F",{"$nulls":23},"","",null,"010102110150FAE28009A0F313FA23F4CCF30D36",303]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1455:F1477)","v":0},null,{"$f":"SUM(H1455:H1477)","v":0},null,{"$f":"SUM(J1455:J1477)","v":0},null,{"$f":"SUM(L1455:L1477)","v":0},null,"TOTAL"]
["0101021102  벽    공    사","■ 인테리어공사 ▶ 지상2층 실명 : 207.청소도구함     개소 :1",{"$nulls":14},"0101021102"]
["지정타일떠붙임 /화장실 (타일 관급)","벽, 몰탈18mm","M2",12.77,null,{"$f":"TRUNC(E1480*D1480, 0)","v":0},null,{"$f":"TRUNC(G1480*D1480, 0)","v":0},null,{"$f":"TRUNC(I1480*D1480, 0)","v":0},{"$f":"TRUNC(E1480+G1480+I1480, 0)","v":0},{"$f":"TRUNC(F1480+H1480+J1480, 0)","v":0},null,"50FAC240091DE2698B2F0344CFCDD6","","","0101021102","T","F","F",{"$nulls":23},"","",null,"010102110250FAC240091DE2698B2F0344CFCDD6",305]
{"$rows_empty":22}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1480:F1502)","v":0},null,{"$f":"SUM(H1480:H1502)","v":0},null,{"$f":"SUM(J1480:J1502)","v":0},null,{"$f":"SUM(L1480:L1502)","v":0},null,"TOTAL"]
["0101021103  천  장  공  사","■ 인테리어공사 ▶ 지상2층 실명 : 207.청소도구함     개소 :1",{"$nulls":14},"0101021103"]
["석고보드","석고보드, 평보드, 방수, 9.5*900*1800mm(㎡)","M2",1.42,null,{"$f":"TRUNC(E1505*D1505, 0)","v":0},null,{"$f":"TRUNC(G1505*D1505, 0)","v":0},null,{"$f":"TRUNC(I1505*D1505, 0)","v":0},{"$f":"TRUNC(E1505+G1505+I1505, 0)","v":0},0,"","57D3722009F9710BAE2ED982F3A1AA138880B3","","","0101021103","F","F","T",{"$nulls":23},"","",null,"010102110357D3722009F9710BAE2ED982F3A1AA138880B3",307]
["등기구타공","다운라이트","EA",1,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101021103","F","F","T",{"$nulls":23},"","",null,"010102110357D3722009F9710B9C21B6DD9D2E4747ACE111",308]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",1.35,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101021103","T","F","F",{"$nulls":23},"","",null,"010102110350FAB2500909EF985820B87BB6AB0D",309]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",1.35,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101021103","T","F","F",{"$nulls":23},"","",null,"010102110350FAF2F0097711FE6F2FE675585AF3",310]
["석고판본드붙임","천장, 방수 9.5mm","M2",1.35,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403862C1FD18B8962","","","0101021103","T","F","F",{"$nulls":23},"","",null,"010102110350FAE28009EEA403862C1FD18B8962",311]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",5.16,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101021103","T","F","F",{"$nulls":23},"","",null,"010102110350FAE280094E44060A2808FF6AAFE4",312]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1505:F1527)","v":0},null,{"$f":"SUM(H1505:H1527)","v":0},null,{"$f":"SUM(J1505:J1527)","v":0},null,{"$f":"SUM(L1505:L1527)","v":0},null,"TOTAL"]
["0101030101  바  닥  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 301.로비     개소 :1",{"$nulls":14},"0101030101"]
["시멘트모르타르바름","바닥, 27mm","M2",432.3,null,{"$f":"TRUNC(E1530*D1530, 0)","v":0},null,{"$f":"TRUNC(G1530*D1530, 0)","v":0},null,{"$f":"TRUNC(I1530*D1530, 0)","v":0},{"$f":"TRUNC(E1530+G1530+I1530, 0)","v":0},{"$f":"TRUNC(F1530+H1530+J1530, 0)","v":0},null,"50FA62D00969ADB3282ADD819FAB85","","","0101030101","T","F","F",{"$nulls":23},"","",null,"010103010150FA62D00969ADB3282ADD819FAB85",843]
["지정비닐타일 깔기","P-타일","M2",432.3,null,{"$f":"TRUNC(E1531*D1531, 0)","v":0},null,{"$f":"TRUNC(G1531*D1531, 0)","v":0},null,{"$f":"TRUNC(I1531*D1531, 0)","v":0},{"$f":"TRUNC(E1531+G1531+I1531, 0)","v":0},{"$f":"TRUNC(F1531+H1531+J1531, 0)","v":0},null,"50FAE28009C3DCCF2C2D6C1FDF1C9C","","","0101030101","T","F","F",{"$nulls":23},"","",null,"010103010150FAE28009C3DCCF2C2D6C1FDF1C9C",689]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1530:F1552)","v":0},null,{"$f":"SUM(H1530:H1552)","v":0},null,{"$f":"SUM(J1530:J1552)","v":0},null,{"$f":"SUM(L1530:L1552)","v":0},null,"TOTAL"]
["0101030102  벽    공    사","■ 인테리어공사 ▶ 지상3층 실명 : 301.로비     개소 :1",{"$nulls":14},"0101030102"]
["엘리베이터출입구 마구리","구로철판1.6t, W:400","M",11.2,null,{"$f":"TRUNC(E1555*D1555, 0)","v":0},null,{"$f":"TRUNC(G1555*D1555, 0)","v":0},null,{"$f":"TRUNC(I1555*D1555, 0)","v":0},{"$f":"TRUNC(E1555+G1555+I1555, 0)","v":0},0,null,"50FAB25009099778C12BFF07E62023","","","0101030102","T","F","F",{"$nulls":23},"","",null,"010103010250FAB25009099778C12BFF07E62023",844]
["걸레받이","구로철판1.6t, W:100","M",3,null,0,null,0,null,0,0,0,null,"50FAB25009099778C12BFF07E6202C","","","0101030102","T","F","F",{"$nulls":23},"","",null,"010103010250FAB25009099778C12BFF07E6202C",845]
["화강석붙임(버너,건식,패턴시공)","벽, 고흥석 30mm","M2",131.16999999999999,null,0,null,0,null,0,0,0,null,"50FAC240092E2412022A0C87E3B371","","","0101030102","T","F","F",{"$nulls":23},"","",null,"010103010250FAC240092E2412022A0C87E3B371",337]
["친환경수성페인트(로울러칠)","내벽 3회. 친환경","M2",248.82,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FEC02D76A50311ED","","","0101030102","T","F","F",{"$nulls":23},"","",null,"010103010250FAF2F0097711FEC02D76A50311ED",338]
["걸레받이용페인트칠","2회","M2",8.76,null,0,null,0,null,0,0,0,null,"50FAF2F00966A2A451265A9E70BECD","","","0101030102","T","F","F",{"$nulls":23},"","",null,"010103010250FAF2F00966A2A451265A9E70BECD",339]
["MDF붙임(벽)","9mm","M2",166.51,null,0,null,0,null,0,0,0,null,"50FAE28009EE89516723B7798FD4FC","","","0101030102","T","F","F",{"$nulls":23},"","",null,"010103010250FAE28009EE89516723B7798FD4FC",340]
["지정무늬목마감","티크","M2",161.56,null,0,null,0,null,0,0,0,null,"50FB62500938F8AF6C2BA268B4F296","","","0101030102","T","F","F",{"$nulls":23},"","",null,"010103010250FB62500938F8AF6C2BA268B4F296",342]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1555:F1577)","v":0},null,{"$f":"SUM(H1555:H1577)","v":0},null,{"$f":"SUM(J1555:J1577)","v":0},null,{"$f":"SUM(L1555:L1577)","v":0},null,"TOTAL"]
["0101030103  천  장  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 301.로비     개소 :1",{"$nulls":14},"0101030103"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",479.84,null,{"$f":"TRUNC(E1580*D1580, 0)","v":0},null,{"$f":"TRUNC(G1580*D1580, 0)","v":0},null,{"$f":"TRUNC(I1580*D1580, 0)","v":0},{"$f":"TRUNC(E1580+G1580+I1580, 0)","v":0},0,null,"57D3722009F9710BAE2ED981ED5CFCF4080C3E","","","0101030103","F","F","T",{"$nulls":23},"","",null,"010103010357D3722009F9710BAE2ED981ED5CFCF4080C3E",344]
["지정타공패널","600*1200","M2",467.25,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C28EF935560ACE7D5C386","","","0101030103","F","F","T",{"$nulls":23},"","",null,"010103010357D3722009F9710B9C28EF935560ACE7D5C386",671]
["등기구타공","다운라이트","EA",74,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101030103","F","F","T",{"$nulls":23},"","",null,"010103010357D3722009F9710B9C21B6DD9D2E4747ACE111",345]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",901.99,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101030103","T","F","F",{"$nulls":23},"","",null,"010103010350FAB2500909EF985820B87BB6AB0D",346]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",456.99,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101030103","T","F","F",{"$nulls":23},"","",null,"010103010350FAF2F0097711FE6F2FE675585AF3",347]
["석고판본드붙임","천장, 일반 9.5mm","M2",456.99,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403B220C4D6970C9E","","","0101030103","T","F","F",{"$nulls":23},"","",null,"010103010350FAE28009EEA403B220C4D6970C9E",348]
["철재커텐박스설치(ㄱ자)","200*200*1.2t, STL. 도장","M",9.0500000000000007,null,0,null,0,null,0,0,0,null,"50FAE2800958DF9CBC23EFCCF16A9D","","","0101030103","T","F","F",{"$nulls":23},"","",null,"010103010350FAE2800958DF9CBC23EFCCF16A9D",349]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",312.23,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101030103","T","F","F",{"$nulls":23},"","",null,"010103010350FAE280094E44060A2808FF6AAFE4",350]
["픽쳐레일","","M",96.71,null,0,null,0,null,0,0,0,null,"51422250099FA2F9AC22E5D3FAE6313ABA61AD","","","0101030103","F","F","T",{"$nulls":23},"","",null,"010103010351422250099FA2F9AC22E5D3FAE6313ABA61AD",696]
{"$rows_empty":14}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1580:F1602)","v":0},null,{"$f":"SUM(H1580:H1602)","v":0},null,{"$f":"SUM(J1580:J1602)","v":0},null,{"$f":"SUM(L1580:L1602)","v":0},null,"TOTAL"]
["0101030201  바  닥  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 302.원장실     개소 :1",{"$nulls":14},"0101030201"]
["시멘트모르타르바름","바닥, 27mm","M2",55.17,null,{"$f":"TRUNC(E1605*D1605, 0)","v":0},null,{"$f":"TRUNC(G1605*D1605, 0)","v":0},null,{"$f":"TRUNC(I1605*D1605, 0)","v":0},{"$f":"TRUNC(E1605+G1605+I1605, 0)","v":0},{"$f":"TRUNC(F1605+H1605+J1605, 0)","v":0},null,"50FA62D00969ADB3282ADD819FAB85","","","0101030201","T","F","F",{"$nulls":23},"","",null,"010103020150FA62D00969ADB3282ADD819FAB85",846]
["지정카펫타일 깔기","고급 7.0mm","M2",55.17,null,{"$f":"TRUNC(E1606*D1606, 0)","v":0},null,{"$f":"TRUNC(G1606*D1606, 0)","v":0},null,{"$f":"TRUNC(I1606*D1606, 0)","v":0},{"$f":"TRUNC(E1606+G1606+I1606, 0)","v":0},{"$f":"TRUNC(F1606+H1606+J1606, 0)","v":0},null,"50FAE28009C3DCCF2C2E721949783B","","","0101030201","T","F","F",{"$nulls":23},"","",null,"010103020150FAE28009C3DCCF2C2E721949783B",847]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1605:F1627)","v":0},null,{"$f":"SUM(H1605:H1627)","v":0},null,{"$f":"SUM(J1605:J1627)","v":0},null,{"$f":"SUM(L1605:L1627)","v":0},null,"TOTAL"]
["0101030202  벽    공    사","■ 인테리어공사 ▶ 지상3층 실명 : 302.원장실     개소 :1",{"$nulls":14},"0101030202"]
["스텐걸레받이","SUS H/L 1.6t, H:100","M",7.99,null,{"$f":"TRUNC(E1630*D1630, 0)","v":0},null,{"$f":"TRUNC(G1630*D1630, 0)","v":0},null,{"$f":"TRUNC(I1630*D1630, 0)","v":0},{"$f":"TRUNC(E1630+G1630+I1630, 0)","v":0},0,null,"50FAB2500947ECFABD256D4BC0E986","","","0101030202","T","F","F",{"$nulls":23},"","",null,"010103020250FAB2500947ECFABD256D4BC0E986",357]
["친환경수성페인트(로울러칠)","내벽 3회. 친환경","M2",9.7200000000000006,null,{"$f":"TRUNC(E1631*D1631, 0)","v":0},null,{"$f":"TRUNC(G1631*D1631, 0)","v":0},null,{"$f":"TRUNC(I1631*D1631, 0)","v":0},0,0,null,"50FAF2F0097711FEC02D76A50311ED","","","0101030202","T","F","F",{"$nulls":23},"","",null,"010103020250FAF2F0097711FEC02D76A50311ED",358]
["걸레받이용페인트칠","2회","M2",0.36,null,{"$f":"TRUNC(E1632*D1632, 0)","v":0},null,{"$f":"TRUNC(G1632*D1632, 0)","v":0},null,{"$f":"TRUNC(I1632*D1632, 0)","v":0},0,0,null,"50FAF2F00966A2A451265A9E70BECD","","","0101030202","T","F","F",{"$nulls":23},"","",null,"010103020250FAF2F00966A2A451265A9E70BECD",359]
["MDF붙임(벽)","9mm","M2",37.93,null,{"$f":"TRUNC(E1633*D1633, 0)","v":0},null,{"$f":"TRUNC(G1633*D1633, 0)","v":0},null,{"$f":"TRUNC(I1633*D1633, 0)","v":0},0,0,null,"50FAE28009EE89516723B7798FD4FC","","","0101030202","T","F","F",{"$nulls":23},"","",null,"010103020250FAE28009EE89516723B7798FD4FC",360]
["지정무늬목마감","티크","M2",23.31,null,{"$f":"TRUNC(E1634*D1634, 0)","v":0},null,{"$f":"TRUNC(G1634*D1634, 0)","v":0},null,{"$f":"TRUNC(I1634*D1634, 0)","v":0},0,0,null,"50FB62500938F8AF6C2BA268B4F296","","","0101030202","T","F","F",{"$nulls":23},"","",null,"010103020250FB62500938F8AF6C2BA268B4F296",362]
{"$rows_empty":18}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1630:F1652)","v":0},null,{"$f":"SUM(H1630:H1652)","v":0},null,{"$f":"SUM(J1630:J1652)","v":0},null,{"$f":"SUM(L1630:L1652)","v":0},null,"TOTAL"]
["0101030203  천  장  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 302.원장실     개소 :1",{"$nulls":14},"0101030203"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",37.1,null,{"$f":"TRUNC(E1655*D1655, 0)","v":0},null,{"$f":"TRUNC(G1655*D1655, 0)","v":0},null,{"$f":"TRUNC(I1655*D1655, 0)","v":0},{"$f":"TRUNC(E1655+G1655+I1655, 0)","v":0},0,null,"57D3722009F9710BAE2ED981ED5CFCF4080C3E","","","0101030203","F","F","T",{"$nulls":23},"","",null,"010103020357D3722009F9710BAE2ED981ED5CFCF4080C3E",364]
["보통합판","보통합판, 1급, 9.0*1220*2440mm","M2",20.420000000000002,null,0,null,0,null,0,0,0,null,"57FE5240098541A8F625467ED95EBC89C0B2EB","","","0101030203","F","F","T",{"$nulls":23},"","",null,"010103020357FE5240098541A8F625467ED95EBC89C0B2EB",882]
["등기구타공","다운라이트","EA",16,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101030203","F","F","T",{"$nulls":23},"","",null,"010103020357D3722009F9710B9C21B6DD9D2E4747ACE111",365]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",55.17,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101030203","T","F","F",{"$nulls":23},"","",null,"010103020350FAB2500909EF985820B87BB6AB0D",366]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",35.340000000000003,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101030203","T","F","F",{"$nulls":23},"","",null,"010103020350FAF2F0097711FE6F2FE675585AF3",367]
["친환경수성페인트(로울러칠)","내천장 3회. 친환경(GB면)","M2",19.829999999999998,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FEC02D7CC9052ABD","","","0101030203","T","F","F",{"$nulls":23},"","",null,"010103020350FAF2F0097711FEC02D7CC9052ABD",883]
["석고판본드붙임","천장, 일반 9.5mm","M2",55.17,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403B220C4D6970C9E","","","0101030203","T","F","F",{"$nulls":23},"","",null,"010103020350FAE28009EEA403B220C4D6970C9E",368]
["철재커텐박스설치(ㄱ자)","200*200*1.2t, STL. 도장","M",14.86,null,0,null,0,null,0,0,0,null,"50FAE2800958DF9CBC23EFCCF16A9D","","","0101030203","T","F","F",{"$nulls":23},"","",null,"010103020350FAE2800958DF9CBC23EFCCF16A9D",370]
["천장단차보강 /원장실","H:350*1.6t갈바/도장, 각파이프틀및달대포함","M",17.829999999999998,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D2807CBFE4","","","0101030203","T","F","F",{"$nulls":23},"","",null,"010103020350FAE2800958DFBF8327D2807CBFE4",371]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",14.86,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101030203","T","F","F",{"$nulls":23},"","",null,"010103020350FAE280094E44060A2808FF6AAFE4",373]
["바리솔마감","","M2",19.829999999999998,null,0,null,0,null,0,0,0,null,"50FB62500938F8A83027CB6CCCEE80","","","0101030203","T","F","F",{"$nulls":23},"","",null,"010103020350FB62500938F8A83027CB6CCCEE80",374]
{"$rows_empty":12}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1655:F1677)","v":0},null,{"$f":"SUM(H1655:H1677)","v":0},null,{"$f":"SUM(J1655:J1677)","v":0},null,{"$f":"SUM(L1655:L1677)","v":0},null,"TOTAL"]
["0101030204  기  타  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 302.원장실     개소 :1",{"$nulls":14},"0101030204"]
["책꽂이","L:3300","개",1,null,{"$f":"TRUNC(E1680*D1680, 0)","v":0},null,{"$f":"TRUNC(G1680*D1680, 0)","v":0},null,{"$f":"TRUNC(I1680*D1680, 0)","v":0},{"$f":"TRUNC(E1680+G1680+I1680, 0)","v":0},{"$f":"TRUNC(F1680+H1680+J1680, 0)","v":0},null,"51422250099FA2F9AC22E5D3FAE6313ABA61A9","","","0101030204","F","F","T",{"$nulls":23},"","",null,"010103020451422250099FA2F9AC22E5D3FAE6313ABA61A9",673]
{"$rows_empty":22}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1680:F1702)","v":0},null,{"$f":"SUM(H1680:H1702)","v":0},null,{"$f":"SUM(J1680:J1702)","v":0},null,{"$f":"SUM(L1680:L1702)","v":0},null,"TOTAL"]
["0101030301  바  닥  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 303.접견실     개소 :1",{"$nulls":14},"0101030301"]
["시멘트모르타르바름","바닥, 27mm","M2",25.14,null,{"$f":"TRUNC(E1705*D1705, 0)","v":0},null,{"$f":"TRUNC(G1705*D1705, 0)","v":0},null,{"$f":"TRUNC(I1705*D1705, 0)","v":0},{"$f":"TRUNC(E1705+G1705+I1705, 0)","v":0},{"$f":"TRUNC(F1705+H1705+J1705, 0)","v":0},null,"50FA62D00969ADB3282ADD819FAB85","","","0101030301","T","F","F",{"$nulls":23},"","",null,"010103030150FA62D00969ADB3282ADD819FAB85",848]
["지정카펫타일 깔기","7.0mm","M2",25.14,null,{"$f":"TRUNC(E1706*D1706, 0)","v":0},null,{"$f":"TRUNC(G1706*D1706, 0)","v":0},null,{"$f":"TRUNC(I1706*D1706, 0)","v":0},{"$f":"TRUNC(E1706+G1706+I1706, 0)","v":0},{"$f":"TRUNC(F1706+H1706+J1706, 0)","v":0},null,"50FAE28009C3DCCF2C2E7219497839","","","0101030301","T","F","F",{"$nulls":23},"","",null,"010103030150FAE28009C3DCCF2C2E7219497839",380]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1705:F1727)","v":0},null,{"$f":"SUM(H1705:H1727)","v":0},null,{"$f":"SUM(J1705:J1727)","v":0},null,{"$f":"SUM(L1705:L1727)","v":0},null,"TOTAL"]
["0101030302  벽    공    사","■ 인테리어공사 ▶ 지상3층 실명 : 303.접견실     개소 :1",{"$nulls":14},"0101030302"]
["스텐걸레받이","SUS H/L 1.6t, H:100","M",12.57,null,{"$f":"TRUNC(E1730*D1730, 0)","v":0},null,{"$f":"TRUNC(G1730*D1730, 0)","v":0},null,{"$f":"TRUNC(I1730*D1730, 0)","v":0},{"$f":"TRUNC(E1730+G1730+I1730, 0)","v":0},0,null,"50FAB2500947ECFABD256D4BC0E986","","","0101030302","T","F","F",{"$nulls":23},"","",null,"010103030250FAB2500947ECFABD256D4BC0E986",383]
["MDF붙임(벽)","9mm","M2",50.11,null,{"$f":"TRUNC(E1731*D1731, 0)","v":0},null,{"$f":"TRUNC(G1731*D1731, 0)","v":0},null,{"$f":"TRUNC(I1731*D1731, 0)","v":0},0,0,null,"50FAE28009EE89516723B7798FD4FC","","","0101030302","T","F","F",{"$nulls":23},"","",null,"010103030250FAE28009EE89516723B7798FD4FC",384]
["지정무늬목마감","티크","M2",35.130000000000003,null,{"$f":"TRUNC(E1732*D1732, 0)","v":0},null,{"$f":"TRUNC(G1732*D1732, 0)","v":0},null,{"$f":"TRUNC(I1732*D1732, 0)","v":0},0,0,null,"50FB62500938F8AF6C2BA268B4F296","","","0101030302","T","F","F",{"$nulls":23},"","",null,"010103030250FB62500938F8AF6C2BA268B4F296",386]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1730:F1752)","v":0},null,{"$f":"SUM(H1730:H1752)","v":0},null,{"$f":"SUM(J1730:J1752)","v":0},null,{"$f":"SUM(L1730:L1752)","v":0},null,"TOTAL"]
["0101030303  천  장  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 303.접견실     개소 :1",{"$nulls":14},"0101030303"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",26.39,null,{"$f":"TRUNC(E1755*D1755, 0)","v":0},null,{"$f":"TRUNC(G1755*D1755, 0)","v":0},null,{"$f":"TRUNC(I1755*D1755, 0)","v":0},{"$f":"TRUNC(E1755+G1755+I1755, 0)","v":0},0,"","57D3722009F9710BAE2ED981ED5CFCF4080C3E","","","0101030303","F","F","T",{"$nulls":23},"","",null,"010103030357D3722009F9710BAE2ED981ED5CFCF4080C3E",388]
["등기구타공","다운라이트","EA",4,null,0,null,0,null,0,0,0,"","57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101030303","F","F","T",{"$nulls":23},"","",null,"010103030357D3722009F9710B9C21B6DD9D2E4747ACE111",389]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",25.14,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101030303","T","F","F",{"$nulls":23},"","",null,"010103030350FAB2500909EF985820B87BB6AB0D",390]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",25.14,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101030303","T","F","F",{"$nulls":23},"","",null,"010103030350FAF2F0097711FE6F2FE675585AF3",391]
["석고판본드붙임","천장, 일반 9.5mm","M2",25.14,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403B220C4D6970C9E","","","0101030303","T","F","F",{"$nulls":23},"","",null,"010103030350FAE28009EEA403B220C4D6970C9E",392]
["철재커텐박스설치(ㄱ자)","200*200*1.2t, STL. 도장","M",3.18,null,0,null,0,null,0,0,0,null,"50FAE2800958DF9CBC23EFCCF16A9D","","","0101030303","T","F","F",{"$nulls":23},"","",null,"010103030350FAE2800958DF9CBC23EFCCF16A9D",393]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",19.440000000000001,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101030303","T","F","F",{"$nulls":23},"","",null,"010103030350FAE280094E44060A2808FF6AAFE4",394]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1755:F1777)","v":0},null,{"$f":"SUM(H1755:H1777)","v":0},null,{"$f":"SUM(J1755:J1777)","v":0},null,{"$f":"SUM(L1755:L1777)","v":0},null,"TOTAL"]
["0101030304  기  타  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 303.접견실     개소 :1",{"$nulls":14},"0101030304"]
["책꽂이","L:5200","개",1,null,{"$f":"TRUNC(E1780*D1780, 0)","v":0},null,{"$f":"TRUNC(G1780*D1780, 0)","v":0},null,{"$f":"TRUNC(I1780*D1780, 0)","v":0},{"$f":"TRUNC(E1780+G1780+I1780, 0)","v":0},{"$f":"TRUNC(F1780+H1780+J1780, 0)","v":0},"","51422250099FA2F9AC22E5D3FAE6313ABA61A8","","","0101030304","F","F","T",{"$nulls":23},"","",null,"010103030451422250099FA2F9AC22E5D3FAE6313ABA61A8",680]
{"$rows_empty":22}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1780:F1802)","v":0},null,{"$f":"SUM(H1780:H1802)","v":0},null,{"$f":"SUM(J1780:J1802)","v":0},null,{"$f":"SUM(L1780:L1802)","v":0},null,"TOTAL"]
["0101030401  바  닥  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 304.원장 행정실     개소 :1",{"$nulls":14},"0101030401"]
["시멘트모르타르바름","바닥, 27mm","M2",19.21,null,{"$f":"TRUNC(E1805*D1805, 0)","v":0},null,{"$f":"TRUNC(G1805*D1805, 0)","v":0},null,{"$f":"TRUNC(I1805*D1805, 0)","v":0},{"$f":"TRUNC(E1805+G1805+I1805, 0)","v":0},0,null,"50FA62D00969ADB3282ADD819FAB85","","","0101030401","T","F","F",{"$nulls":23},"","",null,"010103040150FA62D00969ADB3282ADD819FAB85",849]
["지정카펫타일 깔기","7.0mm","M2",19.21,null,{"$f":"TRUNC(E1806*D1806, 0)","v":0},null,{"$f":"TRUNC(G1806*D1806, 0)","v":0},null,{"$f":"TRUNC(I1806*D1806, 0)","v":0},0,0,null,"50FAE28009C3DCCF2C2E7219497839","","","0101030401","T","F","F",{"$nulls":23},"","",null,"010103040150FAE28009C3DCCF2C2E7219497839",400]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",1,null,{"$f":"TRUNC(E1807*D1807, 0)","v":0},null,{"$f":"TRUNC(G1807*D1807, 0)","v":0},null,{"$f":"TRUNC(I1807*D1807, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101030401","T","F","F",{"$nulls":23},"","",null,"010103040150FAE28009A0F313FA23F4CCF30D36",850]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1805:F1827)","v":0},null,{"$f":"SUM(H1805:H1827)","v":0},null,{"$f":"SUM(J1805:J1827)","v":0},null,{"$f":"SUM(L1805:L1827)","v":0},null,"TOTAL"]
["0101030402  벽    공    사","■ 인테리어공사 ▶ 지상3층 실명 : 304.원장 행정실     개소 :1",{"$nulls":14},"0101030402"]
["스텐걸레받이","SUS H/L 1.6t, H:100","M",17.62,null,{"$f":"TRUNC(E1830*D1830, 0)","v":0},null,{"$f":"TRUNC(G1830*D1830, 0)","v":0},null,{"$f":"TRUNC(I1830*D1830, 0)","v":0},{"$f":"TRUNC(E1830+G1830+I1830, 0)","v":0},0,null,"50FAB2500947ECFABD256D4BC0E986","","","0101030402","T","F","F",{"$nulls":23},"","",null,"010103040250FAB2500947ECFABD256D4BC0E986",403]
["MDF붙임(벽)","9mm","M2",52.14,null,{"$f":"TRUNC(E1831*D1831, 0)","v":0},null,{"$f":"TRUNC(G1831*D1831, 0)","v":0},null,{"$f":"TRUNC(I1831*D1831, 0)","v":0},0,0,null,"50FAE28009EE89516723B7798FD4FC","","","0101030402","T","F","F",{"$nulls":23},"","",null,"010103040250FAE28009EE89516723B7798FD4FC",404]
["지정무늬목마감","티크","M2",49.97,null,{"$f":"TRUNC(E1832*D1832, 0)","v":0},null,{"$f":"TRUNC(G1832*D1832, 0)","v":0},null,{"$f":"TRUNC(I1832*D1832, 0)","v":0},0,0,null,"50FB62500938F8AF6C2BA268B4F296","","","0101030402","T","F","F",{"$nulls":23},"","",null,"010103040250FB62500938F8AF6C2BA268B4F296",406]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1830:F1852)","v":0},null,{"$f":"SUM(H1830:H1852)","v":0},null,{"$f":"SUM(J1830:J1852)","v":0},null,{"$f":"SUM(L1830:L1852)","v":0},null,"TOTAL"]
["0101030403  천  장  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 304.원장 행정실     개소 :1",{"$nulls":14},"0101030403"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",20.170000000000002,null,{"$f":"TRUNC(E1855*D1855, 0)","v":0},null,{"$f":"TRUNC(G1855*D1855, 0)","v":0},null,{"$f":"TRUNC(I1855*D1855, 0)","v":0},{"$f":"TRUNC(E1855+G1855+I1855, 0)","v":0},0,"","57D3722009F9710BAE2ED981ED5CFCF4080C3E","","","0101030403","F","F","T",{"$nulls":23},"","",null,"010103040357D3722009F9710BAE2ED981ED5CFCF4080C3E",408]
["등기구타공","다운라이트","EA",6,null,0,null,0,null,0,0,0,"","57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101030403","F","F","T",{"$nulls":23},"","",null,"010103040357D3722009F9710B9C21B6DD9D2E4747ACE111",409]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",19.21,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101030403","T","F","F",{"$nulls":23},"","",null,"010103040350FAB2500909EF985820B87BB6AB0D",410]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",19.21,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101030403","T","F","F",{"$nulls":23},"","",null,"010103040350FAF2F0097711FE6F2FE675585AF3",411]
["석고판본드붙임","천장, 일반 9.5mm","M2",19.21,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403B220C4D6970C9E","","","0101030403","T","F","F",{"$nulls":23},"","",null,"010103040350FAE28009EEA403B220C4D6970C9E",412]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",21.62,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101030403","T","F","F",{"$nulls":23},"","",null,"010103040350FAE280094E44060A2808FF6AAFE4",413]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1855:F1877)","v":0},null,{"$f":"SUM(H1855:H1877)","v":0},null,{"$f":"SUM(J1855:J1877)","v":0},null,{"$f":"SUM(L1855:L1877)","v":0},null,"TOTAL"]
["0101030404  기  타  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 304.원장 행정실     개소 :1",{"$nulls":14},"0101030404"]
["인포데스크","","개",1,null,{"$f":"TRUNC(E1880*D1880, 0)","v":0},null,{"$f":"TRUNC(G1880*D1880, 0)","v":0},null,{"$f":"TRUNC(I1880*D1880, 0)","v":0},{"$f":"TRUNC(E1880+G1880+I1880, 0)","v":0},{"$f":"TRUNC(F1880+H1880+J1880, 0)","v":0},"","57D3722009F9710B9C28E90B723AB022DF87AA","","","0101030404","F","F","T",{"$nulls":23},"","",null,"010103040457D3722009F9710B9C28E90B723AB022DF87AA",415]
["싱크","","개",1,null,{"$f":"TRUNC(E1881*D1881, 0)","v":0},null,{"$f":"TRUNC(G1881*D1881, 0)","v":0},null,{"$f":"TRUNC(I1881*D1881, 0)","v":0},{"$f":"TRUNC(E1881+G1881+I1881, 0)","v":0},{"$f":"TRUNC(F1881+H1881+J1881, 0)","v":0},"","57D3722009F9710B9C28E90B723AB022DF87AD","","","0101030404","F","F","T",{"$nulls":23},"","",null,"010103040457D3722009F9710B9C28E90B723AB022DF87AD",678]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1880:F1902)","v":0},null,{"$f":"SUM(H1880:H1902)","v":0},null,{"$f":"SUM(J1880:J1902)","v":0},null,{"$f":"SUM(L1880:L1902)","v":0},null,"TOTAL"]
["0101030501  바  닥  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 305.원장 창고     개소 :1",{"$nulls":14},"0101030501"]
["시멘트모르타르바름","바닥, 27mm","M2",10.15,null,{"$f":"TRUNC(E1905*D1905, 0)","v":0},null,{"$f":"TRUNC(G1905*D1905, 0)","v":0},null,{"$f":"TRUNC(I1905*D1905, 0)","v":0},{"$f":"TRUNC(E1905+G1905+I1905, 0)","v":0},{"$f":"TRUNC(F1905+H1905+J1905, 0)","v":0},null,"50FA62D00969ADB3282ADD819FAB85","","","0101030501","T","F","F",{"$nulls":23},"","",null,"010103050150FA62D00969ADB3282ADD819FAB85",851]
["지정카펫타일 깔기","7.0mm","M2",10.15,null,{"$f":"TRUNC(E1906*D1906, 0)","v":0},null,{"$f":"TRUNC(G1906*D1906, 0)","v":0},null,{"$f":"TRUNC(I1906*D1906, 0)","v":0},{"$f":"TRUNC(E1906+G1906+I1906, 0)","v":0},{"$f":"TRUNC(F1906+H1906+J1906, 0)","v":0},null,"50FAE28009C3DCCF2C2E7219497839","","","0101030501","T","F","F",{"$nulls":23},"","",null,"010103050150FAE28009C3DCCF2C2E7219497839",420]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1905:F1927)","v":0},null,{"$f":"SUM(H1905:H1927)","v":0},null,{"$f":"SUM(J1905:J1927)","v":0},null,{"$f":"SUM(L1905:L1927)","v":0},null,"TOTAL"]
["0101030502  벽    공    사","■ 인테리어공사 ▶ 지상3층 실명 : 305.원장 창고     개소 :1",{"$nulls":14},"0101030502"]
["걸레받이용페인트칠","2회","M2",0.84,null,{"$f":"TRUNC(E1930*D1930, 0)","v":0},null,{"$f":"TRUNC(G1930*D1930, 0)","v":0},null,{"$f":"TRUNC(I1930*D1930, 0)","v":0},{"$f":"TRUNC(E1930+G1930+I1930, 0)","v":0},0,null,"50FAF2F00966A2A451265A9E70BECD","","","0101030502","T","F","F",{"$nulls":23},"","",null,"010103050250FAF2F00966A2A451265A9E70BECD",422]
["벽지바름","지정실크벽지","M2",24.36,null,{"$f":"TRUNC(E1931*D1931, 0)","v":0},null,{"$f":"TRUNC(G1931*D1931, 0)","v":0},null,{"$f":"TRUNC(I1931*D1931, 0)","v":0},0,0,null,"50FAE28009FF1B214529ED4347C667","","","0101030502","T","F","F",{"$nulls":23},"","",null,"010103050250FAE28009FF1B214529ED4347C667",423]
["석고판 붙임","벽, 일반 12.5mm 1겹","M2",14.22,null,{"$f":"TRUNC(E1932*D1932, 0)","v":0},null,{"$f":"TRUNC(G1932*D1932, 0)","v":0},null,{"$f":"TRUNC(I1932*D1932, 0)","v":0},0,0,null,"50FAE28009EEB69F052005962D179A","","","0101030502","T","F","F",{"$nulls":23},"","",null,"010103050250FAE28009EEB69F052005962D179A",425]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1930:F1952)","v":0},null,{"$f":"SUM(H1930:H1952)","v":0},null,{"$f":"SUM(J1930:J1952)","v":0},null,{"$f":"SUM(L1930:L1952)","v":0},null,"TOTAL"]
["0101030503  천  장  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 305.원장 창고     개소 :1",{"$nulls":14},"0101030503"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",10.66,null,{"$f":"TRUNC(E1955*D1955, 0)","v":0},null,{"$f":"TRUNC(G1955*D1955, 0)","v":0},null,{"$f":"TRUNC(I1955*D1955, 0)","v":0},{"$f":"TRUNC(E1955+G1955+I1955, 0)","v":0},0,null,"57D3722009F9710BAE2ED981ED5CFCF4080C3E","","","0101030503","F","F","T",{"$nulls":23},"","",null,"010103050357D3722009F9710BAE2ED981ED5CFCF4080C3E",427]
["등기구타공","다운라이트","EA",4,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101030503","F","F","T",{"$nulls":23},"","",null,"010103050357D3722009F9710B9C21B6DD9D2E4747ACE111",428]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",10.15,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101030503","T","F","F",{"$nulls":23},"","",null,"010103050350FAB2500909EF985820B87BB6AB0D",429]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",10.15,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101030503","T","F","F",{"$nulls":23},"","",null,"010103050350FAF2F0097711FE6F2FE675585AF3",430]
["석고판본드붙임","천장, 일반 9.5mm","M2",10.15,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403B220C4D6970C9E","","","0101030503","T","F","F",{"$nulls":23},"","",null,"010103050350FAE28009EEA403B220C4D6970C9E",431]
["철재커텐박스설치(ㄱ자)","200*200*1.2t, STL. 도장","M",4.8,null,0,null,0,null,0,0,0,null,"50FAE2800958DF9CBC23EFCCF16A9D","","","0101030503","T","F","F",{"$nulls":23},"","",null,"010103050350FAE2800958DF9CBC23EFCCF16A9D",432]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",11.2,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101030503","T","F","F",{"$nulls":23},"","",null,"010103050350FAE280094E44060A2808FF6AAFE4",433]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1955:F1977)","v":0},null,{"$f":"SUM(H1955:H1977)","v":0},null,{"$f":"SUM(J1955:J1977)","v":0},null,{"$f":"SUM(L1955:L1977)","v":0},null,"TOTAL"]
["0101030601  바  닥  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 306.원장 화장실     개소 :1",{"$nulls":14},"0101030601"]
["석재.타일보양","하드롱지","M2",4.08,null,{"$f":"TRUNC(E1980*D1980, 0)","v":0},null,{"$f":"TRUNC(G1980*D1980, 0)","v":0},null,{"$f":"TRUNC(I1980*D1980, 0)","v":0},{"$f":"TRUNC(E1980+G1980+I1980, 0)","v":0},0,null,"50FA026009B9885A1F2BAC10AA64C9","","","0101030601","T","F","F",{"$nulls":23},"","",null,"010103060150FA026009B9885A1F2BAC10AA64C9",436]
["지정타일압착붙임 /화장실 (타일 관급)","바닥, 바탕 65mm+압 5mm","M2",4.08,null,{"$f":"TRUNC(E1981*D1981, 0)","v":0},null,{"$f":"TRUNC(G1981*D1981, 0)","v":0},null,{"$f":"TRUNC(I1981*D1981, 0)","v":0},0,0,null,"50FAC240091DE2698B2F0344CE27B1","","","0101030601","T","F","F",{"$nulls":23},"","",null,"010103060150FAC240091DE2698B2F0344CE27B1",437]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",0.82,null,{"$f":"TRUNC(E1982*D1982, 0)","v":0},null,{"$f":"TRUNC(G1982*D1982, 0)","v":0},null,{"$f":"TRUNC(I1982*D1982, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101030601","T","F","F",{"$nulls":23},"","",null,"010103060150FAE28009A0F313FA23F4CCF30D36",438]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F1980:F2002)","v":0},null,{"$f":"SUM(H1980:H2002)","v":0},null,{"$f":"SUM(J1980:J2002)","v":0},null,{"$f":"SUM(L1980:L2002)","v":0},null,"TOTAL"]
["0101030602  벽    공    사","■ 인테리어공사 ▶ 지상3층 실명 : 306.원장 화장실     개소 :1",{"$nulls":14},"0101030602"]
["지정타일떠붙임 /원장화장실 (타일 관급)","벽, 몰탈18mm","M2",21.28,null,{"$f":"TRUNC(E2005*D2005, 0)","v":0},null,{"$f":"TRUNC(G2005*D2005, 0)","v":0},null,{"$f":"TRUNC(I2005*D2005, 0)","v":0},{"$f":"TRUNC(E2005+G2005+I2005, 0)","v":0},{"$f":"TRUNC(F2005+H2005+J2005, 0)","v":0},null,"50FAC240091DE2698B2F0344CFCDD0","","","0101030602","T","F","F",{"$nulls":23},"","",null,"010103060250FAC240091DE2698B2F0344CFCDD0",621]
{"$rows_empty":22}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2005:F2027)","v":0},null,{"$f":"SUM(H2005:H2027)","v":0},null,{"$f":"SUM(J2005:J2027)","v":0},null,{"$f":"SUM(L2005:L2027)","v":0},null,"TOTAL"]
["0101030603  천  장  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 306.원장 화장실     개소 :1",{"$nulls":14},"0101030603"]
["석고보드","석고보드, 평보드, 방수, 9.5*900*1800mm(㎡)","M2",4.28,null,{"$f":"TRUNC(E2030*D2030, 0)","v":0},null,{"$f":"TRUNC(G2030*D2030, 0)","v":0},null,{"$f":"TRUNC(I2030*D2030, 0)","v":0},{"$f":"TRUNC(E2030+G2030+I2030, 0)","v":0},0,null,"57D3722009F9710BAE2ED982F3A1AA138880B3","","","0101030603","F","F","T",{"$nulls":23},"","",null,"010103060357D3722009F9710BAE2ED982F3A1AA138880B3",442]
["등기구타공","다운라이트","EA",2,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101030603","F","F","T",{"$nulls":23},"","",null,"010103060357D3722009F9710B9C21B6DD9D2E4747ACE111",443]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",4.08,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101030603","T","F","F",{"$nulls":23},"","",null,"010103060350FAB2500909EF985820B87BB6AB0D",444]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",4.08,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101030603","T","F","F",{"$nulls":23},"","",null,"010103060350FAF2F0097711FE6F2FE675585AF3",445]
["석고판본드붙임","천장, 방수 9.5mm","M2",4.08,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403862C1FD18B8962","","","0101030603","T","F","F",{"$nulls":23},"","",null,"010103060350FAE28009EEA403862C1FD18B8962",446]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",8.1999999999999993,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101030603","T","F","F",{"$nulls":23},"","",null,"010103060350FAE280094E44060A2808FF6AAFE4",447]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2030:F2052)","v":0},null,{"$f":"SUM(H2030:H2052)","v":0},null,{"$f":"SUM(J2030:J2052)","v":0},null,{"$f":"SUM(L2030:L2052)","v":0},null,"TOTAL"]
["0101030604  기  타  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 306.원장 화장실     개소 :1",{"$nulls":14},"0101030604"]
["수밀코킹(실리콘)","삼각, 5mm이하, 방균용","M",2,null,{"$f":"TRUNC(E2055*D2055, 0)","v":0},null,{"$f":"TRUNC(G2055*D2055, 0)","v":0},null,{"$f":"TRUNC(I2055*D2055, 0)","v":0},{"$f":"TRUNC(E2055+G2055+I2055, 0)","v":0},0,null,"50FA920009DF72024B2E486FEF08DE","","","0101030604","T","F","F",{"$nulls":23},"","",null,"010103060450FA920009DF72024B2E486FEF08DE",449]
["방습거울설치","5mm, 틀 포함","M2",0.24,null,{"$f":"TRUNC(E2056*D2056, 0)","v":0},null,{"$f":"TRUNC(G2056*D2056, 0)","v":0},null,{"$f":"TRUNC(I2056*D2056, 0)","v":0},0,0,null,"50FAD2A009FE1520552E7181DB95CE","","","0101030604","T","F","F",{"$nulls":23},"","",null,"010103060450FAD2A009FE1520552E7181DB95CE",450]
["샤워부스","강화유리12t, W:1640*H:1800","개소",1,null,{"$f":"TRUNC(E2057*D2057, 0)","v":0},null,{"$f":"TRUNC(G2057*D2057, 0)","v":0},null,{"$f":"TRUNC(I2057*D2057, 0)","v":0},0,0,null,"50FB6250091C32460A2B63C2ED68A3","","","0101030604","T","F","F",{"$nulls":23},"","",null,"010103060450FB6250091C32460A2B63C2ED68A3",456]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2055:F2077)","v":0},null,{"$f":"SUM(H2055:H2077)","v":0},null,{"$f":"SUM(J2055:J2077)","v":0},null,{"$f":"SUM(L2055:L2077)","v":0},null,"TOTAL"]
["0101030701  바  닥  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 307.부원장실     개소 :1",{"$nulls":14},"0101030701"]
["시멘트모르타르바름","바닥, 27mm","M2",55.22,null,{"$f":"TRUNC(E2080*D2080, 0)","v":0},null,{"$f":"TRUNC(G2080*D2080, 0)","v":0},null,{"$f":"TRUNC(I2080*D2080, 0)","v":0},{"$f":"TRUNC(E2080+G2080+I2080, 0)","v":0},{"$f":"TRUNC(F2080+H2080+J2080, 0)","v":0},null,"50FA62D00969ADB3282ADD819FAB85","","","0101030701","T","F","F",{"$nulls":23},"","",null,"010103070150FA62D00969ADB3282ADD819FAB85",852]
["지정카펫타일 깔기","고급 7.0mm","M2",55.22,null,{"$f":"TRUNC(E2081*D2081, 0)","v":0},null,{"$f":"TRUNC(G2081*D2081, 0)","v":0},null,{"$f":"TRUNC(I2081*D2081, 0)","v":0},{"$f":"TRUNC(E2081+G2081+I2081, 0)","v":0},{"$f":"TRUNC(F2081+H2081+J2081, 0)","v":0},null,"50FAE28009C3DCCF2C2E721949783B","","","0101030701","T","F","F",{"$nulls":23},"","",null,"010103070150FAE28009C3DCCF2C2E721949783B",853]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2080:F2102)","v":0},null,{"$f":"SUM(H2080:H2102)","v":0},null,{"$f":"SUM(J2080:J2102)","v":0},null,{"$f":"SUM(L2080:L2102)","v":0},null,"TOTAL"]
["0101030702  벽    공    사","■ 인테리어공사 ▶ 지상3층 실명 : 307.부원장실     개소 :1",{"$nulls":14},"0101030702"]
["스텐걸레받이","SUS H/L 1.6t, H:100","M",15.59,null,{"$f":"TRUNC(E2105*D2105, 0)","v":0},null,{"$f":"TRUNC(G2105*D2105, 0)","v":0},null,{"$f":"TRUNC(I2105*D2105, 0)","v":0},{"$f":"TRUNC(E2105+G2105+I2105, 0)","v":0},0,null,"50FAB2500947ECFABD256D4BC0E986","","","0101030702","T","F","F",{"$nulls":23},"","",null,"010103070250FAB2500947ECFABD256D4BC0E986",463]
["MDF붙임(벽)","9mm","M2",44.34,null,{"$f":"TRUNC(E2106*D2106, 0)","v":0},null,{"$f":"TRUNC(G2106*D2106, 0)","v":0},null,{"$f":"TRUNC(I2106*D2106, 0)","v":0},0,0,null,"50FAE28009EE89516723B7798FD4FC","","","0101030702","T","F","F",{"$nulls":23},"","",null,"010103070250FAE28009EE89516723B7798FD4FC",464]
["지정무늬목마감","티크","M2",42.68,null,{"$f":"TRUNC(E2107*D2107, 0)","v":0},null,{"$f":"TRUNC(G2107*D2107, 0)","v":0},null,{"$f":"TRUNC(I2107*D2107, 0)","v":0},0,0,null,"50FB62500938F8AF6C2BA268B4F296","","","0101030702","T","F","F",{"$nulls":23},"","",null,"010103070250FB62500938F8AF6C2BA268B4F296",466]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2105:F2127)","v":0},null,{"$f":"SUM(H2105:H2127)","v":0},null,{"$f":"SUM(J2105:J2127)","v":0},null,{"$f":"SUM(L2105:L2127)","v":0},null,"TOTAL"]
["0101030703  천  장  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 307.부원장실     개소 :1",{"$nulls":14},"0101030703"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",37.090000000000003,null,{"$f":"TRUNC(E2130*D2130, 0)","v":0},null,{"$f":"TRUNC(G2130*D2130, 0)","v":0},null,{"$f":"TRUNC(I2130*D2130, 0)","v":0},{"$f":"TRUNC(E2130+G2130+I2130, 0)","v":0},0,"","57D3722009F9710BAE2ED981ED5CFCF4080C3E","","","0101030703","F","F","T",{"$nulls":23},"","",null,"010103070357D3722009F9710BAE2ED981ED5CFCF4080C3E",468]
["보통합판","보통합판, 1급, 9.0*1220*2440mm","M2",20.5,null,0,null,0,null,0,0,0,"","57FE5240098541A8F625467ED95EBC89C0B2EB","","","0101030703","F","F","T",{"$nulls":23},"","",null,"010103070357FE5240098541A8F625467ED95EBC89C0B2EB",884]
["등기구타공","다운라이트","EA",16,null,0,null,0,null,0,0,0,"","57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101030703","F","F","T",{"$nulls":23},"","",null,"010103070357D3722009F9710B9C21B6DD9D2E4747ACE111",469]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",55.22,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101030703","T","F","F",{"$nulls":23},"","",null,"010103070350FAB2500909EF985820B87BB6AB0D",470]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",35.32,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101030703","T","F","F",{"$nulls":23},"","",null,"010103070350FAF2F0097711FE6F2FE675585AF3",885]
["친환경수성페인트(로울러칠)","내천장 3회. 친환경(GB면)","M2",19.899999999999999,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FEC02D7CC9052ABD","","","0101030703","T","F","F",{"$nulls":23},"","",null,"010103070350FAF2F0097711FEC02D7CC9052ABD",471]
["석고판본드붙임","천장, 일반 9.5mm","M2",55.22,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403B220C4D6970C9E","","","0101030703","T","F","F",{"$nulls":23},"","",null,"010103070350FAE28009EEA403B220C4D6970C9E",472]
["철재커텐박스설치(ㄱ자)","200*200*1.2t, STL. 도장","M",15.29,null,0,null,0,null,0,0,0,null,"50FAE2800958DF9CBC23EFCCF16A9D","","","0101030703","T","F","F",{"$nulls":23},"","",null,"010103070350FAE2800958DF9CBC23EFCCF16A9D",474]
["천장단차보강 /원장실","H:350*1.6t갈바/도장, 각파이프틀및달대포함","M",18.73,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D2807CBFE4","","","0101030703","T","F","F",{"$nulls":23},"","",null,"010103070350FAE2800958DFBF8327D2807CBFE4",475]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",16.59,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101030703","T","F","F",{"$nulls":23},"","",null,"010103070350FAE280094E44060A2808FF6AAFE4",477]
["바리솔마감","","M2",19.899999999999999,null,0,null,0,null,0,0,0,null,"50FB62500938F8A83027CB6CCCEE80","","","0101030703","T","F","F",{"$nulls":23},"","",null,"010103070350FB62500938F8A83027CB6CCCEE80",478]
{"$rows_empty":12}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2130:F2152)","v":0},null,{"$f":"SUM(H2130:H2152)","v":0},null,{"$f":"SUM(J2130:J2152)","v":0},null,{"$f":"SUM(L2130:L2152)","v":0},null,"TOTAL"]
["0101030704  기  타  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 307.부원장실     개소 :1",{"$nulls":14},"0101030704"]
["책꽂이","L:4900","개",1,null,{"$f":"TRUNC(E2155*D2155, 0)","v":0},null,{"$f":"TRUNC(G2155*D2155, 0)","v":0},null,{"$f":"TRUNC(I2155*D2155, 0)","v":0},{"$f":"TRUNC(E2155+G2155+I2155, 0)","v":0},{"$f":"TRUNC(F2155+H2155+J2155, 0)","v":0},"","51422250099FA2F9AC22E5D3FAE6313ABA61AF","","","0101030704","F","F","T",{"$nulls":23},"","",null,"010103070451422250099FA2F9AC22E5D3FAE6313ABA61AF",681]
{"$rows_empty":22}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2155:F2177)","v":0},null,{"$f":"SUM(H2155:H2177)","v":0},null,{"$f":"SUM(J2155:J2177)","v":0},null,{"$f":"SUM(L2155:L2177)","v":0},null,"TOTAL"]
["0101030801  바  닥  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 308.부원장 행정실     개소 :1",{"$nulls":14},"0101030801"]
["시멘트모르타르바름","바닥, 27mm","M2",16.43,null,{"$f":"TRUNC(E2180*D2180, 0)","v":0},null,{"$f":"TRUNC(G2180*D2180, 0)","v":0},null,{"$f":"TRUNC(I2180*D2180, 0)","v":0},{"$f":"TRUNC(E2180+G2180+I2180, 0)","v":0},0,null,"50FA62D00969ADB3282ADD819FAB85","","","0101030801","T","F","F",{"$nulls":23},"","",null,"010103080150FA62D00969ADB3282ADD819FAB85",854]
["지정카펫타일 깔기","7.0mm","M2",16.43,null,{"$f":"TRUNC(E2181*D2181, 0)","v":0},null,{"$f":"TRUNC(G2181*D2181, 0)","v":0},null,{"$f":"TRUNC(I2181*D2181, 0)","v":0},0,0,null,"50FAE28009C3DCCF2C2E7219497839","","","0101030801","T","F","F",{"$nulls":23},"","",null,"010103080150FAE28009C3DCCF2C2E7219497839",482]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",2,null,{"$f":"TRUNC(E2182*D2182, 0)","v":0},null,{"$f":"TRUNC(G2182*D2182, 0)","v":0},null,{"$f":"TRUNC(I2182*D2182, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101030801","T","F","F",{"$nulls":23},"","",null,"010103080150FAE28009A0F313FA23F4CCF30D36",855]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2180:F2202)","v":0},null,{"$f":"SUM(H2180:H2202)","v":0},null,{"$f":"SUM(J2180:J2202)","v":0},null,{"$f":"SUM(L2180:L2202)","v":0},null,"TOTAL"]
["0101030802  벽    공    사","■ 인테리어공사 ▶ 지상3층 실명 : 308.부원장 행정실     개소 :1",{"$nulls":14},"0101030802"]
["스텐걸레받이","SUS H/L 1.6t, H:100","M",11.79,null,{"$f":"TRUNC(E2205*D2205, 0)","v":0},null,{"$f":"TRUNC(G2205*D2205, 0)","v":0},null,{"$f":"TRUNC(I2205*D2205, 0)","v":0},{"$f":"TRUNC(E2205+G2205+I2205, 0)","v":0},0,null,"50FAB2500947ECFABD256D4BC0E986","","","0101030802","T","F","F",{"$nulls":23},"","",null,"010103080250FAB2500947ECFABD256D4BC0E986",485]
["MDF붙임(벽)","9mm","M2",35.1,null,{"$f":"TRUNC(E2206*D2206, 0)","v":0},null,{"$f":"TRUNC(G2206*D2206, 0)","v":0},null,{"$f":"TRUNC(I2206*D2206, 0)","v":0},0,0,null,"50FAE28009EE89516723B7798FD4FC","","","0101030802","T","F","F",{"$nulls":23},"","",null,"010103080250FAE28009EE89516723B7798FD4FC",486]
["지정무늬목마감","티크","M2",33.619999999999997,null,{"$f":"TRUNC(E2207*D2207, 0)","v":0},null,{"$f":"TRUNC(G2207*D2207, 0)","v":0},null,{"$f":"TRUNC(I2207*D2207, 0)","v":0},0,0,null,"50FB62500938F8AF6C2BA268B4F296","","","0101030802","T","F","F",{"$nulls":23},"","",null,"010103080250FB62500938F8AF6C2BA268B4F296",488]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2205:F2227)","v":0},null,{"$f":"SUM(H2205:H2227)","v":0},null,{"$f":"SUM(J2205:J2227)","v":0},null,{"$f":"SUM(L2205:L2227)","v":0},null,"TOTAL"]
["0101030803  천  장  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 308.부원장 행정실     개소 :1",{"$nulls":14},"0101030803"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",17.25,null,{"$f":"TRUNC(E2230*D2230, 0)","v":0},null,{"$f":"TRUNC(G2230*D2230, 0)","v":0},null,{"$f":"TRUNC(I2230*D2230, 0)","v":0},{"$f":"TRUNC(E2230+G2230+I2230, 0)","v":0},0]
["등기구타공","다운라이트","EA",4,null,0,null,0,null,0,0,0]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",16.43,null,0,null,0,null,0,0,0]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",16.43,null,0,null,0,null,0,0,0]
["석고판본드붙임","천장, 일반 9.5mm","M2",16.43,null,0,null,0,null,0,0,0]
["철재커텐박스설치(ㄱ자)","200*200*1.2t, STL. 도장","M",2.73,null,0,null,0,null,0,0,0]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",14.79,null,0,null,0,null,0,0,0]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2230:F2252)","v":0},null,{"$f":"SUM(H2230:H2252)","v":0},null,{"$f":"SUM(J2230:J2252)","v":0},null,{"$f":"SUM(L2230:L2252)","v":0},null,"TOTAL"]
["0101030804  기  타  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 308.부원장 행정실     개소 :1",{"$nulls":14},"0101030804"]
["인포데스크","","개",1,null,{"$f":"TRUNC(E2255*D2255, 0)","v":0},null,{"$f":"TRUNC(G2255*D2255, 0)","v":0},null,{"$f":"TRUNC(I2255*D2255, 0)","v":0},{"$f":"TRUNC(E2255+G2255+I2255, 0)","v":0},{"$f":"TRUNC(F2255+H2255+J2255, 0)","v":0},"","57D3722009F9710B9C28E90B723AB022DF87AA","","","0101030804","F","F","T",{"$nulls":23},"","",null,"010103080457D3722009F9710B9C28E90B723AB022DF87AA",639]
["싱크","","개",1,null,{"$f":"TRUNC(E2256*D2256, 0)","v":0},null,{"$f":"TRUNC(G2256*D2256, 0)","v":0},null,{"$f":"TRUNC(I2256*D2256, 0)","v":0},{"$f":"TRUNC(E2256+G2256+I2256, 0)","v":0},{"$f":"TRUNC(F2256+H2256+J2256, 0)","v":0},"","57D3722009F9710B9C28E90B723AB022DF87AD","","","0101030804","F","F","T",{"$nulls":23},"","",null,"010103080457D3722009F9710B9C28E90B723AB022DF87AD",679]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2255:F2277)","v":0},null,{"$f":"SUM(H2255:H2277)","v":0},null,{"$f":"SUM(J2255:J2277)","v":0},null,{"$f":"SUM(L2255:L2277)","v":0},null,"TOTAL"]
["0101030901  바  닥  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 309.대회의실     개소 :1",{"$nulls":14},"0101030901"]
["시멘트모르타르바름","바닥, 27mm","M2",140.27000000000001,null,{"$f":"TRUNC(E2280*D2280, 0)","v":0},null,{"$f":"TRUNC(G2280*D2280, 0)","v":0},null,{"$f":"TRUNC(I2280*D2280, 0)","v":0},{"$f":"TRUNC(E2280+G2280+I2280, 0)","v":0},0,null,"50FA62D00969ADB3282ADD819FAB85","","","0101030901","T","F","F",{"$nulls":23},"","",null,"010103090150FA62D00969ADB3282ADD819FAB85",856]
["지정카펫타일 깔기","7.0mm","M2",140.27000000000001,null,{"$f":"TRUNC(E2281*D2281, 0)","v":0},null,{"$f":"TRUNC(G2281*D2281, 0)","v":0},null,{"$f":"TRUNC(I2281*D2281, 0)","v":0},0,0,null,"50FAE28009C3DCCF2C2E7219497839","","","0101030901","T","F","F",{"$nulls":23},"","",null,"010103090150FAE28009C3DCCF2C2E7219497839",500]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",3,null,{"$f":"TRUNC(E2282*D2282, 0)","v":0},null,{"$f":"TRUNC(G2282*D2282, 0)","v":0},null,{"$f":"TRUNC(I2282*D2282, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101030901","T","F","F",{"$nulls":23},"","",null,"010103090150FAE28009A0F313FA23F4CCF30D36",857]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2280:F2302)","v":0},null,{"$f":"SUM(H2280:H2302)","v":0},null,{"$f":"SUM(J2280:J2302)","v":0},null,{"$f":"SUM(L2280:L2302)","v":0},null,"TOTAL"]
["0101030902  벽    공    사","■ 인테리어공사 ▶ 지상3층 실명 : 309.대회의실     개소 :1",{"$nulls":14},"0101030902"]
["스텐걸레받이","SUS H/L 1.6t, H:100","M",41.31,null,{"$f":"TRUNC(E2305*D2305, 0)","v":0},null,{"$f":"TRUNC(G2305*D2305, 0)","v":0},null,{"$f":"TRUNC(I2305*D2305, 0)","v":0},{"$f":"TRUNC(E2305+G2305+I2305, 0)","v":0},0,null,"50FAB2500947ECFABD256D4BC0E986","","","0101030902","T","F","F",{"$nulls":23},"","",null,"010103090250FAB2500947ECFABD256D4BC0E986",503]
["MDF붙임(벽)","9mm","M2",36.365000000000002,null,0,null,0,null,0,0,0,null,"50FAE28009EE89516723B7798FD4FC","","","0101030902","T","F","F",{"$nulls":23},"","",null,"010103090250FAE28009EE89516723B7798FD4FC",504]
["합판붙임(벽)","9mm","M2",33.880000000000003,null,0,null,0,null,0,0,0,null,"50FAE28009EED176C1217BAD90B52A","","","0101030902","T","F","F",{"$nulls":23},"","",null,"010103090250FAE28009EED176C1217BAD90B52A",505]
["백페인트글라스설치","5mm","M2",11.07,null,0,null,0,null,0,0,0,null,"50FB624009D672D45B2014F56DE404","","","0101030902","T","F","F",{"$nulls":23},"","",null,"010103090250FB624009D672D45B2014F56DE404",506]
["지정흡음보드붙임","벽, 라인흡음보드","M2",38.81,null,0,null,0,null,0,0,0,null,"50FB62500938F8AF6C2BA31164A680","","","0101030902","T","F","F",{"$nulls":23},"","",null,"010103090250FB62500938F8AF6C2BA31164A680",507]
["지정무늬목마감","티크","M2",57.89,null,0,null,0,null,0,0,0,null,"50FB62500938F8AF6C2BA268B4F296","","","0101030902","T","F","F",{"$nulls":23},"","",null,"010103090250FB62500938F8AF6C2BA268B4F296",509]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2305:F2327)","v":0},null,{"$f":"SUM(H2305:H2327)","v":0},null,{"$f":"SUM(J2305:J2327)","v":0},null,{"$f":"SUM(L2305:L2327)","v":0},null,"TOTAL"]
["0101030903  천  장  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 309.대회의실     개소 :1",{"$nulls":14},"0101030903"]
["석고보드","석고보드, 평보드, 9.5*900*1800mm(㎡)","M2",147.29,null,{"$f":"TRUNC(E2330*D2330, 0)","v":0},null,{"$f":"TRUNC(G2330*D2330, 0)","v":0},null,{"$f":"TRUNC(I2330*D2330, 0)","v":0},{"$f":"TRUNC(E2330+G2330+I2330, 0)","v":0},0,"","57D3722009F9710BAE2ED981ED5CFCF4080C3E","","","0101030903","F","F","T",{"$nulls":23},"","",null,"010103090357D3722009F9710BAE2ED981ED5CFCF4080C3E",511]
["등기구타공","다운라이트","EA",8,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101030903","F","F","T",{"$nulls":23},"","",null,"010103090357D3722009F9710B9C21B6DD9D2E4747ACE111",512]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",140.27000000000001,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101030903","T","F","F",{"$nulls":23},"","",null,"010103090350FAB2500909EF985820B87BB6AB0D",513]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",34.44,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101030903","T","F","F",{"$nulls":23},"","",null,"010103090350FAF2F0097711FE6F2FE675585AF3",514]
["석고판본드붙임","천장, 일반 9.5mm","M2",34.44,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403B220C4D6970C9E","","","0101030903","T","F","F",{"$nulls":23},"","",null,"010103090350FAE28009EEA403B220C4D6970C9E",515]
["철재커텐박스설치(ㄱ자)","200*200*1.2t, STL. 도장","M",10.4,null,0,null,0,null,0,0,0,null,"50FAE2800958DF9CBC23EFCCF16A9D","","","0101030903","T","F","F",{"$nulls":23},"","",null,"010103090350FAE2800958DF9CBC23EFCCF16A9D",516]
["조명박스(J형)","(80+150+200+200)*1.6t갈바/도장, 각파이프틀및달대포함","M",41.2,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D2822A1B8F","","","0101030903","T","F","F",{"$nulls":23},"","",null,"010103090350FAE2800958DFBF8327D2822A1B8F",517]
["지정흡음보드붙임","천장, 타공흡음보드","M2",105.83,null,0,null,0,null,0,0,0,null,"50FB62500938F8AF6C2BA31164A682","","","0101030903","T","F","F",{"$nulls":23},"","",null,"010103090350FB62500938F8AF6C2BA31164A682",508]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",43.46,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101030903","T","F","F",{"$nulls":23},"","",null,"010103090350FAE280094E44060A2808FF6AAFE4",518]
{"$rows_empty":14}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2330:F2352)","v":0},null,{"$f":"SUM(H2330:H2352)","v":0},null,{"$f":"SUM(J2330:J2352)","v":0},null,{"$f":"SUM(L2330:L2352)","v":0},null,"TOTAL"]
["0101031001  바  닥  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 310.공용화장실(남)     개소 :1",{"$nulls":14},"0101031001"]
["석재.타일보양","하드롱지","M2",21.38,null,{"$f":"TRUNC(E2355*D2355, 0)","v":0},null,{"$f":"TRUNC(G2355*D2355, 0)","v":0},null,{"$f":"TRUNC(I2355*D2355, 0)","v":0},{"$f":"TRUNC(E2355+G2355+I2355, 0)","v":0},0,null,"50FA026009B9885A1F2BAC10AA64C9","","","0101031001","T","F","F",{"$nulls":23},"","",null,"010103100150FA026009B9885A1F2BAC10AA64C9",521]
["지정타일압착붙임 /화장실 (타일 관급)","바닥, 바탕 65mm+압 5mm","M2",21.38,null,{"$f":"TRUNC(E2356*D2356, 0)","v":0},null,{"$f":"TRUNC(G2356*D2356, 0)","v":0},null,{"$f":"TRUNC(I2356*D2356, 0)","v":0},0,0,null,"50FAC240091DE2698B2F0344CE27B1","","","0101031001","T","F","F",{"$nulls":23},"","",null,"010103100150FAC240091DE2698B2F0344CE27B1",522]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",1.1000000000000001,null,{"$f":"TRUNC(E2357*D2357, 0)","v":0},null,{"$f":"TRUNC(G2357*D2357, 0)","v":0},null,{"$f":"TRUNC(I2357*D2357, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101031001","T","F","F",{"$nulls":23},"","",null,"010103100150FAE28009A0F313FA23F4CCF30D36",523]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2355:F2377)","v":0},null,{"$f":"SUM(H2355:H2377)","v":0},null,{"$f":"SUM(J2355:J2377)","v":0},null,{"$f":"SUM(L2355:L2377)","v":0},null,"TOTAL"]
["0101031002  벽    공    사","■ 인테리어공사 ▶ 지상3층 실명 : 310.공용화장실(남)     개소 :1",{"$nulls":14},"0101031002"]
["소변기턱설치용 각파이프틀설치","W:200*H:1250, ㅁ-30*30","M",3.25,null,{"$f":"TRUNC(E2380*D2380, 0)","v":0},null,{"$f":"TRUNC(G2380*D2380, 0)","v":0},null,{"$f":"TRUNC(I2380*D2380, 0)","v":0},{"$f":"TRUNC(E2380+G2380+I2380, 0)","v":0},0,null,"50FAB25009099778C12BFF07E62020","","","0101031002","T","F","F",{"$nulls":23},"","",null,"010103100250FAB25009099778C12BFF07E62020",886]
["대변기턱설치용 각파이프틀설치","W:200*H:1000, ㅁ-30*30","M",4,null,0,null,0,null,0,0,0,null,"50FAB25009099778C12BFF07E62021","","","0101031002","T","F","F",{"$nulls":23},"","",null,"010103100250FAB25009099778C12BFF07E62021",887]
["지정타일떠붙임 /화장실 (타일 관급)","벽, 몰탈18mm","M2",50.89,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD6","","","0101031002","T","F","F",{"$nulls":23},"","",null,"010103100250FAC240091DE2698B2F0344CFCDD6",525]
["지정타일본드붙임 /화장실 (타일관급)","벽","M2",8.06,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD1","","","0101031002","T","F","F",{"$nulls":23},"","",null,"010103100250FAC240091DE2698B2F0344CFCDD1",888]
["우레탄도막방수","벽체, 비노출","M2",9.51,null,0,null,0,null,0,0,0,null,"50FA92000987C572F62EA1806E70A5","","","0101031002","T","F","F",{"$nulls":23},"","",null,"010103100250FA92000987C572F62EA1806E70A5",889]
["인조대리석 변기턱","180*30mm, 몰탈30mm","M",7.25,null,0,null,0,null,0,0,0,null,"50FAC240092E47393F289B71873F55","","","0101031002","T","F","F",{"$nulls":23},"","",null,"010103100250FAC240092E47393F289B71873F55",526]
["벽, 합판붙임","방수 12mm 1겹","M2",9.51,null,0,null,0,null,0,0,0,null,"50FAE28009EED176C1217BDCCD06F7","","","0101031002","T","F","F",{"$nulls":23},"","",null,"010103100250FAE28009EED176C1217BDCCD06F7",890]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2380:F2402)","v":0},null,{"$f":"SUM(H2380:H2402)","v":0},null,{"$f":"SUM(J2380:J2402)","v":0},null,{"$f":"SUM(L2380:L2402)","v":0},null,"TOTAL"]
["0101031003  천  장  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 310.공용화장실(남)     개소 :1",{"$nulls":14},"0101031003"]
["석고보드","석고보드, 평보드, 방수, 9.5*900*1800mm(㎡)","M2",22.45,null,{"$f":"TRUNC(E2405*D2405, 0)","v":0},null,{"$f":"TRUNC(G2405*D2405, 0)","v":0},null,{"$f":"TRUNC(I2405*D2405, 0)","v":0},{"$f":"TRUNC(E2405+G2405+I2405, 0)","v":0},0,null,"57D3722009F9710BAE2ED982F3A1AA138880B3","","","0101031003","F","F","T",{"$nulls":23},"","",null,"010103100357D3722009F9710BAE2ED982F3A1AA138880B3",528]
["등기구타공","다운라이트","EA",7,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101031003","F","F","T",{"$nulls":23},"","",null,"010103100357D3722009F9710B9C21B6DD9D2E4747ACE111",529]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",21.38,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101031003","T","F","F",{"$nulls":23},"","",null,"010103100350FAB2500909EF985820B87BB6AB0D",530]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",21.38,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101031003","T","F","F",{"$nulls":23},"","",null,"010103100350FAF2F0097711FE6F2FE675585AF3",531]
["석고판본드붙임","천장, 방수 9.5mm","M2",21.38,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403862C1FD18B8962","","","0101031003","T","F","F",{"$nulls":23},"","",null,"010103100350FAE28009EEA403862C1FD18B8962",532]
["조명박스(J형) /화장실","(160+160+400+400)*1.6t갈바/도장, 각파이프틀및달대포함","M",9.5500000000000007,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D286850A91","","","0101031003","T","F","F",{"$nulls":23},"","",null,"010103100350FAE2800958DFBF8327D286850A91",533]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",22.88,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101031003","T","F","F",{"$nulls":23},"","",null,"010103100350FAE280094E44060A2808FF6AAFE4",534]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2405:F2427)","v":0},null,{"$f":"SUM(H2405:H2427)","v":0},null,{"$f":"SUM(J2405:J2427)","v":0},null,{"$f":"SUM(L2405:L2427)","v":0},null,"TOTAL"]
["0101031004  기  타  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 310.공용화장실(남)     개소 :1",{"$nulls":14},"0101031004"]
["지정화장실칸막이","자작나무합판마감","M2",21.59,null,{"$f":"TRUNC(E2430*D2430, 0)","v":0},null,{"$f":"TRUNC(G2430*D2430, 0)","v":0},null,{"$f":"TRUNC(I2430*D2430, 0)","v":0},{"$f":"TRUNC(E2430+G2430+I2430, 0)","v":0},0,null,"57D3722009F99DF9C123903DCBC8B9718F30A1","","","0101031004","F","F","T",{"$nulls":23},"","",null,"010103100457D3722009F99DF9C123903DCBC8B9718F30A1",536]
["장애인소변기용손잡이","STS304 Ø38,1.5t","EA",1,null,0,null,0,null,0,0,0,null,"50FB12C009000A0DE123F9CD7ADDE2","","","0101031004","T","F","F",{"$nulls":23},"","",null,"010103100450FB12C009000A0DE123F9CD7ADDE2",537]
["수밀코킹(실리콘)","삼각, 5mm이하, 방균용","M",10.7,null,0,null,0,null,0,0,0,null,"50FA920009DF72024B2E486FEF08DE","","","0101031004","T","F","F",{"$nulls":23},"","",null,"010103100450FA920009DF72024B2E486FEF08DE",538]
["방습거울후레임","스테인리스, W50*1.5t","M",6.7,null,0,null,0,null,0,0,0,null,"50FAB2500924C55AE02DCC1BFE2175","","","0101031004","T","F","F",{"$nulls":23},"","",null,"010103100450FAB2500924C55AE02DCC1BFE2175",539]
["출입구 공프레임","구로철판1.6t, 1220*2150","개소",1,null,0,null,0,null,0,0,0,null,"50FAB2500924980282224F9EC8AE99","","","0101031004","T","F","F",{"$nulls":23},"","",null,"010103100450FAB2500924980282224F9EC8AE99",540]
["방습거울설치","5mm, 틀 포함","M2",2.42,null,0,null,0,null,0,0,0,null,"50FAD2A009FE1520552E7181DB95CE","","","0101031004","T","F","F",{"$nulls":23},"","",null,"010103100450FAD2A009FE1520552E7181DB95CE",541]
["인조대리석세면대","W:600*12t,틀포함","M",2.2999999999999998,null,0,null,0,null,0,0,0,null,"50FB12C0090037D9682873AC4EB01D","","","0101031004","T","F","F",{"$nulls":23},"","",null,"010103100450FB12C0090037D9682873AC4EB01D",542]
["소변기칸막이","400*900, 인조대리석13mm","개소",2,null,0,null,0,null,0,0,0,null,"50FB6250091C32460A2B63C3F2AE4D","","","0101031004","T","F","F",{"$nulls":23},"","",null,"010103100450FB6250091C32460A2B63C3F2AE4D",549]
{"$rows_empty":15}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2430:F2452)","v":0},null,{"$f":"SUM(H2430:H2452)","v":0},null,{"$f":"SUM(J2430:J2452)","v":0},null,{"$f":"SUM(L2430:L2452)","v":0},null,"TOTAL"]
["0101031101  바  닥  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 311.공용화장실(여)     개소 :1",{"$nulls":14},"0101031101"]
["석재.타일보양","하드롱지","M2",24.4,null,{"$f":"TRUNC(E2455*D2455, 0)","v":0},null,{"$f":"TRUNC(G2455*D2455, 0)","v":0},null,{"$f":"TRUNC(I2455*D2455, 0)","v":0},{"$f":"TRUNC(E2455+G2455+I2455, 0)","v":0},0,null,"50FA026009B9885A1F2BAC10AA64C9","","","0101031101","T","F","F",{"$nulls":23},"","",null,"010103110150FA026009B9885A1F2BAC10AA64C9",552]
["지정타일압착붙임 /화장실 (타일 관급)","바닥, 바탕 65mm+압 5mm","M2",24.4,null,{"$f":"TRUNC(E2456*D2456, 0)","v":0},null,{"$f":"TRUNC(G2456*D2456, 0)","v":0},null,{"$f":"TRUNC(I2456*D2456, 0)","v":0},0,0,null,"50FAC240091DE2698B2F0344CE27B1","","","0101031101","T","F","F",{"$nulls":23},"","",null,"010103110150FAC240091DE2698B2F0344CE27B1",553]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",1.1000000000000001,null,{"$f":"TRUNC(E2457*D2457, 0)","v":0},null,{"$f":"TRUNC(G2457*D2457, 0)","v":0},null,{"$f":"TRUNC(I2457*D2457, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101031101","T","F","F",{"$nulls":23},"","",null,"010103110150FAE28009A0F313FA23F4CCF30D36",554]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2455:F2477)","v":0},null,{"$f":"SUM(H2455:H2477)","v":0},null,{"$f":"SUM(J2455:J2477)","v":0},null,{"$f":"SUM(L2455:L2477)","v":0},null,"TOTAL"]
["0101031102  벽    공    사","■ 인테리어공사 ▶ 지상3층 실명 : 311.공용화장실(여)     개소 :1",{"$nulls":14},"0101031102"]
["대변기턱설치용 각파이프틀설치","W:200*H:1000, ㅁ-30*30","M",8,null,{"$f":"TRUNC(E2480*D2480, 0)","v":0},null,{"$f":"TRUNC(G2480*D2480, 0)","v":0},null,{"$f":"TRUNC(I2480*D2480, 0)","v":0},{"$f":"TRUNC(E2480+G2480+I2480, 0)","v":0},0,null,"50FAB25009099778C12BFF07E62021","","","0101031102","T","F","F",{"$nulls":23},"","",null,"010103110250FAB25009099778C12BFF07E62021",891]
["지정타일떠붙임 /화장실 (타일 관급)","벽, 몰탈18mm","M2",53.3,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD6","","","0101031102","T","F","F",{"$nulls":23},"","",null,"010103110250FAC240091DE2698B2F0344CFCDD6",556]
["지정타일본드붙임 /화장실 (타일관급)","벽","M2",8,null,0,null,0,null,0,0,0,null,"50FAC240091DE2698B2F0344CFCDD1","","","0101031102","T","F","F",{"$nulls":23},"","",null,"010103110250FAC240091DE2698B2F0344CFCDD1",892]
["우레탄도막방수","벽체, 비노출","M2",9.6,null,0,null,0,null,0,0,0,null,"50FA92000987C572F62EA1806E70A5","","","0101031102","T","F","F",{"$nulls":23},"","",null,"010103110250FA92000987C572F62EA1806E70A5",893]
["인조대리석 변기턱","180*30mm, 몰탈30mm","M",8,null,0,null,0,null,0,0,0,null,"50FAC240092E47393F289B71873F55","","","0101031102","T","F","F",{"$nulls":23},"","",null,"010103110250FAC240092E47393F289B71873F55",557]
["벽, 합판붙임","방수 12mm 1겹","M2",9.6,null,0,null,0,null,0,0,0,null,"50FAE28009EED176C1217BDCCD06F7","","","0101031102","T","F","F",{"$nulls":23},"","",null,"010103110250FAE28009EED176C1217BDCCD06F7",894]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2480:F2502)","v":0},null,{"$f":"SUM(H2480:H2502)","v":0},null,{"$f":"SUM(J2480:J2502)","v":0},null,{"$f":"SUM(L2480:L2502)","v":0},null,"TOTAL"]
["0101031103  천  장  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 311.공용화장실(여)     개소 :1",{"$nulls":14},"0101031103"]
["석고보드","석고보드, 평보드, 방수, 9.5*900*1800mm(㎡)","M2",25.62,null,{"$f":"TRUNC(E2505*D2505, 0)","v":0},null,{"$f":"TRUNC(G2505*D2505, 0)","v":0},null,{"$f":"TRUNC(I2505*D2505, 0)","v":0},{"$f":"TRUNC(E2505+G2505+I2505, 0)","v":0},0,null,"57D3722009F9710BAE2ED982F3A1AA138880B3","","","0101031103","F","F","T",{"$nulls":23},"","",null,"010103110357D3722009F9710BAE2ED982F3A1AA138880B3",559]
["등기구타공","다운라이트","EA",7,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101031103","F","F","T",{"$nulls":23},"","",null,"010103110357D3722009F9710B9C21B6DD9D2E4747ACE111",560]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",24.4,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101031103","T","F","F",{"$nulls":23},"","",null,"010103110350FAB2500909EF985820B87BB6AB0D",561]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",24.4,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101031103","T","F","F",{"$nulls":23},"","",null,"010103110350FAF2F0097711FE6F2FE675585AF3",562]
["석고판본드붙임","천장, 방수 9.5mm","M2",24.4,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403862C1FD18B8962","","","0101031103","T","F","F",{"$nulls":23},"","",null,"010103110350FAE28009EEA403862C1FD18B8962",563]
["조명박스(J형) /화장실","(160+160+400+400)*1.6t갈바/도장, 각파이프틀및달대포함","M",10.1,null,0,null,0,null,0,0,0,null,"50FAE2800958DFBF8327D286850A91","","","0101031103","T","F","F",{"$nulls":23},"","",null,"010103110350FAE2800958DFBF8327D286850A91",564]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",23.72,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101031103","T","F","F",{"$nulls":23},"","",null,"010103110350FAE280094E44060A2808FF6AAFE4",565]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2505:F2527)","v":0},null,{"$f":"SUM(H2505:H2527)","v":0},null,{"$f":"SUM(J2505:J2527)","v":0},null,{"$f":"SUM(L2505:L2527)","v":0},null,"TOTAL"]
["0101031104  기  타  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 311.공용화장실(여)     개소 :1",{"$nulls":14},"0101031104"]
["지정화장실칸막이","자작나무합판마감","M2",43.17,null,{"$f":"TRUNC(E2530*D2530, 0)","v":0},null,{"$f":"TRUNC(G2530*D2530, 0)","v":0},null,{"$f":"TRUNC(I2530*D2530, 0)","v":0},{"$f":"TRUNC(E2530+G2530+I2530, 0)","v":0},0,null,"57D3722009F99DF9C123903DCBC8B9718F30A1","","","0101031104","F","F","T",{"$nulls":23},"","",null,"010103110457D3722009F99DF9C123903DCBC8B9718F30A1",567]
["수밀코킹(실리콘)","삼각, 5mm이하, 방균용","M",10.1,null,0,null,0,null,0,0,0,null,"50FA920009DF72024B2E486FEF08DE","","","0101031104","T","F","F",{"$nulls":23},"","",null,"010103110450FA920009DF72024B2E486FEF08DE",568]
["방습거울후레임","스테인리스, W50*1.5t","M",6.3,null,0,null,0,null,0,0,0,null,"50FAB2500924C55AE02DCC1BFE2175","","","0101031104","T","F","F",{"$nulls":23},"","",null,"010103110450FAB2500924C55AE02DCC1BFE2175",569]
["출입구 공프레임","구로철판1.6t, 1220*2150","개소",1,null,0,null,0,null,0,0,0,null,"50FAB2500924980282224F9EC8AE99","","","0101031104","T","F","F",{"$nulls":23},"","",null,"010103110450FAB2500924980282224F9EC8AE99",570]
["방습거울설치","5mm, 틀 포함","M2",2.21,null,0,null,0,null,0,0,0,null,"50FAD2A009FE1520552E7181DB95CE","","","0101031104","T","F","F",{"$nulls":23},"","",null,"010103110450FAD2A009FE1520552E7181DB95CE",571]
["인조대리석세면대","W:600*12t,틀포함","M",2.1,null,0,null,0,null,0,0,0,null,"50FB12C0090037D9682873AC4EB01D","","","0101031104","T","F","F",{"$nulls":23},"","",null,"010103110450FB12C0090037D9682873AC4EB01D",572]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2530:F2552)","v":0},null,{"$f":"SUM(H2530:H2552)","v":0},null,{"$f":"SUM(J2530:J2552)","v":0},null,{"$f":"SUM(L2530:L2552)","v":0},null,"TOTAL"]
["0101031201  바  닥  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 312.청소도구함     개소 :1",{"$nulls":14},"0101031201"]
["석재.타일보양","하드롱지","M2",1.52,null,{"$f":"TRUNC(E2555*D2555, 0)","v":0},null,{"$f":"TRUNC(G2555*D2555, 0)","v":0},null,{"$f":"TRUNC(I2555*D2555, 0)","v":0},{"$f":"TRUNC(E2555+G2555+I2555, 0)","v":0},0,null,"50FA026009B9885A1F2BAC10AA64C9","","","0101031201","T","F","F",{"$nulls":23},"","",null,"010103120150FA026009B9885A1F2BAC10AA64C9",579]
["지정타일압착붙임 /화장실 (타일 관급)","바닥, 바탕 65mm+압 5mm","M2",1.52,null,{"$f":"TRUNC(E2556*D2556, 0)","v":0},null,{"$f":"TRUNC(G2556*D2556, 0)","v":0},null,{"$f":"TRUNC(I2556*D2556, 0)","v":0},0,0,null,"50FAC240091DE2698B2F0344CE27B1","","","0101031201","T","F","F",{"$nulls":23},"","",null,"010103120150FAC240091DE2698B2F0344CE27B1",580]
["스텐레스재료분리대","바닥, W:6*1.5t, ㅁ-25*25+앵커포함","M",0.82,null,{"$f":"TRUNC(E2557*D2557, 0)","v":0},null,{"$f":"TRUNC(G2557*D2557, 0)","v":0},null,{"$f":"TRUNC(I2557*D2557, 0)","v":0},0,0,null,"50FAE28009A0F313FA23F4CCF30D36","","","0101031201","T","F","F",{"$nulls":23},"","",null,"010103120150FAE28009A0F313FA23F4CCF30D36",581]
{"$rows_empty":20}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2555:F2577)","v":0},null,{"$f":"SUM(H2555:H2577)","v":0},null,{"$f":"SUM(J2555:J2577)","v":0},null,{"$f":"SUM(L2555:L2577)","v":0},null,"TOTAL"]
["0101031202  벽    공    사","■ 인테리어공사 ▶ 지상3층 실명 : 312.청소도구함     개소 :1",{"$nulls":14},"0101031202"]
["지정타일떠붙임 /화장실 (타일 관급)","벽, 몰탈18mm","M2",12.77,null,{"$f":"TRUNC(E2580*D2580, 0)","v":0},null,{"$f":"TRUNC(G2580*D2580, 0)","v":0},null,{"$f":"TRUNC(I2580*D2580, 0)","v":0},{"$f":"TRUNC(E2580+G2580+I2580, 0)","v":0},{"$f":"TRUNC(F2580+H2580+J2580, 0)","v":0},null,"50FAC240091DE2698B2F0344CFCDD6","","","0101031202","T","F","F",{"$nulls":23},"","",null,"010103120250FAC240091DE2698B2F0344CFCDD6",583]
{"$rows_empty":22}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2580:F2602)","v":0},null,{"$f":"SUM(H2580:H2602)","v":0},null,{"$f":"SUM(J2580:J2602)","v":0},null,{"$f":"SUM(L2580:L2602)","v":0},null,"TOTAL"]
["0101031203  천  장  공  사","■ 인테리어공사 ▶ 지상3층 실명 : 312.청소도구함     개소 :1",{"$nulls":14},"0101031203"]
["석고보드","석고보드, 평보드, 방수, 9.5*900*1800mm(㎡)","M2",1.42,null,{"$f":"TRUNC(E2605*D2605, 0)","v":0},null,{"$f":"TRUNC(G2605*D2605, 0)","v":0},null,{"$f":"TRUNC(I2605*D2605, 0)","v":0},{"$f":"TRUNC(E2605+G2605+I2605, 0)","v":0},0,null,"57D3722009F9710BAE2ED982F3A1AA138880B3","","","0101031203","F","F","T",{"$nulls":23},"","",null,"010103120357D3722009F9710BAE2ED982F3A1AA138880B3",585]
["등기구타공","다운라이트","EA",1,null,0,null,0,null,0,0,0,null,"57D3722009F9710B9C21B6DD9D2E4747ACE111","","","0101031203","F","F","T",{"$nulls":23},"","",null,"010103120357D3722009F9710B9C21B6DD9D2E4747ACE111",586]
["경량철골천정틀","M-BAR, H:1m이상. 인써트 유","M2",1.35,null,0,null,0,null,0,0,0,null,"50FAB2500909EF985820B87BB6AB0D","","","0101031203","T","F","F",{"$nulls":23},"","",null,"010103120350FAB2500909EF985820B87BB6AB0D",587]
["비닐페인트(뿜칠)","내천장 3회(GB면)","M2",1.35,null,0,null,0,null,0,0,0,null,"50FAF2F0097711FE6F2FE675585AF3","","","0101031203","T","F","F",{"$nulls":23},"","",null,"010103120350FAF2F0097711FE6F2FE675585AF3",588]
["석고판본드붙임","천장, 방수 9.5mm","M2",1.35,null,0,null,0,null,0,0,0,null,"50FAE28009EEA403862C1FD18B8962","","","0101031203","T","F","F",{"$nulls":23},"","",null,"010103120350FAE28009EEA403862C1FD18B8962",589]
["AL몰딩설치(W형)","15*15*15*15*1.0mm","M",5.16,null,0,null,0,null,0,0,0,null,"50FAE280094E44060A2808FF6AAFE4","","","0101031203","T","F","F",{"$nulls":23},"","",null,"010103120350FAE280094E44060A2808FF6AAFE4",590]
{"$rows_empty":17}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2605:F2627)","v":0},null,{"$f":"SUM(H2605:H2627)","v":0},null,{"$f":"SUM(J2605:J2627)","v":0},null,{"$f":"SUM(L2605:L2627)","v":0},null,"TOTAL"]
["010104  ▶ 골재비및운반비","■ 인테리어공사",{"$nulls":14},"010104"]
["모래","도착도","M3",350,null,{"$f":"TRUNC(E2630*D2630, 0)","v":0},null,{"$f":"TRUNC(G2630*D2630, 0)","v":0},null,{"$f":"TRUNC(I2630*D2630, 0)","v":0},{"$f":"TRUNC(E2630+G2630+I2630, 0)","v":0},{"$f":"TRUNC(F2630+H2630+J2630, 0)","v":0},null,"57FE524009857EC780246BE33745EC1837FA80","","","010104","F","F","T",{"$nulls":23},"","",null,"01010457FE524009857EC780246BE33745EC1837FA80",904]
["시멘트운반","L:10km, 덤프8톤","포",4056,null,{"$f":"TRUNC(E2631*D2631, 0)","v":0},null,{"$f":"TRUNC(G2631*D2631, 0)","v":0},null,{"$f":"TRUNC(I2631*D2631, 0)","v":0},{"$f":"TRUNC(E2631+G2631+I2631, 0)","v":0},{"$f":"TRUNC(F2631+H2631+J2631, 0)","v":0},null,"50FB525009D3352FC120940273CCF0","","","010104","F","T","F",{"$nulls":23},"","",null,"01010450FB525009D3352FC120940273CCF0",688]
{"$rows_empty":21}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2630:F2652)","v":0},null,{"$f":"SUM(H2630:H2652)","v":0},null,{"$f":"SUM(J2630:J2652)","v":0},null,{"$f":"SUM(L2630:L2652)","v":0},null,"TOTAL"]
["010201  ▶ 도급자설치관급자재비","■ 관급공사",{"$nulls":14},"010201"]
["시멘트","40kg/포, 하치장도","포",4056,null,{"$f":"TRUNC(E2655*D2655, 0)","v":0},null,{"$f":"TRUNC(G2655*D2655, 0)","v":0},null,{"$f":"TRUNC(I2655*D2655, 0)","v":0},{"$f":"TRUNC(E2655+G2655+I2655, 0)","v":0},0,null,"57D3722009F90E35B420C8F820FB16E3A0A9AE","","","010201","F","F","T",{"$nulls":23},"","",null,"01020157D3722009F90E35B420C8F820FB16E3A0A9AE",900]
["레미콘","대전,세종,충남, 25-21-15","M3",68,null,0,null,0,null,0,0,0,null,"57D3722009F90E35882C07B428CEC69316067B","","","010201","F","F","T",{"$nulls":23},"","",null,"01020157D3722009F90E35882C07B428CEC69316067B",913]
["지정타일","바닥, 600*600","M2",1815,null,0,null,0,null,0,0,0,null,"57D3722009F92AE1AA2D4ADD2DDCA915AF2228","","","010201","F","F","T",{"$nulls":23},"","",null,"01020157D3722009F92AE1AA2D4ADD2DDCA915AF2228",633]
["지정타일 /화장실 벽","벽, 100*200","M2",536,null,0,null,0,null,0,0,0,null,"57D3722009F92AE1AA2D4ADD2DDCA915AF222B","","","010201","F","F","T",{"$nulls":23},"","",null,"01020157D3722009F92AE1AA2D4ADD2DDCA915AF222B",634]
["지정타일 /원장화장실 벽","벽, 100*200","M2",22,null,0,null,0,null,0,0,0,null,"57D3722009F92AE1AA2D4ADD2DDCA915AF222A","","","010201","F","F","T",{"$nulls":23},"","",null,"01020157D3722009F92AE1AA2D4ADD2DDCA915AF222A",635]
["자연석판석","버너, 30mm, 고흥석","M2",1048,null,0,null,0,null,0,0,0,null,"57D3722009F92AE1AA2D4C8F651530B4255D23","","","010201","F","F","T",{"$nulls":23},"","",null,"01020157D3722009F92AE1AA2D4C8F651530B4255D23",901]
["자연석판석","혼드, 30mm, 고흥석","M2",32,null,0,null,0,null,0,0,0,null,"57D3722009F92AE1AA2D4C8F651530B42AC361","","","010201","F","F","T",{"$nulls":23},"","",null,"01020157D3722009F92AE1AA2D4C8F651530B42AC361",903]
{"$rows_empty":16}
["[ 합           계 ]",{"$nulls":4},{"$f":"SUM(F2655:F2677)","v":0},null,{"$f":"SUM(H2655:H2677)","v":0},null,{"$f":"SUM(J2655:J2677)","v":0},null,{"$f":"SUM(L2655:L2677)","v":0},null,"TOTAL"]

{"sheet":"토목내역","index":4,"n_rows":248,"n_cols":18,"rows_kept":248,"cut":false,"hidden":false,"merged":[[1,8,1,9],[1,10,1,11],[1,12,2,12],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,1,5],[1,6,1,7]]}
["내역서"]
["공 종 명","규 격","수량","단위","재 료 비","","노 무 비","","경    비","","합    계","","비 고"]
["","","","","단 가","금 액","단 가","금 액","단 가","금 액","단 가","금 액",""]
["국토연구원 신청사 건립공사                                                      ","토목150604                                                                      ",1,"식    ",{"$nulls":9},"","02"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"10","",""]
[". 순 공 사 비                                                                   ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"20","*",""]
["..Ⅰ.부대토목공                                                                 ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"30","","0201"]
["..Ⅱ.지하층터파기공                                                             ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"40","","0202"]
["..Ⅲ.기초공사                                                                   ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"50","","0204"]
["..Ⅳ.영구배수공사                                                               ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"60","","0205"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"70","",""]
[". 관 급 자 재 대                                                                ","도급자설치/부가세포함                                                           ",1,"식    ",{"$nulls":9},"",null,"80","*","0206"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"95","",""]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"110","S",""]
[]
["Ⅰ.부대토목공                                                                   ","                                                                                ",1,"식    ",{"$nulls":9},"","0201"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"10","",""]
[".01. 토        공                                                               ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"20","",""]
["..1)터파기                                                                      ","                                                                                ",0,"      ",{"$nulls":9},"",null,"30","",""]
["...토사 굴착 및 상차                                                            ","백호우0.7M3                                                                     ",13106,"M³   ",{"$nulls":9},"",null,"40","","K0010"]
["...리핑암 굴착 및 상차                                                          ","백호우0.7M3                                                                     ",7795,"M³   ",{"$nulls":9},"",null,"50","","K0020"]
["...발파암 굴착 및 상차                                                          ","                                                                                ",745,"M3    ",{"$nulls":9},"",null,"70","","K0056"]
["..2)성토 및 되메우기                                                            ","                                                                                ",0,"      ",{"$nulls":9},"",null,"80","",""]
["...흙쌓기/토사                                                                  ","다짐도90%이상                                                                   ",1366,"m3    ",{"$nulls":9},"",null,"90","","_CDG100100000"]
["...흙쌓기/토사                                                                  ","비다짐                                                                          ",659,"m3    ",{"$nulls":9},"",null,"100","","_CDG100300000"]
["..3)운반                                                                        ","                                                                                ",0,"      ",{"$nulls":9},"",null,"110","",""]
["...운반/토사 (임시적치장)                                                       ","L=1.0KM(덤프)                                                                   ",1974,"M3    ",{"$nulls":9},"",null,"120","","K0060"]
["...운반/상차토사 (되메움용)                                                     ","L=1.0KM(덤프)                                                                   ",1974,"M3    ",{"$nulls":9},"",null,"130","","K0061"]
["...흙운반(적재ㆍ적하)/발파암/집토후상차                                         "," 백호+덤프15톤                                                                  ",745,"m3    ",{"$nulls":9},"",null,"140","","_CDS300201500"]
["...사토/토사                                                                    ","토사,L=30.0km                                                                   ",11351,"M3    ",{"$nulls":9},"",null,"150","","K0086"]
["...토처리                                                                       ","리핑암,L=30.0km                                                                 ",8087,"M3    ",{"$nulls":9},"",null,"160","","K0087A"]
["...잔토처리                                                                     ","발파암,L=30.0km                                                                 ",745,"M3    ",{"$nulls":9},"",null,"170","","K0088"]
["..4)철거비                                                                      ","                                                                                ",0,"      ",{"$nulls":9},"",null,"180","",""]
["...아스팔트포장깨기                                                             ","T=30cm 미만                                                                     ",8,"m3    ",{"$nulls":9},"",null,"190","","_CDC220100000"]
["...포장절단/아스팔트                                                            ","                                                                                ",56,"m     ",{"$nulls":9},"",null,"200","","_CDC220200000"]
["...투수콘포장깨기                                                               ","T=30cm 미만                                                                     ",1,"m3    ",{"$nulls":9},"",null,"210","","_CDC220100000"]
["...포장절단/투수콘                                                              ","                                                                                ",9,"m     ",{"$nulls":9},"",null,"220","","_CDC220200000"]
["...소형고압블록철거                                                             ","인력                                                                            ",50,"m2    ",{"$nulls":9},"",null,"230","","_CDC230000001"]
["...도로/보차도경계석철거                                                        ","굴삭기0.7㎥+대형브레이카                                                        ",6,"m3    ",{"$nulls":9},"",null,"240","","_CDC120100001"]
["...배수구조물철거                                                               ","굴삭기0.7㎥+대형브레이카                                                        ",1,"m3    ",{"$nulls":9},"",null,"250","","_CDC120100002"]
[]
[".02. 우   수   공                                                               ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"260","",""]
["..터파기/육상토사                                                               ","0-2m 기계                                                                       ",2282,"m3    ",{"$nulls":9},"",null,"270","","_CDE110100000"]
["..터파기/풍화암                                                                 ","0-2m 기계                                                                       ",292,"m3    ",{"$nulls":9},"",null,"280","","_CDE210100000"]
["..되메우기/토사                                                                 ","기계90%+인력10%                                                                 ",995,"m3    ",{"$nulls":9},"",null,"290","","_CDH110100000"]
["..되메우기/토사                                                                 ","다짐/기계100%                                                                   ",1236,"m3    ",{"$nulls":9},"",null,"300","","_CDH110000000"]
["..잔토처리                                                                      ","리핑암                                                                          ",292,"m3    ",{"$nulls":9},"",null,"310","","_CDF320000000"]
["..부족토/토사                                                                   ","지하층터파기잔토활용                                                            ",51,"m3    ",{"$nulls":9},"",null,"320","","G_4000"]
["..고강성PVC 이중벽관(자재포함)                                                  ","ø200mm                                                                         ",260,"m     ",{"$nulls":9},"",null,"330","","_CGD020200000"]
["..배수관(흄관)기계부설                                                          ","450mm                                                                           ",332,"m     ",{"$nulls":9},"",null,"340","","_CLK201210450"]
["..배수관(흄관)기계부설                                                          ","600mm                                                                           ",23,"m     ",{"$nulls":9},"",null,"350","","_CLK201210600"]
["..관기초(모래)                                                                  ","Φ250㎜                                                                         ",260,"m     ",{"$nulls":9},"",null,"360","","T000765843"]
["..관기초(콘크리트)                                                              ","Φ450㎜                                                                         ",332,"m     ",{"$nulls":9},"",null,"370","","T000765901"]
["..관기초(콘크리트)                                                              ","Φ600㎜                                                                         ",23,"m     ",{"$nulls":9},"",null,"380","","T000765902"]
["..하수관천공접합                                                                ","Φ450x250㎜                                                                     ",22,"개소  ",{"$nulls":9},"",null,"390","","T0010450"]
["..1호맨홀(우수)                                                                 ","Φ900                                                                           ",6,"개소  ",{"$nulls":9},"",null,"400","","T0007648"]
["..2호맨홀(우수)                                                                 ","Φ1200                                                                          ",6,"개소  ",{"$nulls":9},"",null,"410","","T0007649"]
["..각형맨홀(우수)                                                                ","1.2X1.2                                                                         ",1,"개소  ",{"$nulls":9},"",null,"420","","T0007651"]
["..집수정                                                                        ","600X600                                                                         ",19,"개소  ",{"$nulls":9},"",null,"430","","T00076543"]
["..우수받이                                                                      ","300x400                                                                         ",16,"개소  ",{"$nulls":9},"",null,"440","","T00076521"]
["..트랜치(침투형)                                                                ","300X300                                                                         ",120,"개소  ",{"$nulls":9},"",null,"450","","T00076555"]
["..무소음트랜치                                                                  ","300X400㎜                                                                       ",11,"M     ",{"$nulls":9},"",null,"460","","T00076553"]
["..맨홀접속구                                                                    ","Φ200㎜                                                                         ",11,"EA    ",{"$nulls":9},"",null,"470","","T000765939"]
["..맨홀접속구                                                                    ","Φ450㎜                                                                         ",25,"EA    ",{"$nulls":9},"",null,"480","","T000765942"]
["..맨홀접속구                                                                    ","Φ600㎜                                                                         ",1,"EA    ",{"$nulls":9},"",null,"490","","T000765943"]
["..관로(경고)테이프설치                                                          ","                                                                                ",355,"m     ",{"$nulls":9},"",null,"500","","_CHG120010000"]
["..하수관내 CCTV 조사                                                            ","                                                                                ",355,"m     ",{"$nulls":9},"",null,"510","","YQ0000000"]
["..CCTV 보고서 작성비                                                            ","보고서                                                                          ",355,"m     ",{"$nulls":9},"",null,"520","","YQ0000010"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"530","",""]
[".03. 오   수   공                                                               ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"540","",""]
["..터파기/육상토사                                                               ","0-2m 기계                                                                       ",708,"m3    ",{"$nulls":9},"",null,"550","","_CDE110100000"]
["..되메우기/토사                                                                 ","기계90%+인력10%                                                                 ",180,"m3    ",{"$nulls":9},"",null,"560","","_CDH110100000"]
["..되메우기/토사                                                                 ","다짐/기계100%                                                                   ",468,"m3    ",{"$nulls":9},"",null,"570","","_CDH110000000"]
["..잔토처리                                                                      ","토사                                                                            ",60,"m3    ",{"$nulls":9},"",null,"580","","_CDF310000000"]
["..고강성PVC 이중벽관(자재포함)                                                  ","ø250mm                                                                         ",176,"m     ",{"$nulls":9},"",null,"590","","_CGD020250000"]
["..관기초(모래)                                                                  ","Φ250㎜                                                                         ",176,"m     ",{"$nulls":9},"",null,"600","","T000765843"]
["..1호맨홀(오수)                                                                 ","Φ900                                                                           ",7,"개소  ",{"$nulls":9},"",null,"610","","T0007647"]
["..각형맨홀(오수)                                                                ","1.2X1.2                                                                         ",1,"개소  ",{"$nulls":9},"",null,"620","","T0007650"]
["..맨홀접속구                                                                    ","Φ250㎜                                                                         ",14,"EA    ",{"$nulls":9},"",null,"630","","T000765940"]
["..관로(경고)테이프설치                                                          ","                                                                                ",176,"m     ",{"$nulls":9},"",null,"640","","_CHG120010000"]
["..하수관내 CCTV 조사                                                            ","신설270M당                                                                      ",176,"m     ",{"$nulls":9},"",null,"650","","YQ0000000"]
["..CCTV 보고서 작성비                                                            ","보고서                                                                          ",176,"m     ",{"$nulls":9},"",null,"660","","YQ0000010"]
["..하수관수밀시험                                                                ","Φ250mm                                                                         ",8,"개소  ",{"$nulls":9},"",null,"670","","JH09880250"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"680","",""]
[".04. 상 수  도 공                                                               ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"690","",""]
["..터파기/육상토사                                                               ","기계90%+인력10%                                                                 ",56,"m3    ",{"$nulls":9},"",null,"700","","_CDE100111200"]
["..되메우기/토사                                                                 ","기계90%+인력10%                                                                 ",3,"m3    ",{"$nulls":9},"",null,"710","","_CDH110100000"]
["..되메우기/토사                                                                 ","다짐/기계100%                                                                   ",47,"m3    ",{"$nulls":9},"",null,"720","","_CDH110000000"]
["..잔토처리                                                                      ","토사                                                                            ",7,"m3    ",{"$nulls":9},"",null,"730","","_CDF310000000"]
["..모래부설                                                                      ","재료비별도                                                                      ",7,"M3    ",{"$nulls":9},"",null,"740","","H00901"]
["..주철관(시멘트라이닝닥터일)                                                    ","ø80mm,토사기초KP메카니컬접합                                                   ",41,"m     ",{"$nulls":9},"",null,"750","","_CGB200008000"]
["..주철관절단                                                                    ","ø80mm                                                                          ",2,"개소  ",{"$nulls":9},"",null,"760","","_CGB200008010"]
["..곡관보호공/곡관/자재포함                                                      ","Φ80㎜                                                                          ",2,"EA    ",{"$nulls":9},"",null,"770","","T0007659590"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"780","",""]
[".05. 포   장   공                                                               ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"790","",""]
["..1).아스콘포장                                                                 ","                                                                                ",0,"      ",{"$nulls":9},"",null,"800","",""]
["...아스콘포장/표층 포설및다짐                                                   ","T = 5cm                                                                         ",87,"m2    ",{"$nulls":9},"",null,"810","","_CLC400050000"]
["...아스콘포장/택코팅                                                            ","RSC-4(30ℓ/ａ)                                                                  ",87,"m2    ",{"$nulls":9},"",null,"820","","_CLC210000000"]
["...아스콘포장/기층 포설및다짐                                                   ","T = 10cm                                                                        ",87,"m2    ",{"$nulls":9},"",null,"830","","_CLC300100000"]
["...아스콘포장/프라임코팅                                                        ","RSC-3(80ℓ/ａ)                                                                  ",87,"m2    ",{"$nulls":9},"",null,"840","","_CLC110100000"]
["...보조기층포설및다짐                                                           ","20cm                                                                            ",21,"m3    ",{"$nulls":9},"",null,"850","","_CLA100150000"]
["...동상방지층포설및다짐                                                         ","30cm                                                                            ",32,"m3    ",{"$nulls":9},"",null,"860","","_CLA100200000"]
["..2).기타포장                                                                   ","                                                                                ",0,"      ",{"$nulls":9},"",null,"870","",""]
["...소형고압블럭포장                                                             ","T=650                                                                           ",858,"m2    ",{"$nulls":9},"",null,"880","","T0007303"]
["...소형고압블럭포장                                                             ","T=400(지하층상부)                                                               ",697,"m2    ",{"$nulls":9},"",null,"890","","T00073031"]
["...장애인주차장포장                                                             ","T=400(지하층상부)                                                               ",53,"m2    ",{"$nulls":9},"",null,"900","","T00073061"]
["...잔디블럭주차장포장(조합)                                                     ","T=650                                                                           ",766,"m2    ",{"$nulls":9},"",null,"910","","T00073050A"]
["...잔디블럭주차장포장(조합)                                                     ","T=400                                                                           ",460,"m2    ",{"$nulls":9},"",null,"920","","T00073051A"]
["...투수콘크리트포장                                                             ","T=21cm                                                                          ",7,"m2    ",{"$nulls":9},"",null,"930","","_CLG730307000"]
["...보도블록포장/소형고압블록                                                    ","T=20cm                                                                          ",8,"m2    ",{"$nulls":9},"",null,"940","","_CLG820308000"]
["...APRON포장                                                                    ","보조기층포설                                                                    ",112,"m2    ",{"$nulls":9},"",null,"950","","T0007307"]
["...카스토퍼페드                                                                 ","1.15*0.223*0.2                                                                  ",113,"EA    ",{"$nulls":9},"",null,"960","","T0007308"]
["..3).L형측구및보차도경계석                                                      ","                                                                                ",0,"      ",{"$nulls":9},"",null,"970","",""]
["...보차도경계석(화강석)/L형측구                                                 ","직선,180×200×1000                                                             ",202,"m     ",{"$nulls":9},"",null,"980","","_CLF300318200"]
["...보차도경계석(화강석)/L형측구                                                 ","곡선,180×200×1000                                                             ",26,"m     ",{"$nulls":9},"",null,"990","","_CLF300318210"]
["...턱낮춤구간(화강석)/L형측구/직선,                                             ","180×200×1000                                                                  ",10,"m     ",{"$nulls":9},"",null,"1000","","_CLF300318230"]
["...턱낮춤구간(화강석)/L형측구/곡선,                                             ","180×200×1000                                                                  ",18,"m     ",{"$nulls":9},"",null,"1010","","_CLF300318235"]
["...보차도경계석(화강석)/L형측구/경사,                                           ","180×200~100×1000                                                              ",6,"m     ",{"$nulls":9},"",null,"1020","","_CLF300318240"]
["...재료분리석(직선)                                                             ","180x200                                                                         ",345,"m     ",{"$nulls":9},"",null,"1030","","T000721A"]
["...재료분리석(직선)                                                             ","150x150                                                                         ",4,"M     ",{"$nulls":9},"",null,"1040","","T00070100A"]
["...보조기층포설및다짐                                                           ","15cm                                                                            ",35,"m3    ",{"$nulls":9},"",null,"1050","","_CLA100150010"]
["...동상방지층포설및다짐                                                         ","30cm                                                                            ",46,"m3    ",{"$nulls":9},"",null,"1060","","_CLA100200000"]
["..4).차선도색및카스토퍼                                                         ","                                                                                ",0,"      ",{"$nulls":9},"",null,"1070","",""]
["...차선도색/융착형식 도로형, 수동식                                             ","실선                                                                            ",17,"m2    ",{"$nulls":9},"",null,"1080","","T000703001"]
["...차선도색/융착형식 도로형, 수동식                                             ","문자,기호                                                                       ",29,"m2    ",{"$nulls":9},"",null,"1090","","T000703002"]
["...카스토퍼                                                                     ","                                                                                ",113,"EA    ",{"$nulls":9},"",null,"1100","","H00081001"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"1110","",""]
[".06. 안 전 시설공                                                               ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"1120","",""]
["..장애인표지판                                                                  ","                                                                                ",1,"개    ",{"$nulls":9},"",null,"1130","","T00074010"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"1140","",""]
[".07. 구 조  물 공                                                               ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"1150","",""]
["..터파기/육상토사                                                               ","기계90%+인력10%                                                                 ",190,"m3    ",{"$nulls":9},"",null,"1160","","_CDE100111200"]
["..되메우기/토사(인력10%)                                                        ","기계90%+인력10%                                                                 ",38,"m3    ",{"$nulls":9},"",null,"1170","","_CDH110100000"]
["..잔토처리                                                                      ","토사                                                                            ",153,"m3    ",{"$nulls":9},"",null,"1180","","_CDF310000000"]
["..파쇄암쌓기                                                                    ","0.5㎥ 내외                                                                      ",150,"m2    ",{"$nulls":9},"",null,"1190","","HL2710"]
["..파쇄암쌓기기초                                                                ","                                                                                ",63,"M     ",{"$nulls":9},"",null,"1200","","HL271001"]
["..조경용대석구입운반                                                            ","덤프15TON                                                                       ",120,"㎥    ",{"$nulls":9},"",null,"1210","","HF5900012"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"1220","",""]
[".08. EPS 블 럭 공                                                               ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"1230","",""]
["..EPS 불록성토                                                                  ","                                                                                ",351,"M3    ",{"$nulls":9},"",null,"1240","","K0070001"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"1250","",""]
[".09. 부   대   공                                                               ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"1260","",""]
["..중기운반비                                                                    ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"1270","","H00460"]
["..철근운반                                                                      ","건축단가적용                                                                    ",3.1339999999999999,"TON   ",{"$nulls":9},"",null,"1280","","GS010"]
["..흄관하차비                                                                    ","D 450                                                                           ",137,"본    ",{"$nulls":9},"",null,"1290","","HAM80151"]
["..흄관하차비                                                                    ","D 600                                                                           ",10,"본    ",{"$nulls":9},"",null,"1300","","HAM80152"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"1310","",""]
[".10. 자   재   대                                                               ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"1320","",""]
["..모래                                                                          ","도착도                                                                          ",188,"m3    ",{"$nulls":9},"",null,"1330","","MA001"]
["..자갈                                                                          ","도착도                                                                          ",190,"m3    ",{"$nulls":9},"",null,"1335","","MA002"]
["..잡석                                                                          ","도착도                                                                          ",54,"m3    ",{"$nulls":9},"",null,"1340","","MA003"]
["..보조기층재/도착도                                                             ","                                                                                ",1459,"m3    ",{"$nulls":9},"",null,"1350","","MA005"]
["..동상방지층재/도착도                                                           ","                                                                                ",784,"m3    ",{"$nulls":9},"",null,"1360","","MA0051"]
["..KP닥타일주철관                                                                ","D80 2종                                                                         ",7,"본    ",{"$nulls":9},"",null,"1370","","MX90010080"]
["..맨홀뚜껑(키잠금)받침포함                                                      ","주철재Φ648                                                                     ",7,"조    ",{"$nulls":9},"",null,"1380","","MH81757"]
["..맨홀뚜껑(디자인)받침포함                                                      ","디자인Φ648                                                                     ",14,"조    ",{"$nulls":9},"",null,"1390","","MH817580"]
["..스틸그레이팅(그물망포함)                                                      ","700X700X50                                                                      ",9,"조    ",{"$nulls":9},"",null,"1400","","M3010320120437350"]
["..스틸그레이팅(압연강재)                                                        ","700X700X50                                                                      ",10,"조    ",{"$nulls":9},"",null,"1410","","MD010511"]
["..스틸그레이팅(압연디자인)                                                      ","1000X400X50                                                                     ",120,"조    ",{"$nulls":9},"",null,"1420","","MD01274"]
["..스틸그레이팅(그물망포함)                                                      ","500X400X50                                                                      ",16,"조    ",{"$nulls":9},"",null,"1430","","M3010320120106762"]
["..무소음트랜치                                                                  ","1000X400X50                                                                     ",11,"M     ",{"$nulls":9},"",null,"1440","","MD01010"]
["..소형고압블럭                                                                  ","U형,칼라(T=60mm)                                                                ",9,"㎡    ",{"$nulls":9},"",null,"1450","","MH817441"]
["..소형고압블럭/친환경재                                                         ","U형,칼라(T=80mm)                                                                ",1737,"㎡    ",{"$nulls":9},"",null,"1460","","MH817440"]
["..잔디블럭블럭(칼라)/친환경재                                                   ","T=80mm                                                                          ",1324,"㎡    ",{"$nulls":9},"",null,"1470","","MH8174421"]
["..원심력철근콘크리트관                                                          ","원심력철근콘크리트관, 보통관B2, Φ450mm(강원)                                   ",137,"본    ",{"$nulls":9},"",null,"1480","","M4014210920150865"]
["..원심력철근콘크리트관                                                          ","원심력철근콘크리트관, 보통관B2, Φ600mm(강원)                                   ",10,"본    ",{"$nulls":9},"",null,"1490","","M4014210920150867"]
["..아스팔트콘크리트                                                              ","아스팔트콘크리트, 일반품, 표층용, 밀립도, 13(#78)                               ",10,"톤    ",{"$nulls":9},"",null,"1500","","M3011159720144313"]
["..아스팔트콘크리트                                                              ","아스팔트콘크리트, 일반품, 기층용, BB-2(#467)                                    ",21,"톤    ",{"$nulls":9},"",null,"1510","","M3011159720144314"]
["..아스팔트                                                                      "," 유제RS, C- 4, P/K(200L)                                                        ",0.2,"드럼  ",{"$nulls":9},"",null,"1520","","M3012160120143137"]
["..아스팔트                                                                      "," 유제RS, C- 3, P/K(200L)                                                        ",0.4,"드럼  ",{"$nulls":9},"",null,"1530","","M3012160120143138"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"1570","S",""]
[]
["Ⅱ.지하층터파기공                                                               ","                                                                                ",1,"식    ",{"$nulls":9},"","0202"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"10","*",""]
[".1. 토    공                                                                    ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"20","",""]
["..줄파기                                                                        ","인력+기계                                                                       ",27,"M     ",{"$nulls":9},"",null,"30","","T000010"]
["..토사 굴착 및 상차                                                             ","백호우0.7M3                                                                     ",18856,"M³   ",{"$nulls":9},"",null,"40","","K0010"]
["..리핑암 굴착 및 상차                                                           ","백호우0.7M3                                                                     ",7394,"M3    ",{"$nulls":9},"",null,"50","","K0020"]
["..발파암 굴착 및 상차                                                           ","미진동암파쇄굴                                                                  ",3041,"M3    ",{"$nulls":9},"",null,"60","","K0056"]
["..잔토처리                                                                      ","토사,L=30.0km                                                                   ",2244,"M3    ",{"$nulls":9},"",null,"70","","K0086"]
["..잔토처리                                                                      ","리핑암,L=30.0km                                                                 ",7394,"M3    ",{"$nulls":9},"",null,"80","","K0087A"]
["..잔토처리                                                                      ","발파암,L=30.0km                                                                 ",3041,"M3    ",{"$nulls":9},"",null,"90","","K0088"]
["..운반/토사 (임시적치장)                                                        ","L=1.0KM(덤프)                                                                   ",16612,"M3    ",{"$nulls":9},"",null,"100","","K0060"]
["..운반/상차(되메움용)                                                           ","L=1.0KM(덤프)                                                                   ",16612,"M3    ",{"$nulls":9},"",null,"110","","K0061"]
["..적재,적하/토사                                                                "," 백호+덤프15톤                                                                  ",16612,"M3    ",{"$nulls":9},"",null,"120","","_CDS100201500"]
["..되메우기및다짐                                                                ","다짐도 90% 이상                                                                 ",16612,"M3    ",{"$nulls":9},"",null,"130","","_CDG100100000"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"140","",""]
[".2. 가시설공                                                                    ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"150","",""]
["..H-PILE 천공(H-300×200)                                                       ","(풍화암)                                                                        ",155,"M     ",{"$nulls":9},"",null,"160","","_CJF100020000"]
["..H-PILE 박기                                                                   ","H-300×200×9×14                                                               ",20,"본    ",{"$nulls":9},"",null,"170","","K000060"]
["..H-PILE 뽑기                                                                   ","H-300×200×9×14                                                               ",20,"본    ",{"$nulls":9},"",null,"180","","K000070"]
["..띠장연결 H-300×300×10×15                                                   ","                                                                                ",2,"개소  ",{"$nulls":9},"",null,"190","","K000300"]
["..띠장설치 및 철거                                                              ","H-300×300×10×15                                                              ",26,"M     ",{"$nulls":9},"",null,"200","","K000270"]
["..브라켓트 설치 및 철거                                                         ","L-90x90x10                                                                      ",10,"개소  ",{"$nulls":9},"",null,"210","","K000090"]
["..토류판 설치 및 철거(T=6cm)                                                    "," 3개월이상~6개월미만                                                            ",74,"M2    ",{"$nulls":9},"",null,"220","","_CAE300106000"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"230","",""]
[".3. 운반공                                                                      ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"240","",""]
["..철골운반                                                                      ","건축단가적용                                                                    ",13.462,"TON   ",{"$nulls":9},"",null,"250","","GS020001"]
["..시멘트 운반                                                                   ","건축단가적용                                                                    ",8778,"포    ",{"$nulls":9},"",null,"260","","GS020002"]
["..중기운반비                                                                    ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"270","","H00461"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"280","",""]
[".4. 자재비                                                                      ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"290","",""]
["..강재손료(H-형강 6개월미만)                                                    ","300×200, 300×300                                                              ",13.462,"TON   ",{"$nulls":9},"",null,"300","","YD006220"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"310","",""]
[".5. 계측관리                                                                    ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"320","",""]
["..계측관리                                                                      ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"330","","G_020205_2"]
["  계측기 설치                                                                   ","                                                                                ",0,"      ",{"$nulls":9},"",null,"340","",""]
["   지중경사계                                                                   ","                                                                                ",3,"개소  ",{"$nulls":9},"",null,"350","",""]
["   지하수위계                                                                   ","                                                                                ",2,"개소  ",{"$nulls":9},"",null,"360","",""]
["   지표침하계                                                                   ","                                                                                ",6,"개소  ",{"$nulls":9},"",null,"370","",""]
["  계측분석 및 보고서 작성                                                       ","주2회                                                                           ",5,"개월  ",{"$nulls":9},"",null,"380","",""]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"390","S",""]
[]
["Ⅲ.기초보강공사                                                                 ","                                                                                ",1,"식    ",{"$nulls":9},"","0204"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"10","",""]
[".1. 기초 치환공사                                                               ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"20","",""]
["..치환혼합 및 다짐                                                              ","                                                                                ",1076,"m3    ",{"$nulls":9},"",null,"30","","K0070"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"40","S",""]
[]
["Ⅳ.영구배수공사                                                                 ","                                                                                ",1,"식    ",{"$nulls":9},"","0205"]
[".1. 드레인매트 배수시스템 설치공사                                              ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"10","","G_0204_3"]
["(1) 필터 설치                                                                   ","                                                                                ",0,"      ",{"$nulls":9},"",null,"20","",""]
["  시스템 배수로 감싸기                                                          ","                                                                                ",91,"M2    ",{"$nulls":9},"",null,"30","",""]
["  시스템 유도수로 감싸기                                                        ","                                                                                ",372,"M2    ",{"$nulls":9},"",null,"40","",""]
["  시스템 유도수로 하부 깔기                                                     ","                                                                                ",555,"M2    ",{"$nulls":9},"",null,"50","",""]
["(2) 시스템 배수로 설치                                                          ","                                                                                ",275,"M     ",{"$nulls":9},"",null,"60","",""]
["(3) 시스템 유도수로 설치                                                        ","                                                                                ",555,"M     ",{"$nulls":9},"",null,"70","",""]
["(4) P.E 필름 설치                                                               ","                                                                                ",3871,"M2    ",{"$nulls":9},"",null,"80","",""]
["(5) 잡자재                                                                      ","                                                                                ",1,"식    ",{"$nulls":9},"",null,"90","",""]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"100","S",""]
[]
["1. 관 급 자 재 대                                                               ","부가세포함                                                                      ",1,"식    ",{"$nulls":9},"","0206"]
[".1.레미콘                                                                       ","                                                                                ",0,"      ",{"$nulls":9},"",null,"10","",""]
["..레미콘(부가세포함)                                                            ","레미콘, 대전, 25-21-12                                                          ",121,"㎥    ",{"$nulls":9},"",null,"20","","M3011150520143513"]
["..레미콘(부가세포함)                                                            ","레미콘, 대전, 25-18-08                                                          ",101,"㎥    ",{"$nulls":9},"",null,"30","","M3011150520143509"]
[".2.경계석                                                                       ","                                                                                ",0,"      ",{"$nulls":9},"",null,"40","",""]
["..자연석경계석(부가세포함)                                                      "," 보차도용(직선), 180×200×1000mmR30                                            ",218,"개    ",{"$nulls":9},"",null,"50","","M3013150310025358"]
["..자연석경계석(부가세포함)                                                      "," 보차도용(곡선), 180×200×1000mmR30                                            ",45,"개    ",{"$nulls":9},"",null,"60","","M3013150310063316"]
["..자연석경계석(부가세포함)                                                      "," 보차도용(경사), 180×200~100×1000mmR30                                        ",6,"개    ",{"$nulls":9},"",null,"70","","M3013150320146210"]
["..자연석경계석(부가세포함)                                                      "," 보차도용(직선), 180×200×1000mm                                               ",355,"개    ",{"$nulls":9},"",null,"80","","M3013150310025357"]
["..자연석경계석(부가세포함)                                                      "," 도로용, 직선, 150×150×1000mm                                                 ",4,"개    ",{"$nulls":9},"",null,"90","","M3013150310063320"]
[".3.철근콘크리트용봉강                                                           ","                                                                                ",0,"      ",{"$nulls":9},"",null,"100","",""]
["..철근콘크리트용봉강                                                            ","철근콘크리트용봉강, 이형봉강(SD300), D13                                        ",1.9970000000000001,"톤    ",{"$nulls":9},"",null,"110","","M3010161920160899"]
["..철근콘크리트용봉강                                                            ","철근콘크리트용봉강, 이형봉강(SD300), D16                                        ",0.94499999999999995,"톤    ",{"$nulls":9},"",null,"120","","M3010161920160900"]
["..철근콘크리트용봉강                                                            ","철근콘크리트용봉강, 이형봉강(SD300), D19                                        ",0.192,"톤    ",{"$nulls":9},"",null,"130","","M3010161920160901"]
[".4.시멘트                                                                       ","                                                                                ",0,"      ",{"$nulls":9},"",null,"140","",""]
[".. 시멘트                                                                       ","시멘트, 전지역(제주제외), 40 KG                                                 ",8778,"포    ",{"$nulls":9},"",null,"150","","M3011160120142684"]
["                                                                                ","                                                                                ",0,"      ",{"$nulls":9},"",null,"160","S",""]

{"sheet":"조경내역","index":5,"n_rows":271,"n_cols":34,"rows_kept":271,"cut":false,"hidden":false,"merged":[[1,8,1,9],[1,10,1,11],[1,12,2,12],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,1,5],[1,6,1,7]]}
["국토연구원 신청사 건립공사(조경)_도급 공내역서"]
["공 종 명","규 격","수량","단위","재 료 비","","노 무 비","","경    비","","합    계","","비 고"]
["","","","","단 가","금 액","단 가","금 액","단 가","금 액","단 가","금 액","",{"$nulls":5},"할 증","화폐변환","OP값","EQ","LA","MA","금액계상"]
["1. 조경공사","",1,"식",{"$nulls":8},"","","A0"]
["   ","",null,"",{"$nulls":8},"","",null,"10","S",""]
{"$rows_empty":31}
["1. 조경공사","",{"$nulls":11},"","A1"]
["   1) 식재기반공","",1,"식",{"$nulls":8},"","",null,"10","","B1"]
["   2) 식재공","",1,"식",{"$nulls":8},"","",null,"20","","B2"]
["   3) 시설물공","",1,"식",{"$nulls":8},"","",null,"30","","B3"]
["   4) 포장공","",1,"식",{"$nulls":8},"","",null,"40","","B4"]
["   5) 우배수공","",1,"식",{"$nulls":8},"","",null,"50","","B5"]
["   6) 관급자재운반공사","",1,"식",{"$nulls":8},"","",null,"55","","B6"]
["   >합계","",null,"",{"$nulls":8},"","",null,"57","",""]
["   ","",null,"",{"$nulls":8},"","",null,"60","S",""]
{"$rows_empty":24}
["1) 식재기반공","",null,"",{"$nulls":8},"","","B1"]
["   인공토양","THK600",308.63,"M2",{"$nulls":8},"","",null,"10","","M3012209620162846"]
["   인공토양","THK400",24.5,"M2",{"$nulls":8},"","",null,"20","","M3012209620162845"]
["   인공토양","THK300","448.15","M2",{"$nulls":8},"","",null,"30","","M3012209620162844"]
["   인공토양","THK200","637.96","M2",{"$nulls":8},"","",null,"40","","M3012209620162843"]
["   방근쉬트","",308.63,"M2",{"$nulls":8},"","",null,"50","","M3012209620162849"]
["   투수쉬트","",2130.12,"M2",{"$nulls":8},"","",null,"60","","M3012209620162848"]
["   투수판","THK30",2130.12,"M2",{"$nulls":8},"","",null,"70","","M3012209620162847"]
["   화산석(멀칭)","THK500",24.47,"㎡",{"$nulls":8},"","",null,"75","","M3012209620162850"]
["   점검구","200X200",28,"개소",{"$nulls":8},"","",null,"77","","M3012209620162851"]
["   >소계","",null,"",{"$nulls":8},"","",null,"80","",""]
["   ","",null,"",{"$nulls":8},"","",null,"90","S",""]
{"$rows_empty":21}
["2) 식재공","",null,"",{"$nulls":8},"","","B2",{"$nulls":10},{"$f":"F104+F105+F106+F107+F108+F109+F110+F111+F112+F113+F114+F115+F116+F117+F118+F119+F120+F121+F122+F123+F124+F125+F126+F127+F128+F129+F130+F131+F132+F133+F134+F135+F136+F137+F138+F139+F140","v":0},{"$f":"H104+H105+H106+H107+H108+H109+H110+H111+H112+H113+H114+H115+H116+H117+H118+H119+H120+H121+H122+H123+H124+H125+H126+H127+H128+H129+H130+H131+H132+H133+H134+H135+H136+H137+H138+H139+H140","v":0},{"$f":"J104+J105+J106+J107+J108+J109+J110+J111+J112+J113+J114+J115+J116+J117+J118+J119+J120+J121+J122+J123+J124+J125+J126+J127+J128+J129+J130+J131+J132+J133+J134+J135+J136+J137+J138+J139+J140","v":0}]
["   소나무(장송)","H8.0xR30",9,"주",{"$nulls":8},"","",null,"30","","TA001",null,"T",{"$nulls":5},{"$f":"F141+F142+F143+F144+F145+F146+F147","v":0},{"$f":"H141+H142+H143+H144+H145+H146+H147","v":0},{"$f":"J141+J142+J143+J144+J145+J146+J147","v":0}]
["   소나무(장송)","H8.0xR25",18,"주",{"$nulls":8},"","",null,"40","","TA002",null,"T"]
["   잣나무","H3.0XW1.5",24,"주",{"$nulls":8},"","",null,"50","","TA003",null,"T"]
["   감나무","H3.0*R10",8,"주",{"$nulls":8},"","",null,"75","","TA004",null,"T"]
["   꽃사과","H3.0*R8",8,"주",{"$nulls":8},"","",null,"77","","TA005",null,"T"]
["   느티나무","H5.0xR30",2,"주",{"$nulls":8},"","",null,"80","","TA006",null,"T"]
["   느티나무","H4.5xR20",6,"주",{"$nulls":8},"","",null,"90","","TA008",null,"T"]
["   매화나무","H3.0xR8",15,"주",{"$nulls":8},"","",null,"100","","TA009",null,"T"]
["   모과나무","H3.0xR8",5,"주",{"$nulls":8},"","",null,"105","","TA010",null,"T"]
["   배롱나무","H2.5xR8",3,"주",{"$nulls":8},"","",null,"110","","TA011",null,"T"]
["   산수유","H2.5xW1.5xR8",8,"주",{"$nulls":8},"","",null,"120","","TA012",null,"T"]
["   왕벚나무","H4.0xB12",32,"주",{"$nulls":8},"","",null,"140","","TA013",null,"T"]
["   은행나무","H4.5xB12",46,"주",{"$nulls":8},"","",null,"150","","TA014",null,"T"]
["   이팝나무","H4.5xB12",12,"주",{"$nulls":8},"","",null,"152","","TA0145",null,"T"]
["   청단풍","H3.5xR20",8,"주",{"$nulls":8},"","",null,"153","","TA015",null,"T"]
["   청단풍","H3.0xR10",12,"주",{"$nulls":8},"","",null,"157","","TA016",null,"T"]
["   청단풍","H2.5xR8",18,"주",{"$nulls":8},"","",null,"160","","TA017",null,"T"]
["   층층나무","H3.5xR10",14,"주",{"$nulls":8},"","",null,"170","","TA018",null,"T"]
["   팥배나무","H3.0xR6",25,"주",{"$nulls":8},"","",null,"180","","TA019",null,"T"]
["   홍단풍","H3.0xR10",2,"주",{"$nulls":8},"","",null,"190","","TA020",null,"T"]
["   회화나무","H4.5xR15",25,"주",{"$nulls":8},"","",null,"200","","TA021",null,"T"]
["   남천","H1.0x3가지",160,"주",{"$nulls":8},"","",null,"230","","TA022",null,"T"]
["   회양목","H0.3xW0.3",9070,"주",{"$nulls":8},"","",null,"250","","TA023",null,"T"]
["   백철쭉","H0.3xW0.3",910,"주",{"$nulls":8},"","",null,"265","","TA0235",null,"T"]
["   병꽃나무","H1.0xW0.4",1070,"주",{"$nulls":8},"","",null,"280","","TA024",null,"T"]
["   수수꽃다리","H1.5*W0.6",7,"주",{"$nulls":8},"","",null,"285","","TA025",null,"T"]
["   산수국","H0.3xW0.4",280,"주",{"$nulls":8},"","",null,"290","","TA026",null,"T"]
["   산철쭉","H0.3xW0.3",1050,"주",{"$nulls":8},"","",null,"300","","TA027",null,"T"]
["   영산홍","H0.3xW0.3",1990,"주",{"$nulls":8},"","",null,"310","","TA028",null,"T"]
["   자산홍","H0.3xW0.3",1690,"주",{"$nulls":8},"","",null,"320","","TA029",null,"T"]
["   조팝나무","H0.6XW0.3",60,"주",{"$nulls":8},"","",null,"330","","TA030",null,"T"]
["   좀작살나무","H1.2xW0.4",90,"주",{"$nulls":8},"","",null,"340","","TA031",null,"T"]
["   쥐똥나무","H1.0xW0.3",990,"주",{"$nulls":8},"","",null,"345","","TA0315",null,"T"]
["   황매화","H1.0XW0.4",870,"주",{"$nulls":8},"","",null,"350","","TA032",null,"T"]
["   꽃잔디","8cm",4720,"본",{"$nulls":8},"","",null,"390","","TA033",null,"T"]
["   매발톱꽃","8cm",120,"본",{"$nulls":8},"","",null,"440","","TA034",null,"T"]
["   맥문동","3~5분얼",2930,"본",{"$nulls":8},"","",null,"450","","TA035",null,"T"]
["   벌개미취","8cm",240,"본",{"$nulls":8},"","",null,"470","","TA036",null,"T"]
["   사사(흰줄무늬)","10cm,4치포트",200,"본",{"$nulls":8},"","",null,"520","","TA037",null,"T"]
["   옥잠화","2~3분얼",70,"본",{"$nulls":8},"","",null,"540","","TA038",null,"T"]
["   애란","8cm",8070,"본",{"$nulls":8},"","",null,"550","","TA039",null,"T"]
["   원추리","2~3분얼",50,"본",{"$nulls":8},"","",null,"560","","TA040",null,"T"]
["   세덤","-",18130,"본",{"$nulls":8},"","",null,"595","","TA0405",null,"T"]
["   잔디","0.3x0.3x0.03,평떼",1307.17,"㎡",{"$nulls":8},"평떼","",null,"630","","TA041",null,"T"]
["   >소계","",null,"",{"$nulls":8},"","",null,"635","","",{"$nulls":13},{"$f":"F147+F146+F145+F144+F143+F142+F141+F140+F139+F138+F137+F136+F135+F134+F133+F132+F131+F130+F129+F128+F127+F126+F125+F124+F123+F122+F121+F120+F119+F118+F117+F116+F115+F114+F113+F112+F111","v":0},{"$f":"H147+H146+H145+H144+H143+H142+H141+H140+H139+H138+H137+H136+H135+H134+H133+H132+H131+H130+H129+H128+H127+H126+H125+H124+H123+H122+H121+H120+H119+H118+H117+H116+H115+H114+H113+H112+H111","v":0},{"$f":"J147+J146+J145+J144+J143+J142+J141+J140+J139+J138+J137+J136+J135+J134+J133+J132+J131+J130+J129+J128+J127+J126+J125+J124+J123+J122+J121+J120+J119+J118+J117+J116+J115+J114+J113+J112+J111","v":0}]
["   ","",null,"",{"$nulls":8},"","",null,"640","S","",{"$nulls":13},{"$f":"F110+F109+F108+F107+F106+F105+F104","v":0},{"$f":"H110+H109+H108+H107+H106+H105+H104","v":0},{"$f":"J110+J109+J108+J107+J106+J105+J104","v":0}]
{"$rows_empty":19}
["3) 시설물공","",null,"",{"$nulls":8},"","","B3"]
["   계단","W5350",1,"개소",{"$nulls":8},"","",null,"20","","S-1205-002",null,"T"]
["   날개벽","H200",9.6,"m",{"$nulls":8},"","",null,"30","","S-1205-002-1",null,"T"]
["   핸드레일","",2,"개소",{"$nulls":8},"","",null,"40","","S-1205-003",null,"T"]
["   목재데크A","T20",6,"개소",{"$nulls":8},"","",null,"60","","S-1205-034",null,"T"]
["   목재데크B","T20",252.09,"M2",{"$nulls":8},"","",null,"65","","S-1205-035",null,"T"]
["   목재데크C","T20",863.33,"M2",{"$nulls":8},"","",null,"67","","S-1205-036",null,"T"]
["   플랜터겸 벤치","H450",41.8,"m",{"$nulls":8},"","",null,"69","","S-1205-037",null,"T"]
["   조명열주","D500xH3000",6,"개소",{"$nulls":8},"","",null,"111","","S-1205-010",null,"T"]
["   등의자","560x1800xH440",28,"개소",{"$nulls":8},"","",null,"113","","S-1205-012",null,"T"]
["   휀스A","H1800",12.3,"경간",{"$nulls":8},"","",null,"116","","S-1205-028-1",null,"T"]
["   휀스B","H1800",50.17,"경간",{"$nulls":8},"","",null,"117","","S-1205-028-2",null,"T"]
["   휀스B 출입문","H1800",5,"개소",{"$nulls":8},"","",null,"118","","M4924159620275599"]
["   식재플랜터","1600x1600xH500",6,"개소",{"$nulls":8},"","",null,"119","","S-1205-008-1",null,"T"]
["   목재계단","",15.9,"m",{"$nulls":8},"","",null,"120","","S-1205-027-1",null,"T"]
["   안내해설판","H1000x1200",1,"개소",{"$nulls":8},"","",null,"170","","S-1205-015",null,"T"]
["   돌무더기","D2000xH500",2,"ea",{"$nulls":8},"","",null,"210","","S-1205-019",null,"T"]
["   장작더미","L2500x500x1000",2,"ea",{"$nulls":8},"","",null,"220","","S-1205-020",null,"T"]
["   새집","300x300x300",2,"ea",{"$nulls":8},"","",null,"230","","S-1205-021",null,"T"]
["   디딤돌","300x900",79,"개소",{"$nulls":8},"","",null,"232","","PA0127",null,"T"]
["   화강석디딤석B","400x400",114,"ea",{"$nulls":8},"","",null,"237","","PA0125",null,"T"]
["   장대석놓기","H400",16.55,"M",{"$nulls":8},"","",null,"239","","PA0126",null,"T"]
["   자전거보관대","16151x2000",2,"개소",{"$nulls":8},"","",null,"240","","S-1205-022",null,"T"]
["   ","",null,"",{"$nulls":8},"","",null,"270","S",""]
{"$rows_empty":9}
["4) 포장공","",null,"",{"$nulls":8},"","","B4"]
["   화강석판석포장D","T50,고흥석,정다듬",116.76,"㎡",{"$nulls":8},"","",null,"5","","PA0075",null,"T"]
["   화강석판석포장A","T30,포천석,버너",353.78,"㎡",{"$nulls":8},"","",null,"10","","PA001",null,"T"]
["   화강석판석포장B","T30,고흥석,버너",636.36,"㎡",{"$nulls":8},"","",null,"20","","PA002",null,"T"]
["   화강석판석포장C","T30,마천석,버너",126.34,"㎡",{"$nulls":8},"","",null,"35","","PA003",null,"T"]
["   인조화강석블럭A(지상)","T80,불투수",316.43,"㎡",{"$nulls":8},"","",null,"39","","PA0035",null,"T"]
["   인조화강석블럭A(지상)","T60,투수",1980.82,"㎡",{"$nulls":8},"","",null,"43","","PA004",null,"T"]
["   인조화강석블럭A(옥상)","T60,투수",445.5,"㎡",{"$nulls":8},"","",null,"47","","PA0045",null,"T"]
["   인조화강석블럭B","T60,투수",555.63,"㎡",{"$nulls":8},"","",null,"48","","PA005",null,"T"]
["   인조화강석블럭C","T60,투수",1453.83,"㎡",{"$nulls":8},"","",null,"49","","PA006",null,"T"]
["   자연석판석(잔디줄눈)","THK50",123.92,"M2",{"$nulls":8},"","",null,"60","","PA009",null,"T"]
["   황토길포장","T100",131.19,"㎡",{"$nulls":8},"","",null,"70","","PA010",null,"T"]
["   자갈깔기","T300",64.010000000000005,"㎡",{"$nulls":8},"","",null,"130","","PA011",null,"T"]
["   자갈깔기","T150",697.55,"㎡",{"$nulls":8},"","",null,"165","","PA0115",null,"T"]
["   화강석경계석A(지상)","150x150x1000,직선",952.51,"m",{"$nulls":8},"","",null,"200","","PA013",null,"T"]
["   화강석경계석A(옥상)","150x150x1000,직선",461.64,"m",{"$nulls":8},"","",null,"205","","PA014",null,"T"]
["   화강석경계석B(지상)","100x100x1000,직선",532.58000000000004,"m",{"$nulls":8},"","",null,"210","","PA015",null,"T"]
["   >소계","",null,"",{"$nulls":8},"","",null,"230","",""]
["   ","",null,"",{"$nulls":8},"","",null,"240","S",""]
{"$rows_empty":14}
["5) 우배수공","",null,"",{"$nulls":8},"","","B5"]
["   횡단배수구","W410xH600",150.1,"m",{"$nulls":9},"",null,"30","","W-1205-004",null,"T"]
["   집수정","405x500",9,"개소",{"$nulls":8},"","",null,"60","","W-1205-006",null,"T"]
["   >소계","",null,"",{"$nulls":8},"","",null,"80","",""]
["   ","",null,"",{"$nulls":8},"","",null,"90","S",""]
{"$rows_empty":28}
["6) 관급자재운반공사","",null,"",{"$nulls":8},"","","B6"]
["   시멘트운반비","L:10km, 덤프8톤",883,"포",{"$nulls":8},"","",null,"10","","GE001010102000004"]
["   철근운반비","L:15km, 트레일러20톤",3,"톤",{"$nulls":8},"","",null,"20","","GE001010102000005"]
["   >소계","",null,"",{"$nulls":8},"","",null,"30","",""]

{"sheet":"기계집계","index":6,"n_rows":56,"n_cols":14,"rows_kept":56,"cut":false,"hidden":false,"merged":[[2,12,3,12],[0,0,0,12],[1,0,1,12],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,2,5],[2,6,2,7],[2,8,2,9],[2,10,2,11]]}
["집   계   표"]
["[공사명]  국토연구원 신청사 신축공사"]
["품          명","규       격","단위","수량","재  료  비",null,"노  무  비",null,"경    비",null,"합    계",null,"비고"]
[{"$nulls":4},"단가","금액","단가","금액","단가","금액","단가","금액"]
["01  기계설비공사",null,null,1,{"$nulls":9},"01"]
["0101  장비설치공사",null,null,1,{"$nulls":9},"0101"]
["0102  옥외배관공사",null,null,1,{"$nulls":9},"0102"]
["010201  중온수배관공사",null,null,1,{"$nulls":9},"010201"]
["010202  위생배관공사",null,null,1,{"$nulls":9},"010202"]
["0103  기계실배관공사",null,null,1,{"$nulls":9},"0103"]
["0104  공조배관공사",null,null,1,{"$nulls":9},"0104"]
["0105  공조덕트설치공사",null,null,1,{"$nulls":9},"0105"]
["0106  위생설비공사",null,null,1,{"$nulls":9},"0106"]
["010601  위생기구설치공사",null,null,1,{"$nulls":9},"010601"]
["010602  급수급탕배관공사",null,null,1,{"$nulls":9},"010602"]
["010603  오배수배관공사",null,null,1,{"$nulls":9},"010603"]
["0107  가스배관공사",null,null,1,{"$nulls":9},"0107"]
["0108  연도설치공사",null,null,1,{"$nulls":9},"0108"]
["0109  방음방진설치공사",null,null,1,{"$nulls":9},"0109"]
["0110  동파방지열선공사",null,null,1,{"$nulls":9},"0110"]
["011001  공조(1F,3F,4F,5F)",null,null,1,{"$nulls":9},"011001"]
["011002  위생(2F,4F,5F)",null,null,1,{"$nulls":9},"011002"]
["0111  우수처리시설공사",null,null,1,{"$nulls":9},"0111"]
["0112  쓰레기이송설비공사",null,null,1,{"$nulls":9},"0112"]
["02  T.A.B 공사",null,null,1,{"$nulls":9},"02"]
["03  관급공사",null,null,1,{"$nulls":9},"03"]
["0301  도급자관급",null,null,1,{"$nulls":9},"0301"]
["030101  팬코일유니트",null,null,1,{"$nulls":9},"030101"]
["0302  관급자관급",null,null,1,{"$nulls":9},"0302"]
["030201  냉동기",null,null,1,{"$nulls":9},"030201"]
["030202  콤팩트열교환기",null,null,1,{"$nulls":9},"030202"]
["030203  냉각탑",null,null,1,{"$nulls":9},"030203"]
["030204  공기조화기",null,null,1,{"$nulls":9},"030204"]
["030205  팽창기체분리기",null,null,1,{"$nulls":9},"030205"]
["030206  항온항습기",null,null,1,{"$nulls":9},"030206"]
["030207  저수조",null,null,1,{"$nulls":9},"030207"]
["030208  부스터펌프",null,null,1,{"$nulls":9},"030208"]
["030209  고무발포보온재",null,null,1,{"$nulls":9},"030209"]
["030210  자동제어설치공사",null,null,1,{"$nulls":9},"030210"]
["030211  주방기구설치공사",null,null,1,{"$nulls":9},"030211"]
["030212  EHP설치공사",null,null,1,{"$nulls":9},"030212"]
["030213  환기유니트설치공사",null,null,1,{"$nulls":9},"030213"]
["030214  지열시스템설비공사",null,null,1,{"$nulls":9},"030214"]
["04  분담금공사",null,null,1,{"$nulls":9},"04"]
{"$rows_empty":9}
["[ 합                  계 ]"]
["End Of File(Ver 6.0)"]
["마지막열은 지우지 마시오"]

{"sheet":"기계내역","index":7,"n_rows":2709,"n_cols":29,"rows_kept":2709,"cut":false,"hidden":false,"merged":[[1,12,1,13],[1,14,2,14],[0,2,0,14],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,1,7],[1,8,1,9],[1,10,1,11]]}
[null,null,"[공사명]  국토연구원 신청사 신축공사"]
["공종","코드","품          명","규       격","단위","수량","재  료  비",null,"노  무  비",null,"경    비",null,"합    계",null,"비고"]
[{"$nulls":6},"단가","금액","단가","금액","단가","금액","단가","금액"]
[null,null,"0101  장비설치공사"]
["0101","MM708396907","ACH-1 2단저온수흡수식냉동기","280RT","대",2,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396908","CT-1직교류형냉각탑","700CRT","대",2,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396909","HX-1컴팩트유니트(판형)","684,000KCAL/HR","SET",1,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396910","HX-2컴팩트유니트(판형)","129,000KCAL/HR","",{"$nulls":9},"관급자재",{"$nulls":4},0]
["0101","MM708396911","AHU-1공기조화기(수평형)","46,000CMH","대",1,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396912","AHU-2공기조화기(수평형)","13,000CMH","대",1,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396913","AHU-3공기조화기(수평형)","14,000CMH","대",1,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396914","AHU-4공기조화기(수평형)","12,000CMH","대",1,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396915","AHU-5공기조화기(수평형)","23,000CMH","대",1,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396916","AHU-6공기조화기(수평형)","28,690CMH","대",1,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396917","AHU-7공기조화기(수평형)","30,030CMH","대",1,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396918","HVU-1공기조화기(수평형)","12,000CMH","대",1,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396919","FCU-1팬코일유닛(1WAY천장카세트","6CMM","대",36,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396920","FCU-2팬코일유닛(2WAY천장카세트","16CMM","대",138,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396921","FCU-3팬코일유닛(4WAY천장카세트","18.3CMM","대",11,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396922","FCU-4팬코일유닛(바닥상치형)","18.3CMM","대",219,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396923","FCU-5팬코일유닛(천정매입형)","12.8CMM","대",29,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396924","FCU-6팬코일유닛(천정매입형)","19.8CMM","대",8,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396932","T-1저수조(PDF 361,840L)","6,700*14,800*4,000","대",1,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396937","CHT-1공냉식항온항습기","냉/난:14,250/7,740KCAL/H","대",1,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396938","CHT-2공냉식항온항습기","냉/난:40,500/17,200KCAL/H","대",2,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396939","P-1냉각수순환펌프(인라인)","6,634LPM*29M*55KW","대",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396940","P-2냉수순환펌프(인라인)","2,217LPM*32M*19KW","대",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396941","P-3지열냉온수순환펌프(인라인)","720LPM*27M*5.5KW","대",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396931","P-4급수펌프(부스터)","(395LPM*3)*57M*(7.5KW*3)","SET",1,{"$nulls":8},"관급자재",null,null,0,0,0]
["0101","MM708396942","P-5배수펌프(수중형)","500LPM*14M*2.2KW","대",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396943","P-6배수펌프(수중형)","100LPM*11M*0.75KW","대",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396944","P-7배수펌프(수중형)","50LPM*11M*0.4KW","대",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396945","P-8배수펌프(수중형)","200LPM*13M*1.5KW","대",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396946","P-9배수펌프(수중형)","400LPM*14M*2.2KW","대",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396947","T-2팽창탱크(SS400 200L)","D588*1,094","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396948","FU-1탈취유니트","16,000CMH","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396950","CON-1온수컨벡터","164KCAL/HR 2ROW","대",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396951","CON-2전기컨벡터","1.5KW","대",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396952","F-1원심식인라인휀(D611)","12,000CMH*238PA*2.2KW","대",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396953","F-2소형시로코휀(D250)","1,700CMH*192PA*0.88KW","대",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396954","F-3원심식인라인휀(D543)","4,500CMH*194PA*1.5KW","대",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396955","F-4소형시로코휀(D250)","2,000CMH*192PA*0.88KW","대",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396956","F-5소형시로코휀(D250)","1,700CMH*218PA*0.88KW","대",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396957","F-6소형시로코휀(D250)","500CMH*212PA*0.88KW","대",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396958","F-7편흡입다익형휀(SS#4.5)","12,400CMH*282PA*3.7KW","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396959","F-8편흡입다익형휀(SS#2.5)","3,700CMH*275PA*1.5KW","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396960","F-9천정형휀(D150)","228CMH*17PA*0.03KW","대",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396961","F-11소형시로코휀(D180)","300CMH*192PA*0.13KW","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396962","F-12소형시로코휀(D250)","2,200CMH*242PA*0.88KW","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396963","F-13소형시로코휀(D250)","3,500CMH*256PA*1.2KW","대",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396964","F-14벽부형휀(D200)","540CMH*7PA*0.03KW","대",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396965","F-15소형시로코휀(D250)","1,400CMH*269PA*0.88KW","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396966","F-16양흡입다익형휀(DS#3.5)","13,500CMH*196PA*2.2KW","대",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396967","F-17소형시로코휀(D180)","650CMH*198PA*0.13KW","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396968","F-18소형시로코휀(D250)","800CMH*238PA*0.88KW","대",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396969","F-19소형시로코휀(D250)","700CMH*238PA*0.88KW","대",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","MM708396970","AS-1팽창기체분리기(STS304)","200L 800*1,500*1,558","대",1,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396971","AS-2팽창기체분리기(STS304)","600L 800*1,500*1,200","대",1,{"$nulls":8},"관급자재",{"$nulls":4},0]
["0101","MM708396972","ERD-1천정형전기온풍기","1.5KW","대",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0101","56900017041","노무비","보통인부","인",259,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0101","56900017030","노무비","배관공","인",22,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0101","56900017015","노무비","기계설비공","인",976,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0101","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},"",63,null,1,0,0.03,{"$nulls":8},1]
{"$rows_empty":17}
[null,null,"[ 합           계 ]"]
[null,null,"010201  중온수배관공사"]
["010201","47100607061","이중보온관(단열관)","(SPPS38+HDPE), D150","M",105,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010201","PPS00000001","잡재료비","관의 3%","식",1,{"$nulls":8},"",84,null,0,0,0.03,{"$nulls":8},1]
["010201","47100608101","이중보온관(단열엘보)","(SPPS38+HDPE)D150","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010201","47100608820","이중보온관(단열연결재)","(SPPS38+HDPE)D150","개소",18,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010201","56940130110","강관용접 (S#40)","D150","개소",22,{"$nulls":8},"56940130110",{"$nulls":4},0,{"$nulls":8},1]
["010201","56941530080","X - RAY TEST","","매당",66,{"$nulls":8},"56941530080",{"$nulls":4},0,{"$nulls":8},1]
["010201","56941990020","기계되메우기","","M3",45,{"$nulls":8},"56941990020",{"$nulls":4},0,{"$nulls":8},1]
["010201","56941990010","기계터파기","","M3",60,{"$nulls":8},"56941990010",{"$nulls":4},0,{"$nulls":8},1]
["010201","56941990030","잔토처리","","M3",15,{"$nulls":8},"56941990030",{"$nulls":4},0,{"$nulls":8},1]
["010201","56941990040","모래부설","","M3",15,{"$nulls":8},"56941990040",{"$nulls":4},0,{"$nulls":8},1]
["010201","56900017041","노무비","보통인부","인",13,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["010201","56900017118","노무비","특별인부","인",9,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["010201","56900017125","노무비","플랜트배관공","인",9,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["010201","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},"",96,null,1,0,0.03,{"$nulls":8},1]
{"$rows_empty":10}
[null,null,"[ 합           계 ]"]
[null,null,"010202  위생배관공사"]
["010202","47100487006","배관용 탄소강관","백관 (SPP), D50, 반제품","M",11,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010202","47100487009","배관용 탄소강관","백관 (SPP), D100, 반제품","M",11,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010202","47100727109","일반용 경질염화비닐관","PVC관(VG1,DTS) D100","M",21,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010202","47100727110","일반용 경질염화비닐관","PVC관(VG1,DTS) D125","M",10,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010202","47100787104","수도용 폴리에틸렌관","PE수도관(1종), D25","M",48,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010202","47100787109","수도용 폴리에틸렌관","PE수도관(1종), D75","M",61,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010202","PPS00000001","잡재료비","관의 3%","식",1,{"$nulls":8},"",115,null,0,0,0.03,{"$nulls":8},1]
["010202","47300977003","수도용 폴리에칠렌이음관","90˚엘보(융착식) D25","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010202","47300977008","수도용 폴리에칠렌이음관","90˚엘보(융착식) D75","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010202","47300977122","수도용 폴리에칠렌이음관","소켓 (나사조임식) D25","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010202","47300977272","수도용 폴리에칠렌이음관","밸브소켓(나사조임식) D25","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010202","56940250030","PEM 접합 (수도용)","D25","개소",24,{"$nulls":8},"56940250030",{"$nulls":4},0,{"$nulls":8},1]
["010202","56940250080","PEM 접합 (수도용)","D75","개소",15,{"$nulls":8},"56940250080",{"$nulls":4},0,{"$nulls":8},1]
["010202","47305257662","플랜지(FLANGE)","PE 플랜지 D25","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010202","47305257667","플랜지(FLANGE)","PE 플랜지 D80","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010202","80000011180","청동게이트밸브 (10KG)","D25","EA",2,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["010202","80000011208","주철버터플라이밸브(Lever)","D80","EA",1,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["010202","56941420020","유성페인트칠","철재면2회","M2",5,{"$nulls":8},"56941420020",{"$nulls":4},0,{"$nulls":8},1]
["010202","56941990010","기계터파기","","M3",148,{"$nulls":8},"56941990010",{"$nulls":4},0,{"$nulls":8},1]
["010202","56941990020","기계되메우기","","M3",111,{"$nulls":8},"56941990020",null,null,0,0,0,{"$nulls":8},1]
["010202","56941990030","잔토처리","","M3",37,{"$nulls":8},"56941990030",{"$nulls":4},0,{"$nulls":8},1]
["010202","56941990040","모래부설","","M3",37,{"$nulls":8},"56941990040",{"$nulls":4},0,{"$nulls":8},1]
["010202","56900017041","노무비","보통인부","인",3,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["010202","56900017030","노무비","배관공","인",7,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["010202","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},"",133,null,1,0,0.03,{"$nulls":8},1]
{"$rows_empty":25}
[null,null,"[ 합           계 ]"]
[null,null,"0103  기계실배관공사"]
["0103","47100487003","배관용 탄소강관","백관 (SPP), D25, 반제품","M",11,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100487006","배관용 탄소강관","백관 (SPP), D50, 반제품","M",58,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100487007","배관용 탄소강관","백관 (SPP), D65, 반제품","M",30,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100487008","배관용 탄소강관","백관 (SPP), D80, 반제품","M",44,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100487009","배관용 탄소강관","백관 (SPP), D100, 반제품","M",126,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100487011","배관용 탄소강관","백관 (SPP), D150, 반제품","M",17,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100487012","배관용 탄소강관","백관 (SPP), D200, 반제품","M",23,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100487013","배관용 탄소강관","백관 (SPP), D250, 반제품","M",216,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100487102","배관용 탄소강관","흑관 (SPP), D20, 반제품","M",8,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100537502","압력배관용  탄소강관","흑관 (S#40), D20","M",14,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100537505","압력배관용  탄소강관","흑관 (S#40), D40","M",7,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100537508","압력배관용  탄소강관","흑관 (S#40), D80","M",66,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100537510","압력배관용  탄소강관","흑관 (S#40), D125","M",48,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100537511","압력배관용  탄소강관","흑관 (S#40), D150","M",70,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100047102","동 및 동합금 관","동관 (L-TYPE), D20","M",36,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100047103","동 및 동합금 관","동관 (L-TYPE), D25","M",229,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100047106","동 및 동합금 관","동관 (L-TYPE), D50","M",158,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100407022","일반배관용 스테인리스 강관","K-TYPE, D20","M",46,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100407023","일반배관용 스테인리스 강관","K-TYPE, D25","M",2,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100407024","일반배관용 스테인리스 강관","K-TYPE, D32","M",39,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100407025","일반배관용 스테인리스 강관","K-TYPE, D40","M",78,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100407026","일반배관용 스테인리스 강관","K-TYPE, D50","M",86,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100417247","배관용 스테인리스 강관","D65x3T","M",80,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100417248","배관용 스테인리스 강관","D80x3T","M",18,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100417249","배관용 스테인리스 강관","D100x3T","M",140,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100417250","배관용 스테인리스 강관","D125x3T","M",311,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100417251","배관용 스테인리스 강관","D150x3T","M",232,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100417252","배관용 스테인리스 강관","D200x3T","M",253,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100417507","배관용스테인리스강관(무용접)","D65x3T","M",65,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100417508","배관용스테인리스강관(무용접)","D80x3T","M",85,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100417509","배관용스테인리스강관(무용접)","D100x3T","M",78,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100417510","배관용스테인리스강관(무용접)","D125x3T","M",37,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100417511","배관용스테인리스강관(무용접)","D150x3T","M",22,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","47100727206","INNO AS (PPF) 저소음관","D150","M",11,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0103","PPS00000001","잡재료비","관의 3%","식",1,{"$nulls":8},"",195,null,0,0,0.03,{"$nulls":8},1]
["0103","56940803102","관보온(유리솜.칼라함석)","40TxD20","M",12,{"$nulls":8},"56940803102",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940803194","관보온(유리솜.칼라함석)","50TxD40","M",7,{"$nulls":8},"56940803194",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940803307","관보온(유리솜.칼라함석)","75TxD80","M",60,{"$nulls":8},"56940803307",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940803309","관보온(유리솜.칼라함석)","75TxD125","M",44,{"$nulls":8},"56940803309",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940803310","관보온(유리솜.칼라함석)","75TxD150","M",64,{"$nulls":8},"56940803310",{"$nulls":4},0,{"$nulls":8},1]
["0103","47304017006","나사식 강관제 관이음쇠","백엘보 (나사) D50","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127002","용접식 관이음쇠","백엘보 (용접) D65","EA",19,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127003","용접식 관이음쇠","백엘보 (용접) D80","EA",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127004","용접식 관이음쇠","백엘보 (용접) D100","EA",19,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127006","용접식 관이음쇠","백엘보 (용접) D150","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127007","용접식 관이음쇠","백엘보 (용접) D200","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127008","용접식 관이음쇠","백엘보 (용접) D250","EA",48,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47304017106","나사식 강관제 관이음쇠","백티이 (나사) D50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127216","용접식 관이음쇠","백티이 (용접) D65","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127218","용접식 관이음쇠","백티이 (용접) D100","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127220","용접식 관이음쇠","백티이 (용접) D150","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127222","용접식 관이음쇠","백티이 (용접) D250","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127387","용접식 관이음쇠","백리듀서 (용접) D250","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47304017303","나사식 강관제 관이음쇠","백니플 (나사) D25","EA",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47304017306","나사식 강관제 관이음쇠","백니플 (나사) D50","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47304017406","나사식 강관제 관이음쇠","백유니온 (나사) D50","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127132","용접식 관이음쇠","흑엘보 (용접 S#40) D20","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127135","용접식 관이음쇠","흑엘보 (용접 S#40) D40","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127138","용접식 관이음쇠","흑엘보 (용접 S#40) D80","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127140","용접식 관이음쇠","흑엘보 (용접 S#40) D125","EA",18,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127141","용접식 관이음쇠","흑엘보 (용접 S#40) D150","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127322","용접식 관이음쇠","흑티이 (용접 S#40) D20","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127328","용접식 관이음쇠","흑티이 (용접 S#40) D80","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127331","용접식 관이음쇠","흑티이 (용접 S#40) D150","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127508","용접식 관이음쇠","흑리듀서 (용접 S#40) D80","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127510","용접식 관이음쇠","흑리듀서 (용접 S#40) D125","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127511","용접식 관이음쇠","흑리듀서 (용접 S#40) D150","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127720","단조 SOCKOLET","D15","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127721","단조 SOCKOLET","D20","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127724","단조 THREADOLET","D15","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301127725","단조 THREADOLET","D20","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301018303","동관이음쇠","동엘보 D25","EA",28,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301018306","동관이음쇠","동엘보 D50","EA",22,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301018422","동관이음쇠","동소켓 D25","EA",13,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301018425","동관이음쇠","동소켓 D50","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301018488","동관이음쇠","동유니온 (C*M) D20","EA",39,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301017322","동관이음쇠","황동아답타 (C*M) D20","EA",39,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108029","일반배관용 STS강관 이음쇠","엘보(STS 용접#10) D65","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108030","일반배관용 STS강관 이음쇠","엘보(STS 용접#10) D80","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108031","일반배관용 STS강관 이음쇠","엘보(STS 용접#10) D100","EA",66,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108032","일반배관용 STS강관 이음쇠","엘보(STS 용접#10) D125","EA",95,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108033","일반배관용 STS강관 이음쇠","엘보(STS 용접#10) D150","EA",22,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108034","일반배관용 STS강관 이음쇠","엘보(STS 용접#10) D200","EA",81,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108215","일반배관용 STS강관 이음쇠","티이(STS 용접 S#10) D100","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108216","일반배관용 STS강관 이음쇠","티이(STS 용접 S#10) D125","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108217","일반배관용 STS강관 이음쇠","티이(STS 용접 S#10) D150","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108218","일반배관용 STS강관 이음쇠","티이(STS 용접 S#10) D200","EA",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108459","일반배관용 STS강관 이음쇠","리듀서(STS용접S#10) D100","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108461","일반배관용 STS강관 이음쇠","리듀서(STS용접S#10) D150","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108462","일반배관용 STS강관 이음쇠","리듀서(STS용접S#10) D200","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108045","일반배관용 STS강관 이음쇠","엘보(STS 용접#20) D100","EA",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108951","STS강관이음쇠(원터치삽입식)","90'엘보  D20","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108952","STS강관이음쇠(원터치삽입식)","90'엘보  D25","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108955","STS강관이음쇠(원터치삽입식)","90'엘보  D30","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108956","STS강관이음쇠(원터치삽입식)","90'엘보  D40","EA",18,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108957","STS강관이음쇠(원터치삽입식)","90'엘보  D50","EA",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108989","STS강관이음쇠(원터치삽입식)","티  D40","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301108990","STS강관이음쇠(원터치삽입식)","티  D50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301109009","STS강관이음쇠(원터치삽입식)","레듀셔  D50x40","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301109043","STS강관이음쇠(원터치삽입식)","소켓  D30","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301109044","STS강관이음쇠(원터치삽입식)","소켓  D40","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301109045","STS강관이음쇠(원터치삽입식)","소켓  D50","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301109050","STS강관이음쇠(원터치삽입식)","밸브소켓  D13x15","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301109052","STS강관이음쇠(원터치삽입식)","밸브소켓  D20x20","EA",24,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301109058","STS강관이음쇠(원터치삽입식)","밸브소켓  D40x40","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301109061","STS강관이음쇠(원터치삽입식)","밸브소켓  D50x50","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288002","무용접스텐고정식커플링(일반용)","D50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288003","무용접스텐고정식커플링(일반용)","D65","EA",19,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288004","무용접스텐고정식커플링(일반용)","D80","EA",55,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288005","무용접스텐고정식커플링(일반용)","D100","EA",14,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288006","무용접스텐고정식커플링(일반용)","D125","EA",47,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288007","무용접스텐고정식커플링(일반용)","D150","EA",22,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288066","무용접 스텐90엘보(일반용)","D65","EA",9,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288067","무용접 스텐90엘보(일반용)","D80","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288068","무용접 스텐90엘보(일반용)","D100","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288069","무용접 스텐90엘보(일반용)","D125","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288070","무용접 스텐90엘보(일반용)","D150","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288147","무용접 스텐티이(일반용)","D80","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288148","무용접 스텐티이(일반용)","D100","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288149","무용접 스텐티이(일반용)","D125","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288150","무용접 스텐티이(일반용)","D150","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288222","무용접 스텐레듀셔(일반용)","D80","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288224","무용접 스텐레듀셔(일반용)","D125","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288225","무용접 스텐레듀셔(일반용)","D150","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288262","무용접 스텐캡","D80","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288264","무용접 스텐캡","D125","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288280","무용접스텐후렌지아답타(일반)","D50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288282","무용접스텐후렌지아답타(일반)","D80","EA",17,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288283","무용접스텐후렌지아답타(일반)","D100","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288284","무용접스텐후렌지아답타(일반)","D125","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305288285","무용접스텐후렌지아답타(일반)","D150","EA",13,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47301149421","INNO AS 파이프이음관","45곡관, D150","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940120070","강관용접","D65","개소",41,{"$nulls":8},"56940120070",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940120080","강관용접","D80","개소",32,{"$nulls":8},"56940120080",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940120090","강관용접","D100","개소",41,{"$nulls":8},"56940120090",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940120110","강관용접","D150","개소",26,{"$nulls":8},"56940120110",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940120120","강관용접","D200","개소",6,{"$nulls":8},"56940120120",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940120130","강관용접","D250","개소",134,{"$nulls":8},"56940120130",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940130010","강관용접 (S#40)","D15","개소",12,{"$nulls":8},"56940130010",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940130020","강관용접 (S#40)","D20","개소",56,{"$nulls":8},"56940130020",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940130050","강관용접 (S#40)","D40","개소",8,{"$nulls":8},"56940130050",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940130080","강관용접 (S#40)","D80","개소",39,{"$nulls":8},"56940130080",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940130100","강관용접 (S#40)","D125","개소",44,{"$nulls":8},"56940130100",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940130110","강관용접 (S#40)","D150","개소",32,{"$nulls":8},"56940130110",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940140020","동관용접","D20","개소",78,{"$nulls":8},"56940140020",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940140030","동관용접","D25","개소",82,{"$nulls":8},"56940140030",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940140060","동관용접","D50","개소",60,{"$nulls":8},"56940140060",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940150020","스텐관용접","D20","개소",2,{"$nulls":8},"56940150020",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940150070","스텐관용접","D65","개소",29,{"$nulls":8},"56940150070",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940150080","스텐관용접","D80","개소",8,{"$nulls":8},"56940150080",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940150090","스텐관용접","D100","개소",190,{"$nulls":8},"56940150090",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940150100","스텐관용접","D125","개소",214,{"$nulls":8},"56940150100",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940150110","스텐관용접","D150","개소",67,{"$nulls":8},"56940150110",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940150120","스텐관용접","D200","개소",234,{"$nulls":8},"56940150120",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940330060","용접합후렌지","D50","개소",4,{"$nulls":8},"56940330060",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940330070","용접합후렌지","D65","개소",8,{"$nulls":8},"56940330070",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940330080","용접합후렌지","D80","개소",12,{"$nulls":8},"56940330080",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940330090","용접합후렌지","D100","개소",41,{"$nulls":8},"56940330090",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940330110","용접합후렌지","D150","개소",3,{"$nulls":8},"56940330110",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940330120","용접합후렌지","D200","개소",10,{"$nulls":8},"56940330120",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940330130","용접합후렌지","D250","개소",64,{"$nulls":8},"56940330130",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940330220","용접합후렌지","D20  (20KG/CM2)","개소",12,{"$nulls":8},"56940330220",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940330250","용접합후렌지","D40  (20KG/CM2)","개소",1,{"$nulls":8},"56940330250",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940330280","용접합후렌지","D80  (20KG/CM2)","개소",16,{"$nulls":8},"56940330280",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940330300","용접합후렌지","D125 (20KG/CM2)","개소",24,{"$nulls":8},"56940330300",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940330310","용접합후렌지","D150 (20KG/CM2)","개소",8,{"$nulls":8},"56940330310",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940370070","스텐용접합후렌지","D65","개소",6,{"$nulls":8},"56940370070",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940370080","스텐용접합후렌지","D80","개소",12,{"$nulls":8},"56940370080",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940370090","스텐용접합후렌지","D100","개소",76,{"$nulls":8},"56940370090",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940370100","스텐용접합후렌지","D125","개소",24,{"$nulls":8},"56940370100",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940370110","스텐용접합후렌지","D150","개소",62,{"$nulls":8},"56940370110",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940370120","스텐용접합후렌지","D200","개소",66,{"$nulls":8},"56940370120",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305257199","플랜지(FLANGE)","맹플랜지 (10KG) D100","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305257201","플랜지(FLANGE)","맹플랜지 (10KG) D150","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47305257442","플랜지(FLANGE)","STS맹플랜지(10KG) D200","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","80000011191","황동볼밸브 (10KG)","D20","EA",4,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0103","80000011195","황동볼밸브 (10KG)","D50","EA",1,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0103","80000011179","청동게이트밸브 (10KG)","D20","EA",38,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0103","80000011180","청동게이트밸브 (10KG)","D25","EA",16,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0103","80000011182","청동게이트밸브 (10KG)","D40","EA",2,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0103","80000011183","청동게이트밸브 (10KG)","D50","EA",7,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0103","80000011186","주철게이트밸브 (10KG)","D100","EA",8,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200167502","게이트 밸브(단조,플랜지)","20kg,D20","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200167508","게이트 밸브","주강,20kg,D80","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200167510","게이트 밸브","주강,20kg,D125","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200167511","게이트 밸브","주강,20kg,D150","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200037417","글로브 밸브(단조,플랜지)","단조,20kg,D20","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200137052","버터플라이 밸브","LEVER,10K*D65","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","80000011208","주철버터플라이밸브(Lever)","D80","EA",10,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200137152","버터플라이 밸브","GEAR,10K*D65","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200137153","버터플라이 밸브","GEAR,10K*D80","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200137154","버터플라이 밸브","GEAR,10K*D100","EA",21,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200137155","버터플라이 밸브","GEAR,10K*D125","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200137156","버터플라이 밸브","GEAR,10K*D150","EA",15,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200137157","버터플라이 밸브","GEAR,10K*D200","EA",28,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200137158","버터플라이 밸브","GEAR,10K*D250","EA",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200427201","체크 밸브","주철,10kg,D50","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","80000011203","주철체크밸브(충격완화용,10KG)","D100","EA",11,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200428310","체크 밸브","스모렌스키,D125","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200428312","체크 밸브","스모렌스키,D200","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200428313","체크 밸브","스모렌스키,D250","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300627023","스트레이너","후랜지, 10kg, D100","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300627025","스트레이너","후랜지, 10kg, D150","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300627026","스트레이너","후랜지, 10kg, D200","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300627027","스트레이너","후랜지, 10kg, D250","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300627108","스트레이너","주강, 20kg, D80","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300627111","스트레이너","주강, 20kg, D150","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300627611","스트레이너","여과망, D150","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","80000011246","벨로즈형후렉시블죠인트 (10KG)","D100","EA",6,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0103","80000011247","벨로즈형후렉시블죠인트 (10KG)","D125","EA",1,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0103","80000011248","벨로즈형후렉시블죠인트 (10KG)","D150","EA",1,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0103","80000011249","벨로즈형후렉시블죠인트 (10KG)","D200","EA",10,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300357013","플랙시블 조인트","벨로즈형, D250*10k","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300357040","플랙시블 조인트","벨로즈형, D125*20k","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300857010","수격방지기","W.H.C D125","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941113025","전자변장치 (STS)","D20x20x20","개소",2,{"$nulls":8},"56941113025",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941125090","이방변장치 (흑)20KG","D100x80x100","개소",2,{"$nulls":8},"56941125090",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941162080","차압변장치(STS)","D100x80x100","개소",1,{"$nulls":8},"56941162080",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941162110","차압변장치(STS)","D200x150x200","개소",1,{"$nulls":8},"56941162110",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941128022","차압독립바란싱&유량조절밸브(동","D25x25x25","개소",1,{"$nulls":8},"56941128022",null,null,0,0,0,{"$nulls":8},1]
["0103","56941129084","차압독립바란싱&유량조절밸브(ST","D65x65x65","개소",1,{"$nulls":8},"56941129084",null,null,0,0,0,{"$nulls":8},1]
["0103","56941129090","차압독립바란싱&유량조절밸브(ST","D80x80x80","개소",2,{"$nulls":8},"56941129090",null,null,0,0,0,{"$nulls":8},1]
["0103","56941129100","차압독립바란싱&유량조절밸브(ST","D100x100x100","개소",1,{"$nulls":8},"56941129100",null,null,0,0,0,{"$nulls":8},1]
["0103","56941161895","차압유량조절변장치 (흑)20KG","D100x100x100","개소",1,{"$nulls":8},"56941161895",null,null,0,0,0,{"$nulls":8},1]
["0103","56941161915","차압유량조절변장치 (흑)20KG","D150x150x150","개소",1,{"$nulls":8},"56941161915",null,null,0,0,0,{"$nulls":8},1]
["0103","56941183090","정수위조절밸브(STS)","D80x80x80","개소",1,{"$nulls":8},"56941183090",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200127021","플로우트 밸브","볼탭 (STS) D15","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","48200857256","피스텍밸브","D80","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940660030","신축접수 (동관복식)","D25","개소",2,{"$nulls":8},"56940660030",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940660060","신축접수 (동관복식)","D50","개소",2,{"$nulls":8},"56940660060",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941700200","신축접수고정앙카가대","","개소",4,{"$nulls":8},"56941700200",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940740430","밸브보온 (함석마감)","50TxD80","개소",5,{"$nulls":8},"56940740430",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940740450","밸브보온 (함석마감)","50TxD125","개소",4,{"$nulls":8},"56940740450",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940740460","밸브보온 (함석마감)","50TxD150","개소",3,{"$nulls":8},"56940740460",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940740831","밸브보온 (고무발포)","25TxD65","개소",3,{"$nulls":8},"56940740831",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940740832","밸브보온 (고무발포)","25TxD80","개소",10,{"$nulls":8},"56940740832",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940740833","밸브보온 (고무발포)","25TxD100","개소",25,{"$nulls":8},"56940740833",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940740834","밸브보온 (고무발포)","25TxD125","개소",13,{"$nulls":8},"56940740834",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940740835","밸브보온 (고무발포)","25TxD150","개소",16,{"$nulls":8},"56940740835",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940740836","밸브보온 (고무발포)","25TxD200","개소",44,{"$nulls":8},"56940740836",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941320010","압력계설치(백관)","0-35KG/CM2","조",20,{"$nulls":8},"56941320010",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941320020","압력계설치(흑관)","0-35KG/CM2","조",6,{"$nulls":8},"56941320020",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941320030","압력계설치(동관)","0-35KG/CM2","조",9,{"$nulls":8},"56941320030",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941320040","압력계설치(STS)","0-35KG/CM2","조",74,{"$nulls":8},"56941320040",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941320050","온도계설치(동관)","L형","조",9,{"$nulls":8},"56941320050",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941320060","온도계설치(백관)","L형","조",10,{"$nulls":8},"56941320060",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941320070","온도계설치(흑관)","L형","조",6,{"$nulls":8},"56941320070",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941320080","온도계설치(STS)","L형","조",71,{"$nulls":8},"56941320080",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941220010","자동공기변설치(물용)백","D15","개소",4,{"$nulls":8},"56941220010",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941220060","자동공기변설치(물용)흑","D15","개소",6,{"$nulls":8},"56941220060",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941220080","자동공기변설치(물용)STS","D15","개소",77,{"$nulls":8},"56941220080",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941530080","X - RAY TEST","","매당",18,{"$nulls":8},"56941530080",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940510060","일반행거(달대볼트)","D50","개소",30,{"$nulls":8},"56940510060",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940510070","일반행거(달대볼트)","D65","개소",8,{"$nulls":8},"56940510070",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940510080","일반행거(달대볼트)","D80","개소",2,{"$nulls":8},"56940510080",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940510090","일반행거(달대볼트)","D100","개소",37,{"$nulls":8},"56940510090",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940510110","일반행거(달대볼트)","D150","개소",7,{"$nulls":8},"56940510110",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940510120","일반행거(달대볼트)","D200","개소",6,{"$nulls":8},"56940510120",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940520020","절연행가(달대볼트)","D20","개소",13,{"$nulls":8},"56940520020",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940520030","절연행가(달대볼트)","D25","개소",133,{"$nulls":8},"56940520030",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940520050","절연행가(달대볼트)","D40","개소",8,{"$nulls":8},"56940520050",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940520060","절연행가(달대볼트)","D50","개소",18,{"$nulls":8},"56940520060",{"$nulls":4},0,{"$nulls":8},1]
["0103","53060228340","U자형볼트/너트","비절연, D80","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","53060228343","U자형볼트/너트","비절연, D150","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","53060228345","U자형볼트/너트","비절연, D250","EA",55,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787033","파이프슈","슈(SHOE),절연앙카 D25","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787034","파이프슈","슈(SHOE),절연앙카 D32","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787035","파이프슈","슈(SHOE),절연앙카 D40","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787036","파이프슈","슈(SHOE),절연앙카 D50","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787037","파이프슈","슈(SHOE),절연앙카 D65","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787039","파이프슈","슈(SHOE),절연앙카 D100","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787040","파이프슈","슈(SHOE),절연앙카 D125","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787103","파이프슈","슈(SHOE),절연가이드 D25","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787106","파이프슈","슈(SHOE),절연가이드 D50","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787135","파이프슈","슈(SHOE),레스팅 D40","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787138","파이프슈","슈(SHOE),레스팅 D80","EA",17,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787140","파이프슈","슈(SHOE),레스팅 D125","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787141","파이프슈","슈(SHOE),레스팅 D150","EA",21,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787164","파이프슈","슈(SHOE),절연레스팅 D32","EA",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787165","파이프슈","슈(SHOE),절연레스팅 D40","EA",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787166","파이프슈","슈(SHOE),절연레스팅 D50","EA",56,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787167","파이프슈","슈(SHOE),절연레스팅 D65","EA",40,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787168","파이프슈","슈(SHOE),절연레스팅 D80","EA",28,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787169","파이프슈","슈(SHOE),절연레스팅 D100","EA",46,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787170","파이프슈","슈(SHOE),절연레스팅 D125","EA",93,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787171","파이프슈","슈(SHOE),절연레스팅 D150","EA",49,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","47300787172","파이프슈","슈(SHOE),절연레스팅 D200","EA",66,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940610030","강관스리브(지수판제외,벽체)","D25","개소",2,{"$nulls":8},"56940610030",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940610100","강관스리브(지수판제외,벽체)","D125","개소",4,{"$nulls":8},"56940610100",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940610110","강관스리브(지수판제외,벽체)","D150","개소",2,{"$nulls":8},"56940610110",{"$nulls":4},0,{"$nulls":8},1]
["0103","56940610130","강관스리브(지수판제외,벽체)","D250","개소",4,{"$nulls":8},"56940610130",{"$nulls":4},0,{"$nulls":8},1]
["0103","95200017301","ㄷ형강","100×50×5×7.5mm","KG",2358,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941340020","인서트플레이트","200x200x9T","개소",60,{"$nulls":8},"56941340020",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941491011","펌프가대설치(배수펌프)","펌프2대설치기준","개소",5,{"$nulls":8},"56941491011",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941422020","녹막이페인트칠","2회","M2",1,{"$nulls":8},"56941422020",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941420040","유성페인트칠","철재면2회 (노무비제외)","M2",358,{"$nulls":8},"56941420040",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941422040","녹막이페인트칠","2회 (노무비제외)","M2",214,{"$nulls":8},"56941422040",{"$nulls":4},0,{"$nulls":8},1]
["0103","56941410010","잡철물제작설치","간단","TON",2.246,{"$nulls":8},"56941410010",{"$nulls":4},0,{"$nulls":8},1]
["0103","MM713398666","열량계(열공급자분)","D80","EA",1,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["0103","MM713398667","열량계(열공급자분)","D150","EA",1,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["0103","56900017041","노무비","보통인부","인",318,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0103","56900017118","노무비","특별인부","인",44,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0103","56900017030","노무비","배관공","인",953,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0103","56900017021","노무비","도장공","인",35,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0103","56900017125","노무비","플랜트배관공","인",44,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0103","56900017126","노무비","플랜트용접공","인",88,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0103","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},"",467,null,1,0,0.03,{"$nulls":8},1]
[]
[]
[]
[null,null,"[ 합           계 ]"]
[null,null,"0104  공조배관공사"]
["0104","47100487002","배관용 탄소강관","백관 (SPP), D20, 반제품","M",1271,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100487003","배관용 탄소강관","백관 (SPP), D25, 반제품","M",767,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100487004","배관용 탄소강관","백관 (SPP), D32, 반제품","M",1313,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100487005","배관용 탄소강관","백관 (SPP), D40, 반제품","M",42,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100487006","배관용 탄소강관","백관 (SPP), D50, 반제품","M",64,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100487007","배관용 탄소강관","백관 (SPP), D65, 반제품","M",62,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100487008","배관용 탄소강관","백관 (SPP), D80, 반제품","M",47,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100487009","배관용 탄소강관","백관 (SPP), D100, 반제품","M",136,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100487010","배관용 탄소강관","백관 (SPP), D125, 반제품","M",8,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100487012","배관용 탄소강관","백관 (SPP), D200, 반제품","M",50,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100487013","배관용 탄소강관","백관 (SPP), D250, 반제품","M",328,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100047102","동 및 동합금 관","동관 (L-TYPE), D20","M",2603,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100047103","동 및 동합금 관","동관 (L-TYPE), D25","M",712,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100047104","동 및 동합금 관","동관 (L-TYPE), D32","M",361,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100047105","동 및 동합금 관","동관 (L-TYPE), D40","M",912,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100047106","동 및 동합금 관","동관 (L-TYPE), D50","M",1422,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100417247","배관용 스테인리스 강관","D65x3T","M",1613,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100417248","배관용 스테인리스 강관","D80x3T","M",62,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100417249","배관용 스테인리스 강관","D100x3T","M",53,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100417250","배관용 스테인리스 강관","D125x3T","M",570,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100637001","온돌파이프","XL관(KS), D15","M",613,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","47100607061","이중보온관(단열관)","(SPPS38+HDPE), D150","M",162,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0104","PPS00000001","잡재료비","관의 3%","식",1,{"$nulls":8},"",495,null,0,0,0.03,{"$nulls":8},1]
["0104","47100608101","이중보온관(단열엘보)","(SPPS38+HDPE)D150","EA",24,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47100608820","이중보온관(단열연결재)","(SPPS38+HDPE)D150","개소",44,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940840100","아티론보온(벽체매립)","5TxD15","M",10,{"$nulls":8},"56940840100",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940840102","아티론보온(벽체매립)","5TxD25","M",1,{"$nulls":8},"56940840102",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017002","나사식 강관제 관이음쇠","백엘보 (나사) D20","EA",1323,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017003","나사식 강관제 관이음쇠","백엘보 (나사) D25","EA",93,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017004","나사식 강관제 관이음쇠","백엘보 (나사) D32","EA",109,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017005","나사식 강관제 관이음쇠","백엘보 (나사) D40","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017006","나사식 강관제 관이음쇠","백엘보 (나사) D50","EA",25,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301127002","용접식 관이음쇠","백엘보 (용접) D65","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301127003","용접식 관이음쇠","백엘보 (용접) D80","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301127004","용접식 관이음쇠","백엘보 (용접) D100","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301127005","용접식 관이음쇠","백엘보 (용접) D125","EA",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301127007","용접식 관이음쇠","백엘보 (용접) D200","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301127008","용접식 관이음쇠","백엘보 (용접) D250","EA",41,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017103","나사식 강관제 관이음쇠","백티이 (나사) D25","EA",189,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017104","나사식 강관제 관이음쇠","백티이 (나사) D32","EA",274,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017105","나사식 강관제 관이음쇠","백티이 (나사) D40","EA",29,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017106","나사식 강관제 관이음쇠","백티이 (나사) D50","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301127216","용접식 관이음쇠","백티이 (용접) D65","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301127217","용접식 관이음쇠","백티이 (용접) D80","EA",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301127218","용접식 관이음쇠","백티이 (용접) D100","EA",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301127221","용접식 관이음쇠","백티이 (용접) D200","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301127222","용접식 관이음쇠","백티이 (용접) D250","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017204","나사식 강관제 관이음쇠","백리듀서 (나사) D32","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017206","나사식 강관제 관이음쇠","백리듀서 (나사) D50","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017803","나사식 강관제 관이음쇠","백캡 (나사) D25","EA",41,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017804","나사식 강관제 관이음쇠","백캡 (나사) D32","EA",25,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017805","나사식 강관제 관이음쇠","백캡 (나사) D40","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017806","나사식 강관제 관이음쇠","백캡 (나사) D50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017503","나사식 강관제 관이음쇠","백소켓 (나사) D25","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017504","나사식 강관제 관이음쇠","백소켓 (나사) D32","EA",13,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017506","나사식 강관제 관이음쇠","백소켓 (나사) D50","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017302","나사식 강관제 관이음쇠","백니플 (나사) D20","EA",441,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47304017306","나사식 강관제 관이음쇠","백니플 (나사) D50","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301127706","용접식 관이음쇠","U_TRAP D50","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018302","동관이음쇠","동엘보 D20","EA",2802,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018303","동관이음쇠","동엘보 D25","EA",116,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018304","동관이음쇠","동엘보 D32","EA",59,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018305","동관이음쇠","동엘보 D40","EA",130,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018306","동관이음쇠","동엘보 D50","EA",193,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018307","동관이음쇠","동엘보 D65","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018373","동관이음쇠","동티이 D25","EA",185,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018374","동관이음쇠","동티이 D32","EA",76,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018375","동관이음쇠","동티이 D40","EA",147,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018376","동관이음쇠","동티이 D50","EA",231,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018403","동관이음쇠","동리듀서 D25","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018404","동관이음쇠","동리듀서 D32","EA",57,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018405","동관이음쇠","동리듀서 D40","EA",50,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018406","동관이음쇠","동리듀서 D50","EA",55,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018422","동관이음쇠","동소켓 D25","EA",13,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018423","동관이음쇠","동소켓 D32","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018424","동관이음쇠","동소켓 D40","EA",28,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018425","동관이음쇠","동소켓 D50","EA",31,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018453","동관이음쇠","동캡 D25","EA",88,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018455","동관이음쇠","동캡 D40","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018456","동관이음쇠","동캡 D50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018489","동관이음쇠","동유니온 (C*M) D25","EA",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018490","동관이음쇠","동유니온 (C*M) D32","EA",9,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018491","동관이음쇠","동유니온 (C*M) D40","EA",9,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301018492","동관이음쇠","동유니온 (C*M) D50","EA",24,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301017322","동관이음쇠","황동아답타 (C*M) D20","EA",1042,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301017323","동관이음쇠","황동아답타 (C*M) D25","EA",26,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301017324","동관이음쇠","황동아답타 (C*M) D32","EA",9,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301017325","동관이음쇠","황동아답타 (C*M) D40","EA",9,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301017326","동관이음쇠","황동아답타 (C*M) D50","EA",24,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301108029","일반배관용 STS강관 이음쇠","엘보(STS 용접#10) D65","EA",263,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301108030","일반배관용 STS강관 이음쇠","엘보(STS 용접#10) D80","EA",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301108031","일반배관용 STS강관 이음쇠","엘보(STS 용접#10) D100","EA",17,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301108032","일반배관용 STS강관 이음쇠","엘보(STS 용접#10) D125","EA",78,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301108213","일반배관용 STS강관 이음쇠","티이(STS 용접 S#10) D65","EA",356,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301108214","일반배관용 STS강관 이음쇠","티이(STS 용접 S#10) D80","EA",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301108215","일반배관용 STS강관 이음쇠","티이(STS 용접 S#10) D100","EA",14,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301108216","일반배관용 STS강관 이음쇠","티이(STS 용접 S#10) D125","EA",43,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301108457","일반배관용 STS강관 이음쇠","리듀서(STS용접S#10) D65","EA",34,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301108458","일반배관용 STS강관 이음쇠","리듀서(STS용접S#10) D80","EA",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301108459","일반배관용 STS강관 이음쇠","리듀서(STS용접S#10) D100","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47301108460","일반배관용 STS강관 이음쇠","리듀서(STS용접S#10) D125","EA",37,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47103127458","크립바","","M",136,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47103127459","코일고정U핀","","EA",1428,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300248201","바닥배수구(F.D)","D50","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940120070","강관용접","D65","개소",51,{"$nulls":8},"56940120070",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940120080","강관용접","D80","개소",37,{"$nulls":8},"56940120080",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940120090","강관용접","D100","개소",65,{"$nulls":8},"56940120090",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940120100","강관용접","D125","개소",32,{"$nulls":8},"56940120100",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940120120","강관용접","D200","개소",48,{"$nulls":8},"56940120120",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940120130","강관용접","D250","개소",136,{"$nulls":8},"56940120130",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940130110","강관용접 (S#40)","D150","개소",68,{"$nulls":8},"56940130110",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940140020","동관용접","D20","개소",6646,{"$nulls":8},"56940140020",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940140030","동관용접","D25","개소",955,{"$nulls":8},"56940140030",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940140040","동관용접","D32","개소",484,{"$nulls":8},"56940140040",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940140050","동관용접","D40","개소",876,{"$nulls":8},"56940140050",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940140060","동관용접","D50","개소",1300,{"$nulls":8},"56940140060",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940140070","동관용접","D65","개소",24,{"$nulls":8},"56940140070",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940150070","스텐관용접","D65","개소",1679,{"$nulls":8},"56940150070",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940150080","스텐관용접","D80","개소",120,{"$nulls":8},"56940150080",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940150090","스텐관용접","D100","개소",100,{"$nulls":8},"56940150090",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940150100","스텐관용접","D125","개소",415,{"$nulls":8},"56940150100",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940330070","용접합후렌지","D65","개소",4,{"$nulls":8},"56940330070",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940330080","용접합후렌지","D80","개소",2,{"$nulls":8},"56940330080",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940330090","용접합후렌지","D100","개소",2,{"$nulls":8},"56940330090",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940330100","용접합후렌지","D125","개소",24,{"$nulls":8},"56940330100",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940330120","용접합후렌지","D200","개소",32,{"$nulls":8},"56940330120",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940330130","용접합후렌지","D250","개소",4,{"$nulls":8},"56940330130",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940370070","스텐용접합후렌지","D65","개소",48,{"$nulls":8},"56940370070",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940370080","스텐용접합후렌지","D80","개소",16,{"$nulls":8},"56940370080",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940370090","스텐용접합후렌지","D100","개소",12,{"$nulls":8},"56940370090",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940370100","스텐용접합후렌지","D125","개소",40,{"$nulls":8},"56940370100",{"$nulls":4},0,{"$nulls":8},1]
["0104","47305257197","플랜지(FLANGE)","맹플랜지 (10KG) D65","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47305257198","플랜지(FLANGE)","맹플랜지 (10KG) D80","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47305257199","플랜지(FLANGE)","맹플랜지 (10KG) D100","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47305257202","플랜지(FLANGE)","맹플랜지 (10KG) D200","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47305257203","플랜지(FLANGE)","맹플랜지 (10KG) D250","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","80000011191","황동볼밸브 (10KG)","D20","EA",934,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0104","80000011192","황동볼밸브 (10KG)","D25","EA",2,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0104","80000011179","청동게이트밸브 (10KG)","D20","EA",34,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0104","80000011180","청동게이트밸브 (10KG)","D25","EA",20,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0104","80000011181","청동게이트밸브 (10KG)","D32","EA",9,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0104","80000011182","청동게이트밸브 (10KG)","D40","EA",9,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0104","80000011183","청동게이트밸브 (10KG)","D50","EA",24,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0104","48200137052","버터플라이 밸브","LEVER,10K*D65","EA",24,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","80000011208","주철버터플라이밸브(Lever)","D80","EA",6,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0104","48200137054","버터플라이 밸브","LEVER,10K*D100","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","48200137155","버터플라이 밸브","GEAR,10K*D125","EA",18,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","48200137157","버터플라이 밸브","GEAR,10K*D200","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300627026","스트레이너","후랜지, 10kg, D200","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","80000011247","벨로즈형후렉시블죠인트 (10KG)","D125","EA",8,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0104","80000011249","벨로즈형후렉시블죠인트 (10KG)","D200","EA",4,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128000","차압독립바란싱&유량조절밸브(동","D20x20x20","개소",1,{"$nulls":8},"56941128000",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128021","차압독립바란싱&유량조절밸브(동","D25x15x25","개소",16,{"$nulls":8},"56941128021",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128020","차압독립바란싱&유량조절밸브(동","D25x20x25","개소",7,{"$nulls":8},"56941128020",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128022","차압독립바란싱&유량조절밸브(동","D25x25x25","개소",1,{"$nulls":8},"56941128022",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128032","차압독립바란싱&유량조절밸브(동","D32x20x32","개소",3,{"$nulls":8},"56941128032",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128033","차압독립바란싱&유량조절밸브(동","D32x32x32","개소",3,{"$nulls":8},"56941128033",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128041","차압독립바란싱&유량조절밸브(동","D40x20x40","개소",1,{"$nulls":8},"56941128041",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128042","차압독립바란싱&유량조절밸브(동","D40x25x40","개소",5,{"$nulls":8},"56941128042",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128040","차압독립바란싱&유량조절밸브(동","D40x32x40","개소",4,{"$nulls":8},"56941128040",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128043","차압독립바란싱&유량조절밸브(동","D40x40x40","개소",2,{"$nulls":8},"56941128043",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128056","차압독립바란싱&유량조절밸브(동","D50x20x50","개소",2,{"$nulls":8},"56941128056",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128055","차압독립바란싱&유량조절밸브(동","D50x25x50","개소",9,{"$nulls":8},"56941128055",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128050","차압독립바란싱&유량조절밸브(동","D50x40x50","개소",8,{"$nulls":8},"56941128050",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128051","차압독립바란싱&유량조절밸브(동","D50x50x50","개소",3,{"$nulls":8},"56941128051",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128182","차압독립바란싱&유량조절밸브(ST","D65x32x65","개소",7,{"$nulls":8},"56941128182",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128180","차압독립바란싱&유량조절밸브(ST","D65x50x65","개소",7,{"$nulls":8},"56941128180",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128195","차압독립바란싱&유량조절밸브(ST","D80x80x80","개소",3,{"$nulls":8},"56941128195",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128200","차압독립바란싱&유량조절밸브(ST","D100x65x100","개소",2,{"$nulls":8},"56941128200",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128205","차압독립바란싱&유량조절밸브(ST","D100x100x100","개소",2,{"$nulls":8},"56941128205",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941128230","차압독립바란싱&유량조절밸브(ST","D125x125x125","개소",2,{"$nulls":8},"56941128230",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940680070","신축접수 (STS 복식)","D65","개소",2,{"$nulls":8},"56940680070",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940680090","신축접수 (STS 복식)","D100","개소",1,{"$nulls":8},"56940680090",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940680100","신축접수 (STS 복식)","D125","개소",6,{"$nulls":8},"56940680100",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941700200","신축접수고정앙카가대","","개소",9,{"$nulls":8},"56941700200",{"$nulls":4},0,{"$nulls":8},1]
["0104","45200067205","실별온도유량조절시스템","7 구","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56801977027","전기온돌판넬","2300x850x15T","EA",15,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56801977028","전기온돌판넬","2300x600x15T","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56801977002","전기온돌판넬","2000x850x15T","EA",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56801977011","전기온돌판넬","2000x600x15T","EA",9,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56801977004","전기온돌판넬","1700x850x15T","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56801977024","전기온돌판넬","1500x850x15T","EA",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56801977013","전기온돌판넬","1250x600x15T","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","41400227402","자동온도조절기","전자식중형","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940740831","밸브보온 (고무발포)","25TxD65","개소",24,{"$nulls":8},"56940740831",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940740832","밸브보온 (고무발포)","25TxD80","개소",6,{"$nulls":8},"56940740832",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940740833","밸브보온 (고무발포)","25TxD100","개소",4,{"$nulls":8},"56940740833",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940740834","밸브보온 (고무발포)","25TxD125","개소",18,{"$nulls":8},"56940740834",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941320040","압력계설치(STS)","0-35KG/CM2","조",12,{"$nulls":8},"56941320040",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941320080","온도계설치(STS)","L형","조",12,{"$nulls":8},"56941320080",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941220080","자동공기변설치(물용)STS","D15","개소",37,{"$nulls":8},"56941220080",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941530080","X - RAY TEST","","매당",20,{"$nulls":8},"56941530080",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940510020","일반행거(달대볼트)","D20","개소",441,{"$nulls":8},"56940510020",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940510030","일반행거(달대볼트)","D25","개소",343,{"$nulls":8},"56940510030",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940510040","일반행거(달대볼트)","D32","개소",596,{"$nulls":8},"56940510040",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940510050","일반행거(달대볼트)","D40","개소",18,{"$nulls":8},"56940510050",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940510060","일반행거(달대볼트)","D50","개소",16,{"$nulls":8},"56940510060",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940510070","일반행거(달대볼트)","D65","개소",553,{"$nulls":8},"56940510070",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940510080","일반행거(달대볼트)","D80","개소",4,{"$nulls":8},"56940510080",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940510090","일반행거(달대볼트)","D100","개소",4,{"$nulls":8},"56940510090",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940510100","일반행거(달대볼트)","D125","개소",25,{"$nulls":8},"56940510100",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940510110","일반행거(달대볼트)","D150","개소",32,{"$nulls":8},"56940510110",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940520020","절연행가(달대볼트)","D20","개소",934,{"$nulls":8},"56940520020",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940520030","절연행가(달대볼트)","D25","개소",235,{"$nulls":8},"56940520030",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940520040","절연행가(달대볼트)","D32","개소",127,{"$nulls":8},"56940520040",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940520050","절연행가(달대볼트)","D40","개소",331,{"$nulls":8},"56940520050",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940520060","절연행가(달대볼트)","D50","개소",478,{"$nulls":8},"56940520060",{"$nulls":4},0,{"$nulls":8},1]
["0104","53060228323","U자형볼트/너트","절연, D25","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","53060228324","U자형볼트/너트","절연, D32","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","53060228325","U자형볼트/너트","절연, D40","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","53060228326","U자형볼트/너트","절연, D50","EA",24,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","53060228327","U자형볼트/너트","절연, D65","EA",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","53060228328","U자형볼트/너트","절연, D80","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","53060228329","U자형볼트/너트","절연, D100","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","53060228330","U자형볼트/너트","절연, D125","EA",53,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","53060228339","U자형볼트/너트","비절연, D65","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","53060228340","U자형볼트/너트","비절연, D80","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","53060228341","U자형볼트/너트","비절연, D100","EA",24,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","53060228342","U자형볼트/너트","비절연, D125","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","53060228343","U자형볼트/너트","비절연, D150","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","53060228344","U자형볼트/너트","비절연, D200","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","53060228345","U자형볼트/너트","비절연, D250","EA",84,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787011","파이프슈","슈(SHOE),앙카슈 D150","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787033","파이프슈","슈(SHOE),절연앙카 D25","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787035","파이프슈","슈(SHOE),절연앙카 D40","EA",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787036","파이프슈","슈(SHOE),절연앙카 D50","EA",9,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787037","파이프슈","슈(SHOE),절연앙카 D65","EA",40,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787040","파이프슈","슈(SHOE),절연앙카 D125","EA",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787071","파이프슈","슈(SHOE),가이드 D150","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787103","파이프슈","슈(SHOE),절연가이드 D25","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787105","파이프슈","슈(SHOE),절연가이드 D40","EA",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787106","파이프슈","슈(SHOE),절연가이드 D50","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787107","파이프슈","슈(SHOE),절연가이드 D65","EA",66,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787109","파이프슈","슈(SHOE),절연가이드 D100","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787110","파이프슈","슈(SHOE),절연가이드 D125","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787163","파이프슈","슈(SHOE),절연레스팅 D25","EA",15,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787166","파이프슈","슈(SHOE),절연레스팅 D50","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787167","파이프슈","슈(SHOE),절연레스팅 D65","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787168","파이프슈","슈(SHOE),절연레스팅 D80","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787169","파이프슈","슈(SHOE),절연레스팅 D100","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787170","파이프슈","슈(SHOE),절연레스팅 D125","EA",54,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","47300787171","파이프슈","슈(SHOE),절연레스팅 D150","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610030","강관스리브(지수판제외,벽체)","D25","개소",20,{"$nulls":8},"56940610030",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610040","강관스리브(지수판제외,벽체)","D32","개소",10,{"$nulls":8},"56940610040",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610050","강관스리브(지수판제외,벽체)","D40","개소",16,{"$nulls":8},"56940610050",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610060","강관스리브(지수판제외,벽체)","D50","개소",15,{"$nulls":8},"56940610060",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610070","강관스리브(지수판제외,벽체)","D65","개소",16,{"$nulls":8},"56940610070",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610080","강관스리브(지수판제외,벽체)","D80","개소",6,{"$nulls":8},"56940610080",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610090","강관스리브(지수판제외,벽체)","D100","개소",2,{"$nulls":8},"56940610090",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610100","강관스리브(지수판제외,벽체)","D125","개소",16,{"$nulls":8},"56940610100",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610110","강관스리브(지수판제외,벽체)","D150","개소",4,{"$nulls":8},"56940610110",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610130","강관스리브(지수판제외,벽체)","D250","개소",8,{"$nulls":8},"56940610130",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610320","강관스리브(지수판제외,바닥)","D20","개소",52,{"$nulls":8},"56940610320",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610330","강관스리브(지수판제외,바닥)","D25","개소",7,{"$nulls":8},"56940610330",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610340","강관스리브(지수판제외,바닥)","D32","개소",2,{"$nulls":8},"56940610340",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610350","강관스리브(지수판제외,바닥)","D40","개소",8,{"$nulls":8},"56940610350",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610360","강관스리브(지수판제외,바닥)","D50","개소",24,{"$nulls":8},"56940610360",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610370","강관스리브(지수판제외,바닥)","D65","개소",25,{"$nulls":8},"56940610370",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610380","강관스리브(지수판제외,바닥)","D80","개소",12,{"$nulls":8},"56940610380",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610390","강관스리브(지수판제외,바닥)","D100","개소",22,{"$nulls":8},"56940610390",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610400","강관스리브(지수판제외,바닥)","D125","개소",53,{"$nulls":8},"56940610400",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610410","강관스리브(지수판제외,바닥)","D150","개소",276,{"$nulls":8},"56940610410",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940610430","강관스리브(지수판제외,바닥)","D250","개소",32,{"$nulls":8},"56940610430",{"$nulls":4},0,{"$nulls":8},1]
["0104","56940620110","강관스리브(지수판포함,벽체)","D150","개소",2,{"$nulls":8},"56940620110",{"$nulls":4},0,{"$nulls":8},1]
["0104","56810021002","방화실란트","D20","개소",52,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56810021003","방화실란트","D25","개소",27,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56810021004","방화실란트","D32","개소",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56810021005","방화실란트","D40","개소",24,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56810021006","방화실란트","D50","개소",39,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56810021007","방화실란트","D65","개소",41,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56810021008","방화실란트","D80","개소",18,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56810021009","방화실란트","D100","개소",24,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56810021010","방화실란트","D125","개소",69,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56810021011","방화실란트","D150","개소",280,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56810021013","방화실란트","D250","개소",32,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","95200017301","ㄷ형강","100×50×5×7.5mm","KG",2054,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941340020","인서트플레이트","200x200x9T","개소",74,{"$nulls":8},"56941340020",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941420040","유성페인트칠","철재면2회 (노무비제외)","M2",374,{"$nulls":8},"56941420040",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941422040","녹막이페인트칠","2회 (노무비제외)","M2",129,{"$nulls":8},"56941422040",{"$nulls":4},0,{"$nulls":8},1]
["0104","56941410010","잡철물제작설치","간단","TON",1.954,{"$nulls":8},"56941410010",{"$nulls":4},0,{"$nulls":8},1]
["0104","56900017041","노무비","보통인부","인",492,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0104","56900017118","노무비","특별인부","인",13,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0104","56900017030","노무비","배관공","인",903,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0104","56900017021","노무비","도장공","인",28,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0104","56900017125","노무비","플랜트배관공","인",13,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0104","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},"",758,null,1,0,0.03,{"$nulls":8},1]
{"$rows_empty":24}
[null,null,"[ 합           계 ]"]
[null,null,"0105  공조덕트설치공사"]
["0105","56941310010","각형덕트제작및설치","(0.5T)","M2",2875,{"$nulls":8},"56941310010",{"$nulls":4},0,{"$nulls":8},1]
["0105","56941310020","각형덕트제작및설치","(0.6T)","M2",1095,{"$nulls":8},"56941310020",{"$nulls":4},0,{"$nulls":8},1]
["0105","56941310030","각형덕트제작및설치","(0.8T)","M2",887,{"$nulls":8},"56941310030",{"$nulls":4},0,{"$nulls":8},1]
["0105","56941310040","각형덕트제작및설치","(1.0T)","M2",51,{"$nulls":8},"56941310040",{"$nulls":4},0,{"$nulls":8},1]
["0105","56941310050","각형덕트제작및설치","(1.2T)","M2",68,{"$nulls":8},"56941310050",{"$nulls":4},0,{"$nulls":8},1]
["0105","56941310070","STS덕트제작및설치","(0.5T)","M2",21,{"$nulls":8},"56941310070",{"$nulls":4},0,{"$nulls":8},1]
["0105","56941310080","STS덕트제작및설치","(0.6T)","M2",301,{"$nulls":8},"56941310080",{"$nulls":4},0,{"$nulls":8},1]
["0105","56941310090","STS덕트제작및설치","(0.8T)","M2",5,{"$nulls":8},"56941310090",{"$nulls":4},0,{"$nulls":8},1]
["0105","56941311540","알루미늄복합판넬덕트","(20T)","M2",5575,{"$nulls":8},"56941311540",{"$nulls":4},0,{"$nulls":8},1]
["0105","56941314010","캔버스제작설치","1.2T","M2",86,{"$nulls":8},"56941314010",{"$nulls":4},0,{"$nulls":8},1]
["0105","41400227651","공조덕트(스파이럴)","D100×0.5t, 공조용","M",26,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41400228502","공조 덕트","SPIRAL ELBOW, D100","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41400228812","공조 덕트","SPIRAL HANGER, D100","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41300247422","디퓨져","사각PAN, D150, AL","EA",399,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41300247423","디퓨져","사각PAN, D200, AL","EA",341,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41300247221","디퓨져","원형PAN, D125, AL","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41300247222","디퓨져","원형PAN, D150, AL","EA",117,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41300247223","디퓨져","원형PAN, D200, AL","EA",194,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41300247224","디퓨져","원형PAN, D250, AL","EA",118,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41300247905","B.L.D (1S)","1,200L","EA",230,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41300248002","디퓨저","1 Slot line, 54×1200, 아연도S","EA",30,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41300247827","디퓨저","노즐, D250, AL","EA",39,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41400227418","공조덕트(플렉시블)","(AL비보온), D100","M",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41400227419","공조덕트(플렉시블)","(AL비보온), D125","M",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41400227420","공조덕트(플렉시블)","(AL비보온), D150","M",492,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41400227422","공조덕트(플렉시블)","(AL비보온), D200","M",393,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41400227424","공조덕트(플렉시블)","(AL비보온), D250","M",85,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41400227470","공조덕트(플렉시블)","(AL보온), D150","M",381,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41400227471","공조덕트(플렉시블)","(AL보온), D175","M",126,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41400227472","공조덕트(플렉시블)","(AL보온), D200","M",523,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41400227474","공조덕트(플렉시블)","(AL보온), D250","M",58,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","41400227476","공조덕트(플렉시블)","(AL보온), D300","M",45,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","36940227016","담파모타","","EA",14,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","36940227001","점검구","200x200","EA",133,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","36940227004","점검구","300x200","EA",31,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","36940227010","핸들","F.V.D","EA",55,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","36940227015","FD/FVD 휴즈","","EA",164,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300527212","스텐밴드","D100","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300527213","스텐밴드","D125","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300527214","스텐밴드","D150","EA",1164,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300527215","스텐밴드","D175","EA",168,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300527216","스텐밴드","D200","EA",1222,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300527218","스텐밴드","D250","EA",192,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300527219","스텐밴드","D300","EA",60,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300527234","동망","#24","M2",75,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53350177161","스테인리스 망","STS 304, 24 메쉬×D0.23×1m","M2",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300527321","후드캡","D100","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300527311","원형환기캡","D100","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","56940620130","강관스리브(지수판포함,벽체)","D250","개소",8,{"$nulls":8},"56940620130",{"$nulls":4},0,{"$nulls":8},1]
["0105","56941420020","유성페인트칠","철재면2회","M2",1141,{"$nulls":8},"56941420020",{"$nulls":4},0,{"$nulls":8},1]
["0105","56941422020","녹막이페인트칠","2회","M2",1141,{"$nulls":8},"56941422020",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940309","AIR CHAMBER","1000 x 450*400","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940310","AIR CHAMBER","1100 x 600*400","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940311","AIR CHAMBER","400 x 1300*500","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940312","AIR CHAMBER","600 x 2200*2500","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940313","AIR CHAMBER","600 x 2300*2500","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940314","AIR CHAMBER","700 x 3500*3800","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940315","AIR CHAMBER","800 x 1000*500","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940316","AIR CHAMBER","800 x 4400*3800","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940317","AIR CHAMBER","800 x 600*400","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940318","AIR CHAMBER","800 x 6000*3800","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940319","AIR CHAMBER","900 x 450*400","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940320","B.D.D (STL)","1000 x 1500","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940321","B.D.D (STL)","1000 x 1600","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940322","B.D.D (STL)","1000 x 2700","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940323","B.D.D (STL)","1100 x 2000","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940324","B.D.D (STL)","1150 x 900","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940325","B.D.D (STL)","1250 x 1200","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940326","B.D.D (STL)","1300 x 550","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940327","B.D.D (STL)","1300 x 900","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940328","B.D.D (STL)","250 x 200","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940329","B.D.D (STL)","300 x 150","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940330","B.D.D (STL)","300 x 200","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940331","B.D.D (STL)","350 x 600","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940332","B.D.D (STL)","400 x 500","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940333","B.D.D (STL)","500 x 1200","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940334","B.D.D (STL)","500 x 350","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940335","B.D.D (STL)","500 x 400","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940336","B.D.D (STL)","500 x 600","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940337","B.D.D (STL)","700 x 2000","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940338","B.D.D (STL)","700 x 500","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940339","B.D.D (STL)","700 x 600","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940340","B.D.D (STL)","750 x 450","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940341","B.D.D (STL)","900 x 350","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940342","B.D.D (STL)","900 x 500","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940343","F.D (STL)","1000 x 1500","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940344","F.D (STL)","1000 x 1600","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940346","F.D (STL)","1000 x 2700","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940347","F.D (STL)","1000 x 300","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940348","F.D (STL)","1000 x 600","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940349","F.D (STL)","1000 x 700","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940350","F.D (STL)","1050 x 300","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836188","F.D (STL)","1050 x 600","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940352","F.D (STL)","1050 x 800","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940353","F.D (STL)","1100 x 2000","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940354","F.D (STL)","1100 x 300","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940355","F.D (STL)","1200 x 1000","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836193","F.D (STL)","1200 x 500","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940357","F.D (STL)","1250 x 1200","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940358","F.D (STL)","1250 x 500","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940359","F.D (STL)","1300 x 900","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940360","F.D (STL)","1450 x 500","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940361","F.D (STL)","1550 x 700","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940362","F.D (STL)","1600 x 400","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940363","F.D (STL)","1650 x 400","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940364","F.D (STL)","500 x 1200","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940365","F.D (STL)","700 x 2000","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836196","F.D (STL)","250 x 150","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940367","F.D (STL)","300 x 150","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM632524045","F.D (STL)","300 x 200","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836199","F.D (STL)","350 x 250","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836200","F.D (STL)","350 x 300","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940371","F.D (STL)","350 x 600","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836202","F.D (STL)","400 x 250","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836203","F.D (STL)","400 x 300","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940374","F.D (STL)","400 x 500","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836205","F.D (STL)","450 x 300","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940376","F.D (STL)","500 x 300","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940377","F.D (STL)","500 x 400","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940378","F.D (STL)","500 x 600","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940379","F.D (STL)","550 x 400","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836211","F.D (STL)","650 x 300","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836213","F.D (STL)","650 x 400","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836214","F.D (STL)","650 x 600","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940383","F.D (STL)","700 x 400","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM632524068","F.D (STL)","700 x 500","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940385","F.D (STL)","700 x 600","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940386","F.D (STL)","750 x 450","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940387","F.D (STL)","750 x 550","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836220","F.D (STL)","800 x 300","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940389","F.D (STL)","800 x 400","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836221","F.D (STL)","800 x 500","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940391","F.D (STL)","800 x 600","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836224","F.D (STL)","850 x 300","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836225","F.D (STL)","850 x 500","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836226","F.D (STL)","900 x 300","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940395","F.D (STL)","900 x 350","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940396","F.D (STL)","900 x 750","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940397","F.D (STL)","950 x 750","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940398","F.D (STS)","1100 x 500","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836231","F.D (STS)","900 x 600","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940400","F.V.D (STL)","150 x 150","EA",30,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940402","F.V.D (STL)","250 x 150","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940401","F.V.D (STL)","250 x 200","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940406","F.V.D (STL)","300 x 150","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940405","F.V.D (STL)","300 x 200","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM710358444","F.V.D (STL)","600 x 300","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM710358445","F.V.D (STL)","700 x 400","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM710358446","F.V.D (STL)","900 x 500","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM710358447","F.V.D (STS)","1300 x 700","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM710358449","F.V.D (STS)","800 x 400","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM710358448","F.V.D (STS)","800 x 700","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940415","GRILLE (STL)","100 x 100","EA",30,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940416","GRILLE (STL)","150 x 150","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836239","GRILLE (STL)","200 x 150","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836241","GRILLE (STL)","300 x 200","EA",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM710358454","GRILLE (STL)","300 x 250","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940422","GRILLE (STL)","350 x 250","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836243","GRILLE (STL)","400 x 250","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940425","GRILLE (STL)","650 x 300","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940428","LOUVER (STL)","900 x 350","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836249","M.V.D (STL)","1700 x 400","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940430","M.V.D (STL)","1900 x 400","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940431","M.V.D (STL)","2500 x 600","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940432","M.V.D (STL)","2500 x 700","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940433","M.V.D (STL)","2600 x 700","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940442","T.V (STL)","1300 x 550","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940443","T.V (STL)","1300 x 900","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940444","T.V (STS)","1100 x 500","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940445","T.V (STS)","700 x 650","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836270","V.D (STL)","200 x 150","EA",161,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836271","V.D (STL)","250 x 150","EA",110,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836272","V.D (STL)","250 x 200","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836273","V.D (STL)","300 x 150","EA",36,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836274","V.D (STL)","300 x 200","EA",34,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836275","V.D (STL)","300 x 250","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836277","V.D (STL)","350 x 200","EA",47,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836278","V.D (STL)","350 x 250","EA",15,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836280","V.D (STL)","400 x 250","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836281","V.D (STL)","400 x 300","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836282","V.D (STL)","450 x 250","EA",9,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM631836283","V.D (STL)","450 x 300","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940459","V.D (STL)","500 x 300","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940460","V.D (STL)","700 x 450","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940474","GRILLE (STL)","600 x 400","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940475","GRILLE (STL)","750 x 400","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM707940476","GRILLE (STL)","800 x 250","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300537010","SPIN IN","D125","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300537011","SPIN IN","D150","EA",582,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300537012","SPIN IN","D175","EA",84,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300537013","SPIN IN","D200","EA",611,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300537015","SPIN IN","D250","EA",96,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","53300537017","SPIN IN","D300","EA",30,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","MM708397143","유인휀","","대",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0105","56900017041","노무비","보통인부","인",26,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0105","56900017019","노무비","덕트공","인",1662,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0105","56900017015","노무비","기계설비공","인",41,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0105","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},"",982,null,1,0,0.03,{"$nulls":8},1]
{"$rows_empty":8}
[null,null,"[ 합           계 ]"]
[null,null,"010601  위생기구설치공사"]
["010601","45100077100","양변기(FV,절수형)","VC-1110C","SET",90,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["010601","45100077101","양변기(FV,센서형)","VC-1110C","SET",14,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010601","45100087013","소변기(전자감지식)","VU-312(전기식)","SET",28,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010601","45100017082","원형세면기(S/L,절수형)","VL-1040","SET",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010601","45100017070","원형세면기(S/L,절수형)","VL-1040(센서수전)","SET",14,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010601","45100017076","각형세면기(S/L,절수형)","VL-610","SET",63,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010601","MM708397268","샤워기(입식)","RBT-711A","EA",15,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010601","MM708397269","샤워기(좌식)","RBT-711A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010601","45100237001","청소씽크","VS-210","SET",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010601","45100247048","청소씽크수전","","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010601","45100247029","씽크혼합수전","","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010601","45100247053","조경수전","D25","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010601","45100057001","휴지걸이(STS)","","EA",104,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010601","45100467001","비누대(STS)","","EA",98,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010601","72900477006","핸드드라이어","","EA",46,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010601","56900017041","노무비","보통인부","인",39,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["010601","56900017072","노무비","위생공","인",166,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["010601","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},"",1010,null,1,0,0.03,{"$nulls":8},1]
[]
[]
[]
[]
[]
[]
[null,null,"[ 합           계 ]"]
[null,null,"010602  급수급탕배관공사"]
["010602","47100407021","일반배관용 스테인리스 강관","K-TYPE, D15","M",1169,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010602","47100407022","일반배관용 스테인리스 강관","K-TYPE, D20","M",773,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010602","47100407023","일반배관용 스테인리스 강관","K-TYPE, D25","M",537,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010602","47100407024","일반배관용 스테인리스 강관","K-TYPE, D32","M",402,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010602","47100407025","일반배관용 스테인리스 강관","K-TYPE, D40","M",289,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010602","47100407026","일반배관용 스테인리스 강관","K-TYPE, D50","M",292,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010602","47100417507","배관용스테인리스강관(무용접)","D65x3T","M",95,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010602","47100417508","배관용스테인리스강관(무용접)","D80x3T","M",83,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010602","47100417509","배관용스테인리스강관(무용접)","D100x3T","M",40,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010602","47100417510","배관용스테인리스강관(무용접)","D125x3T","M",21,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010602","PPS00000001","잡재료비","관의 3%","식",1,{"$nulls":8},"",1029,null,0,0,0.03,{"$nulls":8},1]
["010602","56940840100","아티론보온(벽체매립)","5TxD15","M",390,{"$nulls":8},"56940840100",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940840101","아티론보온(벽체매립)","5TxD20","M",9,{"$nulls":8},"56940840101",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940840102","아티론보온(벽체매립)","5TxD25","M",22,{"$nulls":8},"56940840102",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108950","STS강관이음쇠(원터치삽입식)","90'엘보  D13","EA",1056,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108951","STS강관이음쇠(원터치삽입식)","90'엘보  D20","EA",295,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108952","STS강관이음쇠(원터치삽입식)","90'엘보  D25","EA",169,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108955","STS강관이음쇠(원터치삽입식)","90'엘보  D30","EA",117,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108956","STS강관이음쇠(원터치삽입식)","90'엘보  D40","EA",57,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108957","STS강관이음쇠(원터치삽입식)","90'엘보  D50","EA",52,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108976","STS강관이음쇠(원터치삽입식)","수전엘보  D13x15","EA",120,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108978","STS강관이음쇠(원터치삽입식)","수전엘보  D20x20","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108981","STS강관이음쇠(원터치삽입식)","수전엘보  D25x25","EA",23,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108986","STS강관이음쇠(원터치삽입식)","티  D20","EA",184,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108987","STS강관이음쇠(원터치삽입식)","티  D25","EA",101,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108988","STS강관이음쇠(원터치삽입식)","티  D30","EA",129,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108989","STS강관이음쇠(원터치삽입식)","티  D40","EA",83,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108990","STS강관이음쇠(원터치삽입식)","티  D50","EA",60,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109095","STS강관이음쇠(원터치삽입식)","수전티  D13x15","EA",232,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109100","STS강관이음쇠(원터치삽입식)","수전티  D25x25","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108995","STS강관이음쇠(원터치삽입식)","레듀셔  D20x13","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301108997","STS강관이음쇠(원터치삽입식)","레듀셔  D25x20","EA",47,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109000","STS강관이음쇠(원터치삽입식)","레듀셔  D30x25","EA",68,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109004","STS강관이음쇠(원터치삽입식)","레듀셔  D40x30","EA",37,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109009","STS강관이음쇠(원터치삽입식)","레듀셔  D50x40","EA",24,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109041","STS강관이음쇠(원터치삽입식)","소켓  D20","EA",21,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109042","STS강관이음쇠(원터치삽입식)","소켓  D25","EA",22,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109043","STS강관이음쇠(원터치삽입식)","소켓  D30","EA",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109044","STS강관이음쇠(원터치삽입식)","소켓  D40","EA",14,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109045","STS강관이음쇠(원터치삽입식)","소켓  D50","EA",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109052","STS강관이음쇠(원터치삽입식)","밸브소켓  D20x20","EA",164,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109054","STS강관이음쇠(원터치삽입식)","밸브소켓  D25x25","EA",50,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109056","STS강관이음쇠(원터치삽입식)","밸브소켓  D30x32","EA",66,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109058","STS강관이음쇠(원터치삽입식)","밸브소켓  D40x40","EA",42,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109061","STS강관이음쇠(원터치삽입식)","밸브소켓  D50x50","EA",36,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109065","STS강관이음쇠(원터치삽입식)","캡  D13","EA",232,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109066","STS강관이음쇠(원터치삽입식)","캡  D20","EA",55,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109067","STS강관이음쇠(원터치삽입식)","캡  D25","EA",35,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109068","STS강관이음쇠(원터치삽입식)","캡  D30","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109070","STS강관이음쇠(원터치삽입식)","캡  D50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109122","STS강관이음쇠(원터치삽입식)","후렌지  D20","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109123","STS강관이음쇠(원터치삽입식)","후렌지  D25","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109124","STS강관이음쇠(원터치삽입식)","후렌지  D32","EA",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47301109126","STS강관이음쇠(원터치삽입식)","후렌지  D50","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288003","무용접스텐고정식커플링(일반용)","D65","EA",90,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288004","무용접스텐고정식커플링(일반용)","D80","EA",78,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288005","무용접스텐고정식커플링(일반용)","D100","EA",37,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288006","무용접스텐고정식커플링(일반용)","D125","EA",25,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288066","무용접 스텐90엘보(일반용)","D65","EA",18,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288067","무용접 스텐90엘보(일반용)","D80","EA",17,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288068","무용접 스텐90엘보(일반용)","D100","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288069","무용접 스텐90엘보(일반용)","D125","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288146","무용접 스텐티이(일반용)","D65","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288147","무용접 스텐티이(일반용)","D80","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288148","무용접 스텐티이(일반용)","D100","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288149","무용접 스텐티이(일반용)","D125","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288221","무용접 스텐레듀셔(일반용)","D65","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288222","무용접 스텐레듀셔(일반용)","D80","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288223","무용접 스텐레듀셔(일반용)","D100","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288224","무용접 스텐레듀셔(일반용)","D125","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288281","무용접스텐후렌지아답타(일반)","D65","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288282","무용접스텐후렌지아답타(일반)","D80","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288283","무용접스텐후렌지아답타(일반)","D100","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47305288284","무용접스텐후렌지아답타(일반)","D125","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","80000011179","청동게이트밸브 (10KG)","D20","EA",82,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["010602","80000011180","청동게이트밸브 (10KG)","D25","EA",25,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["010602","80000011181","청동게이트밸브 (10KG)","D32","EA",33,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["010602","80000011182","청동게이트밸브 (10KG)","D40","EA",21,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["010602","80000011183","청동게이트밸브 (10KG)","D50","EA",18,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["010602","48200137052","버터플라이 밸브","LEVER,10K*D65","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","80000011208","주철버터플라이밸브(Lever)","D80","EA",4,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["010602","80000011209","주철버터플라이밸브(Lever)","D100","EA",1,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["010602","48200137155","버터플라이 밸브","GEAR,10K*D125","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47300357004","플랙시블 조인트","벨로즈형, D32*10k","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47300857002","수격방지기","W.H.C D20","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","47300857006","수격방지기","W.H.C D50","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","56941113025","전자변장치 (STS)","D20x20x20","개소",6,{"$nulls":8},"56941113025",null,null,0,0,0,{"$nulls":8},1]
["010602","66800287006","수도미터(냉수용)","D50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","66800287085","수도미터(온수용)","D40","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","56941220080","자동공기변설치(물용)STS","D15","개소",2,{"$nulls":8},"56941220080",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940520010","절연행가(달대볼트)","D15","개소",176,{"$nulls":8},"56940520010",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940520020","절연행가(달대볼트)","D20","개소",295,{"$nulls":8},"56940520020",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940520030","절연행가(달대볼트)","D25","개소",201,{"$nulls":8},"56940520030",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940520040","절연행가(달대볼트)","D32","개소",117,{"$nulls":8},"56940520040",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940520050","절연행가(달대볼트)","D40","개소",89,{"$nulls":8},"56940520050",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940520060","절연행가(달대볼트)","D50","개소",58,{"$nulls":8},"56940520060",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940520070","절연행가(달대볼트)","D65","개소",23,{"$nulls":8},"56940520070",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940520080","절연행가(달대볼트)","D80","개소",19,{"$nulls":8},"56940520080",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940520090","절연행가(달대볼트)","D100","개소",4,{"$nulls":8},"56940520090",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940520100","절연행가(달대볼트)","D125","개소",3,{"$nulls":8},"56940520100",{"$nulls":4},0,{"$nulls":8},1]
["010602","53060228322","U자형볼트/너트","절연, D20","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","53060228323","U자형볼트/너트","절연, D25","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","53060228324","U자형볼트/너트","절연, D32","EA",9,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","53060228325","U자형볼트/너트","절연, D40","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","53060228326","U자형볼트/너트","절연, D50","EA",19,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","53060228327","U자형볼트/너트","절연, D65","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","53060228328","U자형볼트/너트","절연, D80","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","53060228329","U자형볼트/너트","절연, D100","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","53060228330","U자형볼트/너트","절연, D125","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610020","강관스리브(지수판제외,벽체)","D20","개소",30,{"$nulls":8},"56940610020",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610030","강관스리브(지수판제외,벽체)","D25","개소",14,{"$nulls":8},"56940610030",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610040","강관스리브(지수판제외,벽체)","D32","개소",18,{"$nulls":8},"56940610040",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610050","강관스리브(지수판제외,벽체)","D40","개소",11,{"$nulls":8},"56940610050",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610060","강관스리브(지수판제외,벽체)","D50","개소",21,{"$nulls":8},"56940610060",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610070","강관스리브(지수판제외,벽체)","D65","개소",5,{"$nulls":8},"56940610070",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610080","강관스리브(지수판제외,벽체)","D80","개소",4,{"$nulls":8},"56940610080",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610090","강관스리브(지수판제외,벽체)","D100","개소",1,{"$nulls":8},"56940610090",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610100","강관스리브(지수판제외,벽체)","D125","개소",1,{"$nulls":8},"56940610100",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610320","강관스리브(지수판제외,바닥)","D20","개소",8,{"$nulls":8},"56940610320",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610330","강관스리브(지수판제외,바닥)","D25","개소",4,{"$nulls":8},"56940610330",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610340","강관스리브(지수판제외,바닥)","D32","개소",7,{"$nulls":8},"56940610340",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610350","강관스리브(지수판제외,바닥)","D40","개소",4,{"$nulls":8},"56940610350",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610360","강관스리브(지수판제외,바닥)","D50","개소",16,{"$nulls":8},"56940610360",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610370","강관스리브(지수판제외,바닥)","D65","개소",2,{"$nulls":8},"56940610370",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610380","강관스리브(지수판제외,바닥)","D80","개소",3,{"$nulls":8},"56940610380",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610390","강관스리브(지수판제외,바닥)","D100","개소",4,{"$nulls":8},"56940610390",{"$nulls":4},0,{"$nulls":8},1]
["010602","56940610400","강관스리브(지수판제외,바닥)","D125","개소",1,{"$nulls":8},"56940610400",{"$nulls":4},0,{"$nulls":8},1]
["010602","56810021002","방화실란트","D20","개소",30,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","56810021003","방화실란트","D25","개소",14,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","56810021004","방화실란트","D32","개소",18,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","56810021005","방화실란트","D40","개소",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","56810021006","방화실란트","D50","개소",21,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","56810021007","방화실란트","D65","개소",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","56810021008","방화실란트","D80","개소",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","56810021009","방화실란트","D100","개소",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","56810021010","방화실란트","D125","개소",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","95200017301","ㄷ형강","100×50×5×7.5mm","KG",73,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","95200027071","ㄱ형강","등변, 50×50×6mm","KG",1339,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010602","56941340020","인서트플레이트","200x200x9T","개소",6,{"$nulls":8},"56941340020",{"$nulls":4},0,{"$nulls":8},1]
["010602","56941420040","유성페인트칠","철재면2회 (노무비제외)","M2",61,{"$nulls":8},"56941420040",{"$nulls":4},0,{"$nulls":8},1]
["010602","56941422040","녹막이페인트칠","2회 (노무비제외)","M2",61,{"$nulls":8},"56941422040",{"$nulls":4},0,{"$nulls":8},1]
["010602","56941410010","잡철물제작설치","간단","TON",1.3460000000000001,{"$nulls":8},"56941410010",{"$nulls":4},0,{"$nulls":8},1]
["010602","56900017041","노무비","보통인부","인",50,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["010602","56900017030","노무비","배관공","인",67,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["010602","56900017021","노무비","도장공","인",11,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["010602","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},"",1164,null,1,0,0.03,{"$nulls":8},1]
{"$rows_empty":8}
[null,null,"[ 합           계 ]"]
[null,null,"010603  오배수배관공사"]
["010603","47100487006","배관용 탄소강관","백관 (SPP), D50, 반제품","M",218,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100487008","배관용 탄소강관","백관 (SPP), D80, 반제품","M",17,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100487009","배관용 탄소강관","백관 (SPP), D100, 반제품","M",373,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100487010","배관용 탄소강관","백관 (SPP), D125, 반제품","M",56,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100487011","배관용 탄소강관","백관 (SPP), D150, 반제품","M",3,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100487012","배관용 탄소강관","백관 (SPP), D200, 반제품","M",3,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100487013","배관용 탄소강관","백관 (SPP), D250, 반제품","M",208,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727106","일반용 경질염화비닐관","PVC관(VG1,DTS) D50","M",28,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727111","일반용 경질염화비닐관","PVC관(VG1,DTS) D150","M",29,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727153","일반용 경질염화비닐관","PVC관(VG2,DTS) D50","M",874,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727155","일반용 경질염화비닐관","PVC관(VG2,DTS) D75","M",6,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727156","일반용 경질염화비닐관","PVC관(VG2,DTS) D100","M",103,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727157","일반용 경질염화비닐관","PVC관(VG2,DTS) D125","M",5,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727158","일반용 경질염화비닐관","PVC관(VG2,DTS) D150","M",5,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727128","일반용 경질염화비닐관","PVC관(VG1,DRF) D100","M",60,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727129","일반용 경질염화비닐관","PVC관(VG1,DRF) D125","M",31,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727200","INNO AS (PPF) 저소음관","D35","M",60,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727201","INNO AS (PPF) 저소음관","D40","M",20,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727202","INNO AS (PPF) 저소음관","D50","M",348,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727203","INNO AS (PPF) 저소음관","D75","M",216,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727204","INNO AS (PPF) 저소음관","D100","M",569,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727205","INNO AS (PPF) 저소음관","D125","M",77,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727206","INNO AS (PPF) 저소음관","D150","M",54,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","47100727207","INNO AS (PPF) 저소음관","D200","M",15,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["010603","PPS00000001","잡재료비","관의 3%","식",1,{"$nulls":8},"",1199,null,0,0,0.03,{"$nulls":8},1]
["010603","47304017006","나사식 강관제 관이음쇠","백엘보 (나사) D50","EA",23,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301127003","용접식 관이음쇠","백엘보 (용접) D80","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301127004","용접식 관이음쇠","백엘보 (용접) D100","EA",34,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301127005","용접식 관이음쇠","백엘보 (용접) D125","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301127008","용접식 관이음쇠","백엘보 (용접) D250","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47304017106","나사식 강관제 관이음쇠","백티이 (나사) D50","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301127218","용접식 관이음쇠","백티이 (용접) D100","EA",19,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301127219","용접식 관이음쇠","백티이 (용접) D125","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301127222","용접식 관이음쇠","백티이 (용접) D250","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47304017506","나사식 강관제 관이음쇠","백소켓 (나사) D50","EA",18,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47304017306","나사식 강관제 관이음쇠","백니플 (나사) D50","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47304017406","나사식 강관제 관이음쇠","백유니온 (나사) D50","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47300248201","바닥배수구(F.D)","D50","EA",66,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148043","배수용 경질염화비닐 이음관","90˚단곡관(DTS) D50","EA",374,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148044","배수용 경질염화비닐 이음관","90˚단곡관(DTS) D75","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148045","배수용 경질염화비닐 이음관","90˚단곡관(DTS) D100","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148063","배수용 경질염화비닐 이음관","45˚단곡관(DTS) D100","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148143","배수용 경질염화비닐 이음관","소켓 (DTS) D50","EA",89,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148146","배수용 경질염화비닐 이음관","소켓 (DTS) D100","EA",18,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148147","배수용 경질염화비닐 이음관","소켓 (DTS) D125","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148148","배수용 경질염화비닐 이음관","소켓 (DTS) D150","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148235","배수용 경질염화비닐 이음관","리듀서(DTS) D75xD50","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148384","배수용 경질염화비닐 이음관","Y관(DTS) D125xD100","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148390","배수용 경질염화비닐 이음관","Y관(DTS) D150x100","EA",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148604","배수용 경질염화비닐 이음관","YT관(DTS) D50xD50","EA",77,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148613","배수용 경질염화비닐 이음관","YT관(DTS) D75xD50","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148614","배수용 경질염화비닐 이음관","YT관(DTS) D100xD100","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148617","배수용 경질염화비닐 이음관","YT관(DTS) D100xD50","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148618","배수용 경질염화비닐 이음관","YT관(DTS) D100xD75","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148622","배수용 경질염화비닐 이음관","YT관(DTS) D125xD50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148628","배수용 경질염화비닐 이음관","YT관(DTS) D150xD50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148630","배수용 경질염화비닐 이음관","YT관(DTS) D150xD100","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148659","배수용 경질염화비닐 이음관","45˚단곡관(DRF) D50","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148660","배수용 경질염화비닐 이음관","45˚단곡관(DRF) D75","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148661","배수용 경질염화비닐 이음관","45˚단곡관(DRF) D100","EA",15,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148671","배수용 경질염화비닐 이음관","Y관 (DRF) D100x50","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148672","배수용 경질염화비닐 이음관","Y관 (DRF) D100x75","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148736","배수용 경질염화비닐 이음관","Y관 (DRF) D125x75","EA",9,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148674","배수용 경질염화비닐 이음관","Y관 (DRF) D125x100","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148684","배수용 경질염화비닐 이음관","LT관 (DRF) D100x100","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148685","배수용 경질염화비닐 이음관","LT관 (DRF) D125x100","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148716","배수용 경질염화비닐 이음관","소켓 (DRF) D100","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149401","INNO AS 파이프이음관","90곡관, D35","EA",82,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149402","INNO AS 파이프이음관","90곡관, D40","EA",28,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149403","INNO AS 파이프이음관","90곡관, D50","EA",116,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149404","INNO AS 파이프이음관","90곡관, D75","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149405","INNO AS 파이프이음관","90곡관, D100","EA",105,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149417","INNO AS 파이프이음관","45곡관, D50","EA",158,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149418","INNO AS 파이프이음관","45곡관, D75","EA",84,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149419","INNO AS 파이프이음관","45곡관, D100","EA",177,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149420","INNO AS 파이프이음관","45곡관, D125","EA",17,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149421","INNO AS 파이프이음관","45곡관, D150","EA",18,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149422","INNO AS 파이프이음관","45곡관, D200","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149434","INNO AS 파이프이음관","Y 관, D50x50","EA",94,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149435","INNO AS 파이프이음관","Y 관, D75x50","EA",109,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149436","INNO AS 파이프이음관","Y 관, D75x75","EA",25,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149437","INNO AS 파이프이음관","Y 관, D100x50","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149438","INNO AS 파이프이음관","Y 관, D100x75","EA",13,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149439","INNO AS 파이프이음관","Y 관, D100x100","EA",166,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149440","INNO AS 파이프이음관","Y 관, D125x50","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149441","INNO AS 파이프이음관","Y 관, D125x75","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149442","INNO AS 파이프이음관","Y 관, D125x100","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149443","INNO AS 파이프이음관","Y 관, D125x125","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149446","INNO AS 파이프이음관","Y 관, D150x100","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149447","INNO AS 파이프이음관","Y 관, D150x125","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149448","INNO AS 파이프이음관","Y 관, D150x150","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149451","INNO AS 파이프이음관","Y 관, D200x100","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149453","INNO AS 파이프이음관","Y 관, D200x150","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149454","INNO AS 파이프이음관","Y 관, D200x200","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149475","INNO AS 파이프이음관","YT 관, D50x50","EA",23,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149476","INNO AS 파이프이음관","YT 관, D75x50","EA",22,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149478","INNO AS 파이프이음관","YT 관, D100x50","EA",47,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149481","INNO AS 파이프이음관","YT 관, D125x50","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149485","INNO AS 파이프이음관","YT 관, D150x50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149490","INNO AS 파이프이음관","YT 관, D200x50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149593","INNO AS 파이프이음관","소켓, D50","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149594","INNO AS 파이프이음관","소켓, D75","EA",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149595","INNO AS 파이프이음관","소켓, D100","EA",31,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149596","INNO AS 파이프이음관","소켓, D125","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149597","INNO AS 파이프이음관","소켓, D150","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149607","INNO AS 파이프이음관","P트랩, D50","EA",66,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149618","INNO AS 파이프이음관","소제구캡, D50","EA",39,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149619","INNO AS 파이프이음관","소제구캡, D75","EA",48,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149620","INNO AS 파이프이음관","소제구캡, D100","EA",84,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149621","INNO AS 파이프이음관","소제구캡, D125","EA",9,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149622","INNO AS 파이프이음관","소제구캡, D150","EA",9,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149623","INNO AS 파이프이음관","소제구캡, D200","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149668","INNO AS 파이프이음관","레듀샤, D50x35","EA",82,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301149669","INNO AS 파이프이음관","레듀샤, D50x40","EA",28,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148900","배수용 경질염화비닐 이음관","V.T.R(PVC) D125","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148901","배수용 경질염화비닐 이음관","V.T.R(PVC) D150","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940120080","강관용접","D80","개소",16,{"$nulls":8},"56940120080",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940120090","강관용접","D100","개소",157,{"$nulls":8},"56940120090",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940120100","강관용접","D125","개소",15,{"$nulls":8},"56940120100",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940120110","강관용접","D150","개소",8,{"$nulls":8},"56940120110",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940120130","강관용접","D250","개소",55,{"$nulls":8},"56940120130",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940330060","용접합후렌지","D50","개소",24,{"$nulls":8},"56940330060",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940330080","용접합후렌지","D80","개소",4,{"$nulls":8},"56940330080",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940330090","용접합후렌지","D100","개소",27,{"$nulls":8},"56940330090",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940330100","용접합후렌지","D125","개소",1,{"$nulls":8},"56940330100",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940330130","용접합후렌지","D250","개소",4,{"$nulls":8},"56940330130",{"$nulls":4},0,{"$nulls":8},1]
["010603","47305257199","플랜지(FLANGE)","맹플랜지 (10KG) D100","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47305257200","플랜지(FLANGE)","맹플랜지 (10KG) D125","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47305257203","플랜지(FLANGE)","맹플랜지 (10KG) D250","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","80000011183","청동게이트밸브 (10KG)","D50","EA",8,{"$nulls":8},"80000011183",null,null,0,0,0,{"$nulls":8},1]
["010603","80000011185","주철게이트밸브 (10KG)","D80","EA",1,{"$nulls":8},"80000011185",null,null,0,0,0,{"$nulls":8},1]
["010603","80000011186","주철게이트밸브 (10KG)","D100","EA",4,{"$nulls":8},"80000011186",null,null,0,0,0,{"$nulls":8},1]
["010603","48200428306","체크 밸브","스모렌스키,D50","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","80000011203","주철체크밸브(충격완화용,10KG)","D100","EA",4,{"$nulls":8},"80000011203",null,null,0,0,0,{"$nulls":8},1]
["010603","56941320010","압력계설치(백관)","0-35KG/CM2","조",12,{"$nulls":8},"56941320010",null,null,0,0,0,{"$nulls":8},1]
["010603","56940510060","일반행거(달대볼트)","D50","개소",678,{"$nulls":8},"56940510060",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940510080","일반행거(달대볼트)","D80","개소",124,{"$nulls":8},"56940510080",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940510090","일반행거(달대볼트)","D100","개소",408,{"$nulls":8},"56940510090",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940510100","일반행거(달대볼트)","D125","개소",60,{"$nulls":8},"56940510100",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940510110","일반행거(달대볼트)","D150","개소",25,{"$nulls":8},"56940510110",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940510120","일반행거(달대볼트)","D200","개소",7,{"$nulls":8},"56940510120",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940510130","일반행거(달대볼트)","D250","개소",31,{"$nulls":8},"56940510130",{"$nulls":4},0,{"$nulls":8},1]
["010603","53060228341","U자형볼트/너트","비절연, D100","EA",25,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","53060228342","U자형볼트/너트","비절연, D125","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","53060228343","U자형볼트/너트","비절연, D150","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","53060228345","U자형볼트/너트","비절연, D250","EA",14,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940610060","강관스리브(지수판제외,벽체)","D50","개소",16,{"$nulls":8},"56940610060",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940610080","강관스리브(지수판제외,벽체)","D80","개소",15,{"$nulls":8},"56940610080",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940610090","강관스리브(지수판제외,벽체)","D100","개소",32,{"$nulls":8},"56940610090",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940610100","강관스리브(지수판제외,벽체)","D125","개소",5,{"$nulls":8},"56940610100",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940610110","강관스리브(지수판제외,벽체)","D150","개소",5,{"$nulls":8},"56940610110",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940610120","강관스리브(지수판제외,벽체)","D200","개소",1,{"$nulls":8},"56940610120",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940610130","강관스리브(지수판제외,벽체)","D250","개소",2,{"$nulls":8},"56940610130",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940610360","강관스리브(지수판제외,바닥)","D50","개소",2,{"$nulls":8},"56940610360",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940610390","강관스리브(지수판제외,바닥)","D100","개소",36,{"$nulls":8},"56940610390",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940610400","강관스리브(지수판제외,바닥)","D125","개소",7,{"$nulls":8},"56940610400",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940610410","강관스리브(지수판제외,바닥)","D150","개소",8,{"$nulls":8},"56940610410",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940610430","강관스리브(지수판제외,바닥)","D250","개소",14,{"$nulls":8},"56940610430",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940620060","강관스리브(지수판포함,벽체)","D50","개소",9,{"$nulls":8},"56940620060",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940620090","강관스리브(지수판포함,벽체)","D100","개소",8,{"$nulls":8},"56940620090",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940620100","강관스리브(지수판포함,벽체)","D125","개소",4,{"$nulls":8},"56940620100",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940620110","강관스리브(지수판포함,벽체)","D150","개소",4,{"$nulls":8},"56940620110",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940620120","강관스리브(지수판포함,벽체)","D200","개소",3,{"$nulls":8},"56940620120",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940620400","강관스리브(지수판포함,바닥)","D125","개소",1,{"$nulls":8},"56940620400",{"$nulls":4},0,{"$nulls":8},1]
["010603","56940620410","강관스리브(지수판포함,바닥)","D150","개소",1,{"$nulls":8},"56940620410",{"$nulls":4},0,{"$nulls":8},1]
["010603","56810021006","방화실란트","D50","개소",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","56810021008","방화실란트","D80","개소",15,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","56810021009","방화실란트","D100","개소",57,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","56810021010","방화실란트","D125","개소",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","56810021011","방화실란트","D150","개소",13,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","56810021012","방화실란트","D200","개소",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","56810021013","방화실란트","D250","개소",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148939","배수용 경질염화비닐 이음관","청소씽크스리브 D75","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148940","배수용 경질염화비닐 이음관","세면기스리브 D35","EA",82,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148943","배수용 경질염화비닐 이음관","소변기스리브 D40","EA",28,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148944","배수용 경질염화비닐 이음관","씽크스리브 D50","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","47301148945","배수용 경질염화비닐 이음관","양변기스리브 D100","EA",105,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["010603","56941491011","펌프가대설치(배수펌프)","펌프2대설치기준","개소",6,{"$nulls":8},"56941491011",{"$nulls":4},0,{"$nulls":8},1]
["010603","56941420040","유성페인트칠","철재면2회 (노무비제외)","M2",144,{"$nulls":8},"56941420040",{"$nulls":4},0,{"$nulls":8},1]
["010603","56941422040","녹막이페인트칠","2회 (노무비제외)","M2",24,{"$nulls":8},"56941422040",{"$nulls":4},0,{"$nulls":8},1]
["010603","56900017041","노무비","보통인부","인",168,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["010603","56900017030","노무비","배관공","인",359,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["010603","56900017021","노무비","도장공","인",13,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["010603","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},"",1358,null,1,0,0.03,{"$nulls":8},1]
{"$rows_empty":22}
[null,null,"[ 합           계 ]"]
[null,null,"0107  가스배관공사"]
["0107","47100487402","가스배관용 탄소강관","백관(KSD3631), D20","M",24,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0107","47100487404","가스배관용 탄소강관","백관(KSD3631), D25","M",7,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0107","47100487406","가스배관용 탄소강관","백관(KSD3631), D32","M",9,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0107","47100487408","가스배관용 탄소강관","백관(KSD3631), D40","M",7,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0107","47100487410","가스배관용 탄소강관","백관(KSD3631), D50","M",169,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0107","47100777005","가스용 폴리에틸렌관","PEM, D63","M",47,{"$nulls":8},"",{"$nulls":4},0,1,{"$nulls":7},1]
["0107","PPS00000001","잡재료비","관의 3%","식",1,{"$nulls":8},"",1389,null,0,0,0.03,{"$nulls":8},1]
["0107","47305257694","가스용 폴리에틸렌관 이음관","90˚엘보(융착식),Φ63","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47305257768","가스용 폴리에틸렌관 이음관","T/F이음관(융착식),Φ63","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017002","나사식 강관제 관이음쇠","백엘보 (나사) D20","EA",21,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017003","나사식 강관제 관이음쇠","백엘보 (나사) D25","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017004","나사식 강관제 관이음쇠","백엘보 (나사) D32","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017005","나사식 강관제 관이음쇠","백엘보 (나사) D40","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017006","나사식 강관제 관이음쇠","백엘보 (나사) D50","EA",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017103","나사식 강관제 관이음쇠","백티이 (나사) D25","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017104","나사식 강관제 관이음쇠","백티이 (나사) D32","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017105","나사식 강관제 관이음쇠","백티이 (나사) D40","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017106","나사식 강관제 관이음쇠","백티이 (나사) D50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017203","나사식 강관제 관이음쇠","백리듀서 (나사) D25","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017204","나사식 강관제 관이음쇠","백리듀서 (나사) D32","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017205","나사식 강관제 관이음쇠","백리듀서 (나사) D40","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017206","나사식 강관제 관이음쇠","백리듀서 (나사) D50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017802","나사식 강관제 관이음쇠","백캡 (나사) D20","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017803","나사식 강관제 관이음쇠","백캡 (나사) D25","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017302","나사식 강관제 관이음쇠","백니플 (나사) D20","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017306","나사식 강관제 관이음쇠","백니플 (나사) D50","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017402","나사식 강관제 관이음쇠","백유니온 (나사) D20","EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","47304017406","나사식 강관제 관이음쇠","백유니온 (나사) D50","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","56940240020","나사접합","D20","개소",57,{"$nulls":8},"56940240020",{"$nulls":4},0,{"$nulls":8},1]
["0107","56940240030","나사접합","D25","개소",11,{"$nulls":8},"56940240030",{"$nulls":4},0,{"$nulls":8},1]
["0107","56940240040","나사접합","D32","개소",16,{"$nulls":8},"56940240040",{"$nulls":4},0,{"$nulls":8},1]
["0107","56940240050","나사접합","D40","개소",9,{"$nulls":8},"56940240050",{"$nulls":4},0,{"$nulls":8},1]
["0107","56940240060","나사접합","D50","개소",41,{"$nulls":8},"56940240060",{"$nulls":4},0,{"$nulls":8},1]
["0107","56941535521","PEM 접합 (가스용)","D63","개소",29,{"$nulls":8},"56941535521",{"$nulls":4},0,{"$nulls":8},1]
["0107","56940330070","용접합후렌지","D65","개소",2,{"$nulls":8},"56940330070",{"$nulls":4},0,{"$nulls":8},1]
["0107","80000011191","황동볼밸브 (10KG)","D20","EA",7,{"$nulls":8},"표준시장단가",{"$nulls":4},0,{"$nulls":8},1]
["0107","48200147506","가스용주강볼밸브","D50","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","48206147730","가스매몰형볼밸브(2-PURGE)","레버식, D63","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","63500327006","A.S.V","D 50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","66800607006","가스미터(G-25)","40㎥/HR이하","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","66800607101","가스미터박스","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","53300137292","가스키트","브라켓트, D20","EA",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","53300137293","가스키트","브라켓트, D25","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","53300137294","가스키트","브라켓트, D32","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","53300137295","가스키트","브라켓트, D40","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","53300137296","가스키트","브라켓트, D50","EA",77,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","53651007131","스페이서","INSUL-SPACER, D50","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","66650097003","가스 감지기","방수형","SET",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","66650097005","가스감지 판넬","6회로용","면",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","56800447011","맨홀뚜껑(철개)","COVER(맨홀) 중형 가스설비용","조",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","56800447012","맨홀(흄관)","D900","조",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","56941530080","X - RAY TEST","","매당",3,{"$nulls":8},"56941530080",{"$nulls":4},0,{"$nulls":8},1]
["0107","56941530120","라인마크설치","","개소",1,{"$nulls":8},"56941530120",{"$nulls":4},0,{"$nulls":8},1]
["0107","56941530110","LOCATING WIRE설치","","M",45,{"$nulls":8},"56941530110",{"$nulls":4},0,{"$nulls":8},1]
["0107","56941530290","표식 SHEET 포설","","M",90,{"$nulls":8},"56941530290",{"$nulls":4},0,{"$nulls":8},1]
["0107","56941533010","공급관기밀시험","50ø이하","구간",2,{"$nulls":8},"56941533010",{"$nulls":4},0,{"$nulls":8},1]
["0107","56941534010","에어후레싱","50ø이하","구간",1,{"$nulls":8},"56941534010",{"$nulls":4},0,{"$nulls":8},1]
["0107","56941534030","배관구배보기","옥외공급관","M당",45,{"$nulls":8},"56941534030",{"$nulls":4},0,{"$nulls":8},1]
["0107","56941534040","배관청소","65ø이하","구간",1,{"$nulls":8},"56941534040",{"$nulls":4},0,{"$nulls":8},1]
["0107","56941521050","용접개소방식처리","D50","개소",1,{"$nulls":8},"56941521050",{"$nulls":4},0,{"$nulls":8},1]
["0107","53060228334","U자형볼트/너트","비절연, D20","EA",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","53060228335","U자형볼트/너트","비절연, D25","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","53060228336","U자형볼트/너트","비절연, D32","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","53060228337","U자형볼트/너트","비절연, D40","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","53060228338","U자형볼트/너트","비절연, D50","EA",77,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","56940610060","강관스리브(지수판제외,벽체)","D50","개소",1,{"$nulls":8},"56940610060",{"$nulls":4},0,{"$nulls":8},1]
["0107","56940620060","강관스리브(지수판포함,벽체)","D50","개소",1,{"$nulls":8},"56940620060",{"$nulls":4},0,{"$nulls":8},1]
["0107","53060037107","볼트너트","M12x150","EA",397,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","56941420040","유성페인트칠","철재면2회 (노무비제외)","M2",33,{"$nulls":8},"56941420040",{"$nulls":4},0,{"$nulls":8},1]
["0107","56941422030","녹막이페인트칠","1회 (노무비제외)","M2",33,{"$nulls":8},"56941422030",{"$nulls":4},0,{"$nulls":8},1]
["0107","59750337001","강제전선관","아연도  16 mm","M",143,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","59750337002","강제전선관","아연도  22 mm","M",22,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","61450357049","제어케이블","CVV 2Cx1.25 ㎟","M",157,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","56941990010","기계터파기","","M3",54,{"$nulls":8},"56941990010",{"$nulls":4},0,{"$nulls":8},1]
["0107","56941990020","기계되메우기","","M3",45,{"$nulls":8},"56941990020",null,null,0,0,0,{"$nulls":8},1]
["0107","56941990030","잔토처리","","M3",9,{"$nulls":8},"56941990030",{"$nulls":4},0,{"$nulls":8},1]
["0107","56941990040","모래부설","","M3",9,{"$nulls":8},"56941990040",{"$nulls":4},0,{"$nulls":8},1]
["0107","81200068043","SAND BAG","","EA",14,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0107","56900017016","노무비","내선전공","인",9,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0107","56900017076","노무비","저압케이블전공","인",2,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0107","56900017007","노무비","계장공","인",2,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0107","56900017041","노무비","보통인부","인",2,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0107","56900017030","노무비","배관공","인",1,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0107","56900017021","노무비","도장공","인",2,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0107","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},"",1467,null,1,0,0.03,{"$nulls":8},1]
{"$rows_empty":17}
[null,null,"[ 합           계 ]"]
[null,null,"0108  연도설치공사"]
["0108","V1504060001","1) ENGINE STACK","STS/AL'STL","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060002","VERTICAL DRAIN TEE CAP","450A-VDC","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060003","STRAIGHT","450A-477","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060004","LATERAL TEE","450A-LT","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060005","PLATE SUPPORT ASS'Y","450A-PA","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060006","INSULATED VALVE","450A-IV","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060007","SLEEVE","450A-SLV","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060008","STRAIGHT","450A-977","EA",39,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060009","FULL ANGLE RING","450A-FR","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060010","SLIP SECTION","450A-SS477","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060011","BELLOWS JOINT","450A-BJ","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060012","STORM COLLAR","450A-SC","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060013","VENTILATED THIMBLE","450A-VT","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060014","CHECK HOLE","450A-CH477","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060015","STACK CAP","450A-SK","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060016","DRAIN PIPE","DP","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060017","SEALANT","SA","EA",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060020","2) ENGINE BREECHING","STS/AL'STL","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060021","FLANGE ADAPTER","450A-FA","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060022","CLAMP FLANGE","450A-CF","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060023","STRAIGHT","450A-977","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060024","PLATE SUPPORT ASSEMBLY","450A-PA","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060025","SLEEVE","450A-SLV","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060026","STORM COLLAR","450A-SC","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060027","ELBOW 45","450A-EL45","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060028","STRAIGHT","450A-477","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060029","SLIP SECTION","450A-SS477","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060030","BELLOWS JOINT","450A-BJ","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060031","STRAIGHT","SA","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0108","V1504060034","3) INSTALLATION COST","","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":20}
[null,null,"[ 합           계 ]"]
[null,null,"0109  방음방진설치공사"]
["0109","V1504241001"," 1. FAN 방진","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241002","F-1","SH-100","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241003","F-3","SH-100","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241004","F-7","SMB2-150","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241005","F-8","SMB2-50","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241006","F-16","SMB2-200","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241008"," 2. 탈취유니트 방진","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241009","FU-1","SMB2-200","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241010","FU-1","VP-100x50x25t","SHT",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241012"," 3. 공조용소음기","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241013","AHU-1(S)","2000×1200×2100","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241014","AHU-1(R)","1700×1200×1800","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241015","AHU-2(S)","1000×800×2400","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241016","AHU-2(R)","1000×700×2100","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241017","AHU-3(S)","1400×600×2100","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241018","AHU-3(R)","1000×600×1800","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241019","AHU-4(S)","900×800×2400","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241020","AHU-4(R)","900×800×2100","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241021","AHU-5(S)","1300×900×2400","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241022","AHU-5(R)","1300×800×2100","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241023","AHU-6(S)","1500×1000×2100","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241024","AHU-6(R)","1200×1000×1800","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241025","AHU-7(S)","1500×1100×2100","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241026","AHU-7(R)","1300×1000×1800","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241027","HVU-1(S)","1200×600×1800","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241029"," 4. 소음 쳄바","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241030","AHU-1(S)","1600×1600×1100","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241031","AHU-2(S)","1000×2000×800","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241032","AHU-3(S)","1000×1400×650","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241033","AHU-4(S)","1000×1500×1000","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241034","AHU-5(S)","1500×2000×1000","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241035","AHU-6(S)","1600×1600×1000","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241036","AHU-7(S)","1600×1600×1000","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241037","HVU-1(S)","800×1200×650","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241039"," 5. 공조실 PO-MAT 이중바닥 시","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241043","PO-MAT","B25T","㎡",244,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241046","아이소핑크","3'x6'x20THK-20K","장",61,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241047","접착제","-","EA",73.2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241048","비닐시트","0.08THK","㎡",512.4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241049","OPP 테이프","50x5000mm","EA",268.39999999999998,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241050","실란트코킹","우레탄계","Kg",683.2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241051","와이어메쉬","#4 5.8Φ100x100","㎡",268.39999999999998,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241052","콘크리트","210-18-15","㎥",24.4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241064"," 6. 냉각탑 PO-MAT 이중바닥 시","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241067","PO-MAT","B25","㎡",130,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241070","아이소핑크","3'x6'x20THK-20K","장",16.25,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241071","접착제","","EA",19.5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241072","비닐시트","0.08THK","㎡",136.5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241073","OPP 테이프","50x5000mm","EA",71.5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241074","실란트코킹","우레탄계","Kg",182,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241075","보강철근","D10","Ton",0.58499999999999996,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241076","콘크리트","25-21-12","㎥",9.75,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","V1504241078","5~6. 설   치   비","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0109","56900017017","노무비","내장공","인",40.700000000000003,{"$nulls":8},"",null,null,0,0,0,null,null,3,{"$nulls":5},1]
["0109","56900017102","노무비","철근공","인",3.3,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0109","56900017108","노무비","콘크리트공","인",20.399999999999999,{"$nulls":8},"",null,null,0,0,0,null,null,3,{"$nulls":5},1]
["0109","56900017029","노무비","방수공","인",20.399999999999999,{"$nulls":8},"",null,null,0,0,0,null,null,3,{"$nulls":5},1]
["0109","56900017041","노무비","보통인부","인",47.2,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["0109","56900017118","노무비","특별인부","인",2,{"$nulls":8},"",null,null,0,0,0,null,null,3,{"$nulls":5},1]
["0109","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},"",1598,null,1,0,0.03,{"$nulls":8},1]
{"$rows_empty":16}
[null,null,"[ 합           계 ]"]
[null,null,"011001  공조(1F,3F,4F,5F)"]
["011001","V1504079001","HEATING CABLE","HSR 16 2-CP","M",735,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079002","POWER CONNECTION KIT","HACC-PK","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079003","END SEAL","ES-10","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079004","SUS BAND","HACC-SB","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079005","GLASS TAPE","GT-66","RL",62,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079006","RTD SENSOR","PT-100","SET",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079007","CONTROL PANEL","1CCT","SET",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079008","CONTROL PANEL","3CCT","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079009","기동전류 제어기","1CCT용","SET",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079010","기동전류 제어기","3CCT용","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079011","자동경보, HTDU 시스템","1CCT용","SET",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079012","자동경보, HTDU 시스템","3CCT용","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079013","STEEL PIPE","16C","M",160,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079014","STEEL PIPE","22C","M",78,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079015","STEEL PIPE","28C","M",35,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079016","STEEL PIPE","36C","M",103,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079017","전선","HFIX 6.0","M",940,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079018","전선","GV 4.0","M",470,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079019","전선","CVVS1.5SQ*3C","M",164,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079020","후렉시블전선관","GW 22C","M",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079021","후렉시블콘넥타","GWCZ 22C","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079022","Pull Box","150*150*100","EA",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079023","Pull Box","200*200*100","EA",17,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079024","전선관 부속품비","전선관의 20%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","V1504079025","잡자재비","자재비의 2%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011001","56900017127","노무비","플랜트전공","인",27,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["011001","56900017016","노무비","내선전공","인",75,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["011001","56900017076","노무비","저압케이블전공","인",4,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["011001","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},"",1645,null,1,0,0.03,{"$nulls":8},1]
{"$rows_empty":21}
[null,null,"[ 합           계 ]"]
[null,null,"011002  위생(2F,4F,5F)"]
["011002","V1504079501","HEATING CABLE","HSR 16 2-CP","M",134,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011002","V1504079502","TEE SPLICE","HACC-TS","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011002","V1504079503","END SEAL","ES-10","EA",13,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011002","V1504079504","SUS BAND","HACC-SB","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011002","V1504079505","GLASS TAPE","GT-66","RL",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011002","V1504079506","THERMOSTAT KIT","TSK","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011002","V1504079507","SENSOR KIT","일자TYPE","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011002","V1504079508","잡자재비","자재비의 2%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["011002","56900017127","노무비","플랜트전공","인",5,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["011002","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},"",1678,null,1,0,0.03,{"$nulls":8},1]
{"$rows_empty":14}
[null,null,"[ 합           계 ]"]
[null,null,"0111  우수처리시설공사"]
["0111","V1504077005","1. 빗물이용시설 기계장비","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077006","SMARTECO","W1,500 x L2,000 x H1,000","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077007","배수펌프","125A x 100A x 1.35㎥/min x 25m","SET",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077008","공급펌프","40A x 40A x 0.06㎥/min x 25mH","SET",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077009","방진가대","15HP","SET",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077010","레벨센서","오뚜기 type","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077011","CONTROL PANEL","W900 x L400 x H1,800","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077029","2. 빗물이용시설 배관공사","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077030","일반배관용스테인레스강관","STS,40A","M",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077031","일반배관용스테인레스강관","STS,100A","M",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077032","일반배관용스테인레스강관","STS,125A","M",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077033","일반배관용스테인레스강관","STS, 200A","M",15,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077034","용접소모자재","STS,40A","개소",21,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077035","용접소모자재","STS,100A","개소",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077036","용접소모자재","STS,125A","개소",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077037","용접소모자재","STS, 200A","개소",17,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077038","스테인레스 접합후렌지","STS, 40A","EA",25,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077039","스테인레스 접합후렌지","STS, 100A","EA",14,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077040","스테인레스 접합후렌지","STS, 125A","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077041","스테인레스 접합후렌지","STS, 200A","EA",9,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077042","버터플라이 밸브","GEAR, 40A","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077043","버터플라이 밸브","GEAR, 100A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077044","버터플라이 밸브","GEAR, 125A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077045","버터플라이 밸브","GEAR, 200A","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077046","스트레이너","200A","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077047","자동밸브","200A","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077048","체크밸브","40A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077049","체크밸브","100A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077050","후렉시블 콘넥타","40A","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077051","후렉시블 콘넥타","100A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077052","후렉시블 콘넥타","125A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077053","일반배관용 스테인레스강관 이음","엘보, STS304, 40A","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077054","일반배관용 스테인레스강관 이음","엘보, STS304, 100A","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077055","일반배관용 스테인레스강관 이음","엘보, STS304, 125A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077056","일반배관용 스테인레스강관 이음","엘보, STS304, 200A","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077057","일반배관용 스테인레스강관 이음","티, STS304, 40A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077058","일반배관용 스테인레스강관 이음","티, STS304, 100A","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077059","일반배관용 스테인레스강관 이음","티, STS304, 125A","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077060","일반배관용 스테인레스강관 이음","티, STS304, 200A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077061","압력계","10kg","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077079","3. 빗물이용시설 잡철물공사","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077080","ANGLE","50 x 50 x 4t","kg",280,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077081","PLATE","150*150*6T","kg",180,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077082","U BOLT","40A","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077083","U BOLT","100A","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077084","U BOLT","125A","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077085","U BOLT","200A","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077086","ANCHOR","M16","EA",19,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077104","4. 빗물이용시설 전기공사","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0111","V1504077105","전기공사","제어 및 2차 배선공사","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
[null,null,"[ 합           계 ]"]
[null,null,"0112  쓰레기이송설비공사"]
["0112","V1504075002","1. 토목공사","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075003","터파기","B.H 06 + 인력","㎥",670,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075004","모래부설 및 다짐","B.H 06 +콤팩트","㎥",280,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075005","되메우기 및 다짐","B.H 06 + 롤러(1ton)","㎥",400,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075009","2. 기자재공사","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075010","음식물쓰레기투입구","10L (공압구동형)","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075011","일반쓰레기투입구","100L 대형(공압구동형)","SET",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075012","공기흡입구","소음기부착","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075015","3. 관로공사","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075016","배관공사비(SPPS직관, SCH20)","400A(3Layer PE코팅)","m",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075017","배관공사비(SPPS직관, SCH20)","500A(3Layer PE코팅)","m",195,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075018","배관공사비(SPPS직관, SCH20)","500A(3Layer PE코팅)15\"","ea",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075019","배관공사비(SPPS직관, SCH20)","500A(3Layer PE코팅)30\"","ea",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075020","배관공사비(SPPS직관, SCH20)","500A(3Layer PE코팅)90\"","ea",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075021","배관공사비(일반곡관)","400A(3Layer PE코팅)90\"","ea",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075022","편심레듀사(흡입구벨브접속부위)","편심레듀샤, SPP 3LPECOATED","ea",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075023","FANGE KS 10K FF SS400","","Set",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075024","점검맨홀","","Set",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075025","관로경고테이프","","m",390,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075026","비파괴검사","R.T검사","개소",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075027","열수축튜브(용접부마감)","1.64*100*12","㎡",56,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075030","4. 전기및자동제어공사","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075031","투입구제어기","LW2-DV(투입구용)","SET",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075032","투입구제어기","LW2-DV(투입구/AV용)","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075033","증폭기+TR","","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075034","ELP전선관","65mm","M",526,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075035","전원케이블","F-CV 4mm2/2C,부속포함","M",150,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075036","제어케이블","UL-2919,부속포함","M",526,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075037","공기관","PB-8,15mm","M",526,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075038","공기관 피팅류","PB-8,15mm","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["0112","V1504075039","supervisor 및 시운전비","","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":19}
[null,null,"[ 합           계 ]"]
[null,null,"02  T.A.B 공사"]
["02","V1504302001","가.직접인건비","","",{"$nulls":9},"",{"$nulls":4},0,{"$nulls":8},1]
["02","V1504302002","1.시스템검토","","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["02","V1504302003","2.공기분배계통","","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["02","V1504302004","3.물분배계통","","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["02","V1504302005","4.소음계통","","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["02","V1504302006","5.마무리작업","","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["02","V1504302007","6.최종보고서 작성","","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["02","V1504302008","나.간접인건비","","",{"$nulls":9},"",{"$nulls":4},0,{"$nulls":8},1]
["02","V1504302009","1.제경비","","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["02","V1504302010","2.기술료","","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":14}
[null,null,"[ 합           계 ]"]
[null,null,"030101  팬코일유니트"]
["030101","MM708396919","FCU-1팬코일유닛(1WAY천장카세트","6CMM","대",36,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030101","MM708396920","FCU-2팬코일유닛(2WAY천장카세트","16CMM","대",138,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030101","MM708396921","FCU-3팬코일유닛(4WAY천장카세트","18.3CMM","대",11,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030101","MM708396922","FCU-4팬코일유닛(바닥상치형)","18.3CMM","대",219,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030101","MM708396923","FCU-5팬코일유닛(천정매입형)","12.8CMM","대",29,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030101","MM708396924","FCU-6팬코일유닛(천정매입형)","19.8CMM","대",8,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030101","Z3000000220","부가가치세","10%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":17}
[null,null,"[ 합           계 ]"]
[null,null,"030201  냉동기"]
["030201","MM708396907","ACH-1 2단저온수흡수식냉동기","280RT","대",2,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030201","Z3000000222","부가가치세","10%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":22}
[null,null,"[ 합           계 ]"]
[null,null,"030202  콤팩트열교환기"]
["030202","MM708396909","HX-1컴팩트유니트(판형)","684,000KCAL/HR","SET",1,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030202","MM708396910","HX-2컴팩트유니트(판형)","129,000KCAL/HR","",1,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030202","Z3000000224","부가가치세","10%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":21}
[null,null,"[ 합           계 ]"]
[null,null,"030203  냉각탑"]
["030203","MM708396908","CT-1직교류형냉각탑","700CRT","대",2,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030203","Z3000000226","부가가치세","10%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":22}
[null,null,"[ 합           계 ]"]
[null,null,"030204  공기조화기"]
["030204","MM708396911","AHU-1공기조화기(수평형)","46,000CMH","대",1,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030204","MM708396912","AHU-2공기조화기(수평형)","13,000CMH","대",1,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030204","MM708396913","AHU-3공기조화기(수평형)","14,000CMH","대",1,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030204","MM708396914","AHU-4공기조화기(수평형)","12,000CMH","대",1,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030204","MM708396915","AHU-5공기조화기(수평형)","23,000CMH","대",1,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030204","MM708396916","AHU-6공기조화기(수평형)","28,690CMH","대",1,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030204","MM708396917","AHU-7공기조화기(수평형)","30,030CMH","대",1,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030204","MM708396918","HVU-1공기조화기(수평형)","12,000CMH","대",1,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030204","Z3000000228","부가가치세","10%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":15}
[null,null,"[ 합           계 ]"]
[null,null,"030205  팽창기체분리기"]
["030205","MM708396970","AS-1팽창기체분리기(STS304)","200L 800*1,500*1,558","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030205","MM708396971","AS-2팽창기체분리기(STS304)","600L 800*1,500*1,200","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030205","Z2000000221","부가가치세","10%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":21}
[null,null,"[ 합           계 ]"]
[null,null,"030206  항온항습기"]
["030206","MM708396937","CHT-1공냉식항온항습기","냉/난:14,250/7,740KCAL/H","대",1,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030206","MM708396938","CHT-2공냉식항온항습기","냉/난:40,500/17,200KCAL/H","대",2,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030206","Z3000000231","부가가치세","10%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":21}
[null,null,"[ 합           계 ]"]
[null,null,"030207  저수조"]
["030207","MM708396932","T-1저수조(PDF 361,840L)","6,700*14,800*4,000","대",1,{"$nulls":8},"",null,null,0,0,0,{"$nulls":8},1]
["030207","Z3000000217","부가가치세","10%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":22}
[null,null,"[ 합           계 ]"]
[null,null,"030208  부스터펌프"]
["030208","MM708396931","P-4급수펌프(부스터)","(395LPM*3)*57M*(7.5KW*3)","SET",1,{"$nulls":8},"21878706",null,null,0,0,0,{"$nulls":8},1]
{"$rows_empty":23}
[null,null,"[ 합           계 ]"]
[null,null,"030209  고무발포보온재"]
["030209","M0002130025","고무발포단열재(동관용)","D25x13T","m",218,{"$nulls":8},"22314367",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0002190050","고무발포단열재(동관용)","D50x19T","m",150,{"$nulls":8},"22314389",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0002250020","고무발포단열재(동관용)","D20x25T","m",2416,{"$nulls":8},"22314362",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0002250025","고무발포단열재(동관용)","D25x25T","m",677,{"$nulls":8},"22314369",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0002250032","고무발포단열재(동관용)","D32x25T","m",344,{"$nulls":8},"22314376",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0002250040","고무발포단열재(동관용)","D40x25T","m",868,{"$nulls":8},"22314383",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0002250050","고무발포단열재(동관용)","D50x25T","m",1354,{"$nulls":8},"22314390",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0002250065","고무발포단열재(동관용)","D65x25T","m",1466,{"$nulls":8},"22314397",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0002250080","고무발포단열재(동관용)","D80x25T","m",56,{"$nulls":8},"22314404",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0002250100","고무발포단열재(동관용)","D100x25T","m",48,{"$nulls":8},"22314410",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0002250125","고무발포단열재(동관용)","D125x25T","m",518,{"$nulls":8},"22314416",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001130050","고무발포단열재(강관용)","D50x13T","m",21,{"$nulls":8},"22314492",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001130065","고무발포단열재(강관용)","D65x13T","m",25,{"$nulls":8},"22314499",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001130080","고무발포단열재(강관용)","D80x13T","m",8,{"$nulls":8},"22314506",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001130100","고무발포단열재(강관용)","D100x13T","m",21,{"$nulls":8},"22314512",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001190015","고무발포단열재(강관용)","D15x19T","m",673,{"$nulls":8},"22314459",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001190020","고무발포단열재(강관용)","D20x19T","m",1847,{"$nulls":8},"22314465",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001190025","고무발포단열재(강관용)","D25x19T","m",1165,{"$nulls":8},"22314472",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001190032","고무발포단열재(강관용)","D32x19T","m",1595,{"$nulls":8},"22314479",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001190040","고무발포단열재(강관용)","D40x19T","m",370,{"$nulls":8},"22314486",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001190050","고무발포단열재(강관용)","D50x19T","m",308,{"$nulls":8},"22314493",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001190065","고무발포단열재(강관용)","D65x19T","m",203,{"$nulls":8},"22314500",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001190080","고무발포단열재(강관용)","D80x19T","m",209,{"$nulls":8},"22314507",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001190100","고무발포단열재(강관용)","D100x19T","m",358,{"$nulls":8},"22314513",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001190125","고무발포단열재(강관용)","D125x19T","m",53,{"$nulls":8},"22314519",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001190150","고무발포단열재(강관용)","D150x19T","m",20,{"$nulls":8},"22314525",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001250050","고무발포단열재(강관용)","D50x25T","m",84,{"$nulls":8},"22314494",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001250065","고무발포단열재(강관용)","D65x25T","m",72,{"$nulls":8},"22314501",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001250080","고무발포단열재(강관용)","D80x25T","m",3,{"$nulls":8},"22314508",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001250100","고무발포단열재(강관용)","D100x25T","m",196,{"$nulls":8},"22314514",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001250125","고무발포단열재(강관용)","D125x25T","m",334,{"$nulls":8},"22314520",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001250150","고무발포단열재(강관용)","D150x25T","m",172,{"$nulls":8},"22314526",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001250200","고무발포단열재(강관용)","D200x25T","m",296,{"$nulls":8},"22314532",{"$nulls":4},0,{"$nulls":8},1]
["030209","M0001250250","고무발포단열재(강관용)","D250x25T","m",124,{"$nulls":8},"22314538",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":16}
[null,null,"[ 합           계 ]"]
[null,null,"030210  자동제어설치공사"]
["030210","V1506052001","1. 중앙관제장치","LGB-F2000(조달우수2012180)","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052002","       *주 요  사 양","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052003","+  HARDWARE","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052004"," -  CPU","INTEL i7 2.93GHz","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052005"," -   MAIN MEMORY","4Gbyte","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052006"," -   보조기억용량","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052007"," -   보조기억용량","H.D.D.  :  1Tbyte","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052008"," -   보조기억용량","O.D.D  : HP Super Multi DVD","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052009","  - WINDOWS 7","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052010","  - EXCEL 2013","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052011"," -  KEY BOARD","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052012"," -  MOUSE","광마우스","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052013","+모니터","23 inch LED","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052014","+PRINTER","칼라잉크젯 (A4용)","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052015","+인터컴","모기","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052016","+인터컴","자기","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052017","+HUB","8PORT","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052018","+DESK&CHAIR","","SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052019","   'SOFTWARE","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052020","- 특징 : 음성지원,멀티테스킹,","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052021","          O/S-한글 WINDOW'XP이","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052022","- 기능 :","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052023"," -  관제점 감시 및 제어 실행","","L/S",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052024","     ( Point Monitoring & Cont","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052025"," -  네트워크 구성 및 관제점 입","","L/S",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052026","     ( Datasheet Program )","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052027"," -  그래픽 감시 및 제어화면 제","","L/S",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052028","     ( Graphic Sheet Editor Pr","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052029"," -  관제점 감시 객체 라이브러","","L/S",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052030","     ( OCX Library )","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052031"," -  네트워크 통신제어 기능","","L/S",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052032","     ( Network Communication P","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052033"," -  데이타베이스 관리 기능","","L/S",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052034","    ( Structured Storage I/O P","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052035"," -  텍스트 감시 및 제어화면 제","","L/S",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052036","    ( Text M&A Editor Program","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052037"," -  멀티미디어 제어기능","","L/S",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052038","    ( Multimedia Control Progr","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052039"," -  보정영상분석을 이용하여 화","","L/S",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052040","         (Smart Fire Detecting","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052041","2. 현장제어반","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052042","DDC - M","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052043","1) ENCLOSURE","900x1800x350","장",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052044","2) 차단기","ABS32a 20A","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052045","3) NOISE FILTER","AC250V 20A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052046","4) CONSENT(노즐) 접지2구형","AC250V 20A","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052047","5) THERMO STAT","0~90C 1A1B","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052048","6) FAN","110x110","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052049","7) FL","AC220V 60W","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052050","8) TERMINAL BLOCK","15A Ass'ry","EA",60,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052051","9) CONTROL CABLE","KIV 1.25","M",80,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052052","10) TR","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052053","11) 아크릴명판","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052054","12)FUSE","","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052055","13)PVC DUCT","","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052056","14) MAIN MODULE","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052057","15) DI CARD","DI : 16","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052058","16) AI CARD","AI : 16","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052059","17) DO CARD","DO : 16","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052060","18) AO CARD","AO : 16","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052061","DDC - 1A - 1","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052062","1) ENCLOSURE","800x1100x250","장",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052063","2) 차단기","ABS32a 20A","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052064","3) NOISE FILTER","AC250V 20A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052065","4) CONSENT(노즐) 접지2구형","AC250V 20A","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052066","5) THERMO STAT","0~90C 1A1B","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052067","6) FAN","110x110","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052068","7) FL","AC220V 60W","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052069","8) TERMINAL BLOCK","15A Ass'ry","EA",60,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052070","9) CONTROL CABLE","KIV 1.25","M",80,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052071","10) TR","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052072","11) 아크릴명판","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052073","12)FUSE","","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052074","13)PVC DUCT","","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052075","14) MAIN MODULE","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052076","15) DI CARD","DI : 16","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052077","16) AI CARD","AI : 16","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052078","17) DO CARD","DO : 16","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052079","18) AO CARD","AO : 16","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052080","DDC - 1A - 2","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052081","1) ENCLOSURE","900x1200x350","장",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052082","2) 차단기","ABS32a 20A","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052083","3) NOISE FILTER","AC250V 20A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052084","4) CONSENT(노즐) 접지2구형","AC250V 20A","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052085","5) THERMO STAT","0~90C 1A1B","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052086","6) FAN","110x110","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052087","7) FL","AC220V 60W","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052088","8) TERMINAL BLOCK","15A Ass'ry","EA",60,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052089","9) CONTROL CABLE","KIV 1.25","M",80,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052090","10) TR","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052091","11) 아크릴명판","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052092","12)FUSE","","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052093","13)PVC DUCT","","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052094","14) MAIN MODULE","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052095","15) DI CARD","DI : 16","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052096","16) AI CARD","AI : 16","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052097","17) DO CARD","DO : 16","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052098","18) AO CARD","AO : 16","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052099","DDC - PH - 1","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052100","1) ENCLOSURE","800x1100x250","장",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052101","2) 차단기","ABS32a 20A","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052102","3) NOISE FILTER","AC250V 20A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052103","4) CONSENT(노즐) 접지2구형","AC250V 20A","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052104","5) THERMO STAT","0~90C 1A1B","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052105","6) FAN","110x110","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052106","7) FL","AC220V 60W","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052107","8) TERMINAL BLOCK","15A Ass'ry","EA",60,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052108","9) CONTROL CABLE","KIV 1.25","M",80,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052109","10) TR","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052110","11) 아크릴명판","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052111","12)FUSE","","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052112","13)PVC DUCT","","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052113","14) MAIN MODULE","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052114","15) DI CARD","DI : 16","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052115","16) AI CARD","AI : 16","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052116","17) DO CARD","DO : 16","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052117","18) AO CARD","AO : 16","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052118","DDC - PH - 2","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052119","1) ENCLOSURE","900x1200x250","장",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052120","2) 차단기","ABS32a 20A","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052121","3) NOISE FILTER","AC250V 20A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052122","4) CONSENT(노즐) 접지2구형","AC250V 20A","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052123","5) THERMO STAT","0~90C 1A1B","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052124","6) FAN","110x110","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052125","7) FL","AC220V 60W","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052126","8) TERMINAL BLOCK","15A Ass'ry","EA",60,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052127","9) CONTROL CABLE","KIV 1.25","M",80,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052128","10) TR","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052129","11) 아크릴명판","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052130","12)FUSE","","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052131","13)PVC DUCT","","EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052132","14) MAIN MODULE","","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052133","15) DI CARD","DI : 16","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052134","16) AI CARD","AI : 16","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052135","17) DO CARD","DO : 16","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052136","18) AO CARD","AO : 16","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052137","3. 현장기자재","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052138","통신중계장치",""," EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052139","GATEWAY",""," EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052140","FVR",""," EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052141","배관 온도 감지기",""," EA",24,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052142","덕트 온도 감지기",""," EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052143","실내 온도 감지기",""," EA",22,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052144","덕트 온도 & 습도 감지기",""," EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052145","실내 온도 & 습도 감지기",""," EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052146","옥외 온도 & 습도 감지기",""," EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052147","비례 댐퍼 구동기",""," EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052148","ON-OFF 댐퍼 구동기",""," EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052149","4. 설치기자재","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052150","정수위 조절 밸브","80A"," EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052151","차압 조절 밸브","80A"," EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052152","차압 조절 밸브","150A"," EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052153","차압 유량 조절 밸브","80A"," EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052154","차압 유량 조절 밸브","150A"," EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052155","차압독립형 바란씽&유량조절밸브","10A"," EA",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052156","차압독립형 바란씽&유량조절밸브","15A"," EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052157","차압독립형 바란씽&유량조절밸브","20A"," EA",13,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052158","차압독립형 바란씽&유량조절밸브","25A"," EA",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052159","차압독립형 바란씽&유량조절밸브","32A"," EA",14,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052160","차압독립형 바란씽&유량조절밸브","40A"," EA",9,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052161","차압독립형 바란씽&유량조절밸브","50A"," EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052162","차압독립형 바란씽&유량조절밸브","65A"," EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052163","차압독립형 바란씽&유량조절밸브","80A"," EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052164","차압독립형 바란씽&유량조절밸브","100A"," EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052165","차압독립형 바란씽&유량조절밸브","125A"," EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052166","차압독립형 바란씽&유량조절밸브","125A HF"," EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052167","버터플라이밸브","150A"," EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052168","버터플라이밸브","200A"," EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052169","전자변(물용)","25A"," EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052170","전자변(물용)","40A"," EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052171","이온화 연감지기",""," EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052172","필터용 차압 스위치",""," EA",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052173","액체유동스위치",""," EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052174","수위 지시 조절기","(부표식,센서1)"," EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052175","수위 지시 조절기","(부표식,센서2)"," EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052176","수위조절기","(오뚜기식,4P)"," EA",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052177","CO DETECTOR",""," EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052178","CO2 DETECTOR",""," EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052179","백엽상",""," SET",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052180","필드판넬","FP-1"," SET",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052181","UPS","3KVA"," EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052182","배관","16C"," M",5297,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052183","배관","22C"," M",1008,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052184","배관","28C"," M",569,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052185","배관","36C"," M",1011,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052186","후렉시블 튜브","16C"," M",220,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052187","후렉시블 튜브","22C"," M",79,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052188","후렉시블 콘넥터","16C"," EA",400,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052189","후렉시블 콘넥터","22C"," EA",144,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052190","전선","HIFX 2.5"," M",14551,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052191","전선","F-CV 4.0/3C"," M",426,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052192","케이블","TJV 1.0/2C"," M",5978,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052193","케이블","TJV 1.0/3C"," M",6252,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052194","케이블","RS-485 2P"," M",1871,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052195","케이블","CPEV 0.65/5P"," M",424,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052196","케이블","F-CVVS 1.5/2C"," M",110,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052197","헹가로드","3/8\""," EA",2007,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052198","앙카볼트","3/8\""," EA",2007,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052199","C-찬넬",""," EA",502,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052200","풀박스","150 x 150 x 100"," EA",19,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052201","풀박스","200 x 200 x100"," EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052202","풀박스","300 x 300 x200"," EA",22,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052203","풀박스","400 x 400 x300"," EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052204","풀박스","600 x 600 x300"," EA",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052205","사각박스","중 형"," EA",272,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052206","관 부 속","20%","L/S",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052207","잡자재비","2%","L/S",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","V1506052208","5. 인건비","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030210","56900017007","노무비","계장공","인",326,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["030210","56900017016","노무비","내선전공","인",1041,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["030210","56900017076","노무비","저압케이블전공","인",9,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["030210","56900017041","노무비","보통인부","인",17,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["030210","56900017111","노무비","통신관련기사","인",61,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["030210","56900017114","노무비","통신설비공","인",3,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["030210","56900017116","노무비","통신케이블공","인",229,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["030210","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},"",2326,null,1,0,0.03,{"$nulls":8},1]
["030210","Z3000000215","부가가치세","10%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":15}
[null,null,"[ 합           계 ]"]
[null,null,"030211  주방기구설치공사"]
["030211","V1504101003","발판소독기(노출형)","1200x600x20","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101004","저울받침대","700x750x200","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101005","전자저울 150KG","CAS:DB-1,150KG","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101006","검수대","1200x750x1800","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101007","작업대찬장","1200x750x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101008","육류분쇄기","FUJEE:MN - 22S","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101009","야채절단기","HALLDE:RG100","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101010","벽찬장","1200x350x500","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101011","울트라바이올렛멀티스틸레이져","HGS-B9002","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101012","울트라바이올렛나이프레이스틸레","HGS-834D","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101013","손세정대/센서식","HGS-S001","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101014","손소독기(센서식)","HGS-HC300","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101015","자동릴호스/역류방지혼합수전(냉","15M(NOZZLE SPRAY)","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101016","이동작업대","1200x750x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101017","이동건조대","1200x750x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101018","주방용다목적전처리가공작업대","1500x750x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101019","2-조세정대/하부선반","1500x750x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101020","작업대/하부선반","1500x750x850","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101021","냉동냉장고","SAMSUNG:CRFF-1141","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101022","조립형STS팬랙1500 3단","1500x600x1600","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101023","엘형운반차","900x600x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101024","조립식냉장실/에어커튼 / 롤인타","3300x2000x3000","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101025","냉동냉장실투시창 / 콤프레사 (","350x10x350","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101026","조립식폴리선반 910MM 3-TIRE","NERKO:910(3)","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101027","조립식폴리선반 1525MM 3-TIRE","NERKO:1525(3)","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101028","보존식냉동고","LASSELE:KF-603F","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101029","발판소독기(노출형)","900x600x20","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101030","작업대/찬장","1500x600x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101031","가스부침기","RINNAI:RSB903H","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101032","가스렌지3구자동점화","RINNAI:RSB-300F","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101033","가스낮은렌지자동점화","RINNAI:RLT-120","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101034","작업대/하부선반","600x750x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101035","콤비스티머 하부받침대 (10단)","1000x655x580","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101036","2/1 10.1GN 플렉시콤비매직파일","MKN:FKE101R_MP.10010259","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101037","2/1GN 쉬팬(530x500) 액세서리.(","AP MKN CGERP","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101038","플렉시콤비매직파일럿콤비스티머","SP MKN CGERP","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101039","가스자동취반기","RINNAI:RRA-150A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101040","가스회전식국솥 400인용스텐","RINNAI:RSK-400S(150LITER)","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101041","스텐레스월마감","1800x20x940","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101042","1-조세정작업대/하부선반","1500x750x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101043","수저식판자동배분대","520x700x1270","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101044","자율배식대 3500","WOOJIN:L3500","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101045","국보온운반차(전기식)","600x600x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101046","잔반처리대(2구형)","1500x750x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101047","잔반통(걸름망)","Ø490xx540","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101048","세척준비대/씽크","2050x750x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101049","컴펙트콘베어시스템","PRIME:PRC-600G","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101050","식기건조대","1500x750x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101051","랙보관선반 벽설치형","900x500x600","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101052","전기식기소독보관고(단면)","LASSELE:LHD-1633LG","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101053","이동세정대","1200x750x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101054","수저회수차","720x600x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101055","울트라바이올렛컵스틸레이져컵리","HGS-CR800","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101056","식수대 찬장","1200x700x500","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101058","배기후드(박스형)","2850x900x600","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101059","급.배기후드/휠타(박스형)","1800x1500x600","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101060","페콘필터","HOOD FECON FILTER","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101061","배기후드/휠타(박스형)","3170x1500x600","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101062","페콘필터","HOOD FECON FILTER","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101063","급.배기후드/휠타(박스형)","2600x1900x600","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101064","페콘필터","HOOD FECON FILTER","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101068","수전","","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101069","보조대/하부선반","300x710x450","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101070","작업대/찬장","1500x750x850","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","V1504101071","운반설치비","","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030211","Z3000000213","부가가치세","10%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":10}
[null,null,"[ 합           계 ]"]
[null,null,"030212  EHP설치공사"]
["030212","V1506051001","실외기(표준형)","14.5/16.3","대",2,{"$nulls":8},"22713522",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051002","실외기(표준형)","16.0/18.0","대",1,{"$nulls":8},"22713521",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051003","실외기(1등급)","23.0/26.5","대",1,{"$nulls":8},"22713563",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051004","실외기(1등급)","29.0/32.6","대",1,{"$nulls":8},"22713562",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051005","실외기(1등급)","46.4/52.2","대",1,{"$nulls":8},"22713559",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051006","실외기(1등급)","81.2/91.7","대",1,{"$nulls":8},"22713553",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051007","실내기(1-WAY)","69.6/0","대",1,{"$nulls":8},"22687574",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051008","실내기(1-WAY)","2.3/2.6","대",1,{"$nulls":8},"22718764",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051009","실내기(1-WAY)","5.2/6.0","대",5,{"$nulls":8},"22718767",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051010","실내기(2-WAY)","5.2/6","대",3,{"$nulls":8},"22718770",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051011","실내기(2-WAY)","6/6.8","대",1,{"$nulls":8},"22718771",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051012","실내기(4-WAY)","5.2/6","대",7,{"$nulls":8},"22718773",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051013","실내기(4-WAY)","6/6.8","대",4,{"$nulls":8},"22718774",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051014","실내기(4-WAY)","7.2/8.1","대",1,{"$nulls":8},"22718775",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051015","실내기(4-WAY)","8.3/9.3","대",2,{"$nulls":8},"22718776",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051016","실내기(4-WAY)","10/11","대",6,{"$nulls":8},"22718777",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051017","실내기(벽걸이형)","3.2/3.6","대",2,{"$nulls":8},"22718793",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051018","실내기(직립형)","29.0/32.6","대",2,{"$nulls":8},"22718796",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051019","싱글형실외기","4.0/5.0","대",3,{"$nulls":8},"22713518",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051020","싱글형실외기","6.0/7.2","대",2,{"$nulls":8},"22713516",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051021","싱글형실외기","6/7.2","대",1,{"$nulls":8},"22713514",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051022","싱글형실내기","4.0/5.0","대",3,{"$nulls":8},"22718813",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051023","싱글형실내기","6.0/7.2","대",2,{"$nulls":8},"22718815",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051024","싱글형실내기","6/7.2","대",1,{"$nulls":8},"22718817",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051025","스탠드형냉난방기","21.0/24.0","대",1,{"$nulls":8},"22425606",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051026","유선 룸컨트롤러","AWR-WE10N","대",36,{"$nulls":8},"22724061",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051027","무선 룸컨트롤러","AR-EH00","대",4,{"$nulls":8},"22724062",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051028","중앙컨트롤러","ACM-A202DN","대",3,{"$nulls":8},"22724063",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051029","중앙제어용 중계기","AIM-B13D","개",8,{"$nulls":8},"22724065",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051030","냉난방공조공사","AXJ-YA2512K이하","개",21,{"$nulls":8},"20469354",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051031","냉난방공조공사","AXJ-YA2812K이상","개",4,{"$nulls":8},"21590439",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051032","냉난방공조공사","AXJ-T3819K 외","개",2,{"$nulls":8},"20687670",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051033","DMS","AIM-D00AN","대",1,{"$nulls":8},"22724067",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051034","분배KIT2실","AXD-E24K200A","개",1,{"$nulls":8},"22724070",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051035","멀티&싱글1식","장비설치(냉매배관제외)","식",41,{"$nulls":8},"21567236",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051036","냉난방공조공사","12.7φ","m",960,{"$nulls":8},"10061680",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051037","냉난방공조공사","15.88φ","m",310,{"$nulls":8},"10061682",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051038","냉난방공조공사","20.0φ","m",224,{"$nulls":8},"10061684",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051039","냉난방공조공사","25.0φ","m",24,{"$nulls":8},"20373317",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051040","냉난방공조공사","28.581φ","m",69,{"$nulls":8},"20918014",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051041","냉난방공조공사","38.1φ","m",118,{"$nulls":8},"20918016",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051042","냉난방공조공사","룸설치전용선,커버제외","m",360,{"$nulls":8},"10061686",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051043","냉난방공조공사","중앙설치전용선,커버제외","m",572,{"$nulls":8},"10061688",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051044","냉난방공조공사","통신용케이블 및 CD관설치","m",834,{"$nulls":8},"22723642",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051045","냉난방공조공사","PVC드레인관설치","m",428,{"$nulls":8},"20373322",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051046","냉난방공조공사","MDF냉매배관커버설치","㎡",21,{"$nulls":8},"20373318",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051047","냉난방공조공사","함석냉매배관커버설치","㎡",48,{"$nulls":8},"20373320",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051048","냉난방공조공사","노출배관커버트레이","조",34,{"$nulls":8},"20912089",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051049","냉난방공조공사","50톤설치용 크레인","대",1,{"$nulls":8},"21624130",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051050","실외기받침대","싱글받침대 SI-LF145","대",9,{"$nulls":8},"22271362",{"$nulls":4},0,{"$nulls":8},1]
["030212","V1506051051","실외기받침대","평균990*830*130mm","조",8,{"$nulls":8},"20912098",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":25}
[null,null,"[ 합           계 ]"]
[null,null,"030213  환기유니트설치공사"]
["030213","V1504074001","공기순환장치","250CMH","대",4,{"$nulls":8},"22684772",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074002","공기순환장치","350CMH","대",3,{"$nulls":8},"22684773",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074003","공기순환장치","500CMH","대",3,{"$nulls":8},"22684774",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074004","공기순환장치","800CMH","대",4,{"$nulls":8},"22684775",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074005","공기순환장치","1,000CMH","대",7,{"$nulls":8},"22684776",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074006","룸 컨트롤세트 및 설치","AWR-VH01","개",21,{"$nulls":8},"20770464",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074007","냉난방기","AIM-B13B-E","개",2,{"$nulls":8},"20918684",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074008","중앙컨트롤세트 및 설치","ACM-A202(중계기필수16실)","개",2,{"$nulls":8},"20770465",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074010","공기순환장치설치","덕트평균,150Ø흡배기,2구[2X2]","식",7,{"$nulls":8},"20770454",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074011","공기순환장치설치","덕트평균,200Ø흡배기,3구[3X3]","식",3,{"$nulls":8},"20770455",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074012","공기순환장치설치","덕트평균,250Ø흡배기,4구[4X4]","식",11,{"$nulls":8},"20770456",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074013","전선 및 전선관[커버없음]","룸컨트롤러설치용전선","M",264,{"$nulls":8},"20770467",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074014","전선 및 전선관[커버없음]","중앙컨트롤러설치용전선","M",352,{"$nulls":8},"20770466",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074015","스파이럴덕트 1M당","평균,200Ø","M",396,{"$nulls":8},"20770457",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074016","플렉시블덕트 1M당","평균,200Ø","M",264,{"$nulls":8},"20770458",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074017","덕트보온단열 1㎡당","평균,200Ø","㎡",396,{"$nulls":8},"20770459",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074018","디퓨져","평균,200Ø","개",146,{"$nulls":8},"20770460",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074019","엘보[ELBO]","평균,200Ø","개",146,{"$nulls":8},"20770461",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074020","Branch","평균,200Ø","개",52,{"$nulls":8},"20770462",{"$nulls":4},0,{"$nulls":8},1]
["030213","V1504074021","Reducing-Branch","평균,200ØX150ØX200Ø","개",56,{"$nulls":8},"20770463",{"$nulls":4},0,{"$nulls":8},1]
[]
[]
[]
[]
[null,null,"[ 합           계 ]"]
[null,null,"030214  지열시스템설비공사"]
["030214","V1506060002","1. 주요 장비비","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060003","지열히트펌프","YTTG-600N(난방 60℃ 인증제품)","대",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060004","지열원순환펌프","720LPM, 5.5kW","대",7,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060005","밀폐형팽창탱크","1500","대",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060006","지열HEADER","@300A x 3,500L","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060026","2. 지열 배관공사 - SUS 관","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060027","스테인리스관","200","m",43,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060028","스테인리스관","125","m",163,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060029","스테인리스관","100","m",179,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060030","스테인리스관","50","m",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060031","스테인리스 엘보","200","ea",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060032","스테인리스 엘보","125","ea",40,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060033","스테인리스 엘보","100","ea",50,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060034","스테인리스 엘보","50","ea",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060035","스테인리스 티이","200","ea",13,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060036","스테인리스 티이","100","ea",14,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060037","스테인리스 레듀셔","200","ea",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060038","스테인리스 레듀셔","100","ea",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060039","절연 슈","200","ea",9,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060040","절연 슈","125","ea",33,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060041","절연 슈","100","ea",36,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060042","절연 슈","50","ea",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060043","버터플라이밸브","200","ea",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060044","버터플라이밸브","125","ea",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060045","버터플라이밸브","100","ea",21,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060046","석션디퓨져","100","ea",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060047","체크밸브","100","ea",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060048","후렉시블 조인트","100","ea",22,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060049","스트레이너","100","ea",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060050","스테인리스 합후렌지","200","ea",4,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060051","스테인리스 합후렌지","125","ea",16,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060052","스테인리스 합후렌지","100","ea",114,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060053","스테인리스 합후렌지","50","ea",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060054","볼밸브 (10K)","50","ea",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060055","볼밸브 (10K)","20","ea",11,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060056","자동공기변","15","ea",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060057","압력계","0~35kgf/cm2","ea",34,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060058","온도계","L 형","ea",22,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060059","스테인리스 강관용접","200","개소",80,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060060","스테인리스 강관용접","125","개소",113,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060061","스테인리스 강관용접","100","개소",210,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060062","스테인리스 강관용접","50","개소",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060063","스테인리스 강관용접","20","개소",67,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060064","관보온(고무발포)","200","m",43,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060065","관보온(고무발포)","125","m",163,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060066","관보온(고무발포)","100","m",179,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060067","관보온(고무발포)","50","m",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060068","밸브보온(고무발포)","200","개소",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060069","밸브보온(고무발포)","125","개소",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060070","밸브보온(고무발포)","100","개소",60,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060071","잡철물제작설치","간단","ton",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060072","부동액","에탄올","ℓ",8622,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060073","잡재료비","재료비의 3%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060074","공구손료","노무비의 3%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060078","3. 지열 배관공사 - PE 배관","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060079","PE Pipe","125","m",420,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060080","PE Pipe","100","m",380,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060081","PE Pipe","80","m",260,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060082","PE Pipe","65","m",284,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060083","PE Pipe","50","m",80,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060084","PE Pipe","40","m",240,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060085","PE 엘보","125","ea",18,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060086","PE 엘보","100","ea",22,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060087","PE 엘보","65","ea",14,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060088","PE 엘보","40","ea",186,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060089","PE 티이","125","ea",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060090","PE 이경티","100","ea",40,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060091","PE 이경티","80","ea",52,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060092","PE 이경티","65","ea",52,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060093","PE 이경티","50","ea",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060094","PE 레듀셔","125","ea",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060095","PE 레듀셔","100","ea",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060096","PE 레듀셔","80","ea",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060097","PE 레듀셔","65","ea",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060098","PE 레듀셔","50","ea",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060099","PE 융착","125","개소",124,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060100","PE 융착","100","개소",212,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060101","PE 융착","80","개소",180,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060102","PE 융착","65","개소",212,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060103","PE 융착","50","개소",90,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060104","PE 융착","40","개소",620,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060105","터파기","","㎥",1900,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060106","모래부설","","㎥",500,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060107","되메우기","","㎥",1450,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060108","잡재료비","재료비의 3%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060130","4. 지중열교환기공사","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060131","지중열교환기","200 m","공",108,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060156","5. 자동제어","","",0,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060157","COMPUTER","PENTIUM 코어2듀오","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060158","MONITOR","23\" LCD COLOR","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060159","DESK & CHAIR","사무용","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060160","CONVERTER","RS-422/RS-232C","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060161","HMI SOFTWARE","기본 512 TAG","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060162","0.6/1KV CVV-S CABLE","CVV-SB 1.5㎟*2C","M",300,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060163","가요전선관","16mm 방수형 후렉시블 튜브","M",200,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060168","PANEL CASE","800W*1200H*200D","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060169","NAME PLATE","MAIN, 속판, 외부 등","LOT",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060170","CPU","GM-CPUA","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060171","POWER","GM-PA2A","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060172","DIGITAL INPUT","G6I-D24A","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060173","DIGITAL OUTPUT","G6Q-RY2A","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060174","ANALOG INPUT","4--20MA/ 10.0 K오옴","EA",3,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060175","ANALOG OUTPUT","4--20MA/0--10VDC","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060176","BASE","GM6-BO6M","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060177","통신 MODULE","G6L-CUEA","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060178","터치스크린(프로그램포함)","7\" TFT LCD","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060179","POWER SUPPLY","AC220V/24V 5A","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060180","NOISE FILTER","250VAC 6A","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060181","NFB","ABS 32/10A","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060182","NFB","BKM-2P/6A","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060183","AUX RELAY","AC 24V SOCKET 포함","EA",15,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060184","CABLE","1.25SQ*200M","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060185","PVC DUCT","60*60 외","EA",8,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060186","FAN","AC220V 100mm","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060187","단자대","1P15A","EA",100,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060188","CONSENT","220V/15A  3구","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060189","TEMP. SENSOR","PT100Ω(WALL포함)","EA",10,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060190","플로우스위치","HFS-25","EA",5,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060191","전력량계","3상4선식/PULSE","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060192","유량계","4~20mA/PULSE","EA",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060193","제어용 케이블(차폐)","CVV-SB 1.5 x 2C","M",50,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060194","제어용 케이블","TJV 1.0 x 2C","M",224,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060195","제어용 케이블","HIV 2.5","M",186,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060196","전선관 Steel","16C","M",94,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060197","전선관 Steel","22C","M",52,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060198","전선관 Steel","28C","M",34,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060199","전선관 Steel","36C","M",18,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060200","전선관 부속","전선관의 20%","L/S",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060201","플렉시블 관","16c","M",50,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060202","플렉시블 연결관","16c","EA",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060203","노말 밴드","28C","EA",12,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060204","노말 밴드","36C","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060205","풀 박스","100 x 100 x 50","EA",14,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060206","풀 박스","150 x 150 x 100","EA",6,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060207","풀 박스","300 x 300 x 200","EA",2,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060208","행가","16C 외","EA",20,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060209","C-찬넬","1.2Tx1.2M","EA",15,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060210","앙카볼트","3/8\"","EA",30,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","V1506060211","잡자재비","주재료비의 5%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["030214","56900017007","노무비","계장공","인",15,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["030214","56900017016","노무비","내선전공","인",20,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["030214","56900017041","노무비","보통인부","인",8,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["030214","56900017076","노무비","저압케이블전공","인",6,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["030214","56900017111","노무비","통신관련기사","인",9,{"$nulls":8},"",{"$nulls":4},0,null,null,3,{"$nulls":5},1]
["030214","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},"",2671,null,1,0,0.03,{"$nulls":8},1]
["030214","Z2000000214","부가가치세","10%","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":8}
[null,null,"[ 합           계 ]"]
[null,null,"04  분담금공사"]
["04","Z2000000217","지역난방분담금","","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["04","Z2000000218","상수도분담금","","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
["04","Z2000000219","도시가스분담금","","식",1,{"$nulls":8},"",{"$nulls":4},0,{"$nulls":8},1]
{"$rows_empty":21}
[null,null,"[ 합           계 ]"]
["End Of File(Ver 6.0)"]
[null,null,"A,B행과 마지막열은 지우지 마시오"]

{"sheet":"소방집계","index":8,"n_rows":31,"n_cols":13,"rows_kept":31,"cut":false,"hidden":false,"merged":[[2,12,3,12],[0,0,0,12],[1,0,1,12],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,2,5],[2,6,2,7],[2,8,2,9],[2,10,2,11]]}
["집   계   표"]
["[공사명]  국토연구원 신청사 설계변경"]
["품          명","규       격","단위","수량","재  료  비",null,"노  무  비",null,"경    비",null,"합    계",null,"비고"]
[{"$nulls":4},"단가","금액","단가","금액","단가","금액","단가","금액"]
["01  소화설비공사",null,null,1]
["0101  소화장비설치공사",null,null,1]
["0102  옥외소화배관공사",null,null,1]
["0103  소화펌프실배관공사",null,null,1]
["0104  옥내소화배관공사",null,null,1]
["0105  스프링클러배관공사",null,null,1]
["0106  제연덕트설치공사",null,null,1]
["0107  동파방지열선설치공사",null,null,1]
["0108  소화가스설치공사",null,null,1]
["0109  주방소화설비공사",null,null,1]
["02  DOOR FAN TEST",null,null,1]
["03  제연 T.A.B",null,null,1]
{"$rows_empty":12}
["[ 합                  계 ]"]
["End Of File(Ver 6.0)"]
["마지막열은 지우지 마시오"]

{"sheet":"소방내역","index":9,"n_rows":629,"n_cols":15,"rows_kept":629,"cut":false,"hidden":false,"merged":[[1,12,1,13],[1,14,2,14],[0,2,0,14],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,1,7],[1,8,1,9],[1,10,1,11]]}
[null,null,"[공사명]  국토연구원 신청사 설계변경"]
["공종","코드","품          명","규       격","단위","수량","재  료  비",null,"노  무  비",null,"경    비",null,"합    계",null,"비고"]
[{"$nulls":6},"단가","금액","단가","금액","단가","금액","단가","금액"]
[null,null,"0101  소화장비설치공사"]
["0101","MM708392715","FP1SP주펌프(다단볼류트)","1,600LPM*75M*37KW","대",1,{"$nulls":8},""]
["0101","MM708392716","FP2SP예비펌프(다단볼류트)","1,600LPM*75M*37KW","대",1,{"$nulls":8},""]
["0101","MM708392717","FP3SP충압펌프(웨스코)","60LPM*75M*3.7KW","대",1,{"$nulls":8},""]
["0101","MM708392718","FP4H주펌프(다단볼류트)","650LPM*75M*15KW","대",1,{"$nulls":8},""]
["0101","MM708392719","FP5H예비펌프(다단볼류트)","650LPM*75M*15KW","대",1,{"$nulls":8},""]
["0101","MM708392720","FP6H충압펌프(웨스코)","60LPM*75M*3.7KW","대",1,{"$nulls":8},""]
["0101","MM708634023","FSF01급기휀(에어포일#4SS)","15,000CMH*95MMAQ*11.25KW","대",2,{"$nulls":8},""]
["0101","MM708392722","FEF01배기휀(시로코#2.5SS)","6,000CMH*55MMAQ*3.7KW","대",2,{"$nulls":8},""]
["0101","53401317004","진동방지장치","펌프(편흡입) 25㎜ 5HP 이하","조",2,{"$nulls":8},""]
["0101","53401317021","진동방지장치","펌프(편흡입) 25㎜ 20HP 이하","조",2,{"$nulls":8},""]
["0101","53401317041","진동방지장치","펌프(편흡입) 25㎜ 50HP 이하","조",2,{"$nulls":8},""]
["0101","56900017041","노무비","보통인부","인",9,{"$nulls":8},""]
["0101","56900017015","노무비","기계설비공","인",29,{"$nulls":8},""]
["0101","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},""]
{"$rows_empty":10}
[null,null,"[ 합           계 ]"]
[null,null,"0102  옥외소화배관공사"]
["0102","47103177520","수도용폴리에틸렌피복 강관","PEP관(KSD3565), D80","M",154,{"$nulls":8},""]
["0102","PPS00000001","잡재료비","관의 3%","식",1,{"$nulls":8},""]
["0102","47301127033","용접식 관이음쇠","흑엘보 (용접) D80","EA",3,{"$nulls":8},""]
["0102","47301127242","용접식 관이음쇠","흑티이 (용접) D80","EA",1,{"$nulls":8},""]
["0102","56940120080","강관용접","D80","개소",31]
["0102","56941440030","지상식소화전(쌍구)","100x65x65","개소",1]
["0102","56941521080","용접개소방식처리","D80","개소",31]
["0102","56941422020","녹막이페인트칠","2회","M2",1]
["0102","56941990010","기계터파기","","M3",177]
["0102","56941990020","기계되메우기","","M3",147.5]
["0102","56941990030","잔토처리","","M3",29.5]
["0102","56941990040","모래부설","","M3",29.5]
["0102","56900017041","노무비","보통인부","인",8,{"$nulls":8},""]
["0102","56900017030","노무비","배관공","인",17,{"$nulls":8},""]
["0102","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},""]
{"$rows_empty":9}
[null,null,"[ 합           계 ]"]
[null,null,"0103  소화펌프실배관공사"]
["0103","47100487002","배관용 탄소강관","백관 (SPP), D20, 반제품","M",6]
["0103","47100487003","배관용 탄소강관","백관 (SPP), D25, 반제품","M",6]
["0103","47100487006","배관용 탄소강관","백관 (SPP), D50, 반제품","M",20]
["0103","47100487047","배관용 탄소강관 (무용접)","백관 (SPP), D65, 반제품","M",3]
["0103","47100487048","배관용 탄소강관 (무용접)","백관 (SPP), D80, 반제품","M",3]
["0103","47100487049","배관용 탄소강관 (무용접)","백관 (SPP), D100, 반제품","M",19]
["0103","47100487051","배관용 탄소강관 (무용접)","백관 (SPP), D150, 반제품","M",37]
["0103","47100487052","배관용 탄소강관 (무용접)","백관 (SPP), D200, 반제품","M",23]
["0103","PPS00000001","잡재료비","관의 3%","식",1]
["0103","47304017003","나사식 강관제 관이음쇠","백엘보 (나사) D25","EA",8]
["0103","47304017006","나사식 강관제 관이음쇠","백엘보 (나사) D50","EA",14]
["0103","47304017106","나사식 강관제 관이음쇠","백티이 (나사) D50","EA",4]
["0103","47304017206","나사식 강관제 관이음쇠","백리듀서 (나사) D50","EA",4]
["0103","47304017302","나사식 강관제 관이음쇠","백니플 (나사) D20","EA",6]
["0103","47304017303","나사식 강관제 관이음쇠","백니플 (나사) D25","EA",8]
["0103","47304017402","나사식 강관제 관이음쇠","백유니온 (나사) D20","EA",6]
["0103","47304017403","나사식 강관제 관이음쇠","백유니온 (나사) D25","EA",8]
["0103","47305289401","무용접엘보","D65","EA",6]
["0103","47305289402","무용접엘보","D80","EA",6]
["0103","47305289403","무용접엘보","D100","EA",13]
["0103","47305289405","무용접엘보","D150","EA",20]
["0103","47305289406","무용접엘보","D200","EA",7]
["0103","47305289417","무용접티이","D100","EA",6]
["0103","47305289419","무용접티이","D150","EA",14]
["0103","47305289420","무용접티이","D200","EA",4]
["0103","47305289433","무용접레듀셔","D100","EA",4]
["0103","47305289435","무용접레듀셔","D150","EA",6]
["0103","47305289455","무용접캡","D150","EA",1]
["0103","47305289456","무용접캡","D200","EA",1]
["0103","47305289551","무용접후렌지아답타니플","D65","EA",12]
["0103","47305289552","무용접후렌지아답타니플","D80","EA",16]
["0103","47305289553","무용접후렌지아답타니플","D100","EA",26]
["0103","47305289554","무용접후렌지아답타니플","D125","EA",4]
["0103","47305289555","무용접후렌지아답타니플","D150","EA",34]
["0103","47305289556","무용접후렌지아답타니플","D200","EA",8]
["0103","47305289591","무용접고정식커플링","D65","EA",24]
["0103","47305289592","무용접고정식커플링","D80","EA",32]
["0103","47305289593","무용접고정식커플링","D100","EA",76]
["0103","47305289594","무용접고정식커플링","D125","EA",8]
["0103","47305289595","무용접고정식커플링","D150","EA",126]
["0103","47305289596","무용접고정식커플링","D200","EA",33]
["0103","56940330050","용접합후렌지","D40","개소",4]
["0103","56940330060","용접합후렌지","D50","개소",24]
["0103","48200428306","체크 밸브","스모렌스키,D50","EA",2]
["0103","47300627006","스트레이너","나사, 10kg, D50","EA",2]
["0103","47300627023","스트레이너","후랜지, 10kg, D100","EA",2]
["0103","47300627025","스트레이너","후랜지, 10kg, D150","EA",2]
["0103","47300627611","스트레이너","여과망, D150","EA",2]
["0103","47300627612","스트레이너","여과망, D200","EA",2]
["0103","47300857009","수격방지기","W.H.C D100","EA",2]
["0103","47300857011","수격방지기","W.H.C D150","EA",2]
["0103","56940740440","밸브보온 (함석마감)","50TxD100","개소",8]
["0103","56940740460","밸브보온 (함석마감)","50TxD150","개소",8]
["0103","42100557202","소방용 밸브","릴리프밸브(소방), D25","EA",4]
["0103","48200168033","게이트 밸브","OS&Y밸브, D65","EA",4]
["0103","48200168034","게이트 밸브","OS&Y밸브, D80","EA",4]
["0103","48200168050","게이트 밸브","OS&Y밸브(W/템퍼스위치) D50","EA",4]
["0103","48200168053","게이트 밸브","OS&Y밸브(W/템퍼스위치) D100","EA",4]
["0103","48200168055","게이트 밸브","OS&Y밸브(W/템퍼스위치) D150","EA",6]
["0103","48200168056","게이트 밸브","OS&Y밸브(W/템퍼스위치) D200","EA",2]
["0103","42101917023","소방유량계","순간유량계(후로셀) D65","EA",2]
["0103","42101917024","소방유량계","순간유량계(후로셀) D80","EA",2]
["0103","53060228338","U자형볼트/너트","비절연, D50","EA",3]
["0103","53060228341","U자형볼트/너트","비절연, D100","EA",3]
["0103","53060228343","U자형볼트/너트","비절연, D150","EA",8]
["0103","53060228344","U자형볼트/너트","비절연, D200","EA",6]
["0103","95200027091","ㄱ형강","등변, 65×65×6mm","KG",260]
["0103","56941340020","인서트플레이트","200x200x9T","개소",42]
["0103","56941420020","조합페인트칠","철재면2회","M2",8]
["0103","56941422020","녹막이페인트칠","2회","M2",8]
["0103","56941410010","잡철물제작설치","간단","TON",0.248]
["0103","80000011114","관보온(발포폴리에틸렌매직)","D50x25T","m",18]
["0103","80000011125","관보온(발포폴리에틸렌매직)","D100x40T","m",18]
["0103","80000011127","관보온(발포폴리에틸렌매직)","D150x40T","m",34]
["0103","80000011128","관보온(발포폴리에틸렌매직)","D200x40T","m",21]
["0103","80000011263","압력계(강관용)","D100*35KG/CM2","EA",6]
["0103","80000011179","청동게이트밸브 (10KG)","D20","EA",6]
["0103","80000011180","청동게이트밸브 (10KG)","D25","EA",4]
["0103","80000011203","주철체크밸브(충격완화용,10KG)","D100","EA",2]
["0103","80000011205","주철체크밸브(충격완화용,10KG)","D150","EA",2]
["0103","80000011243","벨로즈형후렉시블죠인트 (10KG)","D50","EA",4]
["0103","80000011246","벨로즈형후렉시블죠인트 (10KG)","D100","EA",4]
["0103","80000011248","벨로즈형후렉시블죠인트 (10KG)","D150","EA",4]
["0103","80000011907","슬리브 설치","D125mm～D150mm(벽)","개소",1]
["0103","80000011908","슬리브 설치","D200mm～D250mm(벽)","개소",1]
["0103","MM708566847","내화충진재","D150","EA",1]
["0103","MM708566848","내화충진재","D200","EA",1]
["0103","56900017041","노무비","보통인부","인",12]
["0103","56900017030","노무비","배관공","인",41]
["0103","PPS00000003","공구손료","노무비의 3%","식",1]
{"$rows_empty":12}
[null,null,"[ 합           계 ]"]
[null,null,"0104  옥내소화배관공사"]
["0104","47100487002","배관용 탄소강관","백관 (SPP), D20, 반제품","M",4]
["0104","47100487006","배관용 탄소강관","백관 (SPP), D50, 반제품","M",601]
["0104","47100487047","배관용 탄소강관 (무용접)","백관 (SPP), D65, 반제품","M",288]
["0104","47100487048","배관용 탄소강관 (무용접)","백관 (SPP), D80, 반제품","M",118]
["0104","47100487049","배관용 탄소강관 (무용접)","백관 (SPP), D100, 반제품","M",297]
["0104","PPS00000001","잡재료비","관의 3%","식",1]
["0104","47304017006","나사식 강관제 관이음쇠","백엘보 (나사) D50","EA",98]
["0104","47304017206","나사식 강관제 관이음쇠","백리듀서 (나사) D50","EA",33]
["0104","47304017506","나사식 강관제 관이음쇠","백소켓 (나사) D50","EA",54]
["0104","47304017302","나사식 강관제 관이음쇠","백니플 (나사) D20","EA",2]
["0104","47304017305","나사식 강관제 관이음쇠","백니플 (나사) D40","EA",43]
["0104","47304017402","나사식 강관제 관이음쇠","백유니온 (나사) D20","EA",2]
["0104","47305289401","무용접엘보","D65","EA",33]
["0104","47305289402","무용접엘보","D80","EA",9]
["0104","47305289403","무용접엘보","D100","EA",21]
["0104","47305289415","무용접티이","D65","EA",18]
["0104","47305289416","무용접티이","D80","EA",9]
["0104","47305289417","무용접티이","D100","EA",30]
["0104","47305289431","무용접레듀셔","D65","EA",8]
["0104","47305289432","무용접레듀셔","D80","EA",9]
["0104","47305289433","무용접레듀셔","D100","EA",11]
["0104","47305289553","무용접후렌지아답타니플","D100","EA",4]
["0104","47305289591","무용접고정식커플링","D65","EA",155]
["0104","47305289592","무용접고정식커플링","D80","EA",60]
["0104","47305289593","무용접고정식커플링","D100","EA",154]
["0104","47300857009","수격방지기","W.H.C D100","EA",2]
["0104","56941440040","소화전함(일반,ALL STS)","650x1200x180","개소",1]
["0104","56941440052","소화전함(일반,외함STS)","650x1200x180","개소",32]
["0104","56941440053","소화전함(단구,외함STS)","650x1200x180","개소",10]
["0104","56941450042","방수용기구함(외함STS)","1300x800x180 (호스4본)","개소",4]
["0104","42100357004","소화기","분말소화기(ABC) 3.3KG","EA",109]
["0104","42100357017","투척식소화기","4EA*1SET","SET",3]
["0104","42100357022","청정소화기","3.0KG","EA",17]
["0104","42101187003","소화기 받침대","소화기받침대 3.3KG","EA",109]
["0104","MM713493400","소공간자동소화장치(가스식)","15KG(1단)","EA",16]
["0104","MM713493401","소공간자동소화장치(가스식)","20KG(2단)","EA",12]
["0104","56940510060","일반행거(달대볼트)","D50","개소",148]
["0104","56940510070","일반행거(달대볼트)","D65","개소",74]
["0104","56940510080","일반행거(달대볼트)","D80","개소",34]
["0104","56940510090","일반행거(달대볼트)","D100","개소",25]
["0104","53060228341","U자형볼트/너트","비절연, D100","EA",45]
["0104","56940620090","강관스리브(지수판포함)","D100","개소",2]
["0104","80000011114","관보온(발포폴리에틸렌매직)","D50x25T","m",547]
["0104","80000011115","관보온(발포폴리에틸렌매직)","D65x25T","m",262]
["0104","80000011116","관보온(발포폴리에틸렌매직)","D80x25T","m",107]
["0104","80000011125","관보온(발포폴리에틸렌매직)","D100x40T","m",268]
["0104","80000011274","소화오토드립","D20mm","EA",1]
["0104","80000011275","연결송수구(쌍구,노출형)","D100x65x65","EA",1]
["0104","80000011301","완강기","3층용","EA",2]
["0104","80000011302","완강기","4층용","EA",2]
["0104","80000011303","완강기","5층용","EA",2]
["0104","80000011304","완강기","6층용","EA",2]
["0104","80000011305","완강기","7층용","EA",2]
["0104","80000011179","청동게이트밸브 (10KG)","D20","EA",2]
["0104","80000011203","주철체크밸브(충격완화용,10KG)","D100","EA",1]
["0104","80000011902","슬리브 설치","D65mm～D100mm(바닥)","개소",14]
["0104","80000011906","슬리브 설치","D65mm～D100mm(벽)","개소",15]
["0104","MM708567936","내화충진재","D65","EA",1]
["0104","MM708566850","내화충진재","D80","EA",4]
["0104","MM708566846","내화충진재","D100","EA",24]
["0104","56900017041","노무비","보통인부","인",61]
["0104","56900017030","노무비","배관공","인",155]
["0104","PPS00000003","공구손료","노무비의 3%","식",1]
{"$rows_empty":13}
[null,null,"[ 합           계 ]"]
[null,null,"0105  스프링클러배관공사"]
["0105","47100487002","배관용 탄소강관","백관 (SPP), D20, 반제품","M",4]
["0105","47100487003","배관용 탄소강관","백관 (SPP), D25, 반제품","M",6880]
["0105","47100487004","배관용 탄소강관","백관 (SPP), D32, 반제품","M",1339]
["0105","47100487005","배관용 탄소강관","백관 (SPP), D40, 반제품","M",1180]
["0105","47100487006","배관용 탄소강관","백관 (SPP), D50, 반제품","M",770]
["0105","47100487047","배관용 탄소강관 (무용접)","백관 (SPP), D65, 반제품","M",455]
["0105","47100487048","배관용 탄소강관 (무용접)","백관 (SPP), D80, 반제품","M",283]
["0105","47100487049","배관용 탄소강관 (무용접)","백관 (SPP), D100, 반제품","M",331]
["0105","47100487051","배관용 탄소강관 (무용접)","백관 (SPP), D150, 반제품","M",892]
["0105","PPS00000001","잡재료비","관의 3%","식",1]
["0105","47304017003","나사식 강관제 관이음쇠","백엘보 (나사) D25","EA",2460]
["0105","47304017004","나사식 강관제 관이음쇠","백엘보 (나사) D32","EA",51]
["0105","47304017005","나사식 강관제 관이음쇠","백엘보 (나사) D40","EA",46]
["0105","47304017006","나사식 강관제 관이음쇠","백엘보 (나사) D50","EA",79]
["0105","47304017103","나사식 강관제 관이음쇠","백티이 (나사) D25","EA",2141]
["0105","47304017104","나사식 강관제 관이음쇠","백티이 (나사) D32","EA",563]
["0105","47304017105","나사식 강관제 관이음쇠","백티이 (나사) D40","EA",542]
["0105","47304017106","나사식 강관제 관이음쇠","백티이 (나사) D50","EA",483]
["0105","47304017203","나사식 강관제 관이음쇠","백리듀서 (나사) D25","EA",1335]
["0105","47304017204","나사식 강관제 관이음쇠","백리듀서 (나사) D32","EA",574]
["0105","47304017205","나사식 강관제 관이음쇠","백리듀서 (나사) D40","EA",545]
["0105","47304017206","나사식 강관제 관이음쇠","백리듀서 (나사) D50","EA",591]
["0105","47304017803","나사식 강관제 관이음쇠","백캡 (나사) D25","EA",825]
["0105","47304017503","나사식 강관제 관이음쇠","백소켓 (나사) D25","EA",94]
["0105","47304017505","나사식 강관제 관이음쇠","백소켓 (나사) D40","EA",3]
["0105","47304017506","나사식 강관제 관이음쇠","백소켓 (나사) D50","EA",4]
["0105","47304017302","나사식 강관제 관이음쇠","백니플 (나사) D20","EA",2]
["0105","47304017303","나사식 강관제 관이음쇠","백니플 (나사) D25","EA",10]
["0105","47304017402","나사식 강관제 관이음쇠","백유니온 (나사) D20","EA",2]
["0105","47304017403","나사식 강관제 관이음쇠","백유니온 (나사) D25","EA",10]
["0105","47304017406","나사식 강관제 관이음쇠","백유니온 (나사) D50","EA",11]
["0105","47305289401","무용접엘보","D65","EA",13]
["0105","47305289402","무용접엘보","D80","EA",6]
["0105","47305289403","무용접엘보","D100","EA",7]
["0105","47305289405","무용접엘보","D150","EA",59]
["0105","47305289415","무용접티이","D65","EA",196]
["0105","47305289416","무용접티이","D80","EA",91]
["0105","47305289417","무용접티이","D100","EA",97]
["0105","47305289419","무용접티이","D150","EA",236]
["0105","47305289431","무용접레듀셔","D65","EA",55]
["0105","47305289432","무용접레듀셔","D80","EA",25]
["0105","47305289433","무용접레듀셔","D100","EA",19]
["0105","47305289435","무용접레듀셔","D150","EA",38]
["0105","47305289451","무용접캡","D65","EA",33]
["0105","47305289551","무용접후렌지아답타니플","D65","EA",4]
["0105","47305289553","무용접후렌지아답타니플","D100","EA",4]
["0105","47305289554","무용접후렌지아답타니플","D125","EA",2]
["0105","47305289555","무용접후렌지아답타니플","D150","EA",57]
["0105","47305289591","무용접고정식커플링","D65","EA",645]
["0105","47305289592","무용접고정식커플링","D80","EA",250]
["0105","47305289593","무용접고정식커플링","D100","EA",256]
["0105","47305289594","무용접고정식커플링","D125","EA",2]
["0105","47305289595","무용접고정식커플링","D150","EA",758]
["0105","47300857007","수격방지기","W.H.C D65","EA",4]
["0105","47300857010","수격방지기","W.H.C D125","EA",2]
["0105","47300857011","수격방지기","W.H.C D150","EA",11]
["0105","42100557005","소방용 밸브","프리액션밸브, D150","EA",1]
["0105","42100557106","소방용 밸브","알람밸브, D150","EA",10]
["0105","42100557551","사이트그라스","D25","EA",10]
["0105","48200168053","게이트 밸브","OS&Y밸브(W/템퍼스위치) D100","EA",1]
["0105","48200168055","게이트 밸브","OS&Y밸브(W/템퍼스위치) D150","EA",12]
["0105","42100207012","소방용헤드(FLUSH-TY)","스프링클러헤드,(하)72℃","EA",2080]
["0105","42100207013","소방용헤드(FLUSH-TY)","스프링클러헤드,(하)105℃","EA",22]
["0105","42100207014","소방용헤드(GLASS BULB)","스프링클러헤드,(상)68℃","EA",200]
["0105","42100207016","소방용헤드(GLASS BULB)","스프링클러헤드,(하)68℃","EA",132]
["0105","42100207032","소방용헤드(조기반응형,FLUSH)","스프링클러헤드,72℃","EA",43]
["0105","42101647074","후렉시블조인트(소방용)","1.5M","SET",2145]
["0105","54300047247","드라이펜던트(플러쉬형)","290mmm 72도","EA",15]
["0105","MM711507261","드라이펜던트(측벽식)","72℃","EA",2]
["0105","42101207017","차폐판","","EA",123]
["0105","56940510030","일반행거(달대볼트)","D25","개소",2423]
["0105","56940510040","일반행거(달대볼트)","D32","개소",603]
["0105","56940510050","일반행거(달대볼트)","D40","개소",511]
["0105","56940510060","일반행거(달대볼트)","D50","개소",183]
["0105","56940510070","일반행거(달대볼트)","D65","개소",3]
["0105","56940510090","일반행거(달대볼트)","D100","개소",8]
["0105","53060228339","U자형볼트/너트","비절연, D65","EA",121]
["0105","53060228340","U자형볼트/너트","비절연, D80","EA",82]
["0105","53060228341","U자형볼트/너트","비절연, D100","EA",82]
["0105","53060228343","U자형볼트/너트","비절연, D150","EA",238]
["0105","56940620090","강관스리브(지수판포함)","D100","개소",1]
["0105","95200027091","ㄱ형강","등변, 65×65×6mm","KG",6528]
["0105","56941340020","인서트플레이트","200x200x9T","개소",1052]
["0105","56941420020","조합페인트칠","철재면2회","M2",398]
["0105","56941422020","녹막이페인트칠","2회","M2",210]
["0105","56941410010","잡철물제작설치","간단","TON",6.2069999999999999]
["0105","80000011111","관보온(발포폴리에틸렌매직)","D25x25T","m",5578]
["0105","80000011112","관보온(발포폴리에틸렌매직)","D32x25T","m",1078]
["0105","80000011113","관보온(발포폴리에틸렌매직)","D40x25T","m",957]
["0105","80000011114","관보온(발포폴리에틸렌매직)","D50x25T","m",621]
["0105","80000011115","관보온(발포폴리에틸렌매직)","D65x25T","m",315]
["0105","80000011116","관보온(발포폴리에틸렌매직)","D80x25T","m",234]
["0105","80000011125","관보온(발포폴리에틸렌매직)","D100x40T","m",284]
["0105","80000011127","관보온(발포폴리에틸렌매직)","D150x40T","m",744]
["0105","80000011263","압력계(강관용)","D100*35KG/CM2","EA",10]
["0105","80000011273","소화앵글밸브","D40mm","EA",35]
["0105","80000011274","소화오토드립","D20mm","EA",1]
["0105","80000011275","연결송수구(쌍구,노출형)","D100x65x65","EA",2]
["0105","80000011277","스프링클러헤드(폐쇄,상하향형)","79℃이하","EA",986]
["0105","80000011179","청동게이트밸브 (10KG)","D20","EA",2]
["0105","80000011203","주철체크밸브(충격완화용,10KG)","D100","EA",1]
["0105","80000011192","황동볼밸브 (10KG)","D25","EA",10]
["0105","80000011902","슬리브 설치","D65mm～D100mm(바닥)","개소",11]
["0105","80000011903","슬리브 설치","D125mm～D150mm(바닥)","개소",11]
["0105","80000011905","슬리브 설치","D25mm～D50mm(벽)","개소",11]
["0105","80000011907","슬리브 설치","D125mm～D150mm(벽)","개소",15]
["0105","MM708566849","내화충진재","D25","EA",11]
["0105","MM708567936","내화충진재","D65","EA",11]
["0105","MM708566847","내화충진재","D150","EA",26]
["0105","56900017041","노무비","보통인부","인",621]
["0105","56900017030","노무비","배관공","인",1503]
["0105","PPS00000003","공구손료","노무비의 3%","식",1]
{"$rows_empty":16}
[null,null,"[ 합           계 ]"]
[null,null,"0106  제연덕트설치공사"]
["0106","56941311010","각형덕트제작설치(기계)","(0.5T)","M2",92]
["0106","56941311030","각형덕트제작설치(기계)","(0.8T)","M2",837]
["0106","56940790110","각형덕트보온(은박지)","25THK","M2",929]
["0106","56941314010","캔버스제작설치","1.2T","M2",4]
["0106","36940227015","FD/FVD 휴즈","","EA",4]
["0106","36940227001","점검구","200x200","EA",18]
["0106","36940227016","담파모타","","EA",14]
["0106","53300527234","동망","#24","M2",1]
["0106","42101647023","동관","D6","M",140]
["0106","56942000033","차압조절댐퍼설치","","M2당",6]
["0106","MM709750733","F.D (STL)","1000 x 600","EA",1]
["0106","MM709054856","F.D (STL)","800 x 400","EA",3]
["0106","MM708565171","GRILLE (STL)","800 x 300","EA",14]
["0106","MM708565172","M.F.D (STL)","800 x 300","EA",14]
["0106","MM711582589","T.V (STL)","1000 x 600","EA",1]
["0106","MM708565173","V.D (STL)","800 x 400","EA",2]
["0106","MM708565184","자동차압조절담파(W/그릴)","800*600","SET",14]
["0106","MM708565185","차압측정공","","개",14]
["0106","56900017041","노무비","보통인부","인",1]
["0106","56900017030","노무비","배관공","인",3]
["0106","56900017019","노무비","덕트공","인",26]
["0106","PPS00000003","공구손료","노무비의 3%","식",1]
[]
[]
[null,null,"[ 합           계 ]"]
[null,null,"0107  동파방지열선설치공사"]
["0107","S1130000001","관로삽입형 HEATING CABLE","SHE8-2TP","M",116,{"$nulls":8},""]
["0107","S1130000002","SELF-REGULATER HEATING CABLE","SRF16-2CR","M",15,{"$nulls":8},""]
["0107","S1130000003","열선(동파방지,센서부착형,외부","바이메탈 센서형","EA",7,{"$nulls":8},""]
["0107","S1130000004","밀페마감 (메커니컬티) KIT","JC-M(M)","SET",1,{"$nulls":8},""]
["0107","S1130000005","COUPLER","CP","EA",1,{"$nulls":8},""]
["0107","S1130000006","ENDING (메커니컬티) KIT","JC-ED","SET",3,{"$nulls":8},""]
["0107","S1130000007","EXCESS SENSOR","ES","EA",1,{"$nulls":8},""]
["0107","S1130000008","TRUE SENSOR","TS","EA",1,{"$nulls":8},""]
["0107","S1130000009","다회로 HEATER CONTROL","1CCT","LOT",1,{"$nulls":8},""]
["0107","S1130000010","전선","2.5SQ/3C","M",5,{"$nulls":8},""]
["0107","S1130000011","잡재료비","자재비의3%","식",1,{"$nulls":8},""]
["0107","S1130000012","전선관(STEEL PIPE)","16C","M",5,{"$nulls":8},""]
["0107","S1130000013","전선관 부품비","전선관의 20%","식",1,{"$nulls":8},""]
["0107","56900017127","노무비","플랜트전공","인",5,{"$nulls":8},""]
["0107","56900017016","노무비","내선전공","인",1,{"$nulls":8},""]
["0107","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},""]
{"$rows_empty":8}
[null,null,"[ 합           계 ]"]
[null,null,"0108  소화가스설치공사"]
["0108","S1400000001","1. 배관 및 부속자재비","","",{"$nulls":9},""]
["0108","S1400000002","백강관(KSD-3562 SCH#80)","40A","M",2,{"$nulls":8},""]
["0108","S1400000003","백강관(KSD-3562 SCH#80)","65A","M",3,{"$nulls":8},""]
["0108","S1400000004","백강관(KSD-3562 SCH#80)","80A","M",9,{"$nulls":8},""]
["0108","S1400000005","백강관(KSD-3562 SCH#40)","25A","M",19,{"$nulls":8},""]
["0108","S1400000006","백강관(KSD-3562 SCH#40)","32A","M",45,{"$nulls":8},""]
["0108","S1400000007","백강관(KSD-3562 SCH#40)","40A","M",177,{"$nulls":8},""]
["0108","S1400000008","백강관(KSD-3562 SCH#40)","50A","M",11,{"$nulls":8},""]
["0108","S1400000009","백강관(KSD-3562 SCH#40)","65A","M",199,{"$nulls":8},""]
["0108","S1400000010","백강관(KSD-3562 SCH#40)","80A","M",101,{"$nulls":8},""]
["0108","S1400000011","잡재료비","관의 3%","식",1,{"$nulls":8},""]
["0108","S1400000012","백용접엘보(SCH#80)","80A","EA",6,{"$nulls":8},""]
["0108","S1400000013","백용접티이(SCH#80)","80A","EA",5,{"$nulls":8},""]
["0108","S1400000014","백캡(SCH#80)","65A","EA",2,{"$nulls":8},""]
["0108","S1400000015","백캡(SCH#80)","80A","EA",1,{"$nulls":8},""]
["0108","S1400000016","백용접엘보(SCH#40)","25A","EA",20,{"$nulls":8},""]
["0108","S1400000017","백용접엘보(SCH#40)","32A","EA",40,{"$nulls":8},""]
["0108","S1400000018","백용접엘보(SCH#40)","40A","EA",64,{"$nulls":8},""]
["0108","S1400000019","백용접엘보(SCH#40)","65A","EA",38,{"$nulls":8},""]
["0108","S1400000020","백용접엘보(SCH#40)","80A","EA",14,{"$nulls":8},""]
["0108","S1400000021","백용접티이(SCH#40)","40A","EA",5,{"$nulls":8},""]
["0108","S1400000022","백용접티이(SCH#40)","50A","EA",8,{"$nulls":8},""]
["0108","S1400000023","백용접티이(SCH#40)","65A","EA",7,{"$nulls":8},""]
["0108","S1400000024","백용접티이(SCH#40)","80A","EA",2,{"$nulls":8},""]
["0108","S1400000025","백용접레듀샤(SCH#40)","40A","EA",10,{"$nulls":8},""]
["0108","S1400000026","백용접레듀샤(SCH#40)","50A","EA",10,{"$nulls":8},""]
["0108","S1400000027","백용접레듀샤(SCH#40)","65A","EA",14,{"$nulls":8},""]
["0108","S1400000028","백용접레듀샤(SCH#40)","80A","EA",3,{"$nulls":8},""]
["0108","S1400000029","3000파운드 하프커프링(암나사)","15A","EA",28,{"$nulls":8},""]
["0108","S1400000030","U-볼트&너트","25A","EA",7,{"$nulls":8},""]
["0108","S1400000031","U-볼트&너트","32A","EA",14,{"$nulls":8},""]
["0108","S1400000032","U-볼트&너트","40A","EA",54,{"$nulls":8},""]
["0108","S1400000033","U-볼트&너트","50A","EA",4,{"$nulls":8},""]
["0108","S1400000034","U-볼트&너트","65A","EA",60,{"$nulls":8},""]
["0108","S1400000035","U-볼트&너트","80A","EA",30,{"$nulls":8},""]
["0108","S1400000036","앵글","65*65*6T","Kg",2086,{"$nulls":8},""]
["0108","S1400000037","잡철물제작설치","간단","TON",2.0859999999999999,{"$nulls":8},""]
["0108","S1400000038","인서트플레이트 개소","200*200*9t","EA",334,{"$nulls":8},""]
["0108","S1400000039","셋트 앙카","3/8\"*70L","EA",1335,{"$nulls":8},""]
["0108","S1400000040","녹막이페인트","2회","㎡",354,{"$nulls":8},""]
["0108","S1400000041","조합페인트","철재면2회","㎡",105,{"$nulls":8},""]
["0108","S1400000042","2. IG-541 SYSTEM 주자재비","","",0,{"$nulls":8},""]
["0108","S1400000043","HERO IG-541 Cylinder / 300BAR","17.37m³/84LIT","B/T",28,{"$nulls":8},""]
["0108","S1400000044","Cylinder Valve","Rotarex","EA",28,{"$nulls":8},""]
["0108","S1400000045","WIKA Pressure Gauge","360bar","EA",28,{"$nulls":8},""]
["0108","S1400000046","Lever Relese Actuator","M42","EA",8,{"$nulls":8},""]
["0108","S1400000047","Actuator","M42","EA",20,{"$nulls":8},""]
["0108","S1400000048","Check & Pressure Reducing Flex","15A","EA",28,{"$nulls":8},""]
["0108","S1400000049","Actuator Adapter","6.35A","EA",56,{"$nulls":8},""]
["0108","S1400000050","Manifold Safety Relief (SPRING","20A","EA",1,{"$nulls":8},""]
["0108","S1400000051","Pressure Reducing Orifice","40A","EA",3,{"$nulls":8},""]
["0108","S1400000052","Pressure Reducing Orifice","65A","EA",4,{"$nulls":8},""]
["0108","S1400000053","Pressure Reducing Orifice","80A","EA",1,{"$nulls":8},""]
["0108","S1400000054","Selector Valve (W/Flange)","40A","EA",3,{"$nulls":8},""]
["0108","S1400000055","Selector Valve (W/Flange)","65A","EA",4,{"$nulls":8},""]
["0108","S1400000056","Selector Valve (W/Flange)","80A","EA",1,{"$nulls":8},""]
["0108","S1400000057","Actuating Device","1L*0.65KG,steel","SET",8,{"$nulls":8},""]
["0108","S1400000058","Pilot Line Relief Valve","6.35A","EA",8,{"$nulls":8},""]
["0108","S1400000059","Pilot Line Check Valve (BRASS)","6.35A*200bar","EA",16,{"$nulls":8},""]
["0108","S1400000060","Discharge Nozzle (W/Orifice)","25A","EA",9,{"$nulls":8},""]
["0108","S1400000061","Discharge Nozzle (W/Orifice)","32A","EA",12,{"$nulls":8},""]
["0108","S1400000062","Discharge Nozzle (W/Orifice)","40A","EA",6,{"$nulls":8},""]
["0108","S1400000063","Over Pressurisation Vent","600*500","EA",4,{"$nulls":8},""]
["0108","S1400000064","Over Pressurisation Vent","500*500","EA",1,{"$nulls":8},""]
["0108","S1400000065","Over Pressurisation Vent","500*400","EA",1,{"$nulls":8},""]
["0108","S1400000066","Over Pressurisation Vent","400*300","EA",2,{"$nulls":8},""]
["0108","S1400000067","Over Pressurisation Vent","300*300","EA",1,{"$nulls":8},""]
["0108","S1400000068","Operation Name Plate","Acril","EA",1,{"$nulls":8},""]
["0108","S1400000069","Zone Name Plate","Acril","EA",8,{"$nulls":8},""]
["0108","S1400000070","Cylinder Flame (조립식,무용접)","1병당","SET",28,{"$nulls":8},""]
["0108","S1400000071","KFI 제품(설계)심사비","8zone * 2회","EA",16,{"$nulls":8},""]
["0108","S1400000072","Copper Tube","0.8T*6.35A","m",240,{"$nulls":8},""]
["0108","S1400000073","Copper Tee & Nut","6.35A","EA",24,{"$nulls":8},""]
["0108","S1400000074","3. 노무비","","",0,{"$nulls":8},""]
["0108","56900017030","노무비","배관공","인",35,{"$nulls":8},""]
["0108","56900017021","노무비","도장공","인",16,{"$nulls":8},""]
["0108","56900017118","노무비","특별인부","인",51,{"$nulls":8},""]
["0108","56900017126","노무비","플랜트용접공","인",101,{"$nulls":8},""]
["0108","56900017125","노무비","플랜트배관공","인",51,{"$nulls":8},""]
["0108","PPS00000003","공구손료","노무비의 3%","식",1,{"$nulls":8},""]
{"$rows_empty":22}
[null,null,"[ 합           계 ]"]
[null,null,"0109  주방소화설비공사"]
["0109","S1400000100","3 Gallon Tank W/ ANSUL AUTOMAN","","EA",1,{"$nulls":8},""]
["0109","S1400000101","3 Gallon Tank w/single tank","","EA",1,{"$nulls":8},""]
["0109","S1400000102","ANSULEX Low pH Wet Chemical Ag","","EA",2,{"$nulls":8},""]
["0109","S1400000103","Adaptor, 3/8 in pipe compressi","","EA",5,{"$nulls":8},""]
["0109","S1400000104","Adaptor, Quik-Seal","","EA",5,{"$nulls":8},""]
["0109","S1400000105","Alarm initiating Switch , Spdt","","EA",1,{"$nulls":8},""]
["0109","S1400000106","Adaptor, ansul hood seal, 6/pa","","EA",1,{"$nulls":8},""]
["0109","S1400000107","Cartridge, Carbon dioxide,101-","","EA",1,{"$nulls":8},""]
["0109","S1400000108","Detector, Series (Scissor Link","","EA",5,{"$nulls":8},""]
["0109","S1400000109","Detector, Terminal (Scissor Li","","EA",1,{"$nulls":8},""]
["0109","S1400000110","Fusible Link, 360℉, (K Style)","","EA",6,{"$nulls":8},""]
["0109","S1400000111","Nozzle Swivel Adaptor","","EA",6,{"$nulls":8},""]
["0109","S1400000112","Nozzle 1N","","EA",2,{"$nulls":8},""]
["0109","S1400000113","Nozzle 245","","EA",6,{"$nulls":8},""]
["0109","S1400000114","Nozzle 2W","","EA",2,{"$nulls":8},""]
["0109","S1400000115","Pulley elbow, compression type","","EA",15,{"$nulls":8},""]
["0109","S1400000116","Hose/Grommet Package","","EA",2,{"$nulls":8},""]
["0109","S1400000117","Electric Switch (리미트 스위치","","EA",1,{"$nulls":8},""]
["0109","S1400000118","Cocking Lever with Lock Bar","","EA",1,{"$nulls":8},""]
["0109","S1400000119","CB메탈 Blow-Off Cap","","EA",10,{"$nulls":8},""]
["0109","S1400000120","Remote pull station, Aluminum(","","EA",1,{"$nulls":8},""]
["0109","S1400000121","Remote pull station, COVER","","EA",1,{"$nulls":8},""]
["0109","S1400000122","Wire rope , 50ft","","EA",1,{"$nulls":8},""]
["0109","S1400000123","SUS316 MALE CONNETTOR","1/2 * 3/8","EA",15,{"$nulls":8},""]
["0109","S1400000124","SUS316 UNION ELBOW","1/2","EA",25,{"$nulls":8},""]
["0109","S1400000125","SUS316 UNION TEE","1/2","EA",20,{"$nulls":8},""]
["0109","S1400000126","SUS316 UNION","1/2","EA",1,{"$nulls":8},""]
["0109","S1400000127","SUS316  GBU UNION(Seal)","","EA",15,{"$nulls":8},""]
["0109","S1400000128","316 SML'S TUBE (SUS316)","","EA",30,{"$nulls":8},""]
["0109","S1400000129","와이어관(SML'S 도금)","18MM","EA",20,{"$nulls":8},""]
["0109","S1400000130","와이어관 카프링","18MM","EA",5,{"$nulls":8},""]
["0109","S1400000131","와이어관 유니온","18MM","EA",5,{"$nulls":8},""]
["0109","S1400000132","와이어관 유니온 씰","18MM","EA",1,{"$nulls":8},""]
["0109","S1400000133","기타 배관 자재비","","식",1,{"$nulls":8},""]
["0109","S1400000134","8각 복스","54mm","EA",1,{"$nulls":8},""]
["0109","S1400000135","방수 후렉시블(GW)","16C","타",1,{"$nulls":8},""]
["0109","S1400000136","방수 후렉시블 콘넥터(GW)","16C","EA",5,{"$nulls":8},""]
["0109","S1400000137","강제전선관 아연도","16C","M",5,{"$nulls":8},""]
["0109","S1400000138","C찬넬","1.2T,25MM","EA",5,{"$nulls":8},""]
["0109","S1400000139","찬넬 클램프","16C","조",5,{"$nulls":8},""]
["0109","S1400000140","SUS피스","","봉",1,{"$nulls":8},""]
["0109","S1400000141","케이블타이","250mm","봉",1,{"$nulls":8},""]
["0109","S1400000142","전선","HIV-2.5SQ 적색","M",20,{"$nulls":8},""]
["0109","S1400000143","전선","HIV-2.5SQ 흑색","M",20,{"$nulls":8},""]
["0109","S1400000144","잡자재비","","식",1,{"$nulls":8},""]
["0109","S1400000145","ANSUL R-102 주방소화설비 설치","","식",1,{"$nulls":8},""]
["0109","S1400000146","공구손료","","식",1,{"$nulls":8},""]
[]
[]
[]
[null,null,"[ 합           계 ]"]
[null,null,"02  DOOR FAN TEST"]
["02","S1200000100","방호구역","","ZONE",4,{"$nulls":8},""]
{"$rows_empty":23}
[null,null,"[ 합           계 ]"]
[null,null,"03  제연 T.A.B"]
["03","S1300000100","A. 수평덕트 검토","","",{"$nulls":9},""]
["03","S1300000101","a. 부속실 가압","수평덕트당","개소",2,{"$nulls":8},""]
["03","S1300000102","b. 유입공기 배출","수평덕트당","개소",2,{"$nulls":8},""]
["03","S1300000103","B. 입상덕트 검토","","",0,{"$nulls":8},""]
["03","S1300000104","a. 부속실 가압","부속실당","개소",14,{"$nulls":8},""]
["03","S1300000105","b. 유입공기 배출","부속실당","개소",14,{"$nulls":8},""]
["03","S1300000106","2. 시운전 및 조정","","",0,{"$nulls":8},""]
["03","S1300000107","A. 예비점검","","",0,{"$nulls":8},""]
["03","S1300000108","a. 급기계통","부속실당","개소",14,{"$nulls":8},""]
["03","S1300000109","b. 유입공기 배출 계통","부속실당","개소",14,{"$nulls":8},""]
["03","S1300000110","B. 송풍계통 검사","","",0,{"$nulls":8},""]
["03","S1300000111","a. 급기계통","풍량검사 포함","개소",2,{"$nulls":8},""]
["03","S1300000112","b. 유입공기 배출 계통","배기그릴 풍량 측정","개소",2,{"$nulls":8},""]
["03","S1300000113","C. 시스템 조정","급기 계통 조정","개소",2,{"$nulls":8},""]
["03","S1300000114","D. 차압검사","부속실당","개소",14,{"$nulls":8},""]
["03","S1300000115","E. 비개방 차압검사","5개층당 1개소","개소",4,{"$nulls":8},""]
["03","S1300000116","F. 방연풍속 검사","20층 초과 2개소,이하 1개소","개소",2,{"$nulls":8},""]
["03","S1300000117","G. 방화문 개방력 시험","","개소",14,{"$nulls":8},""]
[]
[]
[]
[]
[]
[]
[null,null,"[ 합           계 ]"]
["End Of File(Ver 6.0)"]
[null,null,"A,B행과 마지막열은 지우지 마시오"]

{"sheet":"Sheet8","index":10,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}